(kicad_symbol_lib (version 20231120) (generator "partreel-bundle")
  (symbol "PLACEHOLDER" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0 8.89 0))
    (property "Value" "PartReel part" (at 0 -8.89 0))
    (symbol "PLACEHOLDER_0_1"
      (text "PartReel placeholder" (at 0 2.54 0))
      (text "Real symbol/footprint:" (at 0 0 0))
      (text "see 'PartReel' field URL" (at 0 -2.54 0))
    )
  )
  (symbol "jst_gh_10pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_10pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 10-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 10pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_10pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 12.70 0))
      (property "Value" "JST GH 10-pin (BM10B-GHS-TBT)" (at 3.54 -12.70 0))
      (symbol "jst_gh_10pin_1_1"
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
      )
    )
  (symbol "jst_gh_11pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_11pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 11-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 11pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_11pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 13.97 0))
      (property "Value" "JST GH 11-pin (BM11B-GHS-TBT)" (at 3.54 -13.97 0))
      (symbol "jst_gh_11pin_1_1"
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
      )
    )
  (symbol "jst_gh_12pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 12-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_12pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 15.24 0))
      (property "Value" "JST GH 12-pin (BM12B-GHS-TBT)" (at 3.54 -15.24 0))
      (symbol "jst_gh_12pin_1_1"
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
      )
    )
  (symbol "jst_gh_2pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_2pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 2-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 2pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_2pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 2.54 0))
      (property "Value" "JST GH 2-pin (BM02B-GHS-TBT)" (at 3.54 -2.54 0))
      (symbol "jst_gh_2pin_1_1"
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
      )
    )
  (symbol "jst_gh_3pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 3-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_3pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 3.81 0))
      (property "Value" "JST GH 3-pin (BM03B-GHS-TBT)" (at 3.54 -3.81 0))
      (symbol "jst_gh_3pin_1_1"
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
      )
    )
  (symbol "jst_gh_4pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 4-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_4pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 5.08 0))
      (property "Value" "JST GH 4-pin (BM04B-GHS-TBT)" (at 3.54 -5.08 0))
      (symbol "jst_gh_4pin_1_1"
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
      )
    )
  (symbol "jst_gh_5pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 5-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_5pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 6.35 0))
      (property "Value" "JST GH 5-pin (BM05B-GHS-TBT)" (at 3.54 -6.35 0))
      (symbol "jst_gh_5pin_1_1"
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
      )
    )
  (symbol "jst_gh_6pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 6-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_6pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 7.62 0))
      (property "Value" "JST GH 6-pin (BM06B-GHS-TBT)" (at 3.54 -7.62 0))
      (symbol "jst_gh_6pin_1_1"
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
      )
    )
  (symbol "jst_gh_7pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 7-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_7pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 8.89 0))
      (property "Value" "JST GH 7-pin (BM07B-GHS-TBT)" (at 3.54 -8.89 0))
      (symbol "jst_gh_7pin_1_1"
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
      )
    )
  (symbol "jst_gh_8pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 8-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_8pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 10.16 0))
      (property "Value" "JST GH 8-pin (BM08B-GHS-TBT)" (at 3.54 -10.16 0))
      (symbol "jst_gh_8pin_1_1"
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
      )
    )
  (symbol "jst_gh_9pin" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_gh_9pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST GH series 1.25mm pitch 9-pin SMD connector, vertical top entry. Common in drones/RC (Pixhawk) and compact signal links."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst gh 1.25mm connector smd 9pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_gh_9pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 11.43 0))
      (property "Value" "JST GH 9-pin (BM09B-GHS-TBT)" (at 3.54 -11.43 0))
      (symbol "jst_gh_9pin_1_1"
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
      )
    )
  (symbol "jst_ph_10pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_10pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 10-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 10pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_10pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 12.70 0))
      (property "Value" "JST PH 10-pin (B10B-PH-K-S)" (at 3.54 -12.70 0))
      (symbol "jst_ph_10pin_1_1"
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
      )
    )
  (symbol "jst_ph_11pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_11pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 11-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 11pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_11pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 13.97 0))
      (property "Value" "JST PH 11-pin (B11B-PH-K-S)" (at 3.54 -13.97 0))
      (symbol "jst_ph_11pin_1_1"
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
      )
    )
  (symbol "jst_ph_12pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 12-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_12pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 15.24 0))
      (property "Value" "JST PH 12-pin (B12B-PH-K-S)" (at 3.54 -15.24 0))
      (symbol "jst_ph_12pin_1_1"
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
      )
    )
  (symbol "jst_ph_13pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_13pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 13-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 13pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_13pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 16.51 0))
      (property "Value" "JST PH 13-pin (B13B-PH-K-S)" (at 3.54 -16.51 0))
      (symbol "jst_ph_13pin_1_1"
        (pin passive line (at -5.08 15.24 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -15.24 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
      )
    )
  (symbol "jst_ph_14pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_14pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 14-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 14pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_14pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 17.78 0))
      (property "Value" "JST PH 14-pin (B14B-PH-K-S)" (at 3.54 -17.78 0))
      (symbol "jst_ph_14pin_1_1"
        (pin passive line (at -5.08 16.51 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -16.51 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
      )
    )
  (symbol "jst_ph_15pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_15pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 15-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 15pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_15pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 19.05 0))
      (property "Value" "JST PH 15-pin (B15B-PH-K-S)" (at 3.54 -19.05 0))
      (symbol "jst_ph_15pin_1_1"
        (pin passive line (at -5.08 17.78 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 15.24 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -15.24 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
        (pin passive line (at -5.08 -17.78 0) (length 2.54)
          (name "Pin_15")
          (number "15"))
      )
    )
  (symbol "jst_ph_16pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_16pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 16-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 16pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_16pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 20.32 0))
      (property "Value" "JST PH 16-pin (B16B-PH-K-S)" (at 3.54 -20.32 0))
      (symbol "jst_ph_16pin_1_1"
        (pin passive line (at -5.08 19.05 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 16.51 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
        (pin passive line (at -5.08 -16.51 0) (length 2.54)
          (name "Pin_15")
          (number "15"))
        (pin passive line (at -5.08 -19.05 0) (length 2.54)
          (name "Pin_16")
          (number "16"))
      )
    )
  (symbol "jst_ph_2pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_2pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 2-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 2pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_2pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 2.54 0))
      (property "Value" "JST PH 2-pin (B2B-PH-K-S)" (at 3.54 -2.54 0))
      (symbol "jst_ph_2pin_1_1"
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
      )
    )
  (symbol "jst_ph_3pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 3-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_3pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 3.81 0))
      (property "Value" "JST PH 3-pin (B3B-PH-K-S)" (at 3.54 -3.81 0))
      (symbol "jst_ph_3pin_1_1"
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
      )
    )
  (symbol "jst_ph_4pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 4-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_4pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 5.08 0))
      (property "Value" "JST PH 4-pin (B4B-PH-K-S)" (at 3.54 -5.08 0))
      (symbol "jst_ph_4pin_1_1"
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
      )
    )
  (symbol "jst_ph_5pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 5-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_5pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 6.35 0))
      (property "Value" "JST PH 5-pin (B5B-PH-K-S)" (at 3.54 -6.35 0))
      (symbol "jst_ph_5pin_1_1"
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
      )
    )
  (symbol "jst_ph_6pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 6-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_6pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 7.62 0))
      (property "Value" "JST PH 6-pin (B6B-PH-K-S)" (at 3.54 -7.62 0))
      (symbol "jst_ph_6pin_1_1"
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
      )
    )
  (symbol "jst_ph_7pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 7-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_7pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 8.89 0))
      (property "Value" "JST PH 7-pin (B7B-PH-K-S)" (at 3.54 -8.89 0))
      (symbol "jst_ph_7pin_1_1"
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
      )
    )
  (symbol "jst_ph_8pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 8-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_8pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 10.16 0))
      (property "Value" "JST PH 8-pin (B8B-PH-K-S)" (at 3.54 -10.16 0))
      (symbol "jst_ph_8pin_1_1"
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
      )
    )
  (symbol "jst_ph_9pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_ph_9pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST PH series 2.0mm pitch 9-pin through-hole connector, vertical top entry. Common for LiPo battery and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst ph 2.0mm connector 9pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_ph_9pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 11.43 0))
      (property "Value" "JST PH 9-pin (B9B-PH-K-S)" (at 3.54 -11.43 0))
      (symbol "jst_ph_9pin_1_1"
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
      )
    )
  (symbol "jst_xh_10pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_10pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 10-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 10pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_10pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 12.70 0))
      (property "Value" "JST XH 10-pin (B10B-XH-A)" (at 3.54 -12.70 0))
      (symbol "jst_xh_10pin_1_1"
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
      )
    )
  (symbol "jst_xh_11pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_11pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 11-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 11pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_11pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 13.97 0))
      (property "Value" "JST XH 11-pin (B11B-XH-A)" (at 3.54 -13.97 0))
      (symbol "jst_xh_11pin_1_1"
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
      )
    )
  (symbol "jst_xh_12pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 12-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_12pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 15.24 0))
      (property "Value" "JST XH 12-pin (B12B-XH-A)" (at 3.54 -15.24 0))
      (symbol "jst_xh_12pin_1_1"
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
      )
    )
  (symbol "jst_xh_13pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_13pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 13-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 13pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_13pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 16.51 0))
      (property "Value" "JST XH 13-pin (B13B-XH-A)" (at 3.54 -16.51 0))
      (symbol "jst_xh_13pin_1_1"
        (pin passive line (at -5.08 15.24 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -15.24 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
      )
    )
  (symbol "jst_xh_14pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_14pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 14-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 14pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_14pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 17.78 0))
      (property "Value" "JST XH 14-pin (B14B-XH-A)" (at 3.54 -17.78 0))
      (symbol "jst_xh_14pin_1_1"
        (pin passive line (at -5.08 16.51 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -16.51 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
      )
    )
  (symbol "jst_xh_15pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_15pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 15-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 15pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_15pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 19.05 0))
      (property "Value" "JST XH 15-pin (B15B-XH-A)" (at 3.54 -19.05 0))
      (symbol "jst_xh_15pin_1_1"
        (pin passive line (at -5.08 17.78 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 15.24 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -15.24 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
        (pin passive line (at -5.08 -17.78 0) (length 2.54)
          (name "Pin_15")
          (number "15"))
      )
    )
  (symbol "jst_xh_16pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_16pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 16-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 16pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_16pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 20.32 0))
      (property "Value" "JST XH 16-pin (B16B-XH-A)" (at 3.54 -20.32 0))
      (symbol "jst_xh_16pin_1_1"
        (pin passive line (at -5.08 19.05 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 16.51 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
        (pin passive line (at -5.08 -16.51 0) (length 2.54)
          (name "Pin_15")
          (number "15"))
        (pin passive line (at -5.08 -19.05 0) (length 2.54)
          (name "Pin_16")
          (number "16"))
      )
    )
  (symbol "jst_xh_2pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_2pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 2-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 2pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_2pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 2.54 0))
      (property "Value" "JST XH 2-pin (B2B-XH-A)" (at 3.54 -2.54 0))
      (symbol "jst_xh_2pin_1_1"
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
      )
    )
  (symbol "jst_xh_3pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 3-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_3pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 3.81 0))
      (property "Value" "JST XH 3-pin (B3B-XH-A)" (at 3.54 -3.81 0))
      (symbol "jst_xh_3pin_1_1"
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
      )
    )
  (symbol "jst_xh_4pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 4-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_4pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 5.08 0))
      (property "Value" "JST XH 4-pin (B4B-XH-A)" (at 3.54 -5.08 0))
      (symbol "jst_xh_4pin_1_1"
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
      )
    )
  (symbol "jst_xh_5pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 5-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_5pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 6.35 0))
      (property "Value" "JST XH 5-pin (B5B-XH-A)" (at 3.54 -6.35 0))
      (symbol "jst_xh_5pin_1_1"
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
      )
    )
  (symbol "jst_xh_6pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 6-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_6pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 7.62 0))
      (property "Value" "JST XH 6-pin (B6B-XH-A)" (at 3.54 -7.62 0))
      (symbol "jst_xh_6pin_1_1"
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
      )
    )
  (symbol "jst_xh_7pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 7-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_7pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 8.89 0))
      (property "Value" "JST XH 7-pin (B7B-XH-A)" (at 3.54 -8.89 0))
      (symbol "jst_xh_7pin_1_1"
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
      )
    )
  (symbol "jst_xh_8pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 8-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_8pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 10.16 0))
      (property "Value" "JST XH 8-pin (B8B-XH-A)" (at 3.54 -10.16 0))
      (symbol "jst_xh_8pin_1_1"
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
      )
    )
  (symbol "jst_xh_9pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:jst_xh_9pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eXH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST XH series 2.5mm pitch 9-pin through-hole connector, vertical. Common for batteries, power and signal connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "jst xh 2.5mm connector 9pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/jst_xh_9pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 11.43 0))
      (property "Value" "JST XH 9-pin (B9B-XH-A)" (at 3.54 -11.43 0))
      (symbol "jst_xh_9pin_1_1"
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
      )
    )
  (symbol "pin_header_127_12pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_127_12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "1.27mm pitch 1x12 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 1.27mm connector 12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_127_12pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 15.24 0))
      (property "Value" "Pin Header 1.27mm 12-pin (PinHeader_1x12_P1.27mm)" (at 3.54 -15.24 0))
      (symbol "pin_header_127_12pin_1_1"
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
      )
    )
  (symbol "pin_header_127_8pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_127_8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "1.27mm pitch 1x8 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 1.27mm connector 8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_127_8pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 10.16 0))
      (property "Value" "Pin Header 1.27mm 8-pin (PinHeader_1x08_P1.27mm)" (at 3.54 -10.16 0))
      (symbol "pin_header_127_8pin_1_1"
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
      )
    )
  (symbol "pin_header_254_10pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_10pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x10 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 10pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_10pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 12.70 0))
      (property "Value" "Pin Header 2.54mm 10-pin (PinHeader_1x10_P2.54mm)" (at 3.54 -12.70 0))
      (symbol "pin_header_254_10pin_1_1"
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
      )
    )
  (symbol "pin_header_254_12pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x12 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 12pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_12pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 15.24 0))
      (property "Value" "Pin Header 2.54mm 12-pin (PinHeader_1x12_P2.54mm)" (at 3.54 -15.24 0))
      (symbol "pin_header_254_12pin_1_1"
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
      )
    )
  (symbol "pin_header_254_14pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_14pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x14 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 14pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_14pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 17.78 0))
      (property "Value" "Pin Header 2.54mm 14-pin (PinHeader_1x14_P2.54mm)" (at 3.54 -17.78 0))
      (symbol "pin_header_254_14pin_1_1"
        (pin passive line (at -5.08 16.51 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -16.51 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
      )
    )
  (symbol "pin_header_254_15pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_15pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x15 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 15pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_15pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 19.05 0))
      (property "Value" "Pin Header 2.54mm 15-pin (PinHeader_1x15_P2.54mm)" (at 3.54 -19.05 0))
      (symbol "pin_header_254_15pin_1_1"
        (pin passive line (at -5.08 17.78 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 15.24 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -15.24 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
        (pin passive line (at -5.08 -17.78 0) (length 2.54)
          (name "Pin_15")
          (number "15"))
      )
    )
  (symbol "pin_header_254_20pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_20pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x20 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 20pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_20pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 25.40 0))
      (property "Value" "Pin Header 2.54mm 20-pin (PinHeader_1x20_P2.54mm)" (at 3.54 -25.40 0))
      (symbol "pin_header_254_20pin_1_1"
        (pin passive line (at -5.08 24.13 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 21.59 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 19.05 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 16.51 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 13.97 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 11.43 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
        (pin passive line (at -5.08 -11.43 0) (length 2.54)
          (name "Pin_15")
          (number "15"))
        (pin passive line (at -5.08 -13.97 0) (length 2.54)
          (name "Pin_16")
          (number "16"))
        (pin passive line (at -5.08 -16.51 0) (length 2.54)
          (name "Pin_17")
          (number "17"))
        (pin passive line (at -5.08 -19.05 0) (length 2.54)
          (name "Pin_18")
          (number "18"))
        (pin passive line (at -5.08 -21.59 0) (length 2.54)
          (name "Pin_19")
          (number "19"))
        (pin passive line (at -5.08 -24.13 0) (length 2.54)
          (name "Pin_20")
          (number "20"))
      )
    )
  (symbol "pin_header_254_39pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_39pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x39 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 39pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_39pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 49.53 0))
      (property "Value" "Pin Header 2.54mm 39-pin (PinHeader_1x39_P2.54mm)" (at 3.54 -49.53 0))
      (symbol "pin_header_254_39pin_1_1"
        (pin passive line (at -5.08 48.26 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 45.72 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 43.18 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 40.64 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 38.10 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 35.56 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 33.02 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 30.48 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 27.94 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at -5.08 25.40 0) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at -5.08 22.86 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at -5.08 20.32 0) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at -5.08 17.78 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at -5.08 15.24 0) (length 2.54)
          (name "Pin_14")
          (number "14"))
        (pin passive line (at -5.08 12.70 0) (length 2.54)
          (name "Pin_15")
          (number "15"))
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_16")
          (number "16"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_17")
          (number "17"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_18")
          (number "18"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_19")
          (number "19"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_20")
          (number "20"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_21")
          (number "21"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_22")
          (number "22"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_23")
          (number "23"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_24")
          (number "24"))
        (pin passive line (at -5.08 -12.70 0) (length 2.54)
          (name "Pin_25")
          (number "25"))
        (pin passive line (at -5.08 -15.24 0) (length 2.54)
          (name "Pin_26")
          (number "26"))
        (pin passive line (at -5.08 -17.78 0) (length 2.54)
          (name "Pin_27")
          (number "27"))
        (pin passive line (at -5.08 -20.32 0) (length 2.54)
          (name "Pin_28")
          (number "28"))
        (pin passive line (at -5.08 -22.86 0) (length 2.54)
          (name "Pin_29")
          (number "29"))
        (pin passive line (at -5.08 -25.40 0) (length 2.54)
          (name "Pin_30")
          (number "30"))
        (pin passive line (at -5.08 -27.94 0) (length 2.54)
          (name "Pin_31")
          (number "31"))
        (pin passive line (at -5.08 -30.48 0) (length 2.54)
          (name "Pin_32")
          (number "32"))
        (pin passive line (at -5.08 -33.02 0) (length 2.54)
          (name "Pin_33")
          (number "33"))
        (pin passive line (at -5.08 -35.56 0) (length 2.54)
          (name "Pin_34")
          (number "34"))
        (pin passive line (at -5.08 -38.10 0) (length 2.54)
          (name "Pin_35")
          (number "35"))
        (pin passive line (at -5.08 -40.64 0) (length 2.54)
          (name "Pin_36")
          (number "36"))
        (pin passive line (at -5.08 -43.18 0) (length 2.54)
          (name "Pin_37")
          (number "37"))
        (pin passive line (at -5.08 -45.72 0) (length 2.54)
          (name "Pin_38")
          (number "38"))
        (pin passive line (at -5.08 -48.26 0) (length 2.54)
          (name "Pin_39")
          (number "39"))
      )
    )
  (symbol "pin_header_254_3pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x3 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_3pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 3.81 0))
      (property "Value" "Pin Header 2.54mm 3-pin (PinHeader_1x03_P2.54mm)" (at 3.54 -3.81 0))
      (symbol "pin_header_254_3pin_1_1"
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
      )
    )
  (symbol "pin_header_254_4pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x4 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_4pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 5.08 0))
      (property "Value" "Pin Header 2.54mm 4-pin (PinHeader_1x04_P2.54mm)" (at 3.54 -5.08 0))
      (symbol "pin_header_254_4pin_1_1"
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
      )
    )
  (symbol "pin_header_254_5pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x5 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_5pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 6.35 0))
      (property "Value" "Pin Header 2.54mm 5-pin (PinHeader_1x05_P2.54mm)" (at 3.54 -6.35 0))
      (symbol "pin_header_254_5pin_1_1"
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
      )
    )
  (symbol "pin_header_254_6pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x6 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_6pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 7.62 0))
      (property "Value" "Pin Header 2.54mm 6-pin (PinHeader_1x06_P2.54mm)" (at 3.54 -7.62 0))
      (symbol "pin_header_254_6pin_1_1"
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
      )
    )
  (symbol "pin_header_254_7pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x7 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_7pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 8.89 0))
      (property "Value" "Pin Header 2.54mm 7-pin (PinHeader_1x07_P2.54mm)" (at 3.54 -8.89 0))
      (symbol "pin_header_254_7pin_1_1"
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
      )
    )
  (symbol "pin_header_254_8pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x8 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_8pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 10.16 0))
      (property "Value" "Pin Header 2.54mm 8-pin (PinHeader_1x08_P2.54mm)" (at 3.54 -10.16 0))
      (symbol "pin_header_254_8pin_1_1"
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
      )
    )
  (symbol "pin_header_254_9pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:pin_header_254_9pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://en.wikipedia.org/wiki/Pin_header"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.54mm pitch 1x9 male pin header, THT vertical. Dimensions match the official KiCad Connector_PinHeader library."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "pin header 2.54mm connector 9pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/pin_header_254_9pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 11.43 0))
      (property "Value" "Pin Header 2.54mm 9-pin (PinHeader_1x09_P2.54mm)" (at 3.54 -11.43 0))
      (symbol "pin_header_254_9pin_1_1"
        (pin passive line (at -5.08 10.16 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at -5.08 -10.16 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
      )
    )
  (symbol "screw_terminal_5_08_2pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:screw_terminal_5_08_2pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141810_Cixi-Kefa-Rongda-KF301-5-0-2P_C8465.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5.08mm pitch 2-pole screw terminal block (KF301-compatible), THT. For power and wire-to-board connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "screw terminal 5.08mm connector 2pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/screw_terminal_5_08_2pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 2.54 0))
      (property "Value" "Screw Terminal 5.08mm 2-pin (KF301-5.08-2P)" (at 3.54 -2.54 0))
      (symbol "screw_terminal_5_08_2pin_1_1"
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
      )
    )
  (symbol "screw_terminal_5_08_3pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:screw_terminal_5_08_3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141810_Cixi-Kefa-Rongda-KF301-5-0-2P_C8465.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5.08mm pitch 3-pole screw terminal block (KF301-compatible), THT. For power and wire-to-board connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "screw terminal 5.08mm connector 3pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/screw_terminal_5_08_3pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 3.81 0))
      (property "Value" "Screw Terminal 5.08mm 3-pin (KF301-5.08-3P)" (at 3.54 -3.81 0))
      (symbol "screw_terminal_5_08_3pin_1_1"
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
      )
    )
  (symbol "screw_terminal_5_08_4pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:screw_terminal_5_08_4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141810_Cixi-Kefa-Rongda-KF301-5-0-2P_C8465.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5.08mm pitch 4-pole screw terminal block (KF301-compatible), THT. For power and wire-to-board connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "screw terminal 5.08mm connector 4pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/screw_terminal_5_08_4pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 5.08 0))
      (property "Value" "Screw Terminal 5.08mm 4-pin (KF301-5.08-4P)" (at 3.54 -5.08 0))
      (symbol "screw_terminal_5_08_4pin_1_1"
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
      )
    )
  (symbol "screw_terminal_5_08_5pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:screw_terminal_5_08_5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141810_Cixi-Kefa-Rongda-KF301-5-0-2P_C8465.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5.08mm pitch 5-pole screw terminal block (KF301-compatible), THT. For power and wire-to-board connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "screw terminal 5.08mm connector 5pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/screw_terminal_5_08_5pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 6.35 0))
      (property "Value" "Screw Terminal 5.08mm 5-pin (KF301-5.08-5P)" (at 3.54 -6.35 0))
      (symbol "screw_terminal_5_08_5pin_1_1"
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
      )
    )
  (symbol "screw_terminal_5_08_6pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:screw_terminal_5_08_6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141810_Cixi-Kefa-Rongda-KF301-5-0-2P_C8465.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5.08mm pitch 6-pole screw terminal block (KF301-compatible), THT. For power and wire-to-board connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "screw terminal 5.08mm connector 6pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/screw_terminal_5_08_6pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 7.62 0))
      (property "Value" "Screw Terminal 5.08mm 6-pin (KF301-5.08-6P)" (at 3.54 -7.62 0))
      (symbol "screw_terminal_5_08_6pin_1_1"
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
      )
    )
  (symbol "screw_terminal_5_08_7pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:screw_terminal_5_08_7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141810_Cixi-Kefa-Rongda-KF301-5-0-2P_C8465.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5.08mm pitch 7-pole screw terminal block (KF301-compatible), THT. For power and wire-to-board connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "screw terminal 5.08mm connector 7pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/screw_terminal_5_08_7pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 8.89 0))
      (property "Value" "Screw Terminal 5.08mm 7-pin (KF301-5.08-7P)" (at 3.54 -8.89 0))
      (symbol "screw_terminal_5_08_7pin_1_1"
        (pin passive line (at -5.08 7.62 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -7.62 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
      )
    )
  (symbol "screw_terminal_5_08_8pin" (pin_names hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:screw_terminal_5_08_8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141810_Cixi-Kefa-Rongda-KF301-5-0-2P_C8465.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5.08mm pitch 8-pole screw terminal block (KF301-compatible), THT. For power and wire-to-board connections."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "screw terminal 5.08mm connector 8pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/screw_terminal_5_08_8pin/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 10.16 0))
      (property "Value" "Screw Terminal 5.08mm 8-pin (KF301-5.08-8P)" (at 3.54 -10.16 0))
      (symbol "screw_terminal_5_08_8pin_1_1"
        (pin passive line (at -5.08 8.89 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 6.35 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at -5.08 -6.35 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at -5.08 -8.89 0) (length 2.54)
          (name "Pin_8")
          (number "8"))
      )
    )
  (symbol "sparkfun_audio_jack_trrs_3_5mm_smd"
        (property "Footprint" "PartReel:sparkfun_audio_jack_trrs_3_5mm_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/datasheets/Prototyping/20153.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Audio Jack, 4 Poles (TRRS)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun audio jack receptacle stereo headphones TRRS connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_audio_jack_trrs_3_5mm_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 8.89 0)
    		)
    		(property "Value" "Audio_Jack_TRRS_3.5mm_SMD (SparkFun)"
    			(at 0 6.35 0)
    		)
    		(property "PROD_ID" "CONN-10676"
    			(at 0 -16.51 0)
    		)
    		(property "ki_fp_filters" "Jack*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_audio_jack_trrs_3_5mm_smd_0_1")
    		(symbol "sparkfun_audio_jack_trrs_3_5mm_smd_1_1"
    			(pin passive line
    				(at 5.08 2.54 180)
    				(length 2.54)
    				(name "~")
    				(number "S")
    			)
    			(pin passive line
    				(at 5.08 0 180)
    				(length 2.54)
    				(name "~")
    				(number "R2")
    			)
    			(pin passive line
    				(at 5.08 -2.54 180)
    				(length 2.54)
    				(name "~")
    				(number "R1")
    			)
    			(pin passive line
    				(at 5.08 -5.08 180)
    				(length 2.54)
    				(name "~")
    				(number "T")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_barrel_jack_pth"
        (property "Footprint" "PartReel:sparkfun_barrel_jack_pth"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "DC Barrel Jack with an internal switch."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun DC power barrel jack connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_barrel_jack_pth/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.334 0)
    		)
    		(property "Value" "Barrel_Jack_PTH (SparkFun)"
    			(at 0 -5.08 0)
    		)
    		(property "PROD_ID" "CONN-08197"
    			(at 0 -7.62 0)
    		)
    		(property "ki_fp_filters" "BarrelJack*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_barrel_jack_pth_0_1")
    		(symbol "sparkfun_barrel_jack_pth_1_1"
    			(pin passive line
    				(at 7.62 2.54 180)
    				(length 2.54)
    				(name "PWR")
    				(number "1")
    			)
    			(pin passive line
    				(at 7.62 0 180)
    				(length 2.54)
    				(name "GNDBREAK")
    				(number "3")
    			)
    			(pin passive line
    				(at 7.62 -2.54 180)
    				(length 2.54)
    				(name "GND")
    				(number "2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_barrel_jack_pth_slot"
        (property "Footprint" "PartReel:sparkfun_barrel_jack_pth_slot"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.sparkfun.com/datasheets/Prototyping/Barrel-Connector-PJ-202A.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "DC Barrel Jack with an internal switch."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun DC power barrel jack connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_barrel_jack_pth_slot/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.334 0)
    		)
    		(property "Value" "Barrel_Jack_PTH_Slot (SparkFun)"
    			(at 0 -5.08 0)
    		)
    		(property "PROD_ID" "CONN-08197"
    			(at 0 -7.62 0)
    		)
    		(property "ki_fp_filters" "BarrelJack*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_barrel_jack_pth_slot_0_1")
    		(symbol "sparkfun_barrel_jack_pth_slot_1_1"
    			(pin passive line
    				(at 7.62 2.54 180)
    				(length 2.54)
    				(name "PWR")
    				(number "PWR")
    			)
    			(pin passive line
    				(at 7.62 0 180)
    				(length 2.54)
    				(name "GNDBREAK")
    				(number "GNDBREAK")
    			)
    			(pin passive line
    				(at 7.62 -2.54 180)
    				(length 2.54)
    				(name "GND")
    				(number "GND")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x02_jst_p2_0mm_horizontal_pth"
        (property "Footprint" "PartReel:sparkfun_conn_01x02_jst_p2_0mm_horizontal_pth"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2 Pin 2mm JST Connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x02_jst_p2_0mm_horizontal_pth/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.08 0)
    		)
    		(property "Value" "Conn_01x02_JST_P2.0mm_Horizontal_PTH (SparkFun)"
    			(at 0 -8.89 0)
    		)
    		(property "PROD_ID" "CONN-09863"
    			(at 0 -16.51 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x02_jst_p2_0mm_horizontal_pth_1_1"
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2 Pin 2mm JST Connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.08 0)
    		)
    		(property "Value" "Conn_01x02_JST_P2.0mm_Horizontal_SMD (SparkFun)"
    			(at 0 -8.89 0)
    		)
    		(property "PROD_ID" "CONN-11443"
    			(at 0 -16.51 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin no_connect line
    				(at 1.27 1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC2")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 1.27 -3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC1")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd_lipo"
        (property "Footprint" "PartReel:sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd_lipo"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd_lipo/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2 Pin 2mm JST Connector to match SparkFun LiPo batteries."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd_lipo/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.08 0)
    		)
    		(property "Value" "Conn_01x02_JST_P2.0mm_Horizontal_SMD_LiPo (SparkFun)"
    			(at 0 -8.89 0)
    		)
    		(property "PROD_ID" "CONN-11443"
    			(at 0 -16.51 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x02_jst_p2_0mm_horizontal_smd_lipo_1_1"
    			(text "+"
    				(at 0 0 0)
    			)
    			(text "-"
    				(at 0 -2.54 0)
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "+")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "-")
    				(number "1")
    			)
    			(pin no_connect line
    				(at 1.27 1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC2")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 1.27 -3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC1")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x03_jst_p1_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x03_jst_p1_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "3 Pin 2mm JST Connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x03_jst_p1_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 6.096 0)
    		)
    		(property "Value" "Conn_01x03_JST_P1.0mm_Horizontal_SMD (SparkFun)"
    			(at 0 -6.35 0)
    		)
    		(property "PROD_ID" "CONN-10492"
    			(at 0 -13.97 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x03_jst_p1_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "3")
    				(number "3")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x03_jst_p1_0mm_vertical_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x03_jst_p1_0mm_vertical_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.4uconnector.com/online/object/4udrawing/07265.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "3 Pin 1mm JST Connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x03_jst_p1_0mm_vertical_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 6.096 0)
    		)
    		(property "Value" "Conn_01x03_JST_P1.0mm_Vertical_SMD (SparkFun)"
    			(at 0 -6.35 0)
    		)
    		(property "PROD_ID" "CONN-24642"
    			(at 0 -13.97 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x03_jst_p1_0mm_vertical_smd_1_1"
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "3")
    				(number "3")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x03_jst_p1_25mm_locking_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x03_jst_p1_25mm_locking_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Locking 3 pin JST 1.25mm connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x03_jst_p1_25mm_locking_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 6.35 0)
    		)
    		(property "Value" "Conn_01x03_JST_P1.25mm_Locking_Horizontal_SMD (SparkFun)"
    			(at 0 -6.35 0)
    		)
    		(property "PROD_ID" "CONN-16521"
    			(at 0 -11.43 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x03_jst_p1_25mm_locking_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin no_connect line
    				(at 3.81 -5.08 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 6.35 -5.08 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x04_jst_p1_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x04_jst_p1_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Single row 4 pin connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector 4 pin 1mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x04_jst_p1_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 6.096 0)
    		)
    		(property "Value" "Conn_01x04_JST_P1.0mm_Horizontal_SMD (SparkFun)"
    			(at -0.254 -9.144 0)
    		)
    		(property "SparkFun" "CONN-10310"
    			(at 0 -19.304 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x04_jst_p1_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "4")
    				(number "4")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x04_jst_p1_0mm_vertical_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x04_jst_p1_0mm_vertical_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_conn_01x04_jst_p1_0mm_vertical_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "4 pin JST 1mm polarized connector for I2C."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x04_jst_p1_0mm_vertical_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.08 0)
    		)
    		(property "Value" "Conn_01x04_JST_P1.0mm_Vertical_SMD (SparkFun)"
    			(at 0 -7.62 0)
    		)
    		(property "PROD_ID" "CONN-14483"
    			(at 0 -17.78 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x04_jst_p1_0mm_vertical_smd_1_1"
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x04_jst_p1_25mm_locking_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x04_jst_p1_25mm_locking_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Locking 4 pin JST SMD connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x04_jst_p1_25mm_locking_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.08 0)
    		)
    		(property "Value" "Conn_01x04_JST_P1.25mm_Locking_Horizontal_SMD (SparkFun)"
    			(at 0 -7.62 0)
    		)
    		(property "PROD_ID" "CONN-15303"
    			(at 0 -12.7 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x04_jst_p1_25mm_locking_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin no_connect line
    				(at 3.81 -6.35 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 6.35 -6.35 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x05_jst_p1_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x05_jst_p1_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Right angle SMD polarized connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector 5 pin 1mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x05_jst_p1_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 8.636 0)
    		)
    		(property "Value" "Conn_01x05_JST_P1.0mm_Horizontal_SMD (SparkFun)"
    			(at -0.254 -9.144 0)
    		)
    		(property "PROD_ID" "CONN-20121"
    			(at 0 -19.304 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x05_jst_p1_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "5")
    				(number "5")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x05_jst_p1_25mm_locking_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x05_jst_p1_25mm_locking_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Locking 5-pin JST 1.25mm connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x05_jst_p1_25mm_locking_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 7.62 0)
    		)
    		(property "Value" "Conn_01x05_JST_P1.25mm_Locking_Horizontal_SMD (SparkFun)"
    			(at 0 -7.62 0)
    		)
    		(property "PROD_ID" "CONN-25024"
    			(at 0 -17.78 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x05_jst_p1_25mm_locking_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin no_connect line
    				(at 3.81 -6.35 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 6.35 -6.35 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x05_p2_0mm_socket_vertical_pth"
        (property "Footprint" "PartReel:sparkfun_conn_01x05_p2_0mm_socket_vertical_pth"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.mouser.com/datasheet/2/837/bf085-1994323.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5 pos 2mm pitch 4.4mm tall female header."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun 5 pin 2mm Connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x05_p2_0mm_socket_vertical_pth/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 7.62 0)
    		)
    		(property "Value" "Conn_01x05_P2.0mm_Socket_Vertical_PTH (SparkFun)"
    			(at 0 -7.62 0)
    		)
    		(property "PROD_ID" "CONN-09000"
    			(at 0 -17.78 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x05_p2_0mm_socket_vertical_pth_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x05_p2_0mm_socket_vertical_smd_pin1rightup"
        (property "Footprint" "PartReel:sparkfun_conn_01x05_p2_0mm_socket_vertical_smd_pin1rightup"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://drawings-pdf.s3.amazonaws.com/10489.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "5 pos 2mm pitch 4.4mm tall female SMD header."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun 5 pin 2mm SMD Connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x05_p2_0mm_socket_vertical_smd_pin1rightup/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 7.62 0)
    		)
    		(property "Value" "Conn_01x05_P2.0mm_Socket_Vertical_SMD_Pin1RightUp (SparkFun)"
    			(at 0 -7.62 0)
    		)
    		(property "PROD_ID" "CONN-09344"
    			(at 0 -17.78 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x05_p2_0mm_socket_vertical_smd_pin1rightup_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x06_jst_p1_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x06_jst_p1_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Right angle SMD polarized connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector 6 pin 1mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x06_jst_p1_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 8.636 0)
    		)
    		(property "Value" "Conn_01x06_JST_P1.0mm_Horizontal_SMD (SparkFun)"
    			(at -0.254 -11.684 0)
    		)
    		(property "PROD_ID" "CONN-09659"
    			(at 0 -21.844 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x06_jst_p1_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "6")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x06_jst_p1_0mm_vertical_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x06_jst_p1_0mm_vertical_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Conn_01x06_JST_P1.0mm_Vertical_SMD."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x06_jst_p1_0mm_vertical_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 7.62 0)
    		)
    		(property "Value" "Conn_01x06_JST_P1.0mm_Vertical_SMD (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "CONN-08249"
    			(at -1.27 -15.24 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x06_jst_p1_0mm_vertical_smd_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x06_jst_p1_25mm_locking_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x06_jst_p1_25mm_locking_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST locking connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x06_jst_p1_25mm_locking_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 7.62 0)
    		)
    		(property "Value" "Conn_01x06_JST_P1.25mm_Locking_Horizontal_SMD (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "CONN-16497"
    			(at 0 -20.32 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x06_jst_p1_25mm_locking_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin no_connect line
    				(at 3.81 -8.89 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 6.35 -8.89 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_combined"
        (property "Footprint" "PartReel:sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_combined"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://gct.co/files/drawings/bg125.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_combined/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 7.62 0)
    		)
    		(property "Value" "Conn_01x06_P2.54mm_Socket_Vertical_SMD_Combined (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "CONN-10203"
    			(at 0.254 -20.32 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_combined_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_pin1rightdown"
        (property "Footprint" "PartReel:sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_pin1rightdown"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://gct.co/files/drawings/bg125.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "6 pin female header, SMD."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_pin1rightdown/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 7.62 0)
    		)
    		(property "Value" "Conn_01x06_P2.54mm_Socket_Vertical_SMD_Pin1RightDown (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "CONN-10203"
    			(at 0.254 -20.066 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_pin1rightdown_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_pin1rightdown_passthru"
        (property "Footprint" "PartReel:sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_pin1rightdown_passthru"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://gct.co/files/drawings/bg125.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "6 pin SMD connector passthrough."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_pin1rightdown_passthru/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 7.62 0)
    		)
    		(property "Value" "Conn_01x06_P2.54mm_Socket_Vertical_SMD_Pin1RightDown_Passthru (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "CONN-10203"
    			(at 0.254 -20.066 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x06_p2_54mm_socket_vertical_smd_pin1rightdown_passthru_1_1"
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x07_jst_p1_25mm_locking_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x07_jst_p1_25mm_locking_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "7-pin 1.25mm locking JST connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x07_jst_p1_25mm_locking_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 10.16 0)
    		)
    		(property "Value" "Conn_01x07_JST_P1.25mm_Locking_Horizontal_SMD (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "CONN-25025"
    			(at 0 -20.32 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x07_jst_p1_25mm_locking_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin no_connect line
    				(at 3.81 -8.89 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 6.35 -8.89 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x07_p2_0mm_socket_vertical_pth"
        (property "Footprint" "PartReel:sparkfun_conn_01x07_p2_0mm_socket_vertical_pth"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.mouser.com/datasheet/2/837/bf085-1994323.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "7 pos 2mm pitch 4.4mm tall female."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x07_p2_0mm_socket_vertical_pth/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 10.16 0)
    		)
    		(property "Value" "Conn_01x07_P2.0mm_Socket_Vertical_PTH (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "CONN-09001"
    			(at 0 -12.7 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x07_p2_0mm_socket_vertical_pth_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x07_p2_0mm_socket_vertical_smd_pin1rightup"
        (property "Footprint" "PartReel:sparkfun_conn_01x07_p2_0mm_socket_vertical_smd_pin1rightup"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://drawings-pdf.s3.amazonaws.com/10489.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "7 pos 2mm pitch 4.4mm tall female SMD header."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x07_p2_0mm_socket_vertical_smd_pin1rightup/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 10.16 0)
    		)
    		(property "Value" "Conn_01x07_P2.0mm_Socket_Vertical_SMD_Pin1RightUp (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "CONN-09345"
    			(at 0 -12.7 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x07_p2_0mm_socket_vertical_smd_pin1rightup_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x08_fpc_p1_0mm_horizontal_dualcontact_lif"
        (property "Footprint" "PartReel:sparkfun_conn_01x08_fpc_p1_0mm_horizontal_dualcontact_lif"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/10149903.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Dual contact LIF FPC connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x08_fpc_p1_0mm_horizontal_dualcontact_lif/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 10.16 0)
    		)
    		(property "Value" "Conn_01x08_FPC_P1.0mm_Horizontal_DualContact_LIF (SparkFun)"
    			(at 0 -12.7 0)
    		)
    		(property "PROD_ID" "CONN-..."
    			(at 0.254 -22.606 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x08_fpc_p1_0mm_horizontal_dualcontact_lif_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin no_connect line
    				(at 2.54 1.27 0)
    				(length 3.81)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 2.54 -1.27 0)
    				(length 3.81)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x08_jst_p1_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x08_jst_p1_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Right angle SMD polarized connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector 8 pin 1mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x08_jst_p1_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 11.176 0)
    		)
    		(property "Value" "Conn_01x08_JST_P1.0mm_Horizontal_SMD (SparkFun)"
    			(at 0 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-08435"
    			(at 0.254 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x08_jst_p1_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "8")
    				(number "8")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x08_jst_p1_25mm_locking_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x08_jst_p1_25mm_locking_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST locking connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x08_jst_p1_25mm_locking_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 10.16 0)
    		)
    		(property "Value" "Conn_01x08_JST_P1.25mm_Locking_Horizontal_SMD (SparkFun)"
    			(at 0 -12.7 0)
    		)
    		(property "PROD_ID" "CONN-25026"
    			(at 0 -22.86 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x08_jst_p1_25mm_locking_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin no_connect line
    				(at 3.81 -11.43 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 6.35 -11.43 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_combined"
        (property "Footprint" "PartReel:sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_combined"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_combined/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Conn_01x08_P2.54mm_Socket_Vertical_SMD_Combined."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_combined/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 10.16 0)
    		)
    		(property "Value" "Conn_01x08_P2.54mm_Socket_Vertical_SMD_Combined (SparkFun)"
    			(at 0 -12.7 0)
    		)
    		(property "PROD_ID" "CONN-10204"
    			(at 0.254 -22.606 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_combined_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown"
        (property "Footprint" "PartReel:sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://gct.co/files/drawings/bg125.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "8 pin SMD female header."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 10.16 0)
    		)
    		(property "Value" "Conn_01x08_P2.54mm_Socket_Vertical_SMD_Pin1RightDown (SparkFun)"
    			(at 0 -12.7 0)
    		)
    		(property "PROD_ID" "CONN-10204"
    			(at 0.254 -22.606 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown_passthru"
        (property "Footprint" "PartReel:sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown_passthru"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown_passthru/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "~."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown_passthru/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 10.16 0)
    		)
    		(property "Value" "Conn_01x08_P2.54mm_Socket_Vertical_SMD_Pin1RightDown_Passthru (SparkFun)"
    			(at 0 -12.7 0)
    		)
    		(property "PROD_ID" "CONN-10204"
    			(at 0 -22.86 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x08_p2_54mm_socket_vertical_smd_pin1rightdown_passthru_1_1"
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x09_jst_p1_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x09_jst_p1_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Right angle SMD polarized connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector 9 pin 1mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x09_jst_p1_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 13.716 0)
    		)
    		(property "Value" "Conn_01x09_JST_P1.0mm_Horizontal_SMD (SparkFun)"
    			(at 0 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-25141"
    			(at 0.254 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x09_jst_p1_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "9")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x09_jst_p1_25mm_locking_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x09_jst_p1_25mm_locking_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST locking connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x09_jst_p1_25mm_locking_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 12.7 0)
    		)
    		(property "Value" "Conn_01x09_JST_P1.25mm_Locking_Horizontal_SMD (SparkFun)"
    			(at 0 -12.7 0)
    		)
    		(property "PROD_ID" "CONN-25027"
    			(at 0 -22.86 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x09_jst_p1_25mm_locking_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin no_connect line
    				(at 3.81 -11.43 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 6.35 -11.43 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x10_fpc_p1_0mm_horizontal_dualcontact_lif"
        (property "Footprint" "PartReel:sparkfun_conn_01x10_fpc_p1_0mm_horizontal_dualcontact_lif"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/10149903.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "10 Pin LIF FPC connector dual contact."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x10_fpc_p1_0mm_horizontal_dualcontact_lif/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 12.7 0)
    		)
    		(property "Value" "Conn_01x10_FPC_P1.0mm_Horizontal_DualContact_LIF (SparkFun)"
    			(at 0 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-..."
    			(at 0 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x10_fpc_p1_0mm_horizontal_dualcontact_lif_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin no_connect line
    				(at 5.08 1.27 0)
    				(length 3.81)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 5.08 -1.27 0)
    				(length 3.81)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x10_jst_p1_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x10_jst_p1_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Conn_01x10_JST_P1.0mm_Horizontal_SMD."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector 10 pin 1mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x10_jst_p1_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_numbers
    			(hide yes)
    		)
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 13.716 0)
    		)
    		(property "Value" "Conn_01x10_JST_P1.0mm_Horizontal_SMD (SparkFun)"
    			(at 0 -17.78 0)
    		)
    		(property "PROD_ID" "CONN-25142"
    			(at 0.254 -27.94 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x10_jst_p1_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "10")
    				(number "10")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x10_jst_p1_25mm_locking_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x10_jst_p1_25mm_locking_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eGH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "JST locking connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x10_jst_p1_25mm_locking_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 12.7 0)
    		)
    		(property "Value" "Conn_01x10_JST_P1.25mm_Locking_Horizontal_SMD (SparkFun)"
    			(at 0 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-25028"
    			(at 0 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x10_jst_p1_25mm_locking_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin no_connect line
    				(at 3.81 -13.97 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at 6.35 -13.97 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_combined"
        (property "Footprint" "PartReel:sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_combined"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://gct.co/files/drawings/bg125.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "10 pin SMD female header."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_combined/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 12.7 0)
    		)
    		(property "Value" "Conn_01x10_P2.54mm_Socket_Vertical_SMD_Combined (SparkFun)"
    			(at 0 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-11219"
    			(at 0.254 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_combined_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_pin1rightdown"
        (property "Footprint" "PartReel:sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_pin1rightdown"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://gct.co/files/drawings/bg125.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "10 pin SMD female header."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_pin1rightdown/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 12.7 0)
    		)
    		(property "Value" "Conn_01x10_P2.54mm_Socket_Vertical_SMD_Pin1RightDown (SparkFun)"
    			(at 0 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-11219"
    			(at 0.254 -25.146 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_pin1rightdown_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_pin1rightdown_passthru"
        (property "Footprint" "PartReel:sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_pin1rightdown_passthru"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://gct.co/files/drawings/bg125.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "10 pin SMD female header."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_pin1rightdown_passthru/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 12.7 0)
    		)
    		(property "Value" "Conn_01x10_P2.54mm_Socket_Vertical_SMD_Pin1RightDown_Passthru (SparkFun)"
    			(at 0 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-11219"
    			(at 0.254 -25.146 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x10_p2_54mm_socket_vertical_smd_pin1rightdown_passthru_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x12_jst_p1_0mm_horizontal_smd"
        (property "Footprint" "PartReel:sparkfun_conn_01x12_jst_p1_0mm_horizontal_smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "SMD 12 pin friction fit JST connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x12_jst_p1_0mm_horizontal_smd/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 15.24 0)
    		)
    		(property "Value" "Conn_01x12_JST_P1.0mm_Horizontal_SMD (SparkFun)"
    			(at 0 -17.78 0)
    		)
    		(property "PROD_ID" "CONN-23694"
    			(at 0 -27.94 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x12_jst_p1_0mm_horizontal_smd_1_1"
    			(pin passive line
    				(at -5.08 12.7 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -5.08 -15.24 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x16_fpc_p0_5mm_horizontal_dualcontact"
        (property "Footprint" "PartReel:sparkfun_conn_01x16_fpc_p0_5mm_horizontal_dualcontact"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_conn_01x16_fpc_p0_5mm_horizontal_dualcontact/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Conn_01x16_FPC_P0.5mm_Horizontal_DualContact."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x16_fpc_p0_5mm_horizontal_dualcontact/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 20.32 0)
    		)
    		(property "Value" "Conn_01x16_FPC_P0.5mm_Horizontal_DualContact (SparkFun)"
    			(at 0 -22.86 0)
    		)
    		(property "PROD_ID" "CONN-16066"
    			(at 0 -27.94 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x16_fpc_p0_5mm_horizontal_dualcontact_1_1"
    			(pin passive line
    				(at -5.08 17.78 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 15.24 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 12.7 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at -5.08 -15.24 0)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at -5.08 -17.78 0)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at -5.08 -20.32 0)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin no_connect line
    				(at 8.89 -6.35 0)
    				(length 3.81)
    				(hide yes)
    				(name "MP1")
    				(number "MP1")
    			)
    			(pin no_connect line
    				(at 8.89 -8.89 0)
    				(length 3.81)
    				(hide yes)
    				(name "MP2")
    				(number "MP2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x20_smd_pin1rightup"
        (property "Footprint" "PartReel:sparkfun_conn_01x20_smd_pin1rightup"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2110100430_XKB-Connection-X6511WVS-20H-C60D48R2_C2883777.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "~."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x20_smd_pin1rightup/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 25.4 0)
    		)
    		(property "Value" "Conn_01x20_SMD_Pin1RightUp (SparkFun)"
    			(at 0 -27.94 0)
    		)
    		(property "PROD_ID" "CONN-25435"
    			(at 0 -38.1 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x20_smd_pin1rightup_1_1"
    			(pin passive line
    				(at -5.08 22.86 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 20.32 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 17.78 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 15.24 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 12.7 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at -5.08 -15.24 0)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at -5.08 -17.78 0)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at -5.08 -20.32 0)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at -5.08 -22.86 0)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    			(pin passive line
    				(at -5.08 -25.4 0)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x22_fpc_p0_5mm_vertical_lowercontact"
        (property "Footprint" "PartReel:sparkfun_conn_01x22_fpc_p0_5mm_vertical_lowercontact"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.cvilux.com/uploads/drawings/100/332/CF2081S.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Vertical FPC connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x22_fpc_p0_5mm_vertical_lowercontact/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 27.94 0)
    		)
    		(property "Value" "Conn_01x22_FPC_P0.5mm_Vertical_LowerContact (SparkFun)"
    			(at 0 -30.48 0)
    		)
    		(property "PROD_ID" "CONN-24643"
    			(at -1.016 -40.386 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x22_fpc_p0_5mm_vertical_lowercontact_1_1"
    			(pin passive line
    				(at -5.08 25.4 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 22.86 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 20.32 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 17.78 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 15.24 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 12.7 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at -5.08 -15.24 0)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at -5.08 -17.78 0)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at -5.08 -20.32 0)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    			(pin passive line
    				(at -5.08 -22.86 0)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    			(pin passive line
    				(at -5.08 -25.4 0)
    				(length 3.81)
    				(name "Pin_21")
    				(number "21")
    			)
    			(pin passive line
    				(at -5.08 -27.94 0)
    				(length 3.81)
    				(name "Pin_22")
    				(number "22")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x24_fpc_p0_5mm_horizontal_bottomcontact"
        (property "Footprint" "PartReel:sparkfun_conn_01x24_fpc_p0_5mm_horizontal_bottomcontact"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/7/a/7/f/1/MD-16305-24-Pin_0.5mm_FPC_Connector__Bottom-Contact_.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "FPC connector 24-pin 0.5mm."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector FPC 24 pin 0.5mm Bottom-Contact"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x24_fpc_p0_5mm_horizontal_bottomcontact/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 27.94 0)
    		)
    		(property "Value" "Conn_01x24_FPC_P0.5mm_Horizontal_BottomContact (SparkFun)"
    			(at 0.508 -35.56 0)
    		)
    		(property "PROD_ID" "CONN-14233"
    			(at 0 -45.72 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x24_fpc_p0_5mm_horizontal_bottomcontact_1_1"
    			(pin passive line
    				(at -5.08 25.4 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 22.86 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 20.32 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 17.78 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 15.24 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 12.7 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at -5.08 -15.24 0)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at -5.08 -17.78 0)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at -5.08 -20.32 0)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    			(pin passive line
    				(at -5.08 -22.86 0)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    			(pin passive line
    				(at -5.08 -25.4 0)
    				(length 3.81)
    				(name "Pin_21")
    				(number "21")
    			)
    			(pin passive line
    				(at -5.08 -27.94 0)
    				(length 3.81)
    				(name "Pin_22")
    				(number "22")
    			)
    			(pin passive line
    				(at -5.08 -30.48 0)
    				(length 3.81)
    				(name "Pin_23")
    				(number "23")
    			)
    			(pin passive line
    				(at -5.08 -33.02 0)
    				(length 3.81)
    				(name "Pin_24")
    				(number "24")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_conn_01x24_fpc_p0_5mm_horizontal_dualcontact"
        (property "Footprint" "PartReel:sparkfun_conn_01x24_fpc_p0_5mm_horizontal_dualcontact"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.atom-connector.com/uploads/FPC0.5mm-XP-SMTH1.5.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "FPC connector 24-pin 0.5mm."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector FPC 24 pin 0.5mm Dual Contact"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_conn_01x24_fpc_p0_5mm_horizontal_dualcontact/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 27.94 0)
    		)
    		(property "Value" "Conn_01x24_FPC_P0.5mm_Horizontal_DualContact (SparkFun)"
    			(at 0.508 -35.56 0)
    		)
    		(property "PROD_ID" "CONN-14195"
    			(at 0 -45.72 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_conn_01x24_fpc_p0_5mm_horizontal_dualcontact_1_1"
    			(pin passive line
    				(at -5.08 25.4 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 22.86 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 20.32 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 17.78 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 15.24 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 12.7 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at -5.08 -15.24 0)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at -5.08 -17.78 0)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at -5.08 -20.32 0)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    			(pin passive line
    				(at -5.08 -22.86 0)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    			(pin passive line
    				(at -5.08 -25.4 0)
    				(length 3.81)
    				(name "Pin_21")
    				(number "21")
    			)
    			(pin passive line
    				(at -5.08 -27.94 0)
    				(length 3.81)
    				(name "Pin_22")
    				(number "22")
    			)
    			(pin passive line
    				(at -5.08 -30.48 0)
    				(length 3.81)
    				(name "Pin_23")
    				(number "23")
    			)
    			(pin passive line
    				(at -5.08 -33.02 0)
    				(length 3.81)
    				(name "Pin_24")
    				(number "24")
    			)
    			(pin no_connect line
    				(at 3.81 -24.13 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "MP1")
    			)
    			(pin no_connect line
    				(at 6.35 -24.13 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "MP2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_debug_cortex_2x5_p1_27mm_smd_unshrouded"
        (property "Footprint" "PartReel:sparkfun_debug_cortex_2x5_p1_27mm_smd_unshrouded"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/f/7/4/1/5/21200.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cortex Debug Connector 10 pin."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun swd arm cortex debug debugger 2x5"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_debug_cortex_2x5_p1_27mm_smd_unshrouded/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 8.89 0)
    		)
    		(property "Value" "Debug-Cortex-2x5_P1.27mm-SMD-Unshrouded (SparkFun)"
    			(at 0 -7.62 0)
    		)
    		(property "PROD_ID" "CONN-15353"
    			(at 0 -16.51 0)
    		)
    		(symbol "sparkfun_debug_cortex_2x5_p1_27mm_smd_unshrouded_1_0"
    			(pin power_in line
    				(at -10.16 5.08 0)
    				(length 2.54)
    				(name "VCC")
    				(number "1")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "5")
    			)
    			(pin input line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "9")
    			)
    			(pin open_collector line
    				(at 10.16 5.08 180)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at 10.16 2.54 180)
    				(length 2.54)
    				(name "SWDIO")
    				(number "2")
    			)
    			(pin output line
    				(at 10.16 0 180)
    				(length 2.54)
    				(name "SWDCLK")
    				(number "4")
    			)
    			(pin input line
    				(at 10.16 -2.54 180)
    				(length 2.54)
    				(name "SWO")
    				(number "6")
    			)
    		)
    		(symbol "sparkfun_debug_cortex_2x5_p1_27mm_smd_unshrouded_1_1")
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_microsd_friction"
        (property "Footprint" "PartReel:sparkfun_microsd_friction"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://tools.molex.com/pdm_docs/sd/1050270001_sd.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Micro SD socket External Pin."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector SD microsd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_microsd_friction/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -6.35 15.24 0)
    			(do_not_autoplace)
    		)
    		(property "Value" "microSD_Friction (SparkFun)"
    			(at 0 -12.7 0)
    			(do_not_autoplace)
    		)
    		(property "PROD_ID" "CONN-20948"
    			(at 0 -20.32 0)
    		)
    		(property "ki_fp_filters" "microSD*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_microsd_friction_0_1")
    		(symbol "sparkfun_microsd_friction_1_1"
    			(text "VDD"
    				(at 3.81 -5.08 0)
    			)
    			(pin power_in line
    				(at -8.89 12.7 0)
    				(length 2.54)
    				(name "VDD")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at -8.89 10.16 0)
    				(length 2.54)
    				(name "DAT3/~{CS}")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -8.89 7.62 0)
    				(length 2.54)
    				(name "DAT2")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at -8.89 5.08 0)
    				(length 2.54)
    				(name "DAT1")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at -8.89 2.54 0)
    				(length 2.54)
    				(name "DAT0/SDO")
    				(number "7")
    			)
    			(pin input line
    				(at -8.89 0 0)
    				(length 2.54)
    				(name "CLK/SCK")
    				(number "5")
    			)
    			(pin input line
    				(at -8.89 -2.54 0)
    				(length 2.54)
    				(name "CMD/SDI")
    				(number "3")
    			)
    			(pin passive line
    				(at -8.89 -5.08 0)
    				(length 2.54)
    				(name "DET")
    				(number "9")
    			)
    			(pin passive line
    				(at -8.89 -7.62 0)
    				(length 2.54)
    				(name "SHIELD")
    				(number "10")
    			)
    			(pin power_in line
    				(at -8.89 -10.16 0)
    				(length 2.54)
    				(name "VSS")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_microsd_pushpush"
        (property "Footprint" "PartReel:sparkfun_microsd_pushpush"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/a/d/6/0/8/microSD_Datasheet_msd-1-a.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Micro SD socket External Pin."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector SD microsd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_microsd_pushpush/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -6.35 15.24 0)
    			(do_not_autoplace)
    		)
    		(property "Value" "microSD_PushPush (SparkFun)"
    			(at 0 -12.7 0)
    			(do_not_autoplace)
    		)
    		(property "PROD_ID" "CONN-16110"
    			(at 0 -20.32 0)
    		)
    		(property "ki_fp_filters" "microSD*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_microsd_pushpush_1_1"
    			(pin power_in line
    				(at -8.89 12.7 0)
    				(length 2.54)
    				(name "VDD")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at -8.89 10.16 0)
    				(length 2.54)
    				(name "DAT3/CD")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -8.89 7.62 0)
    				(length 2.54)
    				(name "DAT2")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at -8.89 5.08 0)
    				(length 2.54)
    				(name "DAT1")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at -8.89 2.54 0)
    				(length 2.54)
    				(name "DAT0/SDO")
    				(number "7")
    			)
    			(pin input line
    				(at -8.89 0 0)
    				(length 2.54)
    				(name "CLK/SCK")
    				(number "5")
    			)
    			(pin input line
    				(at -8.89 -2.54 0)
    				(length 2.54)
    				(name "CMD/SDI")
    				(number "3")
    			)
    			(pin passive line
    				(at -8.89 -5.08 0)
    				(length 2.54)
    				(name "~{DET}")
    				(number "9")
    			)
    			(pin passive line
    				(at -8.89 -7.62 0)
    				(length 2.54)
    				(name "SHIELD")
    				(number "10")
    			)
    			(pin power_in line
    				(at -8.89 -10.16 0)
    				(length 2.54)
    				(name "VSS")
    				(number "6")
    			)
    			(pin no_connect line
    				(at 2.54 -8.89 90)
    				(length 2.54)
    				(hide yes)
    				(name "SHIELD")
    				(number "11")
    			)
    			(pin no_connect line
    				(at 3.81 -8.89 90)
    				(length 2.54)
    				(hide yes)
    				(name "SHIELD")
    				(number "12")
    			)
    			(pin no_connect line
    				(at 5.08 -8.89 90)
    				(length 2.54)
    				(hide yes)
    				(name "SHIELD")
    				(number "13")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_qwiic_horizontal"
        (property "Footprint" "PartReel:sparkfun_qwiic_horizontal"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "4 pin JST 1mm polarized connector for I2C."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_qwiic_horizontal/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.08 0)
    		)
    		(property "Value" "Qwiic_Horizontal (SparkFun)"
    			(at 0 -7.62 0)
    		)
    		(property "PROD_ID" "CONN-13694"
    			(at 0 -10.16 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_qwiic_horizontal_0_0")
    		(symbol "sparkfun_qwiic_horizontal_1_1"
    			(text "SCL"
    				(at 1.27 2.54 0)
    			)
    			(text "SDA"
    				(at 1.27 0 0)
    			)
    			(text "3V3"
    				(at 1.27 -2.54 0)
    			)
    			(text "GND"
    				(at 1.27 -5.08 0)
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin no_connect line
    				(at 5.08 3.81 270)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    			(pin no_connect line
    				(at 6.35 3.81 270)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_qwiic_vertical"
        (property "Footprint" "PartReel:sparkfun_qwiic_vertical"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/eSH.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "4 pin JST 1mm polarized connector for I2C."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_qwiic_vertical/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.08 0)
    		)
    		(property "Value" "Qwiic_Vertical (SparkFun)"
    			(at 0 -7.62 0)
    		)
    		(property "PROD_ID" "CONN-14483"
    			(at 0 -10.16 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_qwiic_vertical_0_0")
    		(symbol "sparkfun_qwiic_vertical_1_1"
    			(text "SCL"
    				(at 1.27 2.54 0)
    			)
    			(text "SDA"
    				(at 1.27 0 0)
    			)
    			(text "3V3"
    				(at 1.27 -2.54 0)
    			)
    			(text "GND"
    				(at 1.27 -5.08 0)
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin no_connect line
    				(at 2.54 3.81 270)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    			(pin no_connect line
    				(at 5.08 3.81 270)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_raspberry_pi_2x20_pth"
        (property "Footprint" "PartReel:sparkfun_raspberry_pi_2x20_pth"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "SparkFun header for Raspberry Pi."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Raspberry Pi GPIO Connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_raspberry_pi_2x20_pth/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -17.78 25.4 0)
    		)
    		(property "Value" "Raspberry_Pi_2x20_PTH (SparkFun)"
    			(at 5.08 -22.86 0)
    		)
    		(property "PROD_ID" "CONN-12263"
    			(at 0 -40.64 0)
    		)
    		(property "SF_ID" "PRT-13054"
    			(at 0 -43.18 0)
    		)
    		(property "ki_fp_filters" "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_raspberry_pi_2x20_pth_0_1")
    		(symbol "sparkfun_raspberry_pi_2x20_pth_1_1"
    			(pin bidirectional line
    				(at -20.32 22.86 0)
    				(length 2.54)
    				(name "GPIO14/TXD")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at -20.32 20.32 0)
    				(length 2.54)
    				(name "GPIO15/RXD")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at -20.32 15.24 0)
    				(length 2.54)
    				(name "GPIO16")
    				(number "36")
    			)
    			(pin bidirectional line
    				(at -20.32 12.7 0)
    				(length 2.54)
    				(name "GPIO17")
    				(number "11")
    			)
    			(pin bidirectional line
    				(at -20.32 10.16 0)
    				(length 2.54)
    				(name "GPIO18/PWM0")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at -20.32 5.08 0)
    				(length 2.54)
    				(name "GPIO19/POCI1")
    				(number "35")
    			)
    			(pin bidirectional line
    				(at -20.32 2.54 0)
    				(length 2.54)
    				(name "GPIO20/PICO1")
    				(number "38")
    			)
    			(pin bidirectional line
    				(at -20.32 0 0)
    				(length 2.54)
    				(name "GPIO21/SCLK1")
    				(number "40")
    			)
    			(pin bidirectional line
    				(at -20.32 -5.08 0)
    				(length 2.54)
    				(name "GPIO22")
    				(number "15")
    			)
    			(pin bidirectional line
    				(at -20.32 -7.62 0)
    				(length 2.54)
    				(name "GPIO23")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at -20.32 -10.16 0)
    				(length 2.54)
    				(name "GPIO24")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at -20.32 -12.7 0)
    				(length 2.54)
    				(name "GPIO25")
    				(number "22")
    			)
    			(pin bidirectional line
    				(at -20.32 -15.24 0)
    				(length 2.54)
    				(name "GPIO26")
    				(number "37")
    			)
    			(pin bidirectional line
    				(at -20.32 -17.78 0)
    				(length 2.54)
    				(name "GPIO27")
    				(number "13")
    			)
    			(pin power_in line
    				(at -2.54 26.67 270)
    				(length 2.54)
    				(name "5V")
    				(number "2")
    			)
    			(pin passive line
    				(at -2.54 26.67 270)
    				(length 2.54)
    				(hide yes)
    				(name "5V")
    				(number "4")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "14")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "20")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "25")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "30")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "34")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "39")
    			)
    			(pin power_in line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(name "GND")
    				(number "6")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "9")
    			)
    			(pin power_in line
    				(at 2.54 26.67 270)
    				(length 2.54)
    				(name "3V3")
    				(number "1")
    			)
    			(pin passive line
    				(at 2.54 26.67 270)
    				(length 2.54)
    				(hide yes)
    				(name "3V3")
    				(number "17")
    			)
    			(pin bidirectional line
    				(at 20.32 22.86 180)
    				(length 2.54)
    				(name "ID_SD/GPIO0")
    				(number "27")
    			)
    			(pin bidirectional line
    				(at 20.32 20.32 180)
    				(length 2.54)
    				(name "ID_SC/GPIO1")
    				(number "28")
    			)
    			(pin bidirectional line
    				(at 20.32 15.24 180)
    				(length 2.54)
    				(name "SDA/GPIO2")
    				(number "3")
    			)
    			(pin bidirectional line
    				(at 20.32 12.7 180)
    				(length 2.54)
    				(name "SCL/GPIO3")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 20.32 7.62 180)
    				(length 2.54)
    				(name "GCLK0/GPIO4")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 20.32 5.08 180)
    				(length 2.54)
    				(name "GCLK1/GPIO5")
    				(number "29")
    			)
    			(pin bidirectional line
    				(at 20.32 2.54 180)
    				(length 2.54)
    				(name "GCLK2/GPIO6")
    				(number "31")
    			)
    			(pin bidirectional line
    				(at 20.32 -2.54 180)
    				(length 2.54)
    				(name "~{CE1}/GPIO7")
    				(number "26")
    			)
    			(pin bidirectional line
    				(at 20.32 -5.08 180)
    				(length 2.54)
    				(name "~{CE0}/GPIO8")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 20.32 -7.62 180)
    				(length 2.54)
    				(name "POCI0/GPIO9")
    				(number "21")
    			)
    			(pin bidirectional line
    				(at 20.32 -10.16 180)
    				(length 2.54)
    				(name "PICO0/GPIO10")
    				(number "19")
    			)
    			(pin bidirectional line
    				(at 20.32 -12.7 180)
    				(length 2.54)
    				(name "SCLK0/GPIO11")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 20.32 -17.78 180)
    				(length 2.54)
    				(name "PWM0/GPIO12")
    				(number "32")
    			)
    			(pin bidirectional line
    				(at 20.32 -20.32 180)
    				(length 2.54)
    				(name "PWM1/GPIO13")
    				(number "33")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_raspberry_pi_2x20_pth_nosilk"
        (property "Footprint" "PartReel:sparkfun_raspberry_pi_2x20_pth_nosilk"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/raspberrypi/schematics/rpi_SCH_3bplus_1p0_reduced.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "SparkFun header for Raspberry Pi."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Raspberry Pi GPIO Connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_raspberry_pi_2x20_pth_nosilk/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -17.78 25.4 0)
    		)
    		(property "Value" "Raspberry_Pi_2x20_PTH_NoSilk (SparkFun)"
    			(at 5.08 -22.86 0)
    		)
    		(property "PROD_ID" "CONN-12263"
    			(at 0 -40.64 0)
    		)
    		(property "SF_ID" "PRT-13054"
    			(at 0 -43.18 0)
    		)
    		(property "ki_fp_filters" "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_raspberry_pi_2x20_pth_nosilk_0_1")
    		(symbol "sparkfun_raspberry_pi_2x20_pth_nosilk_1_1"
    			(pin bidirectional line
    				(at -20.32 22.86 0)
    				(length 2.54)
    				(name "GPIO14/TXD")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at -20.32 20.32 0)
    				(length 2.54)
    				(name "GPIO15/RXD")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at -20.32 15.24 0)
    				(length 2.54)
    				(name "GPIO16")
    				(number "36")
    			)
    			(pin bidirectional line
    				(at -20.32 12.7 0)
    				(length 2.54)
    				(name "GPIO17")
    				(number "11")
    			)
    			(pin bidirectional line
    				(at -20.32 10.16 0)
    				(length 2.54)
    				(name "GPIO18/PWM0")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at -20.32 5.08 0)
    				(length 2.54)
    				(name "GPIO19/POCI1")
    				(number "35")
    			)
    			(pin bidirectional line
    				(at -20.32 2.54 0)
    				(length 2.54)
    				(name "GPIO20/PICO1")
    				(number "38")
    			)
    			(pin bidirectional line
    				(at -20.32 0 0)
    				(length 2.54)
    				(name "GPIO21/SCLK1")
    				(number "40")
    			)
    			(pin bidirectional line
    				(at -20.32 -5.08 0)
    				(length 2.54)
    				(name "GPIO22")
    				(number "15")
    			)
    			(pin bidirectional line
    				(at -20.32 -7.62 0)
    				(length 2.54)
    				(name "GPIO23")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at -20.32 -10.16 0)
    				(length 2.54)
    				(name "GPIO24")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at -20.32 -12.7 0)
    				(length 2.54)
    				(name "GPIO25")
    				(number "22")
    			)
    			(pin bidirectional line
    				(at -20.32 -15.24 0)
    				(length 2.54)
    				(name "GPIO26")
    				(number "37")
    			)
    			(pin bidirectional line
    				(at -20.32 -17.78 0)
    				(length 2.54)
    				(name "GPIO27")
    				(number "13")
    			)
    			(pin power_in line
    				(at -2.54 26.67 270)
    				(length 2.54)
    				(name "5V")
    				(number "2")
    			)
    			(pin passive line
    				(at -2.54 26.67 270)
    				(length 2.54)
    				(hide yes)
    				(name "5V")
    				(number "4")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "14")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "20")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "25")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "30")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "34")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "39")
    			)
    			(pin power_in line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(name "GND")
    				(number "6")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "9")
    			)
    			(pin power_in line
    				(at 2.54 26.67 270)
    				(length 2.54)
    				(name "3V3")
    				(number "1")
    			)
    			(pin passive line
    				(at 2.54 26.67 270)
    				(length 2.54)
    				(hide yes)
    				(name "3V3")
    				(number "17")
    			)
    			(pin bidirectional line
    				(at 20.32 22.86 180)
    				(length 2.54)
    				(name "ID_SD/GPIO0")
    				(number "27")
    			)
    			(pin bidirectional line
    				(at 20.32 20.32 180)
    				(length 2.54)
    				(name "ID_SC/GPIO1")
    				(number "28")
    			)
    			(pin bidirectional line
    				(at 20.32 15.24 180)
    				(length 2.54)
    				(name "SDA/GPIO2")
    				(number "3")
    			)
    			(pin bidirectional line
    				(at 20.32 12.7 180)
    				(length 2.54)
    				(name "SCL/GPIO3")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 20.32 7.62 180)
    				(length 2.54)
    				(name "GCLK0/GPIO4")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 20.32 5.08 180)
    				(length 2.54)
    				(name "GCLK1/GPIO5")
    				(number "29")
    			)
    			(pin bidirectional line
    				(at 20.32 2.54 180)
    				(length 2.54)
    				(name "GCLK2/GPIO6")
    				(number "31")
    			)
    			(pin bidirectional line
    				(at 20.32 -2.54 180)
    				(length 2.54)
    				(name "~{CE1}/GPIO7")
    				(number "26")
    			)
    			(pin bidirectional line
    				(at 20.32 -5.08 180)
    				(length 2.54)
    				(name "~{CE0}/GPIO8")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 20.32 -7.62 180)
    				(length 2.54)
    				(name "POCI0/GPIO9")
    				(number "21")
    			)
    			(pin bidirectional line
    				(at 20.32 -10.16 180)
    				(length 2.54)
    				(name "PICO0/GPIO10")
    				(number "19")
    			)
    			(pin bidirectional line
    				(at 20.32 -12.7 180)
    				(length 2.54)
    				(name "SCLK0/GPIO11")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 20.32 -17.78 180)
    				(length 2.54)
    				(name "PWM0/GPIO12")
    				(number "32")
    			)
    			(pin bidirectional line
    				(at 20.32 -20.32 180)
    				(length 2.54)
    				(name "PWM1/GPIO13")
    				(number "33")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_raspberry_pi_2x20_pth_smd_pass_through_top_mount"
        (property "Footprint" "PartReel:sparkfun_raspberry_pi_2x20_pth_smd_pass_through_top_mount"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.4uconnector.com/online/object/4udrawing/10956.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "SparkFun header for Raspberry Pi."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Raspberry Pi GPIO Connector Passthrough"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_raspberry_pi_2x20_pth_smd_pass_through_top_mount/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -17.78 25.4 0)
    		)
    		(property "Value" "Raspberry_Pi_2x20_PTH_SMD_Pass_Through_Top_Mount (SparkFun)"
    			(at 5.08 -22.86 0)
    		)
    		(property "PROD_ID" "CONN-13790"
    			(at 0 -43.18 0)
    		)
    		(property "ki_fp_filters" "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_raspberry_pi_2x20_pth_smd_pass_through_top_mount_0_1")
    		(symbol "sparkfun_raspberry_pi_2x20_pth_smd_pass_through_top_mount_1_1"
    			(pin bidirectional line
    				(at -20.32 22.86 0)
    				(length 2.54)
    				(name "GPIO14/TXD")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at -20.32 20.32 0)
    				(length 2.54)
    				(name "GPIO15/RXD")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at -20.32 15.24 0)
    				(length 2.54)
    				(name "GPIO16")
    				(number "36")
    			)
    			(pin bidirectional line
    				(at -20.32 12.7 0)
    				(length 2.54)
    				(name "GPIO17")
    				(number "11")
    			)
    			(pin bidirectional line
    				(at -20.32 10.16 0)
    				(length 2.54)
    				(name "GPIO18/PWM0")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at -20.32 5.08 0)
    				(length 2.54)
    				(name "GPIO19/POCI1")
    				(number "35")
    			)
    			(pin bidirectional line
    				(at -20.32 2.54 0)
    				(length 2.54)
    				(name "GPIO20/PICO1")
    				(number "38")
    			)
    			(pin bidirectional line
    				(at -20.32 0 0)
    				(length 2.54)
    				(name "GPIO21/SCLK1")
    				(number "40")
    			)
    			(pin bidirectional line
    				(at -20.32 -5.08 0)
    				(length 2.54)
    				(name "GPIO22")
    				(number "15")
    			)
    			(pin bidirectional line
    				(at -20.32 -7.62 0)
    				(length 2.54)
    				(name "GPIO23")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at -20.32 -10.16 0)
    				(length 2.54)
    				(name "GPIO24")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at -20.32 -12.7 0)
    				(length 2.54)
    				(name "GPIO25")
    				(number "22")
    			)
    			(pin bidirectional line
    				(at -20.32 -15.24 0)
    				(length 2.54)
    				(name "GPIO26")
    				(number "37")
    			)
    			(pin bidirectional line
    				(at -20.32 -17.78 0)
    				(length 2.54)
    				(name "GPIO27")
    				(number "13")
    			)
    			(pin power_in line
    				(at -2.54 26.67 270)
    				(length 2.54)
    				(name "5V")
    				(number "2")
    			)
    			(pin passive line
    				(at -2.54 26.67 270)
    				(length 2.54)
    				(hide yes)
    				(name "5V")
    				(number "4")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "14")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "20")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "25")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "30")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "34")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "39")
    			)
    			(pin power_in line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(name "GND")
    				(number "6")
    			)
    			(pin passive line
    				(at 0 -24.13 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "9")
    			)
    			(pin power_in line
    				(at 2.54 26.67 270)
    				(length 2.54)
    				(name "3V3")
    				(number "1")
    			)
    			(pin passive line
    				(at 2.54 26.67 270)
    				(length 2.54)
    				(hide yes)
    				(name "3V3")
    				(number "17")
    			)
    			(pin bidirectional line
    				(at 20.32 22.86 180)
    				(length 2.54)
    				(name "ID_SD/GPIO0")
    				(number "27")
    			)
    			(pin bidirectional line
    				(at 20.32 20.32 180)
    				(length 2.54)
    				(name "ID_SC/GPIO1")
    				(number "28")
    			)
    			(pin bidirectional line
    				(at 20.32 15.24 180)
    				(length 2.54)
    				(name "SDA/GPIO2")
    				(number "3")
    			)
    			(pin bidirectional line
    				(at 20.32 12.7 180)
    				(length 2.54)
    				(name "SCL/GPIO3")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 20.32 7.62 180)
    				(length 2.54)
    				(name "GCLK0/GPIO4")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 20.32 5.08 180)
    				(length 2.54)
    				(name "GCLK1/GPIO5")
    				(number "29")
    			)
    			(pin bidirectional line
    				(at 20.32 2.54 180)
    				(length 2.54)
    				(name "GCLK2/GPIO6")
    				(number "31")
    			)
    			(pin bidirectional line
    				(at 20.32 -2.54 180)
    				(length 2.54)
    				(name "~{CE1}/GPIO7")
    				(number "26")
    			)
    			(pin bidirectional line
    				(at 20.32 -5.08 180)
    				(length 2.54)
    				(name "~{CE0}/GPIO8")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 20.32 -7.62 180)
    				(length 2.54)
    				(name "POCI0/GPIO9")
    				(number "21")
    			)
    			(pin bidirectional line
    				(at 20.32 -10.16 180)
    				(length 2.54)
    				(name "PICO0/GPIO10")
    				(number "19")
    			)
    			(pin bidirectional line
    				(at 20.32 -12.7 180)
    				(length 2.54)
    				(name "SCLK0/GPIO11")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 20.32 -17.78 180)
    				(length 2.54)
    				(name "PWM0/GPIO12")
    				(number "32")
    			)
    			(pin bidirectional line
    				(at 20.32 -20.32 180)
    				(length 2.54)
    				(name "PWM1/GPIO13")
    				(number "33")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_rj45_magjack_poe"
        (property "Footprint" "PartReel:sparkfun_rj45_magjack_poe"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/b/f/e/c/e/LPJ0284GDNL.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Ethernet RJ45 with magnetics and Power-over-Ethernet."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Mag Jack"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_rj45_magjack_poe/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -11.176 20.066 0)
    		)
    		(property "Value" "RJ45_MagJack_PoE (SparkFun)"
    			(at 0 -17.78 0)
    		)
    		(property "PROD_ID" "CONN-16253"
    			(at 0 -20.32 0)
    		)
    		(symbol "sparkfun_rj45_magjack_poe_0_1")
    		(symbol "sparkfun_rj45_magjack_poe_1_0"
    			(pin passive line
    				(at 12.7 15.24 180)
    				(length 2.54)
    				(name "YLW-")
    				(number "12")
    			)
    			(pin passive line
    				(at 12.7 12.7 180)
    				(length 2.54)
    				(name "GRN+")
    				(number "13")
    			)
    			(pin passive line
    				(at 12.7 10.16 180)
    				(length 2.54)
    				(name "GRN-")
    				(number "14")
    			)
    			(pin passive line
    				(at 12.7 7.62 180)
    				(length 2.54)
    				(name "TD+")
    				(number "1")
    			)
    			(pin passive line
    				(at 12.7 5.08 180)
    				(length 2.54)
    				(name "TCT")
    				(number "4")
    			)
    			(pin passive line
    				(at 12.7 2.54 180)
    				(length 2.54)
    				(name "TD-")
    				(number "2")
    			)
    			(pin passive line
    				(at 12.7 0 180)
    				(length 2.54)
    				(name "RD+")
    				(number "3")
    			)
    			(pin passive line
    				(at 12.7 -2.54 180)
    				(length 2.54)
    				(name "RCT")
    				(number "5")
    			)
    			(pin passive line
    				(at 12.7 -5.08 180)
    				(length 2.54)
    				(name "RD-")
    				(number "6")
    			)
    			(pin passive line
    				(at 12.7 -7.62 180)
    				(length 2.54)
    				(name "GND")
    				(number "7")
    			)
    			(pin passive line
    				(at 12.7 -10.16 180)
    				(length 2.54)
    				(name "SHLD")
    				(number "S1")
    			)
    			(pin passive line
    				(at 12.7 -10.16 180)
    				(length 2.54)
    				(hide yes)
    				(name "SHLD")
    				(number "S2")
    			)
    			(pin power_out line
    				(at 12.7 -12.7 180)
    				(length 2.54)
    				(name "PW+")
    				(number "9")
    			)
    			(pin power_out line
    				(at 12.7 -15.24 180)
    				(length 2.54)
    				(name "PW-")
    				(number "10")
    			)
    		)
    		(symbol "sparkfun_rj45_magjack_poe_1_1"
    			(text "J1"
    				(at -10.16 7.62 0)
    			)
    			(text "J2"
    				(at -10.16 2.54 0)
    			)
    			(text "J3"
    				(at -10.16 0 0)
    			)
    			(text "J6"
    				(at -10.16 -5.08 0)
    			)
    			(text "J4"
    				(at -10.16 -7.112 0)
    			)
    			(text "J5"
    				(at -10.16 -8.382 0)
    			)
    			(text "J7"
    				(at -10.16 -13.462 0)
    			)
    			(text "J8"
    				(at -10.16 -14.732 0)
    			)
    			(pin passive line
    				(at 12.7 17.78 180)
    				(length 2.54)
    				(name "YLW+")
    				(number "11")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_screwcage_1x10_p3_5mm_green"
        (property "Footprint" "PartReel:sparkfun_screwcage_1x10_p3_5mm_green"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/b/9/7/3/6/19854.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Screw cage terminal, single row."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun screw terminal (cage only)"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_screwcage_1x10_p3_5mm_green/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 12.7 0)
    		)
    		(property "Value" "ScrewCage_1x10_P3.5mm_Green (SparkFun)"
    			(at -0.254 -15.494 0)
    		)
    		(property "PROD_ID" "CONN-17279"
    			(at 0 -17.78 0)
    		)
    		(property "ki_fp_filters" "TerminalBlock*:*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_screwcage_1x10_p3_5mm_green_1_1"
    			(pin passive line
    				(at -5.08 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 7.62 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 5.08 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "5")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -5.08 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "7")
    			)
    			(pin passive line
    				(at -5.08 -7.62 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "8")
    			)
    			(pin passive line
    				(at -5.08 -10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "9")
    			)
    			(pin passive line
    				(at -5.08 -12.7 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "10")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_screwterminal_1x02_p3_5mm_horizontal_black"
        (property "Footprint" "PartReel:sparkfun_screwterminal_1x02_p3_5mm_horizontal_black"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/8/5/e/4/d/ASS_4091_CO.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Screw terminal."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun screw terminal"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_screwterminal_1x02_p3_5mm_horizontal_black/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 3.81 0)
    		)
    		(property "Value" "ScrewTerminal_1x02_P3.5mm_Horizontal_Black (SparkFun)"
    			(at 0 -3.81 0)
    		)
    		(property "PROD_ID" "CONN-08399"
    			(at 0 -6.35 0)
    		)
    		(property "ki_fp_filters" "TerminalBlock*:*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_screwterminal_1x02_p3_5mm_horizontal_black_1_1"
    			(pin passive line
    				(at -5.08 1.27 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 -1.27 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_screwterminal_1x03_p3_5mm_horizontal_black"
        (property "Footprint" "PartReel:sparkfun_screwterminal_1x03_p3_5mm_horizontal_black"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/b/1/8/d/9/OSTTEXX0104.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Screw terminal."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun screw terminal"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_screwterminal_1x03_p3_5mm_horizontal_black/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at 0 5.08 0)
    		)
    		(property "Value" "ScrewTerminal_1x03_P3.5mm_Horizontal_Black (SparkFun)"
    			(at 0 -5.08 0)
    		)
    		(property "PROD_ID" "CONN-08288"
    			(at 0 -7.62 0)
    		)
    		(property "ki_fp_filters" "TerminalBlock*:*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_screwterminal_1x03_p3_5mm_horizontal_black_1_1"
    			(pin passive line
    				(at -5.08 2.54 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -5.08 0 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -5.08 -2.54 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_usb_c_receptacle"
        (property "Footprint" "PartReel:sparkfun_usb_c_receptacle"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "USB 2.0-only Type-C Receptacle connector."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun usb universal serial bus type-C USB2.0"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_usb_c_receptacle/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -10.16 12.7 0)
    		)
    		(property "Value" "USB_C_Receptacle (SparkFun)"
    			(at 19.05 12.7 0)
    		)
    		(property "PROD_ID" "CONN-14122"
    			(at 1.27 -30.48 0)
    		)
    		(property "ki_fp_filters" "USB*C*Receptacle*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_usb_c_receptacle_0_0")
    		(symbol "sparkfun_usb_c_receptacle_0_1")
    		(symbol "sparkfun_usb_c_receptacle_1_1"
    			(pin passive line
    				(at -7.62 -20.32 90)
    				(length 5.08)
    				(name "SHIELD")
    				(number "S")
    			)
    			(pin no_connect line
    				(at -5.08 -15.24 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC1")
    			)
    			(pin no_connect line
    				(at -3.81 -15.24 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC2")
    			)
    			(pin no_connect line
    				(at -2.54 -15.24 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "NC3")
    			)
    			(pin passive line
    				(at 0 -20.32 90)
    				(length 5.08)
    				(name "GND")
    				(number "GND")
    			)
    			(pin no_connect line
    				(at 2.54 -15.24 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "A8")
    			)
    			(pin no_connect line
    				(at 3.81 -15.24 90)
    				(length 5.08)
    				(hide yes)
    				(name "NC")
    				(number "B8")
    			)
    			(pin power_out line
    				(at 15.24 8.89 180)
    				(length 5.08)
    				(name "VBUS")
    				(number "VBUS")
    			)
    			(pin bidirectional line
    				(at 15.24 0 180)
    				(length 5.08)
    				(name "D+")
    				(number "A6")
    			)
    			(pin bidirectional line
    				(at 15.24 0 180)
    				(length 5.08)
    				(hide yes)
    				(name "D+")
    				(number "B6")
    			)
    			(pin bidirectional line
    				(at 15.24 -2.54 180)
    				(length 5.08)
    				(name "D-")
    				(number "A7")
    			)
    			(pin bidirectional line
    				(at 15.24 -2.54 180)
    				(length 5.08)
    				(hide yes)
    				(name "D-")
    				(number "B7")
    			)
    			(pin bidirectional line
    				(at 15.24 -8.89 180)
    				(length 5.08)
    				(name "CC1")
    				(number "A5")
    			)
    			(pin bidirectional line
    				(at 15.24 -11.43 180)
    				(length 5.08)
    				(name "CC2")
    				(number "B5")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "usb_c_16p" (in_bom yes) (on_board yes)
      (pin_names (offset 1.524))
      (property "Reference" "J" (at 0 13.43 0))
      (property "Value" "USB Type-C Receptacle 16-pin (USB 2.0)" (at 0 -13.43 0))
        (property "Footprint" "PartReel:usb_c_16p"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2304140030_HCTL-CKX-3AH1_C165948.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "USB Type-C receptacle, 16-pin (USB 2.0 + power), SMD with through-hole shield tabs. Pinout matches the common TYPE-C-31-M-12 / HRO 16-pin part."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "usb usb-c type-c receptacle connector 16pin"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/usb_c_16p/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "usb_c_16p_1_1"
        (pin passive line (at -15.24 8.89 0) (length 5.08)
          (name "GND")
          (number "A1"))
        (pin passive line (at -15.24 6.35 0) (length 5.08)
          (name "VBUS")
          (number "A4"))
        (pin passive line (at -15.24 3.81 0) (length 5.08)
          (name "CC1")
          (number "A5"))
        (pin passive line (at -15.24 1.27 0) (length 5.08)
          (name "D+")
          (number "A6"))
        (pin passive line (at -15.24 -1.27 0) (length 5.08)
          (name "D-")
          (number "A7"))
        (pin passive line (at -15.24 -3.81 0) (length 5.08)
          (name "SBU1")
          (number "A8"))
        (pin passive line (at -15.24 -6.35 0) (length 5.08)
          (name "VBUS")
          (number "A9"))
        (pin passive line (at -15.24 -8.89 0) (length 5.08)
          (name "GND")
          (number "A12"))
        (pin passive line (at 15.24 8.89 180) (length 5.08)
          (name "GND")
          (number "B1"))
        (pin passive line (at 15.24 6.35 180) (length 5.08)
          (name "VBUS")
          (number "B4"))
        (pin passive line (at 15.24 3.81 180) (length 5.08)
          (name "CC2")
          (number "B5"))
        (pin passive line (at 15.24 1.27 180) (length 5.08)
          (name "D+")
          (number "B6"))
        (pin passive line (at 15.24 -1.27 180) (length 5.08)
          (name "D-")
          (number "B7"))
        (pin passive line (at 15.24 -3.81 180) (length 5.08)
          (name "SBU2")
          (number "B8"))
        (pin passive line (at 15.24 -6.35 180) (length 5.08)
          (name "VBUS")
          (number "B9"))
        (pin passive line (at 15.24 -8.89 180) (length 5.08)
          (name "GND")
          (number "B12"))
        (pin passive line (at 0 -16.51 90) (length 5.08)
          (name "SH")
          (number "S1"))
      )
    )
  (symbol "yeonho_smw250_03p" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:yeonho_smw250_03p"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.devicemart.co.kr/goods/download?id=33537&rank=1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Yeonho SMW250 series 2.5mm pitch 3-pin wire-to-board wafer, DIP straight, AC/DC 250V 3A. JST XH compatible pattern. Pin row offset: lock front 3.45mm / back 2.35mm."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "yeonho smw250 2.5mm connector wafer 3pin jst xh compatible"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/yeonho_smw250_03p/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 5.08 0))
      (property "Value" "Yeonho SMW250-03P" (at 3.54 -5.08 0))
      (symbol "yeonho_smw250_03p_1_1"
        (pin passive line (at -5.08 2.54 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 0.00 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
      )
    )
  (symbol "yeonho_smw250_04p" (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:yeonho_smw250_04p"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.devicemart.co.kr/goods/download?id=33537&rank=1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Yeonho SMW250 series 2.5mm pitch 4-pin wire-to-board wafer, DIP straight, AC/DC 250V 3A. JST XH compatible pattern. Pin row offset: lock front 3.45mm / back 2.35mm."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "yeonho smw250 2.5mm connector wafer 4pin jst xh compatible"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/yeonho_smw250_04p/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "J" (at 3.54 6.35 0))
      (property "Value" "Yeonho SMW250-04P" (at 3.54 -6.35 0))
      (symbol "yeonho_smw250_04p_1_1"
        (pin passive line (at -5.08 3.81 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at -5.08 1.27 0) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at -5.08 -1.27 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at -5.08 -3.81 0) (length 2.54)
          (name "Pin_4")
          (number "4"))
      )
    )
  (symbol "samtec_ftsh_107_01_l_dv_k" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 2.54 2.54 0))
      (property "Value" "FTSH-107-01-L-DV-K 1.27mm 2x7 SMD header (Samtec)" (at 2.54 -18.41 0))
        (property "Footprint" "PartReel:samtec_ftsh_107_01_l_dv_k"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.samtec.com/products/ftsh-107-01-l-dv-k"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Samtec FTSH series 1.27mm dual-row SMD header, 2x7 (14 pins). FTSH-107 is the STDC14 debug connector (ST UM2448)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "connector header 1.27mm samtec ftsh stdc14"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/samtec_ftsh_107_01_l_dv_k/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "samtec_ftsh_107_01_l_dv_k_1_1"
        (pin passive line (at 0 -0 0) (length 2.54)
          (name "Pin_1")
          (number "1"))
        (pin passive line (at 10.16 -0 180) (length 2.54)
          (name "Pin_2")
          (number "2"))
        (pin passive line (at 0 -2.54 0) (length 2.54)
          (name "Pin_3")
          (number "3"))
        (pin passive line (at 10.16 -2.54 180) (length 2.54)
          (name "Pin_4")
          (number "4"))
        (pin passive line (at 0 -5.08 0) (length 2.54)
          (name "Pin_5")
          (number "5"))
        (pin passive line (at 10.16 -5.08 180) (length 2.54)
          (name "Pin_6")
          (number "6"))
        (pin passive line (at 0 -7.62 0) (length 2.54)
          (name "Pin_7")
          (number "7"))
        (pin passive line (at 10.16 -7.62 180) (length 2.54)
          (name "Pin_8")
          (number "8"))
        (pin passive line (at 0 -10.16 0) (length 2.54)
          (name "Pin_9")
          (number "9"))
        (pin passive line (at 10.16 -10.16 180) (length 2.54)
          (name "Pin_10")
          (number "10"))
        (pin passive line (at 0 -12.7 0) (length 2.54)
          (name "Pin_11")
          (number "11"))
        (pin passive line (at 10.16 -12.7 180) (length 2.54)
          (name "Pin_12")
          (number "12"))
        (pin passive line (at 0 -15.24 0) (length 2.54)
          (name "Pin_13")
          (number "13"))
        (pin passive line (at 10.16 -15.24 180) (length 2.54)
          (name "Pin_14")
          (number "14"))
      ))
  (symbol "microsd_hc" (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 15.97 0))
      (property "Value" "microSD Card Socket (push-push)" (at 0 -18.51 0))
        (property "Footprint" "PartReel:microsd_hc"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.hirose.com/product/series/DM3"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "microSD / TF card socket, push-push, SMD. Land pattern per Hirose DM3AT-SF-PEJM5 datasheet. SD-bus pinout (DAT/CMD/CLK/VDD/VSS)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "microsd sd tf card socket connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/microsd_hc/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "microsd_hc_1_1"
        (pin passive line (at -8.89 11.43 0) (length 2.54)
          (name "DAT2")
          (number "1"))
        (pin passive line (at -8.89 8.89 0) (length 2.54)
          (name "DAT3/CD")
          (number "2"))
        (pin passive line (at -8.89 6.35 0) (length 2.54)
          (name "CMD")
          (number "3"))
        (pin passive line (at -8.89 3.81 0) (length 2.54)
          (name "VDD")
          (number "4"))
        (pin passive line (at -8.89 1.27 0) (length 2.54)
          (name "CLK")
          (number "5"))
        (pin passive line (at -8.89 -1.27 0) (length 2.54)
          (name "VSS")
          (number "6"))
        (pin passive line (at -8.89 -3.81 0) (length 2.54)
          (name "DAT0")
          (number "7"))
        (pin passive line (at -8.89 -6.35 0) (length 2.54)
          (name "DAT1")
          (number "8"))
        (pin passive line (at -8.89 -8.89 0) (length 2.54)
          (name "DET_B")
          (number "9"))
        (pin passive line (at -8.89 -11.43 0) (length 2.54)
          (name "DET_A")
          (number "10"))
        (pin passive line (at 0 -19.05 90) (length 2.54)
          (name "Shield")
          (number "SH"))
      )
    )
  (symbol "nxp_pesd15vs5ud_q"
        (property "Footprint" "PartReel:nxp_pesd15vs5ud_q"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PESD15VS5UD-Q.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "AEC-Q101 automotive-qualified version of PESD15VS5UD (identical fivefold ESD array, SOT457/SC-74 TSOP6). Same package and pinout as PESD15VS5UD per the Nexperia PESD15VS5UD-Q datasheet (pin table cross-checked against PESDXS5UD_SER); footprint/symbol reuse the gate-verified PESD15VS5UD assets."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern fivefold esd protection diode arrays 30kv"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nxp_pesd15vs5ud_q/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "D"
    			(at 3.81 2.54 0)
    		)
    		(property "Value" "PESD15VS5UD-Q"
    			(at 3.81 -2.54 0)
    		)
    		(symbol "nxp_pesd15vs5ud_q_0_0"
    			(pin passive line
    				(at 0 0 0)
    				(length 2.54)
    				(name "A")
    				(number "2")
    			)
    		)
    		(symbol "nxp_pesd15vs5ud_q_1_0"
    			(pin passive line
    				(at 7.62 0 180)
    				(length 2.54)
    				(name "C")
    				(number "1")
    			)
    		)
    		(symbol "nxp_pesd15vs5ud_q_2_0"
    			(pin passive line
    				(at 7.62 0 180)
    				(length 2.54)
    				(name "C")
    				(number "3")
    			)
    		)
    		(symbol "nxp_pesd15vs5ud_q_3_0"
    			(pin passive line
    				(at 7.62 0 180)
    				(length 2.54)
    				(name "C")
    				(number "4")
    			)
    		)
    		(symbol "nxp_pesd15vs5ud_q_4_0"
    			(pin passive line
    				(at 7.62 0 180)
    				(length 2.54)
    				(name "C")
    				(number "5")
    			)
    		)
    		(symbol "nxp_pesd15vs5ud_q_5_0"
    			(pin passive line
    				(at 7.62 0 180)
    				(length 2.54)
    				(name "C")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "diodes_dmp6023le" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (at -3.81 6.35 0))
      (property "Value" "DMP6023LE-13 60V P-channel MOSFET (SOT-223)" (at -3.81 -6.35 0))
        (property "Footprint" "PartReel:diodes_dmp6023le"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP6023LE.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "60V P채널 증가형 파워 MOSFET, RDS(on) 28mΩ @VGS=-10V, ID -7A(TA=25°C), VGS ±20V, PD 2W, AEC-Q101. SOT-223. 24V 산업 전원의 역극성 보호·하이사이드 스위치용 (게이트 RC로 돌입전류 제한 겸용)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "dmp6023le diodes mosfet p-channel pmos 60v sot-223 sot223 reverse polarity power"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/diodes_dmp6023le/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "diodes_dmp6023le_1_1"
        (text "G" (at -4.826 0.381 0))
        (text "D" (at 0.635 5.588 0))
        (text "S" (at 0.635 -6.858 0))
        (pin passive line (at -7.62 0 0) (length 2.54)
          (name "G")
          (number "1"))
        (pin passive line (at 0 7.62 270) (length 2.54)
          (name "D")
          (number "2"))
        (pin passive line (at 0 -7.62 90) (length 2.54)
          (name "S")
          (number "3"))
      ))
  (symbol "ti_tps259520dsgr"
        (property "Footprint" "PartReel:ti_tps259520dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit; 3.8V OV clamp, latch-off after TSD, active-high EN/UVLO. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259520dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259520DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259520dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259521dsgr"
        (property "Footprint" "PartReel:ti_tps259521dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit; 3.8V OV clamp, auto-retry after TSD, active-high EN/UVLO. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259521dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259521DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259521dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259525dsgr"
        (property "Footprint" "PartReel:ti_tps259525dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 3-18V, 0.5-4A adj current limit; 3.8V OV clamp, auto-retry, active-high EN/UVLO, quick output discharge (QOD replaces FLT). Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259525dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259525DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259525dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "QOD")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259530dsgr"
        (property "Footprint" "PartReel:ti_tps259530dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit; 5.7V OV clamp, latch-off after TSD, active-high EN/UVLO. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259530dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259530DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259530dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259531dsgr"
        (property "Footprint" "PartReel:ti_tps259531dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit; 5.7V OV clamp, auto-retry after TSD, active-high EN/UVLO. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259531dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259531DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259531dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259533dsgr"
        (property "Footprint" "PartReel:ti_tps259533dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit, 34mOhm; fixed 5.7V OV clamp, auto-retry, active-low EN/OVLO, no QOD. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259533dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259533DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259533dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "~{EN}/OVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259535dsgr"
        (property "Footprint" "PartReel:ti_tps259535dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 3-18V, 0.5-4A adj current limit; 5.7V OV clamp, auto-retry, active-high EN/UVLO, quick output discharge (QOD replaces FLT). Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259535dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259535DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259535dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "QOD")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259540dsgr"
        (property "Footprint" "PartReel:ti_tps259540dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit; 13.7V OV clamp, latch-off after TSD, active-high EN/UVLO. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259540dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259540DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259540dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259541dsgr"
        (property "Footprint" "PartReel:ti_tps259541dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit; 13.7V OV clamp, auto-retry after TSD, active-high EN/UVLO. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259541dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259541DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259541dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259570dsgr"
        (property "Footprint" "PartReel:ti_tps259570dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit; no OV clamp, latch-off after TSD, active-high EN/UVLO. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259570dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259570DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259570dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps259571dsgr"
        (property "Footprint" "PartReel:ti_tps259571dsgr"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2595.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "eFuse 2.7-18V, 0.5-4A adj current limit; no OV clamp, auto-retry after TSD, active-high EN/UVLO. Same package and pinout as TPS259573DSG per the TI family datasheet; footprint/symbol reuse the gate-verified TPS259573DSG assets (pins renamed per variant)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 18v mohm efuse with fast overvoltage"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps259571dsgr/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS259571DSGR"
    			(at 10.16 -24.13 0)
    		)
    		(symbol "ti_tps259571dsgr_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "4")
    			)
    			(pin input line
    				(at -5.08 -15.24 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "1")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "5")
    			)
    			(pin output line
    				(at 25.4 -7.62 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 25.4 -12.7 180)
    				(length 5.08)
    				(name "ILM")
    				(number "7")
    			)
    			(pin power_in line
    				(at 25.4 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "8")
    			)
    			(pin power_in line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_tps26602pwpt"
        (property "Footprint" "PartReel:ti_tps26602pwpt"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2660.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "60V eFuse with fixed 38V internal overvoltage clamp (vs TPS26600's adjustable overvoltage cut-off); circuit-breaker with auto-retry. Same package and pinout as TPS26600PWP per the TI family datasheet; footprint/symbol reuse the gate-verified TPS26600PWP assets."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 60v industrial efuse with integrated reverse"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_tps26602pwpt/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 10.16 1.27 0)
    		)
    		(property "Value" "TPS26602PWPT"
    			(at 10.16 -36.83 0)
    		)
    		(symbol "ti_tps26602pwpt_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "IN")
    				(number "1")
    			)
    			(pin input line
    				(at -5.08 -5.08 0)
    				(length 5.08)
    				(name "IN")
    				(number "2")
    			)
    			(pin input line
    				(at -5.08 -10.16 0)
    				(length 5.08)
    				(name "UVLO")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -17.78 0)
    				(length 5.08)
    				(name "OVP")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at -5.08 -20.32 0)
    				(length 5.08)
    				(name "dVdT")
    				(number "12")
    			)
    			(pin input line
    				(at -5.08 -25.4 0)
    				(length 5.08)
    				(name "MODE")
    				(number "6")
    			)
    			(pin passive line
    				(at -5.08 -30.48 0)
    				(length 5.08)
    				(name "RTN")
    				(number "8")
    			)
    			(pin power_in line
    				(at -5.08 -33.02 0)
    				(length 5.08)
    				(name "PwPd")
    				(number "17")
    			)
    			(pin output line
    				(at 25.4 -2.54 180)
    				(length 5.08)
    				(name "OUT")
    				(number "15")
    			)
    			(pin output line
    				(at 25.4 -5.08 180)
    				(length 5.08)
    				(name "OUT")
    				(number "16")
    			)
    			(pin output line
    				(at 25.4 -10.16 180)
    				(length 5.08)
    				(name "~{FLT}")
    				(number "14")
    			)
    			(pin input line
    				(at 25.4 -15.24 180)
    				(length 5.08)
    				(name "~{SHDN}")
    				(number "7")
    			)
    			(pin output line
    				(at 25.4 -20.32 180)
    				(length 5.08)
    				(name "IMON")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at 25.4 -25.4 180)
    				(length 5.08)
    				(name "ILIM")
    				(number "11")
    			)
    			(pin passive line
    				(at 25.4 -27.94 180)
    				(length 5.08)
    				(name "N.C.")
    				(number "4")
    			)
    			(pin passive line
    				(at 25.4 -30.48 180)
    				(length 5.08)
    				(name "N.C.")
    				(number "13")
    			)
    			(pin power_in line
    				(at 25.4 -33.02 180)
    				(length 5.08)
    				(name "GND")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_lm5163ddar"
        (property "Footprint" "PartReel:ti_lm5163ddar"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5163.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "100V input COT buck converter, 0.5A output (vs 1A on LM5164), same ultra-low IQ. Same package and pinout as LM5164DDA per the TI family datasheet; footprint/symbol reuse the gate-verified LM5164DDA assets."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 100 input synchronous buck converter with"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_lm5163ddar/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 11.43 1.27 0)
    		)
    		(property "Value" "LM5163DDAR"
    			(at 11.43 -24.13 0)
    		)
    		(symbol "ti_lm5163ddar_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "VIN")
    				(number "2")
    			)
    			(pin input line
    				(at -5.08 -7.62 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -12.7 0)
    				(length 5.08)
    				(name "RON")
    				(number "4")
    			)
    			(pin output line
    				(at -5.08 -17.78 0)
    				(length 5.08)
    				(name "PGOOD")
    				(number "6")
    			)
    			(pin output line
    				(at 27.94 -2.54 180)
    				(length 5.08)
    				(name "SW")
    				(number "8")
    			)
    			(pin input line
    				(at 27.94 -7.62 180)
    				(length 5.08)
    				(name "BST")
    				(number "7")
    			)
    			(pin input line
    				(at 27.94 -12.7 180)
    				(length 5.08)
    				(name "FB")
    				(number "5")
    			)
    			(pin power_in line
    				(at 27.94 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at 27.94 -20.32 180)
    				(length 5.08)
    				(name "EP")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_lm5163hqddarq1"
        (property "Footprint" "PartReel:ti_lm5163hqddarq1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5163h-q1.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "100V input COT buck converter, 0.5A output, AEC-Q100 automotive extended high-temperature (165C junction) grade. Same package and pinout as LM5164DDA per the TI family datasheet; footprint/symbol reuse the gate-verified LM5164DDA assets."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 100 input synchronous buck converter with"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_lm5163hqddarq1/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 11.43 1.27 0)
    		)
    		(property "Value" "LM5163HQDDARQ1"
    			(at 11.43 -24.13 0)
    		)
    		(symbol "ti_lm5163hqddarq1_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "VIN")
    				(number "2")
    			)
    			(pin input line
    				(at -5.08 -7.62 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -12.7 0)
    				(length 5.08)
    				(name "RON")
    				(number "4")
    			)
    			(pin output line
    				(at -5.08 -17.78 0)
    				(length 5.08)
    				(name "PGOOD")
    				(number "6")
    			)
    			(pin output line
    				(at 27.94 -2.54 180)
    				(length 5.08)
    				(name "SW")
    				(number "8")
    			)
    			(pin input line
    				(at 27.94 -7.62 180)
    				(length 5.08)
    				(name "BST")
    				(number "7")
    			)
    			(pin input line
    				(at 27.94 -12.7 180)
    				(length 5.08)
    				(name "FB")
    				(number "5")
    			)
    			(pin power_in line
    				(at 27.94 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at 27.94 -20.32 180)
    				(length 5.08)
    				(name "EP")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_lm5163qddarq1"
        (property "Footprint" "PartReel:ti_lm5163qddarq1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5163-q1.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "100V input COT buck converter, 0.5A output, AEC-Q100 Grade 1 automotive. Same package and pinout as LM5164DDA per the TI family datasheet; footprint/symbol reuse the gate-verified LM5164DDA assets."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 100 input synchronous buck converter with"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_lm5163qddarq1/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 11.43 1.27 0)
    		)
    		(property "Value" "LM5163QDDARQ1"
    			(at 11.43 -24.13 0)
    		)
    		(symbol "ti_lm5163qddarq1_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "VIN")
    				(number "2")
    			)
    			(pin input line
    				(at -5.08 -7.62 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -12.7 0)
    				(length 5.08)
    				(name "RON")
    				(number "4")
    			)
    			(pin output line
    				(at -5.08 -17.78 0)
    				(length 5.08)
    				(name "PGOOD")
    				(number "6")
    			)
    			(pin output line
    				(at 27.94 -2.54 180)
    				(length 5.08)
    				(name "SW")
    				(number "8")
    			)
    			(pin input line
    				(at 27.94 -7.62 180)
    				(length 5.08)
    				(name "BST")
    				(number "7")
    			)
    			(pin input line
    				(at 27.94 -12.7 180)
    				(length 5.08)
    				(name "FB")
    				(number "5")
    			)
    			(pin power_in line
    				(at 27.94 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at 27.94 -20.32 180)
    				(length 5.08)
    				(name "EP")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_lm5164ddar"
        (property "Footprint" "PartReel:ti_lm5164ddar"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5164.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "100V input COT buck converter, 1A output, ultra-low IQ (10.5uA no-load); commercial (non-automotive) tape-and-reel orderable of the LM5164DDA — the part distributors stock. Same package and pinout as LM5164DDA per the TI family datasheet; footprint/symbol reuse the gate-verified LM5164DDA assets."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 100 input synchronous buck converter with"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_lm5164ddar/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 11.43 1.27 0)
    		)
    		(property "Value" "LM5164DDAR"
    			(at 11.43 -24.13 0)
    		)
    		(symbol "ti_lm5164ddar_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "VIN")
    				(number "2")
    			)
    			(pin input line
    				(at -5.08 -7.62 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -12.7 0)
    				(length 5.08)
    				(name "RON")
    				(number "4")
    			)
    			(pin output line
    				(at -5.08 -17.78 0)
    				(length 5.08)
    				(name "PGOOD")
    				(number "6")
    			)
    			(pin output line
    				(at 27.94 -2.54 180)
    				(length 5.08)
    				(name "SW")
    				(number "8")
    			)
    			(pin input line
    				(at 27.94 -7.62 180)
    				(length 5.08)
    				(name "BST")
    				(number "7")
    			)
    			(pin input line
    				(at 27.94 -12.7 180)
    				(length 5.08)
    				(name "FB")
    				(number "5")
    			)
    			(pin power_in line
    				(at 27.94 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at 27.94 -20.32 180)
    				(length 5.08)
    				(name "EP")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "ti_lm5164qddarq1"
        (property "Footprint" "PartReel:ti_lm5164qddarq1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/lm5164-q1.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "100V input COT buck converter, 1A output, AEC-Q100 Grade 1 automotive (Tj -40 to +150C). Same package and pinout as LM5164DDA per the TI family datasheet; footprint/symbol reuse the gate-verified LM5164DDA assets."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cern 100 input synchronous buck converter with"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ti_lm5164qddarq1/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.27)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "IC"
    			(at 11.43 1.27 0)
    		)
    		(property "Value" "LM5164QDDARQ1"
    			(at 11.43 -24.13 0)
    		)
    		(symbol "ti_lm5164qddarq1_1_0"
    			(pin input line
    				(at -5.08 -2.54 0)
    				(length 5.08)
    				(name "VIN")
    				(number "2")
    			)
    			(pin input line
    				(at -5.08 -7.62 0)
    				(length 5.08)
    				(name "EN/UVLO")
    				(number "3")
    			)
    			(pin input line
    				(at -5.08 -12.7 0)
    				(length 5.08)
    				(name "RON")
    				(number "4")
    			)
    			(pin output line
    				(at -5.08 -17.78 0)
    				(length 5.08)
    				(name "PGOOD")
    				(number "6")
    			)
    			(pin output line
    				(at 27.94 -2.54 180)
    				(length 5.08)
    				(name "SW")
    				(number "8")
    			)
    			(pin input line
    				(at 27.94 -7.62 180)
    				(length 5.08)
    				(name "BST")
    				(number "7")
    			)
    			(pin input line
    				(at 27.94 -12.7 180)
    				(length 5.08)
    				(name "FB")
    				(number "5")
    			)
    			(pin power_in line
    				(at 27.94 -17.78 180)
    				(length 5.08)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at 27.94 -20.32 180)
    				(length 5.08)
    				(name "EP")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "nordic_nrf52805_caxx"
        (property "Footprint" "PartReel:nordic_nrf52805_caxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/nRF52805_PS_v1.4/resource/nRF52805_PS_v1.4.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.4GHz Bluetooth 5.4 SoC, 192KB Flash, 24KB RAM, Cortex-M4, ADC, SPI, UART, TWI, QDEC, WLCSP-36."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless ble bluetooth-low-energy arm cortex-m4 soc microcontroller two-layer wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf52805_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF52805-CAXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA?28*6x6*2.482x2.464mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf52805_caxx_1_0"
  				(pin bidirectional line
  					(at -22.86 10.16 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "D6")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -22.86 5.08 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "D5")
  					(alternate "XL2" input line)
  				)
  				(pin bidirectional line
  					(at -22.86 -2.54 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "F5")
  					(alternate "AIN2" input line)
  				)
  				(pin bidirectional line
  					(at -22.86 -5.08 0)
  					(length 2.54)
  					(name "P0.05")
  					(number "F6")
  					(alternate "AIN3" input line)
  				)
  				(pin bidirectional line
  					(at -22.86 -7.62 0)
  					(length 2.54)
  					(name "P0.12")
  					(number "G5")
  				)
  				(pin bidirectional line
  					(at -22.86 -10.16 0)
  					(length 2.54)
  					(name "P0.14")
  					(number "F4")
  				)
  				(pin bidirectional line
  					(at -22.86 -12.7 0)
  					(length 2.54)
  					(name "P0.16")
  					(number "G4")
  				)
  				(pin bidirectional line
  					(at -22.86 -15.24 0)
  					(length 2.54)
  					(name "P0.18")
  					(number "G3")
  				)
  				(pin bidirectional line
  					(at -22.86 -17.78 0)
  					(length 2.54)
  					(name "P0.20")
  					(number "F2")
  				)
  				(pin power_in line
  					(at 0 33.02 270)
  					(length 2.54)
  					(name "VDD")
  					(number "A6")
  				)
  				(pin power_in line
  					(at 0 33.02 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "G6")
  				)
  				(pin power_in line
  					(at 0 -33.02 90)
  					(length 2.54)
  					(name "VSS")
  					(number "B3")
  				)
  				(pin passive line
  					(at 0 -33.02 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "B4")
  				)
  				(pin passive line
  					(at 0 -33.02 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS_PA")
  					(number "C1")
  				)
  				(pin passive line
  					(at 0 -33.02 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D3")
  				)
  				(pin passive line
  					(at 0 -33.02 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D4")
  				)
  				(pin passive line
  					(at 0 -33.02 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E3")
  				)
  				(pin passive line
  					(at 0 -33.02 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E4")
  				)
  				(pin power_out line
  					(at 2.54 33.02 270)
  					(length 2.54)
  					(name "DCC")
  					(number "A5")
  				)
  				(pin passive line
  					(at 22.86 22.86 180)
  					(length 2.54)
  					(name "DEC1")
  					(number "B6")
  				)
  				(pin passive line
  					(at 22.86 20.32 180)
  					(length 2.54)
  					(name "DEC2")
  					(number "A3")
  				)
  				(pin passive line
  					(at 22.86 17.78 180)
  					(length 2.54)
  					(name "DEC4")
  					(number "A4")
  				)
  				(pin bidirectional line
  					(at 22.86 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "E1")
  				)
  				(pin input line
  					(at 22.86 -10.16 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "G2")
  					(alternate "P0.21" bidirectional line)
  				)
  				(pin input line
  					(at 22.86 -15.24 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "G1")
  				)
  				(pin bidirectional line
  					(at 22.86 -17.78 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "F1")
  				)
  			)
  			(symbol "nordic_nrf52805_caxx_1_1"
  				(pin input line
  					(at -22.86 22.86 0)
  					(length 2.54)
  					(name "XC1")
  					(number "A1")
  				)
  				(pin input line
  					(at -22.86 17.78 0)
  					(length 2.54)
  					(name "XC2")
  					(number "A2")
  				)
  			)
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf52810_caxx"
        (property "Footprint" "PartReel:nordic_nrf52810_caxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/nRF52810_PS_v1.5/resource/nRF52810_PS_v1.5.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.4GHz Bluetooth 5.4 SoC, 64MHz Cortex-M4, ADC, PDM, PWM, UART, SPI, TWI, CSP-33."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless ble bluetooth-low-energy arm microcontroller wireless 2mbps ant nrf52-series"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf52810_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF52810-CAXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA?33*6x6*2.482x2.464mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf52810_caxx_0_0"
  				(pin input line
  					(at -22.86 30.48 0)
  					(length 2.54)
  					(name "XC1")
  					(number "A1")
  				)
  				(pin input line
  					(at -22.86 25.4 0)
  					(length 2.54)
  					(name "XC2")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -22.86 -10.16 0)
  					(length 2.54)
  					(name "P0.08")
  					(number "F6")
  				)
  				(pin bidirectional line
  					(at -22.86 -12.7 0)
  					(length 2.54)
  					(name "P0.11")
  					(number "F5")
  				)
  				(pin bidirectional line
  					(at -22.86 -15.24 0)
  					(length 2.54)
  					(name "P0.12")
  					(number "G5")
  				)
  				(pin bidirectional line
  					(at -22.86 -17.78 0)
  					(length 2.54)
  					(name "P0.14")
  					(number "F4")
  				)
  				(pin bidirectional line
  					(at -22.86 -20.32 0)
  					(length 2.54)
  					(name "P0.15")
  					(number "G4")
  				)
  				(pin bidirectional line
  					(at -22.86 -22.86 0)
  					(length 2.54)
  					(name "P0.16")
  					(number "G3")
  				)
  				(pin bidirectional line
  					(at -22.86 -25.4 0)
  					(length 2.54)
  					(name "P0.17")
  					(number "F3")
  				)
  				(pin bidirectional line
  					(at -22.86 -27.94 0)
  					(length 2.54)
  					(name "P0.18")
  					(number "E2")
  				)
  				(pin bidirectional line
  					(at -22.86 -30.48 0)
  					(length 2.54)
  					(name "P0.20")
  					(number "G2")
  				)
  				(pin power_in line
  					(at 0 40.64 270)
  					(length 2.54)
  					(name "VDD")
  					(number "A6")
  				)
  				(pin power_in line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(name "VSS")
  					(number "E3")
  				)
  				(pin power_out line
  					(at 2.54 40.64 270)
  					(length 2.54)
  					(name "DCC")
  					(number "A5")
  				)
  				(pin bidirectional line
  					(at 22.86 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "E1")
  				)
  				(pin input line
  					(at 22.86 -27.94 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "G1")
  				)
  				(pin bidirectional line
  					(at 22.86 -30.48 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "F1")
  				)
  			)
  			(symbol "nordic_nrf52810_caxx_1_0"
  				(pin bidirectional line
  					(at -22.86 17.78 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "B5")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -22.86 12.7 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "D5")
  					(alternate "XL2" input line)
  				)
  				(pin bidirectional line
  					(at -22.86 -2.54 0)
  					(length 2.54)
  					(name "P0.03")
  					(number "D6")
  					(alternate "AIN1" input line)
  				)
  				(pin bidirectional line
  					(at -22.86 -5.08 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "E5")
  					(alternate "AIN2" input line)
  				)
  				(pin bidirectional line
  					(at -22.86 -7.62 0)
  					(length 2.54)
  					(name "P0.05")
  					(number "E6")
  					(alternate "AIN3" input line)
  				)
  				(pin passive line
  					(at 0 40.64 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "G6")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "B3")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "B4")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS_PA")
  					(number "C1")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D3")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D4")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E4")
  				)
  				(pin passive line
  					(at 22.86 30.48 180)
  					(length 2.54)
  					(name "DEC1")
  					(number "B6")
  				)
  				(pin passive line
  					(at 22.86 27.94 180)
  					(length 2.54)
  					(name "DEC2")
  					(number "A3")
  				)
  				(pin passive line
  					(at 22.86 25.4 180)
  					(length 2.54)
  					(name "DEC4")
  					(number "A4")
  				)
  				(pin input line
  					(at 22.86 -22.86 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "F2")
  					(alternate "P0.21" bidirectional line)
  				)
  			)
  			(symbol "nordic_nrf52810_caxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf52820_cfxx"
        (property "Footprint" "PartReel:nordic_nrf52820_cfxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf52820/attach/nRF52820_PS_v1.5.pdf?_LANG=enus"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.4GHz Bluetooth 5.4 USB SoC, 256KB Flash, 32KB RAM, Cortex-M4, Comparator, UART, SPI, TWI, QDEC, CSP-."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless ble bluetooth-low-energy bluetooth-mesh thread zigbee arm microcontroller wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf52820_cfxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF52820-CFXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA?44*7x7*2.531x2.531mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf52820_cfxx_0_0"
  				(pin bidirectional line
  					(at -25.4 45.72 0)
  					(length 2.54)
  					(name "D+")
  					(number "G5")
  				)
  				(pin bidirectional line
  					(at -25.4 43.18 0)
  					(length 2.54)
  					(name "D-")
  					(number "G4")
  				)
  				(pin input line
  					(at -25.4 33.02 0)
  					(length 2.54)
  					(name "XC1")
  					(number "A1")
  				)
  				(pin input line
  					(at -25.4 27.94 0)
  					(length 2.54)
  					(name "XC2")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -25.4 -10.16 0)
  					(length 2.54)
  					(name "P0.06")
  					(number "E6")
  				)
  				(pin bidirectional line
  					(at -25.4 -12.7 0)
  					(length 2.54)
  					(name "P0.07")
  					(number "F6")
  				)
  				(pin bidirectional line
  					(at -25.4 -15.24 0)
  					(length 2.54)
  					(name "P0.08")
  					(number "B3")
  				)
  				(pin bidirectional line
  					(at -25.4 -17.78 0)
  					(length 2.54)
  					(name "P0.14")
  					(number "F4")
  				)
  				(pin bidirectional line
  					(at -25.4 -20.32 0)
  					(length 2.54)
  					(name "P0.15")
  					(number "F3")
  				)
  				(pin bidirectional line
  					(at -25.4 -22.86 0)
  					(length 2.54)
  					(name "P0.16")
  					(number "E3")
  				)
  				(pin bidirectional line
  					(at -25.4 -25.4 0)
  					(length 2.54)
  					(name "P0.17")
  					(number "E2")
  				)
  				(pin bidirectional line
  					(at -25.4 -27.94 0)
  					(length 2.54)
  					(name "P0.20")
  					(number "F2")
  				)
  				(pin bidirectional line
  					(at -25.4 -30.48 0)
  					(length 2.54)
  					(name "P0.28")
  					(number "C5")
  				)
  				(pin bidirectional line
  					(at -25.4 -33.02 0)
  					(length 2.54)
  					(name "P0.29")
  					(number "C4")
  				)
  				(pin bidirectional line
  					(at -25.4 -35.56 0)
  					(length 2.54)
  					(name "P0.30")
  					(number "B4")
  				)
  				(pin power_in line
  					(at -5.08 58.42 270)
  					(length 2.54)
  					(name "VBUS")
  					(number "G7")
  				)
  				(pin passive line
  					(at 0 58.42 270)
  					(length 2.54)
  					(name "VDD")
  					(number "E7")
  				)
  				(pin power_in line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(name "VSS")
  					(number "D3")
  				)
  				(pin power_out line
  					(at 2.54 58.42 270)
  					(length 2.54)
  					(name "DCC")
  					(number "A6")
  				)
  				(pin power_in line
  					(at 7.62 58.42 270)
  					(length 2.54)
  					(name "VDDH")
  					(number "F7")
  				)
  				(pin passive line
  					(at 25.4 35.56 180)
  					(length 2.54)
  					(name "DECUSB")
  					(number "G6")
  				)
  				(pin bidirectional line
  					(at 25.4 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "E1")
  				)
  				(pin input line
  					(at 25.4 -33.02 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "G2")
  				)
  				(pin bidirectional line
  					(at 25.4 -35.56 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "G1")
  				)
  			)
  			(symbol "nordic_nrf52820_cfxx_1_0"
  				(pin bidirectional line
  					(at -25.4 17.78 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "C7")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -25.4 12.7 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "D7")
  					(alternate "XL2" input line)
  				)
  				(pin bidirectional line
  					(at -25.4 0 0)
  					(length 2.54)
  					(name "P0.02")
  					(number "B6")
  					(alternate "AIN0" input line)
  				)
  				(pin bidirectional line
  					(at -25.4 -2.54 0)
  					(length 2.54)
  					(name "P0.03")
  					(number "B5")
  					(alternate "AIN1" input line)
  				)
  				(pin bidirectional line
  					(at -25.4 -5.08 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "C6")
  					(alternate "AIN2" input line)
  				)
  				(pin bidirectional line
  					(at -25.4 -7.62 0)
  					(length 2.54)
  					(name "P0.05")
  					(number "D6")
  					(alternate "AIN3" input line)
  				)
  				(pin passive line
  					(at 0 58.42 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "A3")
  				)
  				(pin passive line
  					(at 0 58.42 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "B7")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "A4")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS_PA")
  					(number "C1")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D4")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D5")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E4")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E5")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "F5")
  				)
  				(pin passive line
  					(at 25.4 45.72 180)
  					(length 2.54)
  					(name "DEC1")
  					(number "A7")
  				)
  				(pin passive line
  					(at 25.4 43.18 180)
  					(length 2.54)
  					(name "DEC4")
  					(number "A5")
  				)
  				(pin passive line
  					(at 25.4 40.64 180)
  					(length 2.54)
  					(name "DEC5")
  					(number "F1")
  				)
  				(pin passive line
  					(at 25.4 38.1 180)
  					(length 2.54)
  					(name "DEC6")
  					(number "C2")
  				)
  				(pin input line
  					(at 25.4 -27.94 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "G3")
  					(alternate "P0.18" bidirectional line)
  				)
  			)
  			(symbol "nordic_nrf52820_cfxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf52832_cixx"
        (property "Footprint" "PartReel:nordic_nrf52832_cixx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/nRF52832_PS_v1.9/resource/nRF52832_PS_v1.9.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.4GHz Bluetooth 5.4 NFC SoC, 64MHz Cortex-M4 FPU, PDM, I2S, CSP-51."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless ble bluetooth-low-energy bluetooth-mesh arm microcontroller wireless 2mbps ant"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf52832_cixx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF52832-CIXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA?51*7x8*2.956x3.226mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf52832_cixx_0_0"
  				(pin input line
  					(at -30.48 45.72 0)
  					(length 2.54)
  					(name "XC1")
  					(number "B2")
  				)
  				(pin input line
  					(at -30.48 40.64 0)
  					(length 2.54)
  					(name "XC2")
  					(number "A1")
  				)
  				(pin bidirectional line
  					(at -30.48 -7.62 0)
  					(length 2.54)
  					(name "P0.06")
  					(number "F7")
  				)
  				(pin bidirectional line
  					(at -30.48 -10.16 0)
  					(length 2.54)
  					(name "P0.07")
  					(number "F6")
  				)
  				(pin bidirectional line
  					(at -30.48 -12.7 0)
  					(length 2.54)
  					(name "P0.08")
  					(number "G7")
  				)
  				(pin bidirectional line
  					(at -30.48 -15.24 0)
  					(length 2.54)
  					(name "P0.11")
  					(number "F4")
  				)
  				(pin bidirectional line
  					(at -30.48 -17.78 0)
  					(length 2.54)
  					(name "P0.12")
  					(number "H6")
  				)
  				(pin bidirectional line
  					(at -30.48 -20.32 0)
  					(length 2.54)
  					(name "P0.13")
  					(number "G4")
  				)
  				(pin bidirectional line
  					(at -30.48 -22.86 0)
  					(length 2.54)
  					(name "P0.17")
  					(number "G3")
  				)
  				(pin bidirectional line
  					(at -30.48 -25.4 0)
  					(length 2.54)
  					(name "P0.19")
  					(number "F3")
  				)
  				(pin bidirectional line
  					(at -30.48 -27.94 0)
  					(length 2.54)
  					(name "P0.22")
  					(number "F2")
  				)
  				(pin bidirectional line
  					(at -30.48 -30.48 0)
  					(length 2.54)
  					(name "P0.23")
  					(number "E2")
  				)
  				(pin bidirectional line
  					(at -30.48 -33.02 0)
  					(length 2.54)
  					(name "P0.24")
  					(number "E1")
  				)
  				(pin bidirectional line
  					(at -30.48 -35.56 0)
  					(length 2.54)
  					(name "P0.25")
  					(number "B3")
  				)
  				(pin bidirectional line
  					(at -30.48 -38.1 0)
  					(length 2.54)
  					(name "P0.26")
  					(number "D3")
  				)
  				(pin bidirectional line
  					(at -30.48 -40.64 0)
  					(length 2.54)
  					(name "P0.27")
  					(number "B4")
  				)
  				(pin power_in line
  					(at 0 63.5 270)
  					(length 2.54)
  					(name "VDD")
  					(number "A7")
  				)
  				(pin power_in line
  					(at 0 -63.5 90)
  					(length 2.54)
  					(name "VSS")
  					(number "C4")
  				)
  				(pin power_out line
  					(at 2.54 63.5 270)
  					(length 2.54)
  					(name "DCC")
  					(number "B6")
  				)
  				(pin bidirectional line
  					(at 30.48 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "D1")
  				)
  				(pin input line
  					(at 30.48 -48.26 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "F1")
  				)
  				(pin bidirectional line
  					(at 30.48 -50.8 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "G1")
  				)
  			)
  			(symbol "nordic_nrf52832_cixx_1_0"
  				(pin bidirectional line
  					(at -30.48 33.02 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "D7")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 27.94 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "C7")
  					(alternate "XL2" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 17.78 0)
  					(length 2.54)
  					(name "P0.09")
  					(number "G6")
  					(alternate "NFC1" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 12.7 0)
  					(length 2.54)
  					(name "P0.10")
  					(number "G5")
  					(alternate "NFC2" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 2.54 0)
  					(length 2.54)
  					(name "P0.02")
  					(number "C6")
  					(alternate "AIN0" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 0 0)
  					(length 2.54)
  					(name "P0.03")
  					(number "D6")
  					(alternate "AIN1" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 -2.54 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "E6")
  					(alternate "AIN2" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 -5.08 0)
  					(length 2.54)
  					(name "P0.05")
  					(number "E7")
  					(alternate "AIN3" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 -43.18 0)
  					(length 2.54)
  					(name "P0.28")
  					(number "A3")
  					(alternate "AIN4" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 -45.72 0)
  					(length 2.54)
  					(name "P0.29")
  					(number "A4")
  					(alternate "AIN5" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 -48.26 0)
  					(length 2.54)
  					(name "P0.30")
  					(number "A5")
  					(alternate "AIN6" input line)
  				)
  				(pin bidirectional line
  					(at -30.48 -50.8 0)
  					(length 2.54)
  					(name "P0.31")
  					(number "B5")
  					(alternate "AIN7" input line)
  				)
  				(pin no_connect line
  					(at -27.94 -53.34 0)
  					(length 2.54)
  					(hide yes)
  					(name "NC")
  					(number "C3")
  				)
  				(pin passive line
  					(at 0 63.5 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "H7")
  				)
  				(pin passive line
  					(at 0 -63.5 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "C5")
  				)
  				(pin passive line
  					(at 0 -63.5 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS_PA")
  					(number "D2")
  				)
  				(pin passive line
  					(at 0 -63.5 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E3")
  				)
  				(pin passive line
  					(at 0 -63.5 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "F5")
  				)
  				(pin passive line
  					(at 30.48 45.72 180)
  					(length 2.54)
  					(name "DEC1")
  					(number "B7")
  				)
  				(pin passive line
  					(at 30.48 43.18 180)
  					(length 2.54)
  					(name "DEC2")
  					(number "A2")
  				)
  				(pin passive line
  					(at 30.48 40.64 180)
  					(length 2.54)
  					(name "DEC3")
  					(number "C2")
  				)
  				(pin passive line
  					(at 30.48 38.1 180)
  					(length 2.54)
  					(name "DEC4")
  					(number "A6")
  				)
  				(pin bidirectional line
  					(at 30.48 -22.86 180)
  					(length 2.54)
  					(name "P0.18")
  					(number "H2")
  					(alternate "TRACEDATA[0]" output line)
  				)
  				(pin bidirectional line
  					(at 30.48 -25.4 180)
  					(length 2.54)
  					(name "P0.16")
  					(number "H3")
  					(alternate "TRACEDATA[1]" output line)
  				)
  				(pin bidirectional line
  					(at 30.48 -27.94 180)
  					(length 2.54)
  					(name "P0.15")
  					(number "H4")
  					(alternate "TRACEDATA[2]" output line)
  				)
  				(pin bidirectional line
  					(at 30.48 -30.48 180)
  					(length 2.54)
  					(name "P0.14")
  					(number "H5")
  					(alternate "TRACEDATA[3]" output line)
  				)
  				(pin bidirectional line
  					(at 30.48 -33.02 180)
  					(length 2.54)
  					(name "P0.20")
  					(number "G2")
  					(alternate "TRACECLK" input line)
  				)
  				(pin input line
  					(at 30.48 -43.18 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "H1")
  					(alternate "P0.21" bidirectional line)
  				)
  			)
  			(symbol "nordic_nrf52832_cixx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf52833_cjxx"
        (property "Footprint" "PartReel:nordic_nrf52833_cjxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf52833/attach/nRF52833_PS_v1.7.pdf?_LANG=enus"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.4GHz Bluetooth 5.4 USB NFC SoC, 512KB Flash, 128KB RAM, 105°C Cortex-M4 FPU, ADC, SPI, UART, TWI, PWM, I2S, PDM, CSP-76."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless ble bluetooth-low-energy bluetooth-mesh thread zigbee arm microcontroller wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf52833_cjxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF52833-CJXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA?76*9x9*3.175x3.175mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf52833_cjxx_0_0"
  				(pin bidirectional line
  					(at -35.56 71.12 0)
  					(length 2.54)
  					(name "D+")
  					(number "J7")
  				)
  				(pin bidirectional line
  					(at -35.56 68.58 0)
  					(length 2.54)
  					(name "D-")
  					(number "H7")
  				)
  				(pin input line
  					(at -35.56 58.42 0)
  					(length 2.54)
  					(name "XC1")
  					(number "A1")
  				)
  				(pin input line
  					(at -35.56 53.34 0)
  					(length 2.54)
  					(name "XC2")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -35.56 -2.54 0)
  					(length 2.54)
  					(name "P0.06")
  					(number "E9")
  				)
  				(pin bidirectional line
  					(at -35.56 -5.08 0)
  					(length 2.54)
  					(name "P0.08")
  					(number "E7")
  				)
  				(pin bidirectional line
  					(at -35.56 -7.62 0)
  					(length 2.54)
  					(name "P0.13")
  					(number "F7")
  				)
  				(pin bidirectional line
  					(at -35.56 -10.16 0)
  					(length 2.54)
  					(name "P0.14")
  					(number "J6")
  				)
  				(pin bidirectional line
  					(at -35.56 -12.7 0)
  					(length 2.54)
  					(name "P0.15")
  					(number "H5")
  				)
  				(pin bidirectional line
  					(at -35.56 -15.24 0)
  					(length 2.54)
  					(name "P0.16")
  					(number "G6")
  				)
  				(pin bidirectional line
  					(at -35.56 -17.78 0)
  					(length 2.54)
  					(name "P0.17")
  					(number "J5")
  				)
  				(pin bidirectional line
  					(at -35.56 -20.32 0)
  					(length 2.54)
  					(name "P0.19")
  					(number "C5")
  				)
  				(pin bidirectional line
  					(at -35.56 -22.86 0)
  					(length 2.54)
  					(name "P0.20")
  					(number "G5")
  				)
  				(pin bidirectional line
  					(at -35.56 -25.4 0)
  					(length 2.54)
  					(name "P0.21")
  					(number "G4")
  				)
  				(pin bidirectional line
  					(at -35.56 -27.94 0)
  					(length 2.54)
  					(name "P0.22")
  					(number "J3")
  				)
  				(pin bidirectional line
  					(at -35.56 -30.48 0)
  					(length 2.54)
  					(name "P0.23")
  					(number "D7")
  				)
  				(pin bidirectional line
  					(at -35.56 -33.02 0)
  					(length 2.54)
  					(name "P0.24")
  					(number "G3")
  				)
  				(pin bidirectional line
  					(at -35.56 -35.56 0)
  					(length 2.54)
  					(name "P0.25")
  					(number "A3")
  				)
  				(pin bidirectional line
  					(at -35.56 -38.1 0)
  					(length 2.54)
  					(name "P0.26")
  					(number "C9")
  				)
  				(pin bidirectional line
  					(at -35.56 -40.64 0)
  					(length 2.54)
  					(name "P0.27")
  					(number "C8")
  				)
  				(pin bidirectional line
  					(at -35.56 -53.34 0)
  					(length 2.54)
  					(name "P1.01")
  					(number "F3")
  				)
  				(pin bidirectional line
  					(at -35.56 -55.88 0)
  					(length 2.54)
  					(name "P1.02")
  					(number "H1")
  				)
  				(pin bidirectional line
  					(at -35.56 -58.42 0)
  					(length 2.54)
  					(name "P1.03")
  					(number "B4")
  				)
  				(pin bidirectional line
  					(at -35.56 -60.96 0)
  					(length 2.54)
  					(name "P1.04")
  					(number "G2")
  				)
  				(pin bidirectional line
  					(at -35.56 -63.5 0)
  					(length 2.54)
  					(name "P1.05")
  					(number "C4")
  				)
  				(pin bidirectional line
  					(at -35.56 -66.04 0)
  					(length 2.54)
  					(name "P1.06")
  					(number "E3")
  				)
  				(pin bidirectional line
  					(at -35.56 -68.58 0)
  					(length 2.54)
  					(name "P1.07")
  					(number "G1")
  				)
  				(pin bidirectional line
  					(at -35.56 -71.12 0)
  					(length 2.54)
  					(name "P1.08")
  					(number "F9")
  				)
  				(pin passive line
  					(at 0 83.82 270)
  					(length 2.54)
  					(name "VDD")
  					(number "J4")
  				)
  				(pin power_in line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(name "VSS")
  					(number "D6")
  				)
  				(pin power_out line
  					(at 2.54 83.82 270)
  					(length 2.54)
  					(name "DCC")
  					(number "A8")
  				)
  				(pin power_in line
  					(at 7.62 83.82 270)
  					(length 2.54)
  					(name "VDDH")
  					(number "H9")
  				)
  				(pin passive line
  					(at 35.56 60.96 180)
  					(length 2.54)
  					(name "DECUSB")
  					(number "J8")
  				)
  				(pin bidirectional line
  					(at 35.56 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "E1")
  				)
  				(pin input line
  					(at 35.56 -68.58 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "H2")
  				)
  				(pin bidirectional line
  					(at 35.56 -71.12 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "J2")
  				)
  			)
  			(symbol "nordic_nrf52833_cjxx_1_0"
  				(pin bidirectional line
  					(at -35.56 43.18 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "B8")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 38.1 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "B7")
  					(alternate "XL2" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 22.86 0)
  					(length 2.54)
  					(name "P0.09")
  					(number "F2")
  					(alternate "NFC1" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 17.78 0)
  					(length 2.54)
  					(name "P0.10")
  					(number "E2")
  					(alternate "NFC2" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 7.62 0)
  					(length 2.54)
  					(name "P0.02")
  					(number "C6")
  					(alternate "AIN0" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 5.08 0)
  					(length 2.54)
  					(name "P0.03")
  					(number "A4")
  					(alternate "AIN1" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 2.54 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "D8")
  					(alternate "AIN2" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 0 0)
  					(length 2.54)
  					(name "P0.05")
  					(number "D9")
  					(alternate "AIN3" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 -43.18 0)
  					(length 2.54)
  					(name "P0.28")
  					(number "C7")
  					(alternate "AIN4" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 -45.72 0)
  					(length 2.54)
  					(name "P0.29")
  					(number "A5")
  					(alternate "AIN5" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 -48.26 0)
  					(length 2.54)
  					(name "P0.30")
  					(number "B5")
  					(alternate "AIN6" input line)
  				)
  				(pin bidirectional line
  					(at -35.56 -50.8 0)
  					(length 2.54)
  					(name "P0.31")
  					(number "B6")
  					(alternate "AIN7" input line)
  				)
  				(pin power_in line
  					(at -5.08 83.82 270)
  					(length 2.54)
  					(name "VBUS")
  					(number "H8")
  				)
  				(pin passive line
  					(at 0 83.82 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "A9")
  				)
  				(pin passive line
  					(at 0 83.82 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "B3")
  				)
  				(pin passive line
  					(at 0 83.82 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "G9")
  				)
  				(pin passive line
  					(at 0 83.82 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "J1")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "A7")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS_PA")
  					(number "C1")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D3")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D4")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D5")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E4")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E5")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "E6")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "F4")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "F5")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "F6")
  				)
  				(pin passive line
  					(at 0 -83.82 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "J9")
  				)
  				(pin passive line
  					(at 35.56 71.12 180)
  					(length 2.54)
  					(name "DEC1")
  					(number "B9")
  				)
  				(pin passive line
  					(at 35.56 68.58 180)
  					(length 2.54)
  					(name "DEC4")
  					(number "A6")
  				)
  				(pin passive line
  					(at 35.56 66.04 180)
  					(length 2.54)
  					(name "DEC5")
  					(number "F1")
  					(alternate "NC" no_connect line)
  				)
  				(pin passive line
  					(at 35.56 63.5 180)
  					(length 2.54)
  					(name "DEC6")
  					(number "C2")
  				)
  				(pin bidirectional line
  					(at 35.56 -43.18 180)
  					(length 2.54)
  					(name "P1.00")
  					(number "H3")
  					(alternate "TRACEDATA[0]" output line)
  				)
  				(pin bidirectional line
  					(at 35.56 -45.72 180)
  					(length 2.54)
  					(name "P0.12")
  					(number "H6")
  					(alternate "TRACEDATA[1]" output line)
  				)
  				(pin bidirectional line
  					(at 35.56 -48.26 180)
  					(length 2.54)
  					(name "P0.11")
  					(number "G8")
  					(alternate "TRACEDATA[2]" output line)
  				)
  				(pin bidirectional line
  					(at 35.56 -50.8 180)
  					(length 2.54)
  					(name "P1.09")
  					(number "F8")
  					(alternate "TRACEDATA[3]" output line)
  				)
  				(pin bidirectional line
  					(at 35.56 -53.34 180)
  					(length 2.54)
  					(name "P0.07")
  					(number "E8")
  					(alternate "TRACECLK" input line)
  				)
  				(pin input line
  					(at 35.56 -63.5 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "H4")
  					(alternate "P0.18" bidirectional line)
  				)
  			)
  			(symbol "nordic_nrf52833_cjxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf52840_ckxx"
        (property "Footprint" "PartReel:nordic_nrf52840_ckxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf52840/attach/nRF52840_PS_v1.11.pdf?_LANG=enus"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.4GHz Bluetooth 5.4 USB NFC SoC, 64MHz Cortex-M4 FPU, CryptoCell, PDM, I2S, QSPI, CSP-94."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless ble bluetooth-low-energy bluetooth-mesh thread zigbee arm microcontroller wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf52840_ckxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF52840-CKXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA?94*10x10*3.544x3.607mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf52840_ckxx_0_0"
  				(pin bidirectional line
  					(at -34.29 76.2 0)
  					(length 3.81)
  					(name "D+")
  					(number "K8")
  				)
  				(pin bidirectional line
  					(at -34.29 73.66 0)
  					(length 3.81)
  					(name "D-")
  					(number "J8")
  				)
  				(pin input line
  					(at -34.29 63.5 0)
  					(length 3.81)
  					(name "XC1")
  					(number "A1")
  				)
  				(pin input line
  					(at -34.29 58.42 0)
  					(length 3.81)
  					(name "XC2")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -34.29 7.62 0)
  					(length 3.81)
  					(name "P0.06")
  					(number "E9")
  				)
  				(pin bidirectional line
  					(at -34.29 5.08 0)
  					(length 3.81)
  					(name "P0.08")
  					(number "E10")
  				)
  				(pin bidirectional line
  					(at -34.29 2.54 0)
  					(length 3.81)
  					(name "P0.13")
  					(number "H7")
  				)
  				(pin bidirectional line
  					(at -34.29 0 0)
  					(length 3.81)
  					(name "P0.14")
  					(number "J7")
  				)
  				(pin bidirectional line
  					(at -34.29 -2.54 0)
  					(length 3.81)
  					(name "P0.15")
  					(number "K7")
  				)
  				(pin bidirectional line
  					(at -34.29 -5.08 0)
  					(length 3.81)
  					(name "P0.16")
  					(number "H6")
  				)
  				(pin bidirectional line
  					(at -34.29 -7.62 0)
  					(length 3.81)
  					(name "P0.17")
  					(number "J6")
  				)
  				(pin bidirectional line
  					(at -34.29 -10.16 0)
  					(length 3.81)
  					(name "P0.19")
  					(number "K4")
  				)
  				(pin bidirectional line
  					(at -34.29 -12.7 0)
  					(length 3.81)
  					(name "P0.20")
  					(number "J5")
  				)
  				(pin bidirectional line
  					(at -34.29 -15.24 0)
  					(length 3.81)
  					(name "P0.21")
  					(number "J4")
  				)
  				(pin bidirectional line
  					(at -34.29 -17.78 0)
  					(length 3.81)
  					(name "P0.22")
  					(number "K3")
  				)
  				(pin bidirectional line
  					(at -34.29 -20.32 0)
  					(length 3.81)
  					(name "P0.23")
  					(number "H5")
  				)
  				(pin bidirectional line
  					(at -34.29 -22.86 0)
  					(length 3.81)
  					(name "P0.24")
  					(number "H4")
  				)
  				(pin bidirectional line
  					(at -34.29 -25.4 0)
  					(length 3.81)
  					(name "P0.25")
  					(number "K2")
  				)
  				(pin bidirectional line
  					(at -34.29 -27.94 0)
  					(length 3.81)
  					(name "P0.26")
  					(number "C9")
  				)
  				(pin bidirectional line
  					(at -34.29 -30.48 0)
  					(length 3.81)
  					(name "P0.27")
  					(number "D9")
  				)
  				(pin bidirectional line
  					(at -34.29 -43.18 0)
  					(length 3.81)
  					(name "P1.01")
  					(number "J1")
  				)
  				(pin bidirectional line
  					(at -34.29 -45.72 0)
  					(length 3.81)
  					(name "P1.02")
  					(number "G3")
  				)
  				(pin bidirectional line
  					(at -34.29 -48.26 0)
  					(length 3.81)
  					(name "P1.03")
  					(number "F3")
  				)
  				(pin bidirectional line
  					(at -34.29 -50.8 0)
  					(length 3.81)
  					(name "P1.04")
  					(number "H1")
  				)
  				(pin bidirectional line
  					(at -34.29 -53.34 0)
  					(length 3.81)
  					(name "P1.05")
  					(number "G2")
  				)
  				(pin bidirectional line
  					(at -34.29 -55.88 0)
  					(length 3.81)
  					(name "P1.06")
  					(number "E3")
  				)
  				(pin bidirectional line
  					(at -34.29 -58.42 0)
  					(length 3.81)
  					(name "P1.07")
  					(number "G1")
  				)
  				(pin bidirectional line
  					(at -34.29 -60.96 0)
  					(length 3.81)
  					(name "P1.08")
  					(number "G9")
  				)
  				(pin bidirectional line
  					(at -34.29 -63.5 0)
  					(length 3.81)
  					(name "P1.10")
  					(number "B4")
  				)
  				(pin bidirectional line
  					(at -34.29 -66.04 0)
  					(length 3.81)
  					(name "P1.11")
  					(number "A3")
  				)
  				(pin bidirectional line
  					(at -34.29 -68.58 0)
  					(length 3.81)
  					(name "P1.12")
  					(number "C5")
  				)
  				(pin bidirectional line
  					(at -34.29 -71.12 0)
  					(length 3.81)
  					(name "P1.13")
  					(number "A4")
  				)
  				(pin bidirectional line
  					(at -34.29 -73.66 0)
  					(length 3.81)
  					(name "P1.14")
  					(number "B5")
  				)
  				(pin bidirectional line
  					(at -34.29 -76.2 0)
  					(length 3.81)
  					(name "P1.15")
  					(number "C6")
  				)
  				(pin power_in line
  					(at -7.62 87.63 270)
  					(length 3.81)
  					(name "VBUS")
  					(number "J9")
  				)
  				(pin passive line
  					(at -2.54 87.63 270)
  					(length 3.81)
  					(name "VDD")
  					(number "K1")
  				)
  				(pin power_out line
  					(at 0 87.63 270)
  					(length 3.81)
  					(name "DCC")
  					(number "A9")
  				)
  				(pin power_in line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(name "VSS")
  					(number "K10")
  				)
  				(pin power_in line
  					(at 5.08 87.63 270)
  					(length 3.81)
  					(name "VDDH")
  					(number "J10")
  				)
  				(pin power_out line
  					(at 7.62 87.63 270)
  					(length 3.81)
  					(name "DCCH")
  					(number "H9")
  				)
  				(pin passive line
  					(at 34.29 66.04 180)
  					(length 3.81)
  					(name "DECUSB")
  					(number "K9")
  				)
  				(pin bidirectional line
  					(at 34.29 0 180)
  					(length 3.81)
  					(name "ANT")
  					(number "E1")
  				)
  				(pin input line
  					(at 34.29 -73.66 180)
  					(length 3.81)
  					(name "SWDCLK")
  					(number "H2")
  				)
  				(pin bidirectional line
  					(at 34.29 -76.2 180)
  					(length 3.81)
  					(name "SWDIO")
  					(number "J2")
  				)
  			)
  			(symbol "nordic_nrf52840_ckxx_1_0"
  				(pin bidirectional line
  					(at -34.29 48.26 0)
  					(length 3.81)
  					(name "P0.00")
  					(number "B9")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 43.18 0)
  					(length 3.81)
  					(name "P0.01")
  					(number "B10")
  					(alternate "XL2" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 33.02 0)
  					(length 3.81)
  					(name "P0.09")
  					(number "F1")
  					(alternate "NFC1" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 27.94 0)
  					(length 3.81)
  					(name "P0.10")
  					(number "E2")
  					(alternate "NFC2" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 17.78 0)
  					(length 3.81)
  					(name "P0.02")
  					(number "B6")
  					(alternate "AIN0" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 15.24 0)
  					(length 3.81)
  					(name "P0.03")
  					(number "A5")
  					(alternate "AIN1" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 12.7 0)
  					(length 3.81)
  					(name "P0.04")
  					(number "C10")
  					(alternate "AIN2" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 10.16 0)
  					(length 3.81)
  					(name "P0.05")
  					(number "D10")
  					(alternate "AIN3" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 -33.02 0)
  					(length 3.81)
  					(name "P0.28")
  					(number "A6")
  					(alternate "AIN4" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 -35.56 0)
  					(length 3.81)
  					(name "P0.29")
  					(number "C7")
  					(alternate "AIN5" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 -38.1 0)
  					(length 3.81)
  					(name "P0.30")
  					(number "A7")
  					(alternate "AIN6" input line)
  				)
  				(pin bidirectional line
  					(at -34.29 -40.64 0)
  					(length 3.81)
  					(name "P0.31")
  					(number "C8")
  					(alternate "AIN7" input line)
  				)
  				(pin passive line
  					(at -2.54 87.63 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "B3")
  				)
  				(pin passive line
  					(at -2.54 87.63 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "B8")
  				)
  				(pin passive line
  					(at -2.54 87.63 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "H10")
  				)
  				(pin passive line
  					(at -2.54 87.63 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "K5")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "B7")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS_PA")
  					(number "C1")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "C4")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "D3")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "D4")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "D5")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "D6")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "D7")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "D8")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "E4")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "E5")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "E6")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "E7")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "E8")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "F4")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "F5")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "F6")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "F7")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "F8")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "G4")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "G5")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "G6")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "G7")
  				)
  				(pin passive line
  					(at 0 -87.63 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "G8")
  				)
  				(pin passive line
  					(at 34.29 76.2 180)
  					(length 3.81)
  					(name "DEC1")
  					(number "A10")
  				)
  				(pin passive line
  					(at 34.29 73.66 180)
  					(length 3.81)
  					(name "DEC4")
  					(number "A8")
  				)
  				(pin passive line
  					(at 34.29 71.12 180)
  					(length 3.81)
  					(name "DEC5/NC")
  					(number "F2")
  				)
  				(pin passive line
  					(at 34.29 68.58 180)
  					(length 3.81)
  					(name "DEC6")
  					(number "C2")
  				)
  				(pin bidirectional line
  					(at 34.29 -48.26 180)
  					(length 3.81)
  					(name "P1.00")
  					(number "J3")
  					(alternate "TRACEDATA[0]" output line)
  				)
  				(pin bidirectional line
  					(at 34.29 -50.8 180)
  					(length 3.81)
  					(name "P0.12")
  					(number "G10")
  					(alternate "TRACEDATA[1]" output line)
  				)
  				(pin bidirectional line
  					(at 34.29 -53.34 180)
  					(length 3.81)
  					(name "P0.11")
  					(number "H8")
  					(alternate "TRACEDATA[2]" output line)
  				)
  				(pin bidirectional line
  					(at 34.29 -55.88 180)
  					(length 3.81)
  					(name "P1.09")
  					(number "F10")
  					(alternate "TRACEDATA[3]" output line)
  				)
  				(pin bidirectional line
  					(at 34.29 -58.42 180)
  					(length 3.81)
  					(name "P0.07")
  					(number "F9")
  					(alternate "TRACECLK" input line)
  				)
  				(pin input line
  					(at 34.29 -68.58 180)
  					(length 3.81)
  					(name "~{RESET}")
  					(number "K6")
  					(alternate "P0.18" bidirectional line)
  				)
  			)
  			(symbol "nordic_nrf52840_ckxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf5340_clxx"
        (property "Footprint" "PartReel:nordic_nrf5340_clxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf5340/attach/nRF5340_PS_v1.5.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF5340-CLXX."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf5340_clxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF5340-CLXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_locked" ""
  				(at 0 0 0)
  			)
  			(property "ki_fp_filters" "BGA?132*12x11*4.39x3.994mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf5340_clxx_1_0"
  				(pin bidirectional line
  					(at -30.48 58.42 0)
  					(length 5.08)
  					(name "XC1")
  					(number "A1")
  				)
  				(pin bidirectional line
  					(at -30.48 53.34 0)
  					(length 5.08)
  					(name "XC2")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -30.48 43.18 0)
  					(length 5.08)
  					(name "P0.00/XL1")
  					(number "F11")
  				)
  				(pin bidirectional line
  					(at -30.48 38.1 0)
  					(length 5.08)
  					(name "P0.01/XL2")
  					(number "F12")
  				)
  				(pin bidirectional line
  					(at -30.48 25.4 0)
  					(length 5.08)
  					(name "D+")
  					(number "A12")
  				)
  				(pin bidirectional line
  					(at -30.48 22.86 0)
  					(length 5.08)
  					(name "D-")
  					(number "A11")
  				)
  				(pin bidirectional line
  					(at -30.48 15.24 0)
  					(length 5.08)
  					(name "P0.02/NFC1")
  					(number "G11")
  				)
  				(pin bidirectional line
  					(at -30.48 12.7 0)
  					(length 5.08)
  					(name "P0.03/NFC2")
  					(number "H12")
  				)
  				(pin bidirectional line
  					(at -30.48 5.08 0)
  					(length 5.08)
  					(name "P0.04/AIN0")
  					(number "G10")
  				)
  				(pin bidirectional line
  					(at -30.48 2.54 0)
  					(length 5.08)
  					(name "P0.05/AIN1")
  					(number "F10")
  				)
  				(pin bidirectional line
  					(at -30.48 0 0)
  					(length 5.08)
  					(name "P0.06/AIN2")
  					(number "H10")
  				)
  				(pin bidirectional line
  					(at -30.48 -2.54 0)
  					(length 5.08)
  					(name "P0.07/AIN3")
  					(number "J10")
  				)
  				(pin bidirectional line
  					(at -30.48 -5.08 0)
  					(length 5.08)
  					(name "P0.25/AIN4")
  					(number "L1")
  				)
  				(pin bidirectional line
  					(at -30.48 -7.62 0)
  					(length 5.08)
  					(name "P0.26/AIN5")
  					(number "J2")
  				)
  				(pin bidirectional line
  					(at -30.48 -10.16 0)
  					(length 5.08)
  					(name "P0.27/AIN6")
  					(number "H1")
  				)
  				(pin bidirectional line
  					(at -30.48 -12.7 0)
  					(length 5.08)
  					(name "P0.28/AIN7")
  					(number "E3")
  				)
  				(pin bidirectional line
  					(at -30.48 -20.32 0)
  					(length 5.08)
  					(name "P1.02/TWI")
  					(number "J11")
  				)
  				(pin bidirectional line
  					(at -30.48 -22.86 0)
  					(length 5.08)
  					(name "P1.03/TWI")
  					(number "K12")
  				)
  				(pin bidirectional line
  					(at -30.48 -30.48 0)
  					(length 5.08)
  					(name "P0.13/IO0")
  					(number "K10")
  				)
  				(pin bidirectional line
  					(at -30.48 -33.02 0)
  					(length 5.08)
  					(name "P0.14/IO1")
  					(number "K9")
  				)
  				(pin bidirectional line
  					(at -30.48 -35.56 0)
  					(length 5.08)
  					(name "P0.15/IO2")
  					(number "L9")
  				)
  				(pin bidirectional line
  					(at -30.48 -38.1 0)
  					(length 5.08)
  					(name "P0.16/IO3")
  					(number "K8")
  				)
  				(pin bidirectional line
  					(at -30.48 -40.64 0)
  					(length 5.08)
  					(name "P0.17/SCK")
  					(number "L7")
  				)
  				(pin bidirectional line
  					(at -30.48 -43.18 0)
  					(length 5.08)
  					(name "P0.18/~{CS}")
  					(number "K7")
  				)
  				(pin bidirectional line
  					(at -30.48 -50.8 0)
  					(length 5.08)
  					(name "P0.09/TRACEDATA2/MOSI")
  					(number "J9")
  				)
  				(pin bidirectional line
  					(at -30.48 -53.34 0)
  					(length 5.08)
  					(name "P0.10/TRACEDATA1/MISO")
  					(number "J8")
  				)
  				(pin bidirectional line
  					(at -30.48 -55.88 0)
  					(length 5.08)
  					(name "P0.08/TRACEDATA3/SCK")
  					(number "L12")
  				)
  				(pin bidirectional line
  					(at -30.48 -58.42 0)
  					(length 5.08)
  					(name "P0.11/TRACEDATA0/~{CS}")
  					(number "J7")
  				)
  				(pin bidirectional line
  					(at -30.48 -60.96 0)
  					(length 5.08)
  					(name "P0.12/TRACECLK/DCX")
  					(number "J6")
  				)
  				(pin bidirectional line
  					(at 30.48 58.42 180)
  					(length 5.08)
  					(name "P0.19")
  					(number "J5")
  				)
  				(pin bidirectional line
  					(at 30.48 55.88 180)
  					(length 5.08)
  					(name "P0.20")
  					(number "K5")
  				)
  				(pin bidirectional line
  					(at 30.48 53.34 180)
  					(length 5.08)
  					(name "P0.21")
  					(number "J4")
  				)
  				(pin bidirectional line
  					(at 30.48 50.8 180)
  					(length 5.08)
  					(name "P0.22")
  					(number "K4")
  				)
  				(pin bidirectional line
  					(at 30.48 48.26 180)
  					(length 5.08)
  					(name "P0.23")
  					(number "H3")
  				)
  				(pin bidirectional line
  					(at 30.48 45.72 180)
  					(length 5.08)
  					(name "P0.24")
  					(number "K2")
  				)
  				(pin bidirectional line
  					(at 30.48 43.18 180)
  					(length 5.08)
  					(name "P0.29")
  					(number "E2")
  				)
  				(pin bidirectional line
  					(at 30.48 40.64 180)
  					(length 5.08)
  					(name "P0.30")
  					(number "C4")
  				)
  				(pin bidirectional line
  					(at 30.48 38.1 180)
  					(length 5.08)
  					(name "P0.31")
  					(number "C5")
  				)
  				(pin bidirectional line
  					(at 30.48 35.56 180)
  					(length 5.08)
  					(name "P1.00")
  					(number "D10")
  				)
  				(pin bidirectional line
  					(at 30.48 33.02 180)
  					(length 5.08)
  					(name "P1.01")
  					(number "E10")
  				)
  				(pin bidirectional line
  					(at 30.48 30.48 180)
  					(length 5.08)
  					(name "P1.04")
  					(number "K3")
  				)
  				(pin bidirectional line
  					(at 30.48 27.94 180)
  					(length 5.08)
  					(name "P1.05")
  					(number "L3")
  				)
  				(pin bidirectional line
  					(at 30.48 25.4 180)
  					(length 5.08)
  					(name "P1.06")
  					(number "J3")
  				)
  				(pin bidirectional line
  					(at 30.48 22.86 180)
  					(length 5.08)
  					(name "P1.07")
  					(number "G3")
  				)
  				(pin bidirectional line
  					(at 30.48 20.32 180)
  					(length 5.08)
  					(name "P1.08")
  					(number "F3")
  				)
  				(pin bidirectional line
  					(at 30.48 17.78 180)
  					(length 5.08)
  					(name "P1.09")
  					(number "H2")
  				)
  				(pin bidirectional line
  					(at 30.48 15.24 180)
  					(length 5.08)
  					(name "P1.10")
  					(number "E4")
  				)
  				(pin bidirectional line
  					(at 30.48 12.7 180)
  					(length 5.08)
  					(name "P1.11")
  					(number "C6")
  				)
  				(pin bidirectional line
  					(at 30.48 10.16 180)
  					(length 5.08)
  					(name "P1.12")
  					(number "C7")
  				)
  				(pin bidirectional line
  					(at 30.48 7.62 180)
  					(length 5.08)
  					(name "P1.13")
  					(number "C8")
  				)
  				(pin bidirectional line
  					(at 30.48 5.08 180)
  					(length 5.08)
  					(name "P1.14")
  					(number "C9")
  				)
  				(pin bidirectional line
  					(at 30.48 2.54 180)
  					(length 5.08)
  					(name "P1.15")
  					(number "C10")
  				)
  				(pin bidirectional line
  					(at 30.48 -7.62 180)
  					(length 5.08)
  					(name "ANT")
  					(number "D1")
  				)
  				(pin input line
  					(at 30.48 -17.78 180)
  					(length 5.08)
  					(name "~{RESET}")
  					(number "G2")
  				)
  				(pin input line
  					(at 30.48 -22.86 180)
  					(length 5.08)
  					(name "SWDCLK")
  					(number "F2")
  				)
  				(pin bidirectional line
  					(at 30.48 -25.4 180)
  					(length 5.08)
  					(name "SWDIO")
  					(number "F1")
  				)
  			)
  			(symbol "nordic_nrf5340_clxx_1_1"
  				(text "nordic_nrf5340_clxx\nI/O"
  					(at 0 -5.08 0)
  				)
  			)
  			(symbol "nordic_nrf5340_clxx_2_0"
  				(pin passive line
  					(at -22.86 7.62 0)
  					(length 5.08)
  					(name "DCC")
  					(number "B6")
  				)
  				(pin passive line
  					(at -22.86 2.54 0)
  					(length 5.08)
  					(name "DECR")
  					(number "B4")
  				)
  				(pin passive line
  					(at -22.86 0 0)
  					(length 5.08)
  					(name "DECRF")
  					(number "B1")
  				)
  				(pin passive line
  					(at -22.86 -5.08 0)
  					(length 5.08)
  					(name "DCCD")
  					(number "A9")
  				)
  				(pin passive line
  					(at -22.86 -10.16 0)
  					(length 5.08)
  					(name "DECD")
  					(number "A7")
  				)
  				(pin passive line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(hide yes)
  					(name "VDD")
  					(number "B10")
  				)
  				(pin passive line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(hide yes)
  					(name "VDD")
  					(number "B7")
  				)
  				(pin passive line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(hide yes)
  					(name "VDD")
  					(number "D2")
  				)
  				(pin passive line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(hide yes)
  					(name "VDD")
  					(number "E11")
  				)
  				(pin power_in line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(name "VDD")
  					(number "H11")
  				)
  				(pin passive line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(hide yes)
  					(name "VDD")
  					(number "K1")
  				)
  				(pin passive line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(hide yes)
  					(name "VDD")
  					(number "L11")
  				)
  				(pin passive line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(hide yes)
  					(name "VDD")
  					(number "L5")
  				)
  				(pin power_in line
  					(at 0 20.32 270)
  					(length 5.08)
  					(name "VDDH")
  					(number "B12")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "A5")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "B2")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "B9")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "C2")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "D12")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "E5")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "E6")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "E7")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "E8")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "F5")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "F6")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "F7")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "F8")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "AVSS")
  					(number "G5")
  				)
  				(pin power_in line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(name "VSS")
  					(number "G6")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "G7")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "VSS")
  					(number "G8")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "AVSS")
  					(number "K11")
  				)
  				(pin passive line
  					(at 0 -20.32 90)
  					(length 5.08)
  					(hide yes)
  					(name "AVSS")
  					(number "K6")
  				)
  				(pin power_in line
  					(at 2.54 20.32 270)
  					(length 5.08)
  					(name "VBUS")
  					(number "B11")
  				)
  				(pin passive line
  					(at 22.86 7.62 180)
  					(length 5.08)
  					(name "DECA")
  					(number "B8")
  				)
  				(pin passive line
  					(at 22.86 5.08 180)
  					(length 5.08)
  					(name "DECN")
  					(number "B5")
  				)
  				(pin passive line
  					(at 22.86 -5.08 180)
  					(length 5.08)
  					(name "DCCH")
  					(number "D11")
  				)
  				(pin passive line
  					(at 22.86 -7.62 180)
  					(length 5.08)
  					(name "DECUSB")
  					(number "C11")
  				)
  			)
  			(symbol "nordic_nrf5340_clxx_2_1"
  				(text "nordic_nrf5340_clxx\nPWR"
  					(at 0 -5.08 0)
  				)
  				(pin passive line
  					(at -2.54 20.32 270)
  					(length 5.08)
  					(hide yes)
  					(name "VDD")
  					(number "A3")
  				)
  			)
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf54l15_caxx"
        (property "Footprint" "PartReel:nordic_nrf54l15_caxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf54L15/page/keyfeatures_html5.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF54L Dual Core Multiprotocol BLE SoC."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless BLE SoC nRF"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf54l15_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(in_pos_files yes)
  			(duplicate_pin_numbers_are_jumpers no)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "Value" "nRF54L15-CAXX"
  				(at 0 -2.54 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_fp_filters" "BGA?47*7x7*2.451x2.245mm*"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  				(hide yes)
  			)
  			(symbol "nordic_nrf54l15_caxx_1_0"
  				(pin bidirectional line
  					(at -27.94 50.8 0)
  					(length 2.54)
  					(name "XC1")
  					(number "A1")
  				)
  				(pin bidirectional line
  					(at -27.94 45.72 0)
  					(length 2.54)
  					(name "XC2")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -27.94 -15.24 0)
  					(length 2.54)
  					(name "P1.12")
  					(number "A3")
  					(alternate "AIN5" input line)
  					(alternate "ASI[3]" input line)
  					(alternate "RADIO[3]" bidirectional line)
  				)
  				(pin passive line
  					(at 27.94 50.8 180)
  					(length 2.54)
  					(name "DECA")
  					(number "A4")
  				)
  				(pin passive line
  					(at 27.94 45.72 180)
  					(length 2.54)
  					(name "DECD")
  					(number "A5")
  				)
  				(pin power_in line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(name "VSS")
  					(number "A6")
  				)
  				(pin power_out line
  					(at 27.94 40.64 180)
  					(length 2.54)
  					(name "DCC")
  					(number "A7")
  				)
  				(pin bidirectional line
  					(at -27.94 -7.62 0)
  					(length 2.54)
  					(name "P1.09")
  					(number "B3")
  					(alternate "ASO[2]" output line)
  					(alternate "RADIO[0]" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 -17.78 0)
  					(length 2.54)
  					(name "P1.13")
  					(number "B4")
  					(alternate "AIN6" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -20.32 0)
  					(length 2.54)
  					(name "P1.14")
  					(number "B5")
  					(alternate "AIN7" input line)
  					(alternate "RADIO[5]" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 -22.86 0)
  					(length 2.54)
  					(name "P1.15")
  					(number "B6")
  				)
  				(pin power_in line
  					(at 0 58.42 270)
  					(length 2.54)
  					(name "VDD")
  					(number "B7")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS_PA")
  					(number "C2")
  				)
  				(pin bidirectional line
  					(at -27.94 -10.16 0)
  					(length 2.54)
  					(name "P1.10")
  					(number "C3")
  					(alternate "ASI[2]" input line)
  					(alternate "RADIO[1]" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 -12.7 0)
  					(length 2.54)
  					(name "P1.11")
  					(number "C4")
  					(alternate "AIN4" input line)
  					(alternate "ASO[3]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 38.1 0)
  					(length 2.54)
  					(name "P1.00")
  					(number "C5")
  					(alternate "XL1" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 33.02 0)
  					(length 2.54)
  					(name "P1.01")
  					(number "C6")
  					(alternate "XL2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 10.16 0)
  					(length 2.54)
  					(name "P1.02")
  					(number "C7")
  					(alternate "NFC1" bidirectional line)
  				)
  				(pin output line
  					(at 27.94 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "D1")
  				)
  				(pin input line
  					(at 27.94 -43.18 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "D2")
  				)
  				(pin bidirectional line
  					(at -27.94 15.24 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "D3")
  					(alternate "GRTCLFCLKOUT" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -48.26 0)
  					(length 2.54)
  					(name "P2.08")
  					(number "D4")
  					(alternate "SPIM_MOSI" output line)
  					(alternate "SPIS_MISO" input line)
  					(alternate "TRACEDATA[1]" output line)
  					(alternate "UARTE_TXD" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 7.62 0)
  					(length 2.54)
  					(name "P1.03")
  					(number "D5")
  					(alternate "NFC2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 5.08 0)
  					(length 2.54)
  					(name "P1.04")
  					(number "D6")
  					(alternate "AIN0" input line)
  					(alternate "ASO[0]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 0 0)
  					(length 2.54)
  					(name "P1.06")
  					(number "D7")
  					(alternate "AIN2" input line)
  					(alternate "ASO[1]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 17.78 0)
  					(length 2.54)
  					(name "P0.03")
  					(number "E1")
  					(alternate "GRTCPWM" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 20.32 0)
  					(length 2.54)
  					(name "P0.02")
  					(number "E2")
  				)
  				(pin input line
  					(at 27.94 -48.26 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "E3")
  				)
  				(pin bidirectional line
  					(at -27.94 -45.72 0)
  					(length 2.54)
  					(name "P2.07")
  					(number "E4")
  					(alternate "SPIM_DCX" output line)
  					(alternate "SWO" output line)
  					(alternate "TRACEDATA[0]" output line)
  					(alternate "UARTE_RXD" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -35.56 0)
  					(length 2.54)
  					(name "P2.03")
  					(number "E5")
  					(alternate "QSPI_D2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 2.54 0)
  					(length 2.54)
  					(name "P1.05")
  					(number "E6")
  					(alternate "AIN1" bidirectional line)
  					(alternate "ASI[0]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -2.54 0)
  					(length 2.54)
  					(name "P1.07")
  					(number "E7")
  					(alternate "AIN3" input line)
  					(alternate "ASI[1]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 22.86 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "F1")
  				)
  				(pin bidirectional line
  					(at 27.94 -50.8 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "F2")
  				)
  				(pin bidirectional line
  					(at -27.94 -50.8 0)
  					(length 2.54)
  					(name "P2.09")
  					(number "F3")
  					(alternate "SPIM_MISO" input line)
  					(alternate "SPIS_MOSI" input line)
  					(alternate "TRACEDATA[2]" output line)
  					(alternate "UARTE_CTS" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -43.18 0)
  					(length 2.54)
  					(name "P2.06")
  					(number "F4")
  					(alternate "SPIM_SCK" output line)
  					(alternate "SPIS_SCK" input line)
  					(alternate "TRACE_CLK" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -38.1 0)
  					(length 2.54)
  					(name "P2.04")
  					(number "F5")
  					(alternate "QSPI_D1" bidirectional line)
  					(alternate "SPIM_MISO" input line)
  					(alternate "SPIS_MOSI" input line)
  					(alternate "UARTE_CTS" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -33.02 0)
  					(length 2.54)
  					(name "P2.02")
  					(number "F6")
  					(alternate "QSPI_D0" bidirectional line)
  					(alternate "SPIM_MOSI" output line)
  					(alternate "SPIS_MISO" output line)
  					(alternate "SWO" output line)
  					(alternate "UARTE_TXD" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -5.08 0)
  					(length 2.54)
  					(name "P1.08")
  					(number "F7")
  					(alternate "EXTREF" input line)
  					(alternate "GRTCHFOUT" output line)
  					(alternate "TAMPC.EXT" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 25.4 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "G1")
  				)
  				(pin bidirectional line
  					(at -27.94 -53.34 0)
  					(length 2.54)
  					(name "P2.10")
  					(number "G2")
  					(alternate "SPIM_CS" output line)
  					(alternate "TRACEDATA[3]" output line)
  					(alternate "UARTE_RTS" output line)
  				)
  				(pin passive line
  					(at 0 58.42 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "G3")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "G4")
  				)
  				(pin bidirectional line
  					(at -27.94 -40.64 0)
  					(length 2.54)
  					(name "P2.05")
  					(number "G5")
  					(alternate "QSPI_CS" output line)
  					(alternate "SPIM_CS" output line)
  					(alternate "UARTE_RTS" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -27.94 0)
  					(length 2.54)
  					(name "P2.00")
  					(number "G6")
  					(alternate "QSPI_D3" bidirectional line)
  					(alternate "SPIM_DCX" output line)
  					(alternate "UARTE_RXD" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -30.48 0)
  					(length 2.54)
  					(name "P2.01")
  					(number "G7")
  					(alternate "QSPI_SCK" output line)
  					(alternate "SPIM_SCK" output line)
  					(alternate "SPIS_SCK" output line)
  				)
  			)
  			(symbol "nordic_nrf54l15_caxx_1_1"
  				(text "CLK"
  					(at -15.24 17.78 0)
  				)
  				(text "CLK"
  					(at -15.24 15.24 0)
  				)
  				(text "CLK"
  					(at -15.24 7.62 0)
  				)
  				(text "CLK"
  					(at -15.24 5.08 0)
  				)
  				(text "CLK"
  					(at -15.24 -5.08 0)
  				)
  				(text "CLK"
  					(at -15.24 -12.7 0)
  				)
  				(text "CLK"
  					(at -15.24 -15.24 0)
  				)
  				(text "CLK"
  					(at -15.24 -30.48 0)
  				)
  				(text "CLK"
  					(at -15.24 -43.18 0)
  				)
  				(pin passive line
  					(at 27.94 48.26 180)
  					(length 2.54)
  					(name "DECRF")
  					(number "B1")
  				)
  			)
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf54l15_qgxx"
        (property "Footprint" "PartReel:nordic_nrf54l15_qgxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf54L15"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF54L Dual Core Multiprotocol BLE SoC."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless BLE SoC nRF QFN48"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf54l15_qgxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(in_pos_files yes)
  			(duplicate_pin_numbers_are_jumpers no)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace yes)
  			)
  			(property "Value" "nRF54L15-QGXX"
  				(at 0 -2.54 0)
  				(show_name no)
  				(do_not_autoplace yes)
  			)
  			(property "ki_fp_filters" "QFN*52*1EP*6x6mm*P0.4mm*EP4.7x4.7mm*"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  				(hide yes)
  			)
  			(symbol "nordic_nrf54l15_qgxx_1_0"
  				(pin bidirectional line
  					(at -27.94 43.18 0)
  					(length 2.54)
  					(name "P1.00")
  					(number "1")
  					(alternate "XL1" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 38.1 0)
  					(length 2.54)
  					(name "P1.01")
  					(number "2")
  					(alternate "XL2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 10.16 0)
  					(length 2.54)
  					(name "P1.02")
  					(number "3")
  					(alternate "NFC1" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 7.62 0)
  					(length 2.54)
  					(name "P1.03")
  					(number "4")
  					(alternate "NFC2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 5.08 0)
  					(length 2.54)
  					(name "P1.04")
  					(number "5")
  					(alternate "AIN0" input line)
  					(alternate "ASO[0]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -25.4 0)
  					(length 2.54)
  					(name "P1.16")
  					(number "6")
  				)
  				(pin bidirectional line
  					(at -27.94 2.54 0)
  					(length 2.54)
  					(name "P1.05")
  					(number "7")
  					(alternate "AIN1" bidirectional line)
  					(alternate "ASI[0]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 0 0)
  					(length 2.54)
  					(name "P1.06")
  					(number "8")
  					(alternate "AIN2" input line)
  					(alternate "ASO[1]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -2.54 0)
  					(length 2.54)
  					(name "P1.07")
  					(number "9")
  					(alternate "AIN3" input line)
  					(alternate "ASI[1]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -5.08 0)
  					(length 2.54)
  					(name "P1.08")
  					(number "10")
  					(alternate "EXTREF" input line)
  					(alternate "GRTCHFOUT" output line)
  					(alternate "TAMPC.EXT" bidirectional line)
  				)
  				(pin power_in line
  					(at 0 63.5 270)
  					(length 2.54)
  					(name "VDD")
  					(number "11")
  				)
  				(pin bidirectional line
  					(at -27.94 -30.48 0)
  					(length 2.54)
  					(name "P2.00")
  					(number "12")
  					(alternate "QSPI_D3" bidirectional line)
  					(alternate "SPIM_DCX" output line)
  					(alternate "UARTE_RXD" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -33.02 0)
  					(length 2.54)
  					(name "P2.01")
  					(number "13")
  					(alternate "QSPI_SCK" output line)
  					(alternate "SPIM_SCK" output line)
  					(alternate "SPIS_SCK" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -35.56 0)
  					(length 2.54)
  					(name "P2.02")
  					(number "14")
  					(alternate "QSPI_D0" bidirectional line)
  					(alternate "SPIM_MOSI" output line)
  					(alternate "SPIS_MISO" output line)
  					(alternate "SWO" output line)
  					(alternate "UARTE_TXD" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -38.1 0)
  					(length 2.54)
  					(name "P2.03")
  					(number "15")
  					(alternate "QSPI_D2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 -40.64 0)
  					(length 2.54)
  					(name "P2.04")
  					(number "16")
  					(alternate "QSPI_D1" bidirectional line)
  					(alternate "SPIM_MISO" input line)
  					(alternate "SPIS_MOSI" input line)
  					(alternate "UARTE_CTS" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -43.18 0)
  					(length 2.54)
  					(name "P2.05")
  					(number "17")
  					(alternate "QSPI_CS" output line)
  					(alternate "SPIM_CS" output line)
  					(alternate "UARTE_RTS" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -45.72 0)
  					(length 2.54)
  					(name "P2.06")
  					(number "18")
  					(alternate "SPIM_SCK" output line)
  					(alternate "SPIS_SCK" input line)
  					(alternate "TRACE_CLK" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -48.26 0)
  					(length 2.54)
  					(name "P2.07")
  					(number "19")
  					(alternate "SPIM_DCX" output line)
  					(alternate "SWO" output line)
  					(alternate "TRACEDATA[0]" output line)
  					(alternate "UARTE_RXD" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -50.8 0)
  					(length 2.54)
  					(name "P2.08")
  					(number "20")
  					(alternate "SPIM_MOSI" output line)
  					(alternate "SPIS_MISO" input line)
  					(alternate "TRACEDATA[1]" output line)
  					(alternate "UARTE_TXD" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -53.34 0)
  					(length 2.54)
  					(name "P2.09")
  					(number "21")
  					(alternate "SPIM_MISO" input line)
  					(alternate "SPIS_MOSI" input line)
  					(alternate "TRACEDATA[2]" output line)
  					(alternate "UARTE_CTS" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -55.88 0)
  					(length 2.54)
  					(name "P2.10")
  					(number "22")
  					(alternate "SPIM_CS" output line)
  					(alternate "TRACEDATA[3]" output line)
  					(alternate "UARTE_RTS" output line)
  				)
  				(pin passive line
  					(at 0 63.5 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "23")
  				)
  				(pin bidirectional line
  					(at -27.94 15.24 0)
  					(length 2.54)
  					(name "P0.06")
  					(number "24")
  					(alternate "GRTCLFCLKOUT" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 30.48 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "25")
  				)
  				(pin bidirectional line
  					(at -27.94 27.94 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "26")
  				)
  				(pin bidirectional line
  					(at 27.94 -55.88 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "27")
  				)
  				(pin input line
  					(at 27.94 -53.34 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "28")
  				)
  				(pin bidirectional line
  					(at -27.94 25.4 0)
  					(length 2.54)
  					(name "P0.02")
  					(number "29")
  				)
  				(pin bidirectional line
  					(at -27.94 22.86 0)
  					(length 2.54)
  					(name "P0.03")
  					(number "30")
  					(alternate "GRTCPWM" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 20.32 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "31")
  					(alternate "GRTCLFCLKOUT" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 17.78 0)
  					(length 2.54)
  					(name "P0.05")
  					(number "32")
  					(alternate "GRTCLFCLKOUT" output line)
  				)
  				(pin input line
  					(at 27.94 -48.26 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "33")
  				)
  				(pin output line
  					(at 27.94 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "34")
  				)
  				(pin passive line
  					(at 0 -63.5 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS_PA")
  					(number "35")
  				)
  				(pin passive line
  					(at 27.94 53.34 180)
  					(length 2.54)
  					(name "DECRF")
  					(number "36")
  				)
  				(pin bidirectional line
  					(at -27.94 55.88 0)
  					(length 2.54)
  					(name "XC1")
  					(number "37")
  				)
  				(pin bidirectional line
  					(at -27.94 50.8 0)
  					(length 2.54)
  					(name "XC2")
  					(number "38")
  				)
  				(pin passive line
  					(at 0 63.5 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "39")
  				)
  				(pin bidirectional line
  					(at -27.94 -7.62 0)
  					(length 2.54)
  					(name "P1.09")
  					(number "40")
  					(alternate "ASO[2]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -10.16 0)
  					(length 2.54)
  					(name "P1.10")
  					(number "41")
  					(alternate "ASI[2]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -12.7 0)
  					(length 2.54)
  					(name "P1.11")
  					(number "42")
  					(alternate "AIN4" input line)
  					(alternate "ASO[3]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -15.24 0)
  					(length 2.54)
  					(name "P1.12")
  					(number "43")
  					(alternate "AIN5" input line)
  					(alternate "ASI[3]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -17.78 0)
  					(length 2.54)
  					(name "P1.13")
  					(number "44")
  					(alternate "AIN6" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -20.32 0)
  					(length 2.54)
  					(name "P1.14")
  					(number "45")
  					(alternate "AIN7" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -22.86 0)
  					(length 2.54)
  					(name "P1.15")
  					(number "46")
  				)
  				(pin passive line
  					(at 27.94 55.88 180)
  					(length 2.54)
  					(name "DECA")
  					(number "47")
  				)
  				(pin power_in line
  					(at 0 -63.5 90)
  					(length 2.54)
  					(name "VSS")
  					(number "48")
  				)
  				(pin passive line
  					(at 27.94 50.8 180)
  					(length 2.54)
  					(name "DECD")
  					(number "49")
  				)
  				(pin power_out line
  					(at 27.94 45.72 180)
  					(length 2.54)
  					(name "DCC")
  					(number "50")
  				)
  				(pin passive line
  					(at 0 63.5 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "51")
  				)
  				(pin passive line
  					(at 0 63.5 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "52")
  				)
  				(pin passive line
  					(at 0 -63.5 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "53")
  				)
  			)
  			(symbol "nordic_nrf54l15_qgxx_1_1"
  				(text "CLK"
  					(at -15.24 22.86 0)
  				)
  				(text "CLK"
  					(at -15.24 20.32 0)
  				)
  				(text "CLK"
  					(at -15.24 7.62 0)
  				)
  				(text "CLK"
  					(at -15.24 5.08 0)
  				)
  				(text "CLK"
  					(at -15.24 -5.08 0)
  				)
  				(text "CLK"
  					(at -15.24 -12.7 0)
  				)
  				(text "CLK"
  					(at -15.24 -15.24 0)
  				)
  				(text "CLK"
  					(at -15.24 -33.02 0)
  				)
  				(text "CLK"
  					(at -15.24 -45.72 0)
  				)
  			)
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf54lm20a_paxx"
        (property "Footprint" "PartReel:nordic_nrf54lm20a_paxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf54LM20A/page/pdf/nRF54LM20A_Preliminary_Datasheet_v0.7.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF54LM20A-PAXX."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf54lm20a_paxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(in_pos_files yes)
  			(duplicate_pin_numbers_are_jumpers no)
  			(property "Reference" "U"
  				(at 0 1.27 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "Value" "nRF54LM20A-PAXX"
  				(at 0 -1.27 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_locked" ""
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_fp_filters" "Nordic?FCCSP?98*3.67x3.85mm*P0.35mm*"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  				(hide yes)
  			)
  			(symbol "nordic_nrf54lm20a_paxx_1_0"
  				(pin power_in line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(name "VSS")
  					(number "A1")
  				)
  				(pin input line
  					(at -19.05 15.24 0)
  					(length 3.81)
  					(name "XC1")
  					(number "A2")
  				)
  				(pin power_in line
  					(at 0 34.29 270)
  					(length 3.81)
  					(name "VDD")
  					(number "A3")
  				)
  				(pin passive line
  					(at 0 34.29 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "A4")
  				)
  				(pin passive line
  					(at 19.05 25.4 180)
  					(length 3.81)
  					(name "DCC")
  					(number "A5")
  				)
  				(pin passive line
  					(at 19.05 20.32 180)
  					(length 3.81)
  					(name "DECD")
  					(number "A6")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "A7")
  				)
  				(pin passive line
  					(at 19.05 15.24 180)
  					(length 3.81)
  					(name "DECA")
  					(number "A8")
  				)
  				(pin passive line
  					(at 0 34.29 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "A9")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "A10")
  				)
  				(pin output line
  					(at -19.05 10.16 0)
  					(length 3.81)
  					(name "XC2")
  					(number "B1")
  				)
  				(pin passive line
  					(at 19.05 7.62 180)
  					(length 3.81)
  					(name "DECRF")
  					(number "C1")
  				)
  				(pin bidirectional line
  					(at -19.05 2.54 0)
  					(length 3.81)
  					(name "P1.20")
  					(number "C6")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -19.05 -2.54 0)
  					(length 3.81)
  					(name "P1.21")
  					(number "C7")
  					(alternate "XL2" output line)
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "D1")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "D2")
  				)
  				(pin passive line
  					(at 19.05 -10.16 180)
  					(length 3.81)
  					(name "ANT")
  					(number "E1")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "E5")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "E6")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "F1")
  				)
  				(pin input line
  					(at 19.05 -17.78 180)
  					(length 3.81)
  					(name "~{RESET}")
  					(number "F2")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "F5")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "F6")
  				)
  				(pin input line
  					(at 19.05 -22.86 180)
  					(length 3.81)
  					(name "SWDCLK")
  					(number "G1")
  				)
  				(pin bidirectional line
  					(at 19.05 -25.4 180)
  					(length 3.81)
  					(name "SWDIO")
  					(number "G2")
  				)
  				(pin passive line
  					(at 0 34.29 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "G10")
  				)
  				(pin passive line
  					(at 0 34.29 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "H1")
  				)
  				(pin bidirectional line
  					(at -19.05 -20.32 0)
  					(length 3.81)
  					(name "TXRTUNE")
  					(number "J5")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "K1")
  				)
  				(pin bidirectional line
  					(at -19.05 -15.24 0)
  					(length 3.81)
  					(name "D-")
  					(number "K4")
  				)
  				(pin bidirectional line
  					(at -19.05 -12.7 0)
  					(length 3.81)
  					(name "D+")
  					(number "K5")
  				)
  				(pin passive line
  					(at -19.05 -25.4 0)
  					(length 3.81)
  					(name "DECUSB")
  					(number "K6")
  				)
  				(pin power_in line
  					(at -19.05 25.4 0)
  					(length 3.81)
  					(name "VBUS")
  					(number "K7")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "K10")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_paxx_1_1")
  			(symbol "nordic_nrf54lm20a_paxx_2_0"
  				(pin bidirectional line
  					(at 19.05 -11.43 180)
  					(length 3.81)
  					(name "P0.09")
  					(number "E3")
  				)
  				(pin bidirectional line
  					(at 19.05 -8.89 180)
  					(length 3.81)
  					(name "P0.08")
  					(number "F3")
  				)
  				(pin bidirectional line
  					(at 19.05 -6.35 180)
  					(length 3.81)
  					(name "P0.07")
  					(number "G3")
  				)
  				(pin bidirectional line
  					(at 19.05 -3.81 180)
  					(length 3.81)
  					(name "P0.06")
  					(number "H2")
  				)
  				(pin bidirectional line
  					(at 19.05 -1.27 180)
  					(length 3.81)
  					(name "P0.05")
  					(number "H3")
  				)
  				(pin bidirectional line
  					(at 19.05 1.27 180)
  					(length 3.81)
  					(name "P0.04")
  					(number "J1")
  				)
  				(pin bidirectional line
  					(at 19.05 3.81 180)
  					(length 3.81)
  					(name "P0.03")
  					(number "J2")
  				)
  				(pin bidirectional line
  					(at 19.05 6.35 180)
  					(length 3.81)
  					(name "P0.02")
  					(number "J3")
  				)
  				(pin bidirectional line
  					(at 19.05 8.89 180)
  					(length 3.81)
  					(name "P0.01")
  					(number "K2")
  				)
  				(pin bidirectional line
  					(at 19.05 11.43 180)
  					(length 3.81)
  					(name "P0.00")
  					(number "K3")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_paxx_2_1")
  			(symbol "nordic_nrf54lm20a_paxx_3_0"
  				(pin bidirectional line
  					(at 19.05 -1.27 180)
  					(length 3.81)
  					(name "P1.15")
  					(number "B2")
  				)
  				(pin bidirectional line
  					(at 19.05 -3.81 180)
  					(length 3.81)
  					(name "P1.16")
  					(number "B3")
  				)
  				(pin bidirectional line
  					(at 19.05 -6.35 180)
  					(length 3.81)
  					(name "P1.17")
  					(number "B4")
  				)
  				(pin bidirectional line
  					(at 19.05 -8.89 180)
  					(length 3.81)
  					(name "P1.18")
  					(number "B5")
  				)
  				(pin bidirectional line
  					(at 19.05 -11.43 180)
  					(length 3.81)
  					(name "P1.19")
  					(number "B6")
  				)
  				(pin bidirectional line
  					(at 19.05 -16.51 180)
  					(length 3.81)
  					(name "P1.23")
  					(number "B7")
  				)
  				(pin bidirectional line
  					(at 19.05 -24.13 180)
  					(length 3.81)
  					(name "P1.26")
  					(number "B8")
  				)
  				(pin bidirectional line
  					(at 19.05 1.27 180)
  					(length 3.81)
  					(name "P1.14")
  					(number "C2")
  				)
  				(pin bidirectional line
  					(at 19.05 3.81 180)
  					(length 3.81)
  					(name "P1.13")
  					(number "C3")
  				)
  				(pin bidirectional line
  					(at 19.05 6.35 180)
  					(length 3.81)
  					(name "P1.12")
  					(number "C4")
  				)
  				(pin bidirectional line
  					(at 19.05 8.89 180)
  					(length 3.81)
  					(name "P1.11")
  					(number "C5")
  				)
  				(pin bidirectional line
  					(at 19.05 -26.67 180)
  					(length 3.81)
  					(name "P1.27")
  					(number "C8")
  				)
  				(pin bidirectional line
  					(at 19.05 11.43 180)
  					(length 3.81)
  					(name "P1.10")
  					(number "D5")
  				)
  				(pin bidirectional line
  					(at 19.05 -13.97 180)
  					(length 3.81)
  					(name "P1.22")
  					(number "D6")
  				)
  				(pin bidirectional line
  					(at 19.05 -19.05 180)
  					(length 3.81)
  					(name "P1.24")
  					(number "D7")
  				)
  				(pin bidirectional line
  					(at 19.05 -29.21 180)
  					(length 3.81)
  					(name "P1.28")
  					(number "D8")
  				)
  				(pin bidirectional line
  					(at 19.05 -21.59 180)
  					(length 3.81)
  					(name "P1.25")
  					(number "E7")
  				)
  				(pin bidirectional line
  					(at 19.05 13.97 180)
  					(length 3.81)
  					(name "P1.09")
  					(number "E8")
  				)
  				(pin bidirectional line
  					(at 19.05 16.51 180)
  					(length 3.81)
  					(name "P1.08")
  					(number "F8")
  				)
  				(pin bidirectional line
  					(at 19.05 19.05 180)
  					(length 3.81)
  					(name "P1.07")
  					(number "G8")
  				)
  				(pin bidirectional line
  					(at 19.05 24.13 180)
  					(length 3.81)
  					(name "P1.05")
  					(number "H8")
  				)
  				(pin bidirectional line
  					(at 19.05 29.21 180)
  					(length 3.81)
  					(name "P1.03")
  					(number "H9")
  				)
  				(pin bidirectional line
  					(at 19.05 -31.75 180)
  					(length 3.81)
  					(name "P1.29")
  					(number "H10")
  				)
  				(pin bidirectional line
  					(at 19.05 34.29 180)
  					(length 3.81)
  					(name "P1.01")
  					(number "J6")
  				)
  				(pin bidirectional line
  					(at 19.05 31.75 180)
  					(length 3.81)
  					(name "P1.02")
  					(number "J7")
  				)
  				(pin bidirectional line
  					(at 19.05 21.59 180)
  					(length 3.81)
  					(name "P1.06")
  					(number "J8")
  				)
  				(pin bidirectional line
  					(at 19.05 26.67 180)
  					(length 3.81)
  					(name "P1.04")
  					(number "J9")
  				)
  				(pin bidirectional line
  					(at 19.05 -34.29 180)
  					(length 3.81)
  					(name "P1.30")
  					(number "J10")
  				)
  				(pin bidirectional line
  					(at 19.05 36.83 180)
  					(length 3.81)
  					(name "P1.00")
  					(number "K8")
  				)
  				(pin bidirectional line
  					(at 19.05 -36.83 180)
  					(length 3.81)
  					(name "P1.31")
  					(number "K9")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_paxx_3_1")
  			(symbol "nordic_nrf54lm20a_paxx_4_0"
  				(pin bidirectional line
  					(at 19.05 -2.54 180)
  					(length 3.81)
  					(name "P2.06")
  					(number "B9")
  				)
  				(pin bidirectional line
  					(at 19.05 12.7 180)
  					(length 3.81)
  					(name "P2.00")
  					(number "B10")
  				)
  				(pin bidirectional line
  					(at 19.05 -5.08 180)
  					(length 3.81)
  					(name "P2.07")
  					(number "C9")
  				)
  				(pin bidirectional line
  					(at 19.05 10.16 180)
  					(length 3.81)
  					(name "P2.01")
  					(number "C10")
  				)
  				(pin bidirectional line
  					(at 19.05 -7.62 180)
  					(length 3.81)
  					(name "P2.08")
  					(number "D9")
  				)
  				(pin bidirectional line
  					(at 19.05 7.62 180)
  					(length 3.81)
  					(name "P2.02")
  					(number "D10")
  				)
  				(pin bidirectional line
  					(at 19.05 -10.16 180)
  					(length 3.81)
  					(name "P2.09")
  					(number "E9")
  				)
  				(pin bidirectional line
  					(at 19.05 5.08 180)
  					(length 3.81)
  					(name "P2.03")
  					(number "E10")
  				)
  				(pin bidirectional line
  					(at 19.05 -12.7 180)
  					(length 3.81)
  					(name "P2.10")
  					(number "F9")
  				)
  				(pin bidirectional line
  					(at 19.05 2.54 180)
  					(length 3.81)
  					(name "P2.04")
  					(number "F10")
  				)
  				(pin bidirectional line
  					(at 19.05 0 180)
  					(length 3.81)
  					(name "P2.05")
  					(number "G9")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_paxx_4_1")
  			(symbol "nordic_nrf54lm20a_paxx_5_0"
  				(pin bidirectional line
  					(at 19.05 -15.24 180)
  					(length 3.81)
  					(name "P3.12")
  					(number "D4")
  				)
  				(pin bidirectional line
  					(at 19.05 -12.7 180)
  					(length 3.81)
  					(name "P3.11")
  					(number "E4")
  				)
  				(pin bidirectional line
  					(at 19.05 -10.16 180)
  					(length 3.81)
  					(name "P3.10")
  					(number "F4")
  				)
  				(pin bidirectional line
  					(at 19.05 -7.62 180)
  					(length 3.81)
  					(name "P3.09")
  					(number "F7")
  				)
  				(pin bidirectional line
  					(at 19.05 -5.08 180)
  					(length 3.81)
  					(name "P3.08")
  					(number "G4")
  				)
  				(pin bidirectional line
  					(at 19.05 -2.54 180)
  					(length 3.81)
  					(name "P3.07")
  					(number "G5")
  				)
  				(pin bidirectional line
  					(at 19.05 0 180)
  					(length 3.81)
  					(name "P3.06")
  					(number "G6")
  				)
  				(pin bidirectional line
  					(at 19.05 2.54 180)
  					(length 3.81)
  					(name "P3.05")
  					(number "G7")
  				)
  				(pin bidirectional line
  					(at 19.05 7.62 180)
  					(length 3.81)
  					(name "P3.03")
  					(number "H4")
  				)
  				(pin bidirectional line
  					(at 19.05 10.16 180)
  					(length 3.81)
  					(name "P3.02")
  					(number "H5")
  				)
  				(pin bidirectional line
  					(at 19.05 12.7 180)
  					(length 3.81)
  					(name "P3.01")
  					(number "H6")
  				)
  				(pin bidirectional line
  					(at 19.05 15.24 180)
  					(length 3.81)
  					(name "P3.00")
  					(number "H7")
  				)
  				(pin bidirectional line
  					(at 19.05 5.08 180)
  					(length 3.81)
  					(name "P3.04")
  					(number "J4")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_paxx_5_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf54lm20a_qgaa"
        (property "Footprint" "PartReel:nordic_nrf54lm20a_qgaa"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf54LM20A/page/pdf/nRF54LM20A_Preliminary_Datasheet_v0.7.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF54LM20A-QGAA."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf54lm20a_qgaa/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(in_pos_files yes)
  			(duplicate_pin_numbers_are_jumpers no)
  			(property "Reference" "U"
  				(at -12.7 35.56 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "Value" "nRF54LM20A-QGAA"
  				(at -13.97 33.02 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_locked" ""
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_fp_filters" "QFN*52*1EP*6x6mm*P0.4mm*EP4.7x4.7mm*"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  				(hide yes)
  			)
  			(symbol "nordic_nrf54lm20a_qgaa_1_0"
  				(pin power_in line
  					(at 0 34.29 270)
  					(length 3.81)
  					(name "VDD")
  					(number "6")
  				)
  				(pin power_in line
  					(at -19.05 25.4 0)
  					(length 3.81)
  					(name "VBUS")
  					(number "17")
  				)
  				(pin passive line
  					(at -19.05 -25.4 0)
  					(length 3.81)
  					(name "DECUSB")
  					(number "18")
  				)
  				(pin bidirectional line
  					(at -19.05 -12.7 0)
  					(length 3.81)
  					(name "D+")
  					(number "19")
  				)
  				(pin bidirectional line
  					(at -19.05 -15.24 0)
  					(length 3.81)
  					(name "D-")
  					(number "20")
  				)
  				(pin bidirectional line
  					(at -19.05 -20.32 0)
  					(length 3.81)
  					(name "TXRTUNE")
  					(number "21")
  				)
  				(pin input line
  					(at 19.05 -22.86 180)
  					(length 3.81)
  					(name "SWDCLK")
  					(number "31")
  				)
  				(pin bidirectional line
  					(at 19.05 -25.4 180)
  					(length 3.81)
  					(name "SWDIO")
  					(number "32")
  				)
  				(pin input line
  					(at 19.05 -17.78 180)
  					(length 3.81)
  					(name "~{RESET}")
  					(number "33")
  				)
  				(pin passive line
  					(at 19.05 0 180)
  					(length 3.81)
  					(name "ANT")
  					(number "34")
  				)
  				(pin power_in line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(name "VSS")
  					(number "35")
  				)
  				(pin passive line
  					(at 19.05 12.7 180)
  					(length 3.81)
  					(name "DECRF")
  					(number "36")
  				)
  				(pin input line
  					(at -19.05 15.24 0)
  					(length 3.81)
  					(name "XC1")
  					(number "37")
  				)
  				(pin output line
  					(at -19.05 10.16 0)
  					(length 3.81)
  					(name "XC2")
  					(number "38")
  				)
  				(pin passive line
  					(at 0 34.29 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "42")
  				)
  				(pin passive line
  					(at 19.05 25.4 180)
  					(length 3.81)
  					(name "DCC")
  					(number "43")
  				)
  				(pin passive line
  					(at 19.05 20.32 180)
  					(length 3.81)
  					(name "DECD")
  					(number "44")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "45")
  				)
  				(pin passive line
  					(at 19.05 15.24 180)
  					(length 3.81)
  					(name "DECA")
  					(number "46")
  				)
  				(pin bidirectional line
  					(at -19.05 2.54 0)
  					(length 3.81)
  					(name "P1.20")
  					(number "48")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -19.05 -2.54 0)
  					(length 3.81)
  					(name "P1.21")
  					(number "49")
  					(alternate "XL2" output line)
  				)
  				(pin passive line
  					(at 0 34.29 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "51")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "53")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_qgaa_1_1")
  			(symbol "nordic_nrf54lm20a_qgaa_2_0"
  				(pin bidirectional line
  					(at 19.05 6.35 180)
  					(length 3.81)
  					(name "P0.03")
  					(number "25")
  				)
  				(pin bidirectional line
  					(at 19.05 3.81 180)
  					(length 3.81)
  					(name "P0.04")
  					(number "26")
  				)
  				(pin bidirectional line
  					(at 19.05 1.27 180)
  					(length 3.81)
  					(name "P0.06")
  					(number "27")
  				)
  				(pin bidirectional line
  					(at 19.05 -1.27 180)
  					(length 3.81)
  					(name "P0.07")
  					(number "28")
  				)
  				(pin bidirectional line
  					(at 19.05 -3.81 180)
  					(length 3.81)
  					(name "P0.08")
  					(number "29")
  				)
  				(pin bidirectional line
  					(at 19.05 -6.35 180)
  					(length 3.81)
  					(name "P0.09")
  					(number "30")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_qgaa_2_1")
  			(symbol "nordic_nrf54lm20a_qgaa_3_0"
  				(pin bidirectional line
  					(at 19.05 -16.51 180)
  					(length 3.81)
  					(name "P1.29")
  					(number "7")
  				)
  				(pin bidirectional line
  					(at 19.05 -19.05 180)
  					(length 3.81)
  					(name "P1.30")
  					(number "8")
  				)
  				(pin bidirectional line
  					(at 19.05 -21.59 180)
  					(length 3.81)
  					(name "P1.31")
  					(number "9")
  				)
  				(pin bidirectional line
  					(at 19.05 21.59 180)
  					(length 3.81)
  					(name "P1.00")
  					(number "10")
  				)
  				(pin bidirectional line
  					(at 19.05 19.05 180)
  					(length 3.81)
  					(name "P1.01")
  					(number "11")
  				)
  				(pin bidirectional line
  					(at 19.05 16.51 180)
  					(length 3.81)
  					(name "P1.02")
  					(number "12")
  				)
  				(pin bidirectional line
  					(at 19.05 13.97 180)
  					(length 3.81)
  					(name "P1.03")
  					(number "13")
  				)
  				(pin bidirectional line
  					(at 19.05 11.43 180)
  					(length 3.81)
  					(name "P1.04")
  					(number "14")
  				)
  				(pin bidirectional line
  					(at 19.05 8.89 180)
  					(length 3.81)
  					(name "P1.05")
  					(number "15")
  				)
  				(pin bidirectional line
  					(at 19.05 6.35 180)
  					(length 3.81)
  					(name "P1.06")
  					(number "16")
  				)
  				(pin bidirectional line
  					(at 19.05 3.81 180)
  					(length 3.81)
  					(name "P1.07")
  					(number "22")
  				)
  				(pin bidirectional line
  					(at 19.05 1.27 180)
  					(length 3.81)
  					(name "P1.08")
  					(number "23")
  				)
  				(pin bidirectional line
  					(at 19.05 -1.27 180)
  					(length 3.81)
  					(name "P1.09")
  					(number "24")
  				)
  				(pin bidirectional line
  					(at 19.05 -3.81 180)
  					(length 3.81)
  					(name "P1.15")
  					(number "39")
  				)
  				(pin bidirectional line
  					(at 19.05 -6.35 180)
  					(length 3.81)
  					(name "P1.16")
  					(number "40")
  				)
  				(pin bidirectional line
  					(at 19.05 -8.89 180)
  					(length 3.81)
  					(name "P1.18")
  					(number "41")
  				)
  				(pin bidirectional line
  					(at 19.05 -11.43 180)
  					(length 3.81)
  					(name "P1.19")
  					(number "47")
  				)
  				(pin bidirectional line
  					(at 19.05 -13.97 180)
  					(length 3.81)
  					(name "P1.24")
  					(number "50")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_qgaa_3_1")
  			(symbol "nordic_nrf54lm20a_qgaa_4_0"
  				(pin bidirectional line
  					(at 19.05 3.81 180)
  					(length 3.81)
  					(name "P2.01")
  					(number "1")
  				)
  				(pin bidirectional line
  					(at 19.05 1.27 180)
  					(length 3.81)
  					(name "P2.02")
  					(number "2")
  				)
  				(pin bidirectional line
  					(at 19.05 -1.27 180)
  					(length 3.81)
  					(name "P2.03")
  					(number "3")
  				)
  				(pin bidirectional line
  					(at 19.05 -3.81 180)
  					(length 3.81)
  					(name "P2.04")
  					(number "4")
  				)
  				(pin bidirectional line
  					(at 19.05 -6.35 180)
  					(length 3.81)
  					(name "P2.05")
  					(number "5")
  				)
  				(pin bidirectional line
  					(at 19.05 6.35 180)
  					(length 3.81)
  					(name "P2.00")
  					(number "52")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_qgaa_4_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf54lm20a_qgxx"
        (property "Footprint" "PartReel:nordic_nrf54lm20a_qgxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_nrf54LM20A/page/pdf/nRF54LM20A_Preliminary_Datasheet_v0.7.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF54LM20A-QGXX."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf54lm20a_qgxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(in_pos_files yes)
  			(duplicate_pin_numbers_are_jumpers no)
  			(property "Reference" "U"
  				(at -12.7 35.56 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "Value" "nRF54LM20A-QGXX"
  				(at -13.97 33.02 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_locked" ""
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_fp_filters" "QFN*52*1EP*6x6mm*P0.4mm*EP4.7x4.7mm*"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  				(hide yes)
  			)
  			(symbol "nordic_nrf54lm20a_qgxx_1_0"
  				(pin power_in line
  					(at 0 34.29 270)
  					(length 3.81)
  					(name "VDD")
  					(number "6")
  				)
  				(pin power_in line
  					(at -19.05 25.4 0)
  					(length 3.81)
  					(name "VBUS")
  					(number "17")
  				)
  				(pin passive line
  					(at -19.05 -25.4 0)
  					(length 3.81)
  					(name "DECUSB")
  					(number "18")
  				)
  				(pin bidirectional line
  					(at -19.05 -12.7 0)
  					(length 3.81)
  					(name "D+")
  					(number "19")
  				)
  				(pin bidirectional line
  					(at -19.05 -15.24 0)
  					(length 3.81)
  					(name "D-")
  					(number "20")
  				)
  				(pin bidirectional line
  					(at -19.05 -20.32 0)
  					(length 3.81)
  					(name "TXRTUNE")
  					(number "21")
  				)
  				(pin input line
  					(at 19.05 -22.86 180)
  					(length 3.81)
  					(name "SWDCLK")
  					(number "31")
  				)
  				(pin bidirectional line
  					(at 19.05 -25.4 180)
  					(length 3.81)
  					(name "SWDIO")
  					(number "32")
  				)
  				(pin input line
  					(at 19.05 -17.78 180)
  					(length 3.81)
  					(name "~{RESET}")
  					(number "33")
  				)
  				(pin passive line
  					(at 19.05 0 180)
  					(length 3.81)
  					(name "ANT")
  					(number "34")
  				)
  				(pin power_in line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(name "VSS")
  					(number "35")
  				)
  				(pin passive line
  					(at 19.05 12.7 180)
  					(length 3.81)
  					(name "DECRF")
  					(number "36")
  				)
  				(pin input line
  					(at -19.05 15.24 0)
  					(length 3.81)
  					(name "XC1")
  					(number "37")
  				)
  				(pin output line
  					(at -19.05 10.16 0)
  					(length 3.81)
  					(name "XC2")
  					(number "38")
  				)
  				(pin passive line
  					(at 0 34.29 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "42")
  				)
  				(pin passive line
  					(at 19.05 25.4 180)
  					(length 3.81)
  					(name "DCC")
  					(number "43")
  				)
  				(pin passive line
  					(at 19.05 20.32 180)
  					(length 3.81)
  					(name "DECD")
  					(number "44")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "45")
  				)
  				(pin passive line
  					(at 19.05 15.24 180)
  					(length 3.81)
  					(name "DECA")
  					(number "46")
  				)
  				(pin bidirectional line
  					(at -19.05 2.54 0)
  					(length 3.81)
  					(name "P1.20")
  					(number "48")
  					(alternate "XL1" input line)
  				)
  				(pin bidirectional line
  					(at -19.05 -2.54 0)
  					(length 3.81)
  					(name "P1.21")
  					(number "49")
  					(alternate "XL2" output line)
  				)
  				(pin passive line
  					(at 0 34.29 270)
  					(length 3.81)
  					(hide yes)
  					(name "VDD")
  					(number "51")
  				)
  				(pin passive line
  					(at 0 -34.29 90)
  					(length 3.81)
  					(hide yes)
  					(name "VSS")
  					(number "53")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_qgxx_1_1")
  			(symbol "nordic_nrf54lm20a_qgxx_2_0"
  				(pin bidirectional line
  					(at 19.05 6.35 180)
  					(length 3.81)
  					(name "P0.03")
  					(number "25")
  				)
  				(pin bidirectional line
  					(at 19.05 3.81 180)
  					(length 3.81)
  					(name "P0.04")
  					(number "26")
  				)
  				(pin bidirectional line
  					(at 19.05 1.27 180)
  					(length 3.81)
  					(name "P0.06")
  					(number "27")
  				)
  				(pin bidirectional line
  					(at 19.05 -1.27 180)
  					(length 3.81)
  					(name "P0.07")
  					(number "28")
  				)
  				(pin bidirectional line
  					(at 19.05 -3.81 180)
  					(length 3.81)
  					(name "P0.08")
  					(number "29")
  				)
  				(pin bidirectional line
  					(at 19.05 -6.35 180)
  					(length 3.81)
  					(name "P0.09")
  					(number "30")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_qgxx_2_1")
  			(symbol "nordic_nrf54lm20a_qgxx_3_0"
  				(pin bidirectional line
  					(at 19.05 -16.51 180)
  					(length 3.81)
  					(name "P1.29")
  					(number "7")
  				)
  				(pin bidirectional line
  					(at 19.05 -19.05 180)
  					(length 3.81)
  					(name "P1.30")
  					(number "8")
  				)
  				(pin bidirectional line
  					(at 19.05 -21.59 180)
  					(length 3.81)
  					(name "P1.31")
  					(number "9")
  				)
  				(pin bidirectional line
  					(at 19.05 21.59 180)
  					(length 3.81)
  					(name "P1.00")
  					(number "10")
  				)
  				(pin bidirectional line
  					(at 19.05 19.05 180)
  					(length 3.81)
  					(name "P1.01")
  					(number "11")
  				)
  				(pin bidirectional line
  					(at 19.05 16.51 180)
  					(length 3.81)
  					(name "P1.02")
  					(number "12")
  				)
  				(pin bidirectional line
  					(at 19.05 13.97 180)
  					(length 3.81)
  					(name "P1.03")
  					(number "13")
  				)
  				(pin bidirectional line
  					(at 19.05 11.43 180)
  					(length 3.81)
  					(name "P1.04")
  					(number "14")
  				)
  				(pin bidirectional line
  					(at 19.05 8.89 180)
  					(length 3.81)
  					(name "P1.05")
  					(number "15")
  				)
  				(pin bidirectional line
  					(at 19.05 6.35 180)
  					(length 3.81)
  					(name "P1.06")
  					(number "16")
  				)
  				(pin bidirectional line
  					(at 19.05 3.81 180)
  					(length 3.81)
  					(name "P1.07")
  					(number "22")
  				)
  				(pin bidirectional line
  					(at 19.05 1.27 180)
  					(length 3.81)
  					(name "P1.08")
  					(number "23")
  				)
  				(pin bidirectional line
  					(at 19.05 -1.27 180)
  					(length 3.81)
  					(name "P1.09")
  					(number "24")
  				)
  				(pin bidirectional line
  					(at 19.05 -3.81 180)
  					(length 3.81)
  					(name "P1.15")
  					(number "39")
  				)
  				(pin bidirectional line
  					(at 19.05 -6.35 180)
  					(length 3.81)
  					(name "P1.16")
  					(number "40")
  				)
  				(pin bidirectional line
  					(at 19.05 -8.89 180)
  					(length 3.81)
  					(name "P1.18")
  					(number "41")
  				)
  				(pin bidirectional line
  					(at 19.05 -11.43 180)
  					(length 3.81)
  					(name "P1.19")
  					(number "47")
  				)
  				(pin bidirectional line
  					(at 19.05 -13.97 180)
  					(length 3.81)
  					(name "P1.24")
  					(number "50")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_qgxx_3_1")
  			(symbol "nordic_nrf54lm20a_qgxx_4_0"
  				(pin bidirectional line
  					(at 19.05 3.81 180)
  					(length 3.81)
  					(name "P2.01")
  					(number "1")
  				)
  				(pin bidirectional line
  					(at 19.05 1.27 180)
  					(length 3.81)
  					(name "P2.02")
  					(number "2")
  				)
  				(pin bidirectional line
  					(at 19.05 -1.27 180)
  					(length 3.81)
  					(name "P2.03")
  					(number "3")
  				)
  				(pin bidirectional line
  					(at 19.05 -3.81 180)
  					(length 3.81)
  					(name "P2.04")
  					(number "4")
  				)
  				(pin bidirectional line
  					(at 19.05 -6.35 180)
  					(length 3.81)
  					(name "P2.05")
  					(number "5")
  				)
  				(pin bidirectional line
  					(at 19.05 6.35 180)
  					(length 3.81)
  					(name "P2.00")
  					(number "52")
  				)
  			)
  			(symbol "nordic_nrf54lm20a_qgxx_4_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf54lv10a_caaa"
        (property "Footprint" "PartReel:nordic_nrf54lv10a_caaa"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf54LV10/page/keyfeatures_html5.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF54LV Ultra-low power Bluetooth 5.4 SoC, 1.5V-3.6V, CSP29."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless BLE Bluetooth SoC nRF nRF54 ultra-low-power WLCSP"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf54lv10a_caaa/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(in_pos_files yes)
  			(duplicate_pin_numbers_are_jumpers no)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "Value" "nRF54LV10A-CAAA"
  				(at 0 -2.54 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_fp_filters" "*CSP?29*"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  				(hide yes)
  			)
  			(symbol "nordic_nrf54lv10a_caaa_1_0"
  				(pin passive line
  					(at 17.78 27.94 180)
  					(length 2.54)
  					(name "DECRF")
  					(number "A1")
  				)
  				(pin bidirectional line
  					(at -17.78 33.02 0)
  					(length 2.54)
  					(name "XC1")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -17.78 27.94 0)
  					(length 2.54)
  					(name "XC2")
  					(number "A3")
  				)
  				(pin bidirectional line
  					(at -17.78 -17.78 0)
  					(length 2.54)
  					(name "P1.03")
  					(number "A4")
  					(alternate "AIN3" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 -27.94 0)
  					(length 2.54)
  					(name "P1.10")
  					(number "A5")
  					(alternate "AIN5" input line)
  					(alternate "ASO[1]" output line)
  					(alternate "TRACECLK" output line)
  				)
  				(pin bidirectional line
  					(at 17.78 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "B1")
  				)
  				(pin bidirectional line
  					(at -17.78 -25.4 0)
  					(length 2.54)
  					(name "P1.09")
  					(number "B3")
  				)
  				(pin bidirectional line
  					(at -17.78 -20.32 0)
  					(length 2.54)
  					(name "P1.05")
  					(number "B4")
  					(alternate "ASO[0]" output line)
  					(alternate "EXTREF" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 20.32 0)
  					(length 2.54)
  					(name "P1.13")
  					(number "B5")
  					(alternate "TRACEDATA[2]" output line)
  					(alternate "XL1" bidirectional line)
  				)
  				(pin power_in line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(name "VSS")
  					(number "C1")
  				)
  				(pin input line
  					(at 17.78 -25.4 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "C2")
  				)
  				(pin bidirectional line
  					(at -17.78 -12.7 0)
  					(length 2.54)
  					(name "P1.01")
  					(number "C3")
  					(alternate "AIN1" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 -22.86 0)
  					(length 2.54)
  					(name "P1.07")
  					(number "C4")
  					(alternate "AIN4" input line)
  					(alternate "ASI[0]" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 15.24 0)
  					(length 2.54)
  					(name "P1.14")
  					(number "C5")
  					(alternate "TRACEDATA[3]" output line)
  					(alternate "XL2" bidirectional line)
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D1")
  				)
  				(pin input line
  					(at 17.78 -30.48 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "D2")
  				)
  				(pin bidirectional line
  					(at -17.78 -15.24 0)
  					(length 2.54)
  					(name "P1.02")
  					(number "D3")
  					(alternate "AIN2" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 -30.48 0)
  					(length 2.54)
  					(name "P1.11")
  					(number "D4")
  					(alternate "AIN6" input line)
  					(alternate "ASI[1]" input line)
  					(alternate "SWO" output line)
  					(alternate "TRACEDATA[0]" output line)
  				)
  				(pin passive line
  					(at 17.78 33.02 180)
  					(length 2.54)
  					(name "DECA")
  					(number "D5")
  				)
  				(pin passive line
  					(at 17.78 30.48 180)
  					(length 2.54)
  					(name "DECB")
  					(number "E1")
  				)
  				(pin bidirectional line
  					(at 17.78 -33.02 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "E2")
  				)
  				(pin bidirectional line
  					(at -17.78 -10.16 0)
  					(length 2.54)
  					(name "P1.00")
  					(number "E3")
  					(alternate "AIN0" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 -33.02 0)
  					(length 2.54)
  					(name "P1.12")
  					(number "E4")
  					(alternate "AIN7" input line)
  					(alternate "TRACEDATA[1]" output line)
  				)
  				(pin passive line
  					(at 17.78 25.4 180)
  					(length 2.54)
  					(name "DECD")
  					(number "E5")
  				)
  				(pin passive line
  					(at 17.78 12.7 180)
  					(length 2.54)
  					(name "CFLYH")
  					(number "F1")
  				)
  				(pin passive line
  					(at 17.78 7.62 180)
  					(length 2.54)
  					(name "CFLYL")
  					(number "F2")
  				)
  				(pin power_in line
  					(at 0 40.64 270)
  					(length 2.54)
  					(name "VDDL")
  					(number "F3")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "F4")
  				)
  				(pin power_out line
  					(at 17.78 20.32 180)
  					(length 2.54)
  					(name "DCC")
  					(number "F5")
  				)
  			)
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf54lv10a_caxx"
        (property "Footprint" "PartReel:nordic_nrf54lv10a_caxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf54LV10/page/keyfeatures_html5.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF54LV Ultra-low power Bluetooth 5.4 SoC, 1.5V-3.6V, CSP29."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless BLE Bluetooth SoC nRF nRF54 ultra-low-power WLCSP"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf54lv10a_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(in_pos_files yes)
  			(duplicate_pin_numbers_are_jumpers no)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "Value" "nRF54LV10A-CAXX"
  				(at 0 -2.54 0)
  				(show_name no)
  				(do_not_autoplace no)
  			)
  			(property "ki_fp_filters" "*CSP?29*"
  				(at 0 0 0)
  				(show_name no)
  				(do_not_autoplace no)
  				(hide yes)
  			)
  			(symbol "nordic_nrf54lv10a_caxx_1_0"
  				(pin passive line
  					(at 17.78 27.94 180)
  					(length 2.54)
  					(name "DECRF")
  					(number "A1")
  				)
  				(pin bidirectional line
  					(at -17.78 33.02 0)
  					(length 2.54)
  					(name "XC1")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -17.78 27.94 0)
  					(length 2.54)
  					(name "XC2")
  					(number "A3")
  				)
  				(pin bidirectional line
  					(at -17.78 -17.78 0)
  					(length 2.54)
  					(name "P1.03")
  					(number "A4")
  					(alternate "AIN3" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 -27.94 0)
  					(length 2.54)
  					(name "P1.10")
  					(number "A5")
  					(alternate "AIN5" input line)
  					(alternate "ASO[1]" output line)
  					(alternate "TRACECLK" output line)
  				)
  				(pin bidirectional line
  					(at 17.78 0 180)
  					(length 2.54)
  					(name "ANT")
  					(number "B1")
  				)
  				(pin bidirectional line
  					(at -17.78 -25.4 0)
  					(length 2.54)
  					(name "P1.09")
  					(number "B3")
  				)
  				(pin bidirectional line
  					(at -17.78 -20.32 0)
  					(length 2.54)
  					(name "P1.05")
  					(number "B4")
  					(alternate "ASO[0]" output line)
  					(alternate "EXTREF" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 20.32 0)
  					(length 2.54)
  					(name "P1.13")
  					(number "B5")
  					(alternate "TRACEDATA[2]" output line)
  					(alternate "XL1" bidirectional line)
  				)
  				(pin power_in line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(name "VSS")
  					(number "C1")
  				)
  				(pin input line
  					(at 17.78 -25.4 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "C2")
  				)
  				(pin bidirectional line
  					(at -17.78 -12.7 0)
  					(length 2.54)
  					(name "P1.01")
  					(number "C3")
  					(alternate "AIN1" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 -22.86 0)
  					(length 2.54)
  					(name "P1.07")
  					(number "C4")
  					(alternate "AIN4" input line)
  					(alternate "ASI[0]" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 15.24 0)
  					(length 2.54)
  					(name "P1.14")
  					(number "C5")
  					(alternate "TRACEDATA[3]" output line)
  					(alternate "XL2" bidirectional line)
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "D1")
  				)
  				(pin input line
  					(at 17.78 -30.48 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "D2")
  				)
  				(pin bidirectional line
  					(at -17.78 -15.24 0)
  					(length 2.54)
  					(name "P1.02")
  					(number "D3")
  					(alternate "AIN2" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 -30.48 0)
  					(length 2.54)
  					(name "P1.11")
  					(number "D4")
  					(alternate "AIN6" input line)
  					(alternate "ASI[1]" input line)
  					(alternate "SWO" output line)
  					(alternate "TRACEDATA[0]" output line)
  				)
  				(pin passive line
  					(at 17.78 33.02 180)
  					(length 2.54)
  					(name "DECA")
  					(number "D5")
  				)
  				(pin passive line
  					(at 17.78 30.48 180)
  					(length 2.54)
  					(name "DECB")
  					(number "E1")
  				)
  				(pin bidirectional line
  					(at 17.78 -33.02 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "E2")
  				)
  				(pin bidirectional line
  					(at -17.78 -10.16 0)
  					(length 2.54)
  					(name "P1.00")
  					(number "E3")
  					(alternate "AIN0" input line)
  				)
  				(pin bidirectional line
  					(at -17.78 -33.02 0)
  					(length 2.54)
  					(name "P1.12")
  					(number "E4")
  					(alternate "AIN7" input line)
  					(alternate "TRACEDATA[1]" output line)
  				)
  				(pin passive line
  					(at 17.78 25.4 180)
  					(length 2.54)
  					(name "DECD")
  					(number "E5")
  				)
  				(pin passive line
  					(at 17.78 12.7 180)
  					(length 2.54)
  					(name "CFLYH")
  					(number "F1")
  				)
  				(pin passive line
  					(at 17.78 7.62 180)
  					(length 2.54)
  					(name "CFLYL")
  					(number "F2")
  				)
  				(pin power_in line
  					(at 0 40.64 270)
  					(length 2.54)
  					(name "VDDL")
  					(number "F3")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "F4")
  				)
  				(pin power_out line
  					(at 17.78 20.32 180)
  					(length 2.54)
  					(name "DCC")
  					(number "F5")
  				)
  			)
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf7002_cexx"
        (property "Footprint" "PartReel:nordic_nrf7002_cexx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf7002/page/keyfeatures_html5.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2.4/5GHz Wi-Fi 6 Companion IC, SSID scanning, Matter support, CSP-90."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless wifi6 802.11ax matter companion-ic locationing ssid-scan low-power coexistence"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf7002_cexx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF7002-CEXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA?90*10x9*3.7495x3.385mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf7002_cexx_0_0"
  				(pin output line
  					(at -38.1 -25.4 0)
  					(length 5.08)
  					(name "COEX_GRANT")
  					(number "A11")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "A13")
  				)
  				(pin output line
  					(at -38.1 -30.48 0)
  					(length 5.08)
  					(name "SW_CTRL0")
  					(number "A16")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "A18")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "A20")
  				)
  				(pin bidirectional line
  					(at -38.1 -10.16 0)
  					(length 5.08)
  					(name "QSPI_DATA2")
  					(number "A3")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "A7")
  				)
  				(pin bidirectional line
  					(at -38.1 -33.02 0)
  					(length 5.08)
  					(name "SW_CTRL1")
  					(number "A9")
  				)
  				(pin output line
  					(at -38.1 -27.94 0)
  					(length 5.08)
  					(name "HOST_IRQ")
  					(number "B10")
  				)
  				(pin power_in line
  					(at -2.54 40.64 270)
  					(length 5.08)
  					(name "IOVDD")
  					(number "B12")
  				)
  				(pin no_connect line
  					(at 22.86 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "B15")
  				)
  				(pin power_in line
  					(at 2.54 40.64 270)
  					(length 5.08)
  					(name "OTPVDD")
  					(number "B17")
  				)
  				(pin no_connect line
  					(at 25.4 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "B19")
  				)
  				(pin bidirectional line
  					(at -38.1 -12.7 0)
  					(length 5.08)
  					(name "QSPI_DATA3")
  					(number "B6")
  				)
  				(pin bidirectional line
  					(at -38.1 -20.32 0)
  					(length 5.08)
  					(name "COEX_STATUS0")
  					(number "B8")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "C11")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "C13")
  				)
  				(pin no_connect line
  					(at 27.94 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "C16")
  				)
  				(pin no_connect line
  					(at 7.62 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "C18")
  				)
  				(pin no_connect line
  					(at 10.16 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "C20")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "C5")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "C7")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "C9")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "D1")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "D11")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "D13")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "D16")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "D20")
  				)
  				(pin power_in line
  					(at 5.08 40.64 270)
  					(length 5.08)
  					(name "PWRIOVDD")
  					(number "D3")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "D5")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "D7")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "D9")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "E11")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "E13")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "E3")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "E5")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "E7")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "E9")
  				)
  				(pin passive line
  					(at 38.1 -30.48 180)
  					(length 5.08)
  					(name "DIGVDD")
  					(number "F1")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "F11")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "F13")
  				)
  				(pin passive line
  					(at 38.1 -22.86 180)
  					(length 5.08)
  					(name "PWRBUCKVDD")
  					(number "F3")
  				)
  				(pin power_in line
  					(at 38.1 -7.62 180)
  					(length 5.08)
  					(name "BUCKVBATS")
  					(number "F5")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "F7")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "F9")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "H20")
  				)
  				(pin passive line
  					(at 38.1 -17.78 180)
  					(length 5.08)
  					(name "XOLDO")
  					(number "J11")
  				)
  				(pin input line
  					(at -38.1 -17.78 0)
  					(length 5.08)
  					(name "BUCKEN")
  					(number "J5")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "J7")
  				)
  				(pin passive line
  					(at 38.1 -33.02 180)
  					(length 5.08)
  					(name "AFELDO")
  					(number "J9")
  				)
  				(pin passive line
  					(at 38.1 -25.4 180)
  					(length 5.08)
  					(name "RFVDD")
  					(number "K13")
  				)
  				(pin passive line
  					(at 38.1 -15.24 180)
  					(length 5.08)
  					(name "SXLDO")
  					(number "K16")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "K20")
  				)
  				(pin power_out line
  					(at 38.1 15.24 180)
  					(length 5.08)
  					(name "BUCKOUT")
  					(number "K3")
  				)
  				(pin no_connect line
  					(at 12.7 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "K5")
  				)
  				(pin no_connect line
  					(at 15.24 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "K7")
  				)
  				(pin power_in line
  					(at 38.1 -5.08 180)
  					(length 5.08)
  					(name "BUCKVBAT")
  					(number "L1")
  				)
  				(pin passive line
  					(at 38.1 -20.32 180)
  					(length 5.08)
  					(name "RFBUCKVDD")
  					(number "L13")
  				)
  				(pin power_in line
  					(at -12.7 40.64 270)
  					(length 5.08)
  					(name "VBAT")
  					(number "L16")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "L18")
  				)
  				(pin power_out line
  					(at 38.1 7.62 180)
  					(length 5.08)
  					(name "PALDO")
  					(number "L20")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "L3")
  				)
  				(pin no_connect line
  					(at 17.78 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "L5")
  				)
  				(pin no_connect line
  					(at 20.32 -35.56 90)
  					(length 5.08) hide
  					(name "NC")
  					(number "L7")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "GND")
  					(number "L9")
  				)
  			)
  			(symbol "nordic_nrf7002_cexx_1_0"
  				(pin power_in line
  					(at 0 -40.64 90)
  					(length 5.08)
  					(name "VSS")
  					(number "A1")
  				)
  				(pin bidirectional line
  					(at -38.1 -22.86 0)
  					(length 5.08)
  					(name "COEX_REQ")
  					(number "A5")
  				)
  				(pin bidirectional line
  					(at -38.1 -5.08 0)
  					(length 5.08)
  					(name "QSPI_DATA0")
  					(number "B2")
  					(alternate "SPI_MOSI" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -38.1 -7.62 0)
  					(length 5.08)
  					(name "QSPI_DATA1")
  					(number "B4")
  					(alternate "SPI_MISO" bidirectional line)
  				)
  				(pin input line
  					(at -38.1 0 0)
  					(length 5.08)
  					(name "QSPI_CLK")
  					(number "C1")
  					(alternate "SPI_CLK" input line)
  				)
  				(pin input line
  					(at -38.1 -2.54 0)
  					(length 5.08)
  					(name "~{QSPI_SS}")
  					(number "C3")
  					(alternate "~{SPI_SS}" input line)
  				)
  				(pin bidirectional line
  					(at 38.1 22.86 180)
  					(length 5.08)
  					(name "TXRF1")
  					(number "D18")
  				)
  				(pin power_in line
  					(at 38.1 2.54 180)
  					(length 5.08)
  					(name "PAVDD1")
  					(number "E16")
  				)
  				(pin bidirectional line
  					(at 38.1 27.94 180)
  					(length 5.08)
  					(name "TXRF0")
  					(number "G16")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "BUCKVSSS")
  					(number "J1")
  				)
  				(pin power_in line
  					(at 38.1 5.08 180)
  					(length 5.08)
  					(name "PAVDD0")
  					(number "J14")
  				)
  				(pin passive line
  					(at 38.1 -27.94 180)
  					(length 5.08)
  					(name "BUCKVMID")
  					(number "J3")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 5.08) hide
  					(name "BUCKVSS")
  					(number "K1")
  				)
  				(pin input line
  					(at -38.1 20.32 0)
  					(length 5.08)
  					(name "XOP")
  					(number "K11")
  				)
  				(pin power_in line
  					(at 38.1 -2.54 180)
  					(length 5.08)
  					(name "AFEVBAT")
  					(number "K9")
  				)
  				(pin output line
  					(at -38.1 15.24 0)
  					(length 5.08)
  					(name "XON")
  					(number "L11")
  				)
  			)
  			(symbol "nordic_nrf7002_cexx_1_1")
  		)
  (symbol "nordic_nrf9151_laxx"
        (property "Footprint" "PartReel:nordic_nrf9151_laxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf9151/page/nRF9151_html5_keyfeatures.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "LTE-M/NB-IoT/DECT-NR+ SiP, ARM Cortex-M33, GNSS, LGA-100."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless cellular iot lte-m nb-iot dect-nr+ non-terrestrial-network gnss trustzone"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf9151_laxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF9151-LAXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "LGA?9151*12.1x11.1mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf9151_laxx_0_0"
  				(pin input line
  					(at -33.02 58.42 0)
  					(length 5.08)
  					(name "ENABLE")
  					(number "10")
  				)
  				(pin bidirectional line
  					(at -33.02 48.26 0)
  					(length 5.08)
  					(name "P0.01")
  					(number "57")
  				)
  				(pin bidirectional line
  					(at -33.02 45.72 0)
  					(length 5.08)
  					(name "P0.02")
  					(number "58")
  				)
  				(pin bidirectional line
  					(at -33.02 43.18 0)
  					(length 5.08)
  					(name "P0.03")
  					(number "59")
  				)
  				(pin bidirectional line
  					(at -33.02 40.64 0)
  					(length 5.08)
  					(name "P0.04")
  					(number "61")
  				)
  				(pin bidirectional line
  					(at -33.02 38.1 0)
  					(length 5.08)
  					(name "P0.05")
  					(number "62")
  				)
  				(pin bidirectional line
  					(at -33.02 35.56 0)
  					(length 5.08)
  					(name "P0.06")
  					(number "63")
  				)
  				(pin bidirectional line
  					(at -33.02 33.02 0)
  					(length 5.08)
  					(name "P0.07")
  					(number "64")
  				)
  				(pin bidirectional line
  					(at -33.02 30.48 0)
  					(length 5.08)
  					(name "P0.08")
  					(number "67")
  				)
  				(pin bidirectional line
  					(at -33.02 27.94 0)
  					(length 5.08)
  					(name "P0.09")
  					(number "68")
  				)
  				(pin bidirectional line
  					(at -33.02 25.4 0)
  					(length 5.08)
  					(name "P0.10")
  					(number "69")
  				)
  				(pin bidirectional line
  					(at -33.02 22.86 0)
  					(length 5.08)
  					(name "P0.11")
  					(number "70")
  				)
  				(pin bidirectional line
  					(at -33.02 20.32 0)
  					(length 5.08)
  					(name "P0.12")
  					(number "72")
  				)
  				(pin bidirectional line
  					(at -33.02 17.78 0)
  					(length 5.08)
  					(name "P0.13/AIN0")
  					(number "73")
  				)
  				(pin bidirectional line
  					(at -33.02 15.24 0)
  					(length 5.08)
  					(name "P0.14/AIN1")
  					(number "74")
  				)
  				(pin bidirectional line
  					(at -33.02 12.7 0)
  					(length 5.08)
  					(name "P0.15/AIN2")
  					(number "75")
  				)
  				(pin bidirectional line
  					(at -33.02 10.16 0)
  					(length 5.08)
  					(name "P0.16/AIN3")
  					(number "77")
  				)
  				(pin bidirectional line
  					(at -33.02 7.62 0)
  					(length 5.08)
  					(name "P0.17/AIN4")
  					(number "78")
  				)
  				(pin bidirectional line
  					(at -33.02 5.08 0)
  					(length 5.08)
  					(name "P0.18/AIN5")
  					(number "79")
  				)
  				(pin bidirectional line
  					(at -33.02 2.54 0)
  					(length 5.08)
  					(name "P0.19/AIN6")
  					(number "80")
  				)
  				(pin bidirectional line
  					(at -33.02 0 0)
  					(length 5.08)
  					(name "P0.20/AIN7")
  					(number "2")
  				)
  				(pin bidirectional line
  					(at -33.02 -2.54 0)
  					(length 5.08)
  					(name "P0.26")
  					(number "44")
  				)
  				(pin bidirectional line
  					(at -33.02 -5.08 0)
  					(length 5.08)
  					(name "P0.27")
  					(number "45")
  				)
  				(pin bidirectional line
  					(at -33.02 -7.62 0)
  					(length 5.08)
  					(name "P0.28")
  					(number "47")
  				)
  				(pin bidirectional line
  					(at -33.02 -10.16 0)
  					(length 5.08)
  					(name "P0.29")
  					(number "48")
  				)
  				(pin bidirectional line
  					(at -33.02 -12.7 0)
  					(length 5.08)
  					(name "P0.30")
  					(number "49")
  				)
  				(pin bidirectional line
  					(at -33.02 -15.24 0)
  					(length 5.08)
  					(name "P0.31")
  					(number "50")
  				)
  				(pin bidirectional line
  					(at -33.02 -25.4 0)
  					(length 5.08)
  					(name "MAGPIO0")
  					(number "21")
  				)
  				(pin bidirectional line
  					(at -33.02 -27.94 0)
  					(length 5.08)
  					(name "MAGPIO1")
  					(number "22")
  				)
  				(pin bidirectional line
  					(at -33.02 -30.48 0)
  					(length 5.08)
  					(name "MAGPIO2")
  					(number "23")
  				)
  				(pin bidirectional line
  					(at -33.02 -40.64 0)
  					(length 5.08)
  					(name "SIM_CLK")
  					(number "18")
  				)
  				(pin bidirectional line
  					(at -33.02 -43.18 0)
  					(length 5.08)
  					(name "SIM_IO")
  					(number "17")
  				)
  				(pin bidirectional line
  					(at -33.02 -45.72 0)
  					(length 5.08)
  					(name "SIM_RST")
  					(number "16")
  				)
  				(pin bidirectional line
  					(at -33.02 -48.26 0)
  					(length 5.08)
  					(name "SIM_DET")
  					(number "26")
  				)
  				(pin bidirectional line
  					(at -33.02 -55.88 0)
  					(length 5.08)
  					(name "COEX0")
  					(number "52")
  				)
  				(pin bidirectional line
  					(at -33.02 -58.42 0)
  					(length 5.08)
  					(name "COEX1")
  					(number "53")
  				)
  				(pin bidirectional line
  					(at -33.02 -60.96 0)
  					(length 5.08)
  					(name "COEX2")
  					(number "54")
  				)
  				(pin no_connect line
  					(at -25.4 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "97")
  				)
  				(pin no_connect line
  					(at -22.86 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "88")
  				)
  				(pin no_connect line
  					(at -20.32 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "89")
  				)
  				(pin no_connect line
  					(at -17.78 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "90")
  				)
  				(pin no_connect line
  					(at -15.24 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "91")
  				)
  				(pin no_connect line
  					(at -12.7 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "92")
  				)
  				(pin no_connect line
  					(at -10.16 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "93")
  				)
  				(pin no_connect line
  					(at -7.62 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "94")
  				)
  				(pin no_connect line
  					(at -5.08 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "95")
  				)
  				(pin power_in line
  					(at -2.54 73.66 270)
  					(length 5.08)
  					(name "VDD")
  					(number "14")
  				)
  				(pin no_connect line
  					(at -2.54 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "96")
  				)
  				(pin power_in line
  					(at 0 73.66 270)
  					(length 5.08)
  					(name "VDD_GPIO")
  					(number "65")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "105")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "106")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "107")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "108")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "109")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "110")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "111")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "112")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "113")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "13")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "15")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "20")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "25")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "30")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "34")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "36")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "38")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "39")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "40")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "41")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "43")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "46")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "51")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "55")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "60")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "66")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "7")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "71")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND")
  					(number "76")
  				)
  				(pin power_in line
  					(at 5.08 73.66 270)
  					(length 5.08)
  					(name "SIM_1V8")
  					(number "19")
  				)
  				(pin no_connect line
  					(at 10.16 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "81")
  				)
  				(pin no_connect line
  					(at 12.7 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "82")
  				)
  				(pin no_connect line
  					(at 15.24 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "83")
  				)
  				(pin no_connect line
  					(at 17.78 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "84")
  				)
  				(pin no_connect line
  					(at 20.32 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "85")
  				)
  				(pin no_connect line
  					(at 22.86 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "86")
  				)
  				(pin no_connect line
  					(at 25.4 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "87")
  				)
  				(pin no_connect line
  					(at 27.94 -50.8 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "102")
  				)
  				(pin no_connect line
  					(at 27.94 -53.34 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "103")
  				)
  				(pin no_connect line
  					(at 27.94 -55.88 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "104")
  				)
  				(pin no_connect line
  					(at 27.94 -58.42 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "101")
  				)
  				(pin no_connect line
  					(at 27.94 -60.96 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "100")
  				)
  				(pin no_connect line
  					(at 27.94 -63.5 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "99")
  				)
  				(pin no_connect line
  					(at 27.94 -66.04 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "98")
  				)
  				(pin passive line
  					(at 33.02 58.42 180)
  					(length 5.08)
  					(name "DEC0")
  					(number "24")
  				)
  				(pin bidirectional line
  					(at 33.02 38.1 180)
  					(length 5.08)
  					(name "ANT")
  					(number "35")
  				)
  				(pin bidirectional line
  					(at 33.02 35.56 180)
  					(length 5.08)
  					(name "AUX")
  					(number "37")
  				)
  				(pin power_in line
  					(at 33.02 -27.94 180)
  					(length 5.08)
  					(name "VIO")
  					(number "29")
  				)
  				(pin bidirectional line
  					(at 33.02 -30.48 180)
  					(length 5.08)
  					(name "SCLK")
  					(number "28")
  				)
  				(pin bidirectional line
  					(at 33.02 -33.02 180)
  					(length 5.08)
  					(name "SDATA")
  					(number "27")
  				)
  			)
  			(symbol "nordic_nrf9151_laxx_1_0"
  				(pin bidirectional line
  					(at -33.02 50.8 0)
  					(length 5.08)
  					(name "P0.00")
  					(number "56")
  				)
  				(pin power_in line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(name "GND")
  					(number "1")
  				)
  				(pin no_connect line
  					(at 2.54 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "31")
  				)
  				(pin no_connect line
  					(at 5.08 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "32")
  				)
  				(pin no_connect line
  					(at 7.62 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "33")
  				)
  				(pin input line
  					(at 33.02 15.24 180)
  					(length 5.08)
  					(name "GPS")
  					(number "42")
  				)
  				(pin bidirectional line
  					(at 33.02 -5.08 180)
  					(length 5.08)
  					(name "P0.21/TRACECLK")
  					(number "5")
  				)
  				(pin bidirectional line
  					(at 33.02 -7.62 180)
  					(length 5.08)
  					(name "P0.22/TRACEDATA0")
  					(number "6")
  				)
  				(pin bidirectional line
  					(at 33.02 -10.16 180)
  					(length 5.08)
  					(name "P0.23/TRACEDATA1")
  					(number "8")
  				)
  				(pin bidirectional line
  					(at 33.02 -12.7 180)
  					(length 5.08)
  					(name "P0.24/TRACEDATA2")
  					(number "11")
  				)
  				(pin bidirectional line
  					(at 33.02 -15.24 180)
  					(length 5.08)
  					(name "P0.25/TRACEDATA3")
  					(number "12")
  				)
  				(pin input line
  					(at 33.02 -40.64 180)
  					(length 5.08)
  					(name "~{RESET}")
  					(number "9")
  				)
  				(pin input line
  					(at 33.02 -45.72 180)
  					(length 5.08)
  					(name "SWDCLK")
  					(number "3")
  				)
  				(pin bidirectional line
  					(at 33.02 -48.26 180)
  					(length 5.08)
  					(name "SWDIO")
  					(number "4")
  				)
  			)
  			(symbol "nordic_nrf9151_laxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf9160_sixx"
        (property "Footprint" "PartReel:nordic_nrf9160_sixx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf9160/page/nRF9160_html5_keyfeatures.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "LTE-M/NB-IoT SiP, 1MB Flash, 256KB RAM, Cortex-M33, GNSS, ADC, SPI, I2C, I2S, UART, PDM, PWM, LGA-100."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless cellular iot lte-m nb-iot gnss trustzone cryptocell arm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf9160_sixx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF9160-SIXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "LGA?9160*16.0x10.5m*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf9160_sixx_0_0"
  				(pin input line
  					(at -33.02 58.42 0)
  					(length 5.08)
  					(name "ENABLE")
  					(number "101")
  				)
  				(pin bidirectional line
  					(at -33.02 50.8 0)
  					(length 5.08)
  					(name "P0.00")
  					(number "95")
  				)
  				(pin bidirectional line
  					(at -33.02 48.26 0)
  					(length 5.08)
  					(name "P0.01")
  					(number "96")
  				)
  				(pin bidirectional line
  					(at -33.02 45.72 0)
  					(length 5.08)
  					(name "P0.02")
  					(number "97")
  				)
  				(pin bidirectional line
  					(at -33.02 43.18 0)
  					(length 5.08)
  					(name "P0.03")
  					(number "99")
  				)
  				(pin bidirectional line
  					(at -33.02 40.64 0)
  					(length 5.08)
  					(name "P0.04")
  					(number "100")
  				)
  				(pin bidirectional line
  					(at -33.02 38.1 0)
  					(length 5.08)
  					(name "P0.05")
  					(number "2")
  				)
  				(pin bidirectional line
  					(at -33.02 35.56 0)
  					(length 5.08)
  					(name "P0.06")
  					(number "3")
  				)
  				(pin bidirectional line
  					(at -33.02 33.02 0)
  					(length 5.08)
  					(name "P0.07")
  					(number "4")
  				)
  				(pin bidirectional line
  					(at -33.02 30.48 0)
  					(length 5.08)
  					(name "P0.08")
  					(number "15")
  				)
  				(pin bidirectional line
  					(at -33.02 27.94 0)
  					(length 5.08)
  					(name "P0.09")
  					(number "16")
  				)
  				(pin bidirectional line
  					(at -33.02 25.4 0)
  					(length 5.08)
  					(name "P0.10")
  					(number "18")
  				)
  				(pin bidirectional line
  					(at -33.02 22.86 0)
  					(length 5.08)
  					(name "P0.11")
  					(number "19")
  				)
  				(pin bidirectional line
  					(at -33.02 20.32 0)
  					(length 5.08)
  					(name "P0.12")
  					(number "20")
  				)
  				(pin bidirectional line
  					(at -33.02 17.78 0)
  					(length 5.08)
  					(name "P0.13/AIN0")
  					(number "23")
  				)
  				(pin bidirectional line
  					(at -33.02 15.24 0)
  					(length 5.08)
  					(name "P0.14/AIN1")
  					(number "24")
  				)
  				(pin bidirectional line
  					(at -33.02 12.7 0)
  					(length 5.08)
  					(name "P0.15/AIN2")
  					(number "25")
  				)
  				(pin bidirectional line
  					(at -33.02 10.16 0)
  					(length 5.08)
  					(name "P0.16/AIN3")
  					(number "26")
  				)
  				(pin bidirectional line
  					(at -33.02 7.62 0)
  					(length 5.08)
  					(name "P0.17/AIN4")
  					(number "28")
  				)
  				(pin bidirectional line
  					(at -33.02 5.08 0)
  					(length 5.08)
  					(name "P0.18/AIN5")
  					(number "29")
  				)
  				(pin bidirectional line
  					(at -33.02 2.54 0)
  					(length 5.08)
  					(name "P0.19/AIN6")
  					(number "30")
  				)
  				(pin bidirectional line
  					(at -33.02 0 0)
  					(length 5.08)
  					(name "P0.20/AIN7")
  					(number "35")
  				)
  				(pin bidirectional line
  					(at -33.02 -2.54 0)
  					(length 5.08)
  					(name "P0.26")
  					(number "83")
  				)
  				(pin bidirectional line
  					(at -33.02 -5.08 0)
  					(length 5.08)
  					(name "P0.27")
  					(number "84")
  				)
  				(pin bidirectional line
  					(at -33.02 -7.62 0)
  					(length 5.08)
  					(name "P0.28")
  					(number "86")
  				)
  				(pin bidirectional line
  					(at -33.02 -10.16 0)
  					(length 5.08)
  					(name "P0.29")
  					(number "87")
  				)
  				(pin bidirectional line
  					(at -33.02 -12.7 0)
  					(length 5.08)
  					(name "P0.30")
  					(number "88")
  				)
  				(pin bidirectional line
  					(at -33.02 -15.24 0)
  					(length 5.08)
  					(name "P0.31")
  					(number "89")
  				)
  				(pin bidirectional line
  					(at -33.02 -25.4 0)
  					(length 5.08)
  					(name "MAGPIO0")
  					(number "55")
  				)
  				(pin bidirectional line
  					(at -33.02 -27.94 0)
  					(length 5.08)
  					(name "MAGPIO1")
  					(number "54")
  				)
  				(pin bidirectional line
  					(at -33.02 -30.48 0)
  					(length 5.08)
  					(name "MAGPIO2")
  					(number "53")
  				)
  				(pin bidirectional line
  					(at -33.02 -40.64 0)
  					(length 5.08)
  					(name "SIM_CLK")
  					(number "46")
  				)
  				(pin bidirectional line
  					(at -33.02 -43.18 0)
  					(length 5.08)
  					(name "SIM_IO")
  					(number "48")
  				)
  				(pin bidirectional line
  					(at -33.02 -45.72 0)
  					(length 5.08)
  					(name "SIM_RST")
  					(number "43")
  				)
  				(pin bidirectional line
  					(at -33.02 -48.26 0)
  					(length 5.08)
  					(name "SIM_DET")
  					(number "45")
  				)
  				(pin bidirectional line
  					(at -33.02 -55.88 0)
  					(length 5.08)
  					(name "COEX0")
  					(number "93")
  				)
  				(pin bidirectional line
  					(at -33.02 -58.42 0)
  					(length 5.08)
  					(name "COEX1")
  					(number "92")
  				)
  				(pin bidirectional line
  					(at -33.02 -60.96 0)
  					(length 5.08)
  					(name "COEX2")
  					(number "91")
  				)
  				(pin power_in line
  					(at -5.08 73.66 270)
  					(length 5.08)
  					(name "VDD1")
  					(number "102")
  				)
  				(pin power_in line
  					(at -2.54 73.66 270)
  					(length 5.08)
  					(name "VDD2")
  					(number "22")
  				)
  				(pin power_in line
  					(at 0 73.66 270)
  					(length 5.08)
  					(name "VDD_GPIO")
  					(number "12")
  				)
  				(pin power_in line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(name "VSS")
  					(number "103")
  				)
  				(pin power_in line
  					(at 5.08 73.66 270)
  					(length 5.08)
  					(name "SIM_1V8")
  					(number "49")
  				)
  				(pin bidirectional line
  					(at 33.02 38.1 180)
  					(length 5.08)
  					(name "ANT")
  					(number "61")
  				)
  				(pin bidirectional line
  					(at 33.02 35.56 180)
  					(length 5.08)
  					(name "AUX")
  					(number "64")
  				)
  				(pin bidirectional line
  					(at 33.02 -5.08 180)
  					(length 5.08)
  					(name "P0.21/TRACECLK")
  					(number "37")
  				)
  				(pin bidirectional line
  					(at 33.02 -7.62 180)
  					(length 5.08)
  					(name "P0.22/TRACEDATA0")
  					(number "38")
  				)
  				(pin bidirectional line
  					(at 33.02 -10.16 180)
  					(length 5.08)
  					(name "P0.23/TRACEDATA1")
  					(number "39")
  				)
  				(pin bidirectional line
  					(at 33.02 -12.7 180)
  					(length 5.08)
  					(name "P0.24/TRACEDATA2")
  					(number "40")
  				)
  				(pin bidirectional line
  					(at 33.02 -15.24 180)
  					(length 5.08)
  					(name "P0.25/TRACEDATA3")
  					(number "42")
  				)
  				(pin bidirectional line
  					(at 33.02 -30.48 180)
  					(length 5.08)
  					(name "SCLK")
  					(number "58")
  				)
  				(pin bidirectional line
  					(at 33.02 -33.02 180)
  					(length 5.08)
  					(name "SDATA")
  					(number "59")
  				)
  				(pin bidirectional line
  					(at 33.02 -45.72 180)
  					(length 5.08)
  					(name "SWDCLK")
  					(number "33")
  				)
  				(pin bidirectional line
  					(at 33.02 -48.26 180)
  					(length 5.08)
  					(name "SWDIO")
  					(number "34")
  				)
  			)
  			(symbol "nordic_nrf9160_sixx_1_0"
  				(pin no_connect line
  					(at -27.94 -50.8 0)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "115")
  				)
  				(pin no_connect line
  					(at -27.94 -53.34 0)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "125")
  				)
  				(pin no_connect line
  					(at -25.4 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "117")
  				)
  				(pin no_connect line
  					(at -22.86 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "114")
  				)
  				(pin no_connect line
  					(at -20.32 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "106")
  				)
  				(pin no_connect line
  					(at -17.78 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "118")
  				)
  				(pin no_connect line
  					(at -15.24 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "107")
  				)
  				(pin no_connect line
  					(at -12.7 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "108")
  				)
  				(pin no_connect line
  					(at -10.16 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "127")
  				)
  				(pin no_connect line
  					(at -7.62 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "70")
  				)
  				(pin no_connect line
  					(at -5.08 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "119")
  				)
  				(pin no_connect line
  					(at -2.54 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "71")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "1")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "11")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "14")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "17")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "21")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "27")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "31")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "36")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "41")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "44")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "47")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "5")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "50")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "52")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "56")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "6")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "60")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "62")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "63")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "65")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "66")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "68")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "69")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "7")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "72")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "74")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "75")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "76")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "77")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "78")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "79")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "8")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "80")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "81")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "82")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "85")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "9")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "90")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "94")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "98")
  				)
  				(pin no_connect line
  					(at 2.54 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "104")
  				)
  				(pin no_connect line
  					(at 5.08 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "122")
  				)
  				(pin no_connect line
  					(at 7.62 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "111")
  				)
  				(pin no_connect line
  					(at 10.16 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "51")
  				)
  				(pin no_connect line
  					(at 12.7 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "73")
  				)
  				(pin no_connect line
  					(at 15.24 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "110")
  				)
  				(pin no_connect line
  					(at 17.78 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "121")
  				)
  				(pin no_connect line
  					(at 20.32 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "10")
  				)
  				(pin no_connect line
  					(at 22.86 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "109")
  				)
  				(pin no_connect line
  					(at 25.4 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "120")
  				)
  				(pin no_connect line
  					(at 27.94 -22.86 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "112")
  				)
  				(pin no_connect line
  					(at 27.94 -35.56 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "123")
  				)
  				(pin no_connect line
  					(at 27.94 -38.1 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "124")
  				)
  				(pin no_connect line
  					(at 27.94 -50.8 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "113")
  				)
  				(pin no_connect line
  					(at 27.94 -53.34 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "105")
  				)
  				(pin no_connect line
  					(at 27.94 -55.88 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "126")
  				)
  				(pin no_connect line
  					(at 27.94 -66.04 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "116")
  				)
  				(pin passive line
  					(at 33.02 58.42 180)
  					(length 5.08)
  					(name "DEC0")
  					(number "13")
  				)
  				(pin input line
  					(at 33.02 15.24 180)
  					(length 5.08)
  					(name "GPS")
  					(number "67")
  				)
  				(pin power_in line
  					(at 33.02 -27.94 180)
  					(length 5.08)
  					(name "VIO")
  					(number "57")
  				)
  				(pin input line
  					(at 33.02 -40.64 180)
  					(length 5.08)
  					(name "~{RESET}")
  					(number "32")
  				)
  			)
  			(symbol "nordic_nrf9160_sixx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_nrf9161_sixx"
        (property "Footprint" "PartReel:nordic_nrf9161_sixx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf9161/page/nRF9161_html5_keyfeatures.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "LTE-M/NB-IoT/DECT-NR+ SiP, ARM Cortex-M33, GNSS, LTE PC3, LGA-100."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless cellular iot lte-m nb-iot dect-nr+ gnss trustzone arm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_nrf9161_sixx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nRF9161-SIXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "LGA?9161*16.0x10.5mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_nrf9161_sixx_0_0"
  				(pin bidirectional line
  					(at -33.02 50.8 0)
  					(length 5.08)
  					(name "P0.00")
  					(number "95")
  				)
  				(pin bidirectional line
  					(at -33.02 48.26 0)
  					(length 5.08)
  					(name "P0.01")
  					(number "96")
  				)
  				(pin bidirectional line
  					(at -33.02 45.72 0)
  					(length 5.08)
  					(name "P0.02")
  					(number "97")
  				)
  				(pin bidirectional line
  					(at -33.02 43.18 0)
  					(length 5.08)
  					(name "P0.03")
  					(number "99")
  				)
  				(pin bidirectional line
  					(at -33.02 40.64 0)
  					(length 5.08)
  					(name "P0.04")
  					(number "100")
  				)
  				(pin bidirectional line
  					(at -33.02 38.1 0)
  					(length 5.08)
  					(name "P0.05")
  					(number "2")
  				)
  				(pin bidirectional line
  					(at -33.02 35.56 0)
  					(length 5.08)
  					(name "P0.06")
  					(number "3")
  				)
  				(pin bidirectional line
  					(at -33.02 33.02 0)
  					(length 5.08)
  					(name "P0.07")
  					(number "4")
  				)
  				(pin bidirectional line
  					(at -33.02 30.48 0)
  					(length 5.08)
  					(name "P0.08")
  					(number "15")
  				)
  				(pin bidirectional line
  					(at -33.02 27.94 0)
  					(length 5.08)
  					(name "P0.09")
  					(number "16")
  				)
  				(pin bidirectional line
  					(at -33.02 25.4 0)
  					(length 5.08)
  					(name "P0.10")
  					(number "18")
  				)
  				(pin bidirectional line
  					(at -33.02 22.86 0)
  					(length 5.08)
  					(name "P0.11")
  					(number "19")
  				)
  				(pin bidirectional line
  					(at -33.02 20.32 0)
  					(length 5.08)
  					(name "P0.12")
  					(number "20")
  				)
  				(pin bidirectional line
  					(at -33.02 17.78 0)
  					(length 5.08)
  					(name "P0.13/AIN0")
  					(number "23")
  				)
  				(pin bidirectional line
  					(at -33.02 15.24 0)
  					(length 5.08)
  					(name "P0.14/AIN1")
  					(number "24")
  				)
  				(pin bidirectional line
  					(at -33.02 12.7 0)
  					(length 5.08)
  					(name "P0.15/AIN2")
  					(number "25")
  				)
  				(pin bidirectional line
  					(at -33.02 10.16 0)
  					(length 5.08)
  					(name "P0.16/AIN3")
  					(number "26")
  				)
  				(pin bidirectional line
  					(at -33.02 7.62 0)
  					(length 5.08)
  					(name "P0.17/AIN4")
  					(number "28")
  				)
  				(pin bidirectional line
  					(at -33.02 5.08 0)
  					(length 5.08)
  					(name "P0.18/AIN5")
  					(number "29")
  				)
  				(pin bidirectional line
  					(at -33.02 2.54 0)
  					(length 5.08)
  					(name "P0.19/AIN6")
  					(number "30")
  				)
  				(pin bidirectional line
  					(at -33.02 0 0)
  					(length 5.08)
  					(name "P0.20/AIN7")
  					(number "35")
  				)
  				(pin bidirectional line
  					(at -33.02 -2.54 0)
  					(length 5.08)
  					(name "P0.26")
  					(number "83")
  				)
  				(pin bidirectional line
  					(at -33.02 -5.08 0)
  					(length 5.08)
  					(name "P0.27")
  					(number "84")
  				)
  				(pin bidirectional line
  					(at -33.02 -7.62 0)
  					(length 5.08)
  					(name "P0.28")
  					(number "86")
  				)
  				(pin bidirectional line
  					(at -33.02 -10.16 0)
  					(length 5.08)
  					(name "P0.29")
  					(number "87")
  				)
  				(pin bidirectional line
  					(at -33.02 -12.7 0)
  					(length 5.08)
  					(name "P0.30")
  					(number "88")
  				)
  				(pin bidirectional line
  					(at -33.02 -15.24 0)
  					(length 5.08)
  					(name "P0.31")
  					(number "89")
  				)
  				(pin bidirectional line
  					(at -33.02 -25.4 0)
  					(length 5.08)
  					(name "MAGPIO0")
  					(number "55")
  				)
  				(pin bidirectional line
  					(at -33.02 -27.94 0)
  					(length 5.08)
  					(name "MAGPIO1")
  					(number "54")
  				)
  				(pin bidirectional line
  					(at -33.02 -30.48 0)
  					(length 5.08)
  					(name "MAGPIO2")
  					(number "53")
  				)
  				(pin bidirectional line
  					(at -33.02 -40.64 0)
  					(length 5.08)
  					(name "SIM_CLK")
  					(number "46")
  				)
  				(pin bidirectional line
  					(at -33.02 -43.18 0)
  					(length 5.08)
  					(name "SIM_IO")
  					(number "48")
  				)
  				(pin bidirectional line
  					(at -33.02 -45.72 0)
  					(length 5.08)
  					(name "SIM_RST")
  					(number "43")
  				)
  				(pin bidirectional line
  					(at -33.02 -48.26 0)
  					(length 5.08)
  					(name "SIM_DET")
  					(number "45")
  				)
  				(pin bidirectional line
  					(at -33.02 -55.88 0)
  					(length 5.08)
  					(name "COEX0")
  					(number "93")
  				)
  				(pin bidirectional line
  					(at -33.02 -58.42 0)
  					(length 5.08)
  					(name "COEX1")
  					(number "92")
  				)
  				(pin bidirectional line
  					(at -33.02 -60.96 0)
  					(length 5.08)
  					(name "COEX2")
  					(number "91")
  				)
  				(pin power_in line
  					(at -2.54 73.66 270)
  					(length 5.08)
  					(name "VDD2")
  					(number "22")
  				)
  				(pin power_in line
  					(at 0 73.66 270)
  					(length 5.08)
  					(name "VDD_GPIO")
  					(number "12")
  				)
  				(pin power_in line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(name "VSS")
  					(number "103")
  				)
  				(pin power_in line
  					(at 5.08 73.66 270)
  					(length 5.08)
  					(name "SIM_1V8")
  					(number "49")
  				)
  				(pin bidirectional line
  					(at 33.02 38.1 180)
  					(length 5.08)
  					(name "ANT")
  					(number "61")
  				)
  				(pin bidirectional line
  					(at 33.02 35.56 180)
  					(length 5.08)
  					(name "AUX")
  					(number "64")
  				)
  				(pin bidirectional line
  					(at 33.02 -5.08 180)
  					(length 5.08)
  					(name "P0.21/TRACECLK")
  					(number "37")
  				)
  				(pin bidirectional line
  					(at 33.02 -7.62 180)
  					(length 5.08)
  					(name "P0.22/TRACEDATA0")
  					(number "38")
  				)
  				(pin bidirectional line
  					(at 33.02 -10.16 180)
  					(length 5.08)
  					(name "P0.23/TRACEDATA1")
  					(number "39")
  				)
  				(pin bidirectional line
  					(at 33.02 -12.7 180)
  					(length 5.08)
  					(name "P0.24/TRACEDATA2")
  					(number "40")
  				)
  				(pin bidirectional line
  					(at 33.02 -15.24 180)
  					(length 5.08)
  					(name "P0.25/TRACEDATA3")
  					(number "42")
  				)
  				(pin bidirectional line
  					(at 33.02 -30.48 180)
  					(length 5.08)
  					(name "SCLK")
  					(number "58")
  				)
  				(pin bidirectional line
  					(at 33.02 -33.02 180)
  					(length 5.08)
  					(name "SDATA")
  					(number "59")
  				)
  				(pin bidirectional line
  					(at 33.02 -45.72 180)
  					(length 5.08)
  					(name "SWDCLK")
  					(number "33")
  				)
  				(pin bidirectional line
  					(at 33.02 -48.26 180)
  					(length 5.08)
  					(name "SWDIO")
  					(number "34")
  				)
  			)
  			(symbol "nordic_nrf9161_sixx_1_0"
  				(pin input line
  					(at -33.02 58.42 0)
  					(length 5.08)
  					(name "ENABLE")
  					(number "101")
  				)
  				(pin no_connect line
  					(at -27.94 -50.8 0)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "115")
  				)
  				(pin no_connect line
  					(at -27.94 -53.34 0)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "125")
  				)
  				(pin no_connect line
  					(at -25.4 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "117")
  				)
  				(pin no_connect line
  					(at -22.86 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "114")
  				)
  				(pin no_connect line
  					(at -20.32 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "106")
  				)
  				(pin no_connect line
  					(at -17.78 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "118")
  				)
  				(pin no_connect line
  					(at -15.24 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "107")
  				)
  				(pin no_connect line
  					(at -12.7 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "108")
  				)
  				(pin no_connect line
  					(at -10.16 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "127")
  				)
  				(pin no_connect line
  					(at -7.62 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "70")
  				)
  				(pin power_in line
  					(at -5.08 73.66 270)
  					(length 5.08)
  					(name "VDD1")
  					(number "102")
  				)
  				(pin no_connect line
  					(at -5.08 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "119")
  				)
  				(pin no_connect line
  					(at -2.54 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "71")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "1")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "11")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "14")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "17")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "21")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "27")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "31")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "36")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "41")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "44")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "47")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "5")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "50")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "52")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "56")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "6")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "60")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "62")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "63")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "65")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "66")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "68")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "69")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "7")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "72")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "74")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "75")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "76")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "77")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "78")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "79")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "8")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "80")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "81")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "82")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "85")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "9")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "90")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "94")
  				)
  				(pin passive line
  					(at 0 -73.66 90)
  					(length 5.08)
  					(hide yes)
  					(name "GND_Shield")
  					(number "98")
  				)
  				(pin no_connect line
  					(at 2.54 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "104")
  				)
  				(pin no_connect line
  					(at 5.08 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "122")
  				)
  				(pin no_connect line
  					(at 7.62 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "111")
  				)
  				(pin no_connect line
  					(at 10.16 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "51")
  				)
  				(pin no_connect line
  					(at 12.7 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "73")
  				)
  				(pin no_connect line
  					(at 15.24 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "110")
  				)
  				(pin no_connect line
  					(at 17.78 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "121")
  				)
  				(pin no_connect line
  					(at 20.32 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "10")
  				)
  				(pin no_connect line
  					(at 22.86 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "109")
  				)
  				(pin no_connect line
  					(at 25.4 -68.58 90)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "120")
  				)
  				(pin no_connect line
  					(at 27.94 -22.86 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "112")
  				)
  				(pin no_connect line
  					(at 27.94 -35.56 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "123")
  				)
  				(pin no_connect line
  					(at 27.94 -38.1 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "124")
  				)
  				(pin no_connect line
  					(at 27.94 -50.8 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "113")
  				)
  				(pin no_connect line
  					(at 27.94 -53.34 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "105")
  				)
  				(pin no_connect line
  					(at 27.94 -55.88 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "126")
  				)
  				(pin no_connect line
  					(at 27.94 -66.04 180)
  					(length 5.08)
  					(hide yes)
  					(name "NC")
  					(number "116")
  				)
  				(pin passive line
  					(at 33.02 58.42 180)
  					(length 5.08)
  					(name "DEC0")
  					(number "13")
  				)
  				(pin input line
  					(at 33.02 15.24 180)
  					(length 5.08)
  					(name "GPS")
  					(number "67")
  				)
  				(pin power_in line
  					(at 33.02 -27.94 180)
  					(length 5.08)
  					(name "VIO")
  					(number "57")
  				)
  				(pin input line
  					(at 33.02 -40.64 180)
  					(length 5.08)
  					(name "~{RESET}")
  					(number "32")
  				)
  			)
  			(symbol "nordic_nrf9161_sixx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "es8311" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 15.97 0))
      (property "Value" "ES8311 Mono Audio Codec" (at 0 -18.51 0))
        (property "Footprint" "PartReel:es8311"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.everest-semi.com/pdf/ES8311%20PB.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Everest ES8311 low-power mono audio codec - Espressif's reference codec (ESP32-S3-Box, Korvo, most ESP32 voice kits). I2S/PCM + I2C (0x18/0x19 via CE), 1.6-3.6V, QFN-20 3x3."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "es8311 everest codec audio i2s esp32 qfn"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/es8311/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "es8311_1_1"
        (pin passive line (at -16.29 11.43 0) (length 2.54)
          (name "CCLK")
          (number "1"))
        (pin passive line (at -16.29 8.89 0) (length 2.54)
          (name "MCLK")
          (number "2"))
        (pin passive line (at -16.29 6.35 0) (length 2.54)
          (name "PVDD")
          (number "3"))
        (pin passive line (at -16.29 3.81 0) (length 2.54)
          (name "DVDD")
          (number "4"))
        (pin passive line (at -16.29 1.27 0) (length 2.54)
          (name "DGND")
          (number "5"))
        (pin passive line (at -16.29 -1.27 0) (length 2.54)
          (name "SCLK/DMIC_SCL")
          (number "6"))
        (pin passive line (at -16.29 -3.81 0) (length 2.54)
          (name "ASDOUT")
          (number "7"))
        (pin passive line (at -16.29 -6.35 0) (length 2.54)
          (name "LRCK")
          (number "8"))
        (pin passive line (at -16.29 -8.89 0) (length 2.54)
          (name "DSDIN")
          (number "9"))
        (pin passive line (at -16.29 -11.43 0) (length 2.54)
          (name "AGND")
          (number "10"))
        (pin passive line (at 16.29 11.43 180) (length 2.54)
          (name "AVDD")
          (number "11"))
        (pin passive line (at 16.29 8.89 180) (length 2.54)
          (name "OUTP")
          (number "12"))
        (pin passive line (at 16.29 6.35 180) (length 2.54)
          (name "OUTN")
          (number "13"))
        (pin passive line (at 16.29 3.81 180) (length 2.54)
          (name "DACVREF")
          (number "14"))
        (pin passive line (at 16.29 1.27 180) (length 2.54)
          (name "ADCVREF")
          (number "15"))
        (pin passive line (at 16.29 -1.27 180) (length 2.54)
          (name "VMID")
          (number "16"))
        (pin passive line (at 16.29 -3.81 180) (length 2.54)
          (name "MIC1N")
          (number "17"))
        (pin passive line (at 16.29 -6.35 180) (length 2.54)
          (name "MIC1P/DMIC_SDA")
          (number "18"))
        (pin passive line (at 16.29 -8.89 180) (length 2.54)
          (name "CDATA")
          (number "19"))
        (pin passive line (at 16.29 -11.43 180) (length 2.54)
          (name "CE")
          (number "20"))
        (pin passive line (at 0.00 -19.05 90) (length 2.54)
          (name "EP/GND")
          (number "21"))
      )
    )
  (symbol "inmp441" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 9.62 0))
      (property "Value" "INMP441 I2S MEMS Microphone" (at 0 -9.62 0))
        (property "Footprint" "PartReel:inmp441"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.farnell.com/datasheets/1824785.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "TDK InvenSense INMP441 omnidirectional bottom-port MEMS microphone with 24-bit I2S output, 1.8-3.3V. The default ESP32 I2S mic. Footprint includes the required PCB sound hole (0.8mm NPTH) under the port ring - keep solder paste off the hole."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "inmp441 invensense mems microphone i2s esp32 audio"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/inmp441/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "inmp441_1_1"
        (pin passive line (at -11.43 5.08 0) (length 2.54)
          (name "SCK")
          (number "1"))
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "SD")
          (number "2"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "WS")
          (number "3"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "L/R")
          (number "4"))
        (pin passive line (at -11.43 -5.08 0) (length 2.54)
          (name "GND")
          (number "5"))
        (pin passive line (at 11.43 5.08 180) (length 2.54)
          (name "GND")
          (number "6"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "VDD")
          (number "7"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "CHIPEN")
          (number "8"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "GND")
          (number "9"))
      )
    )
  (symbol "vs1053b" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 33.75 0))
      (property "Value" "VS1053B MP3/Ogg Audio Codec" (at 0 -33.75 0))
        (property "Footprint" "PartReel:vs1053b"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.vlsi.fi/fileadmin/datasheets/vs1053.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "VLSI VS1053B MP3/Ogg Vorbis/AAC/WMA/MIDI audio codec with headphone driver, SPI control/data, LQFP-48. The Adafruit Music Maker chip. GBUF must never be grounded; CVDD 1.8V core."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "vs1053 vlsi mp3 ogg codec audio spi lqfp"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/vs1053b/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "vs1053b_1_1"
        (pin passive line (at -17.64 29.21 0) (length 2.54)
          (name "MICP/LINE1")
          (number "1"))
        (pin passive line (at -17.64 26.67 0) (length 2.54)
          (name "MICN")
          (number "2"))
        (pin passive line (at -17.64 24.13 0) (length 2.54)
          (name "XRESET")
          (number "3"))
        (pin passive line (at -17.64 21.59 0) (length 2.54)
          (name "DGND0")
          (number "4"))
        (pin passive line (at -17.64 19.05 0) (length 2.54)
          (name "CVDD0")
          (number "5"))
        (pin passive line (at -17.64 16.51 0) (length 2.54)
          (name "IOVDD0")
          (number "6"))
        (pin passive line (at -17.64 13.97 0) (length 2.54)
          (name "CVDD1")
          (number "7"))
        (pin passive line (at -17.64 11.43 0) (length 2.54)
          (name "DREQ")
          (number "8"))
        (pin passive line (at -17.64 8.89 0) (length 2.54)
          (name "GPIO2/DCLK")
          (number "9"))
        (pin passive line (at -17.64 6.35 0) (length 2.54)
          (name "GPIO3/SDATA")
          (number "10"))
        (pin passive line (at -17.64 3.81 0) (length 2.54)
          (name "GPIO6/I2S_SCLK")
          (number "11"))
        (pin passive line (at -17.64 1.27 0) (length 2.54)
          (name "GPIO7/I2S_SDATA")
          (number "12"))
        (pin passive line (at -17.64 -1.27 0) (length 2.54)
          (name "XDCS/BSYNC")
          (number "13"))
        (pin passive line (at -17.64 -3.81 0) (length 2.54)
          (name "IOVDD1")
          (number "14"))
        (pin passive line (at -17.64 -6.35 0) (length 2.54)
          (name "VCO")
          (number "15"))
        (pin passive line (at -17.64 -8.89 0) (length 2.54)
          (name "DGND1")
          (number "16"))
        (pin passive line (at -17.64 -11.43 0) (length 2.54)
          (name "XTALO")
          (number "17"))
        (pin passive line (at -17.64 -13.97 0) (length 2.54)
          (name "XTALI")
          (number "18"))
        (pin passive line (at -17.64 -16.51 0) (length 2.54)
          (name "IOVDD2")
          (number "19"))
        (pin passive line (at -17.64 -19.05 0) (length 2.54)
          (name "DGND2")
          (number "20"))
        (pin passive line (at -17.64 -21.59 0) (length 2.54)
          (name "DGND3")
          (number "21"))
        (pin passive line (at -17.64 -24.13 0) (length 2.54)
          (name "DGND4")
          (number "22"))
        (pin passive line (at -17.64 -26.67 0) (length 2.54)
          (name "XCS")
          (number "23"))
        (pin passive line (at -17.64 -29.21 0) (length 2.54)
          (name "CVDD2")
          (number "24"))
        (pin passive line (at 17.64 29.21 180) (length 2.54)
          (name "GPIO5/I2S_MCLK")
          (number "25"))
        (pin passive line (at 17.64 26.67 180) (length 2.54)
          (name "RX")
          (number "26"))
        (pin passive line (at 17.64 24.13 180) (length 2.54)
          (name "TX")
          (number "27"))
        (pin passive line (at 17.64 21.59 180) (length 2.54)
          (name "SCLK")
          (number "28"))
        (pin passive line (at 17.64 19.05 180) (length 2.54)
          (name "SI")
          (number "29"))
        (pin passive line (at 17.64 16.51 180) (length 2.54)
          (name "SO")
          (number "30"))
        (pin passive line (at 17.64 13.97 180) (length 2.54)
          (name "CVDD3")
          (number "31"))
        (pin passive line (at 17.64 11.43 180) (length 2.54)
          (name "XTEST")
          (number "32"))
        (pin passive line (at 17.64 8.89 180) (length 2.54)
          (name "GPIO0")
          (number "33"))
        (pin passive line (at 17.64 6.35 180) (length 2.54)
          (name "GPIO1")
          (number "34"))
        (pin passive line (at 17.64 3.81 180) (length 2.54)
          (name "GND")
          (number "35"))
        (pin passive line (at 17.64 1.27 180) (length 2.54)
          (name "GPIO4/I2S_LROUT")
          (number "36"))
        (pin passive line (at 17.64 -1.27 180) (length 2.54)
          (name "AGND0")
          (number "37"))
        (pin passive line (at 17.64 -3.81 180) (length 2.54)
          (name "AVDD0")
          (number "38"))
        (pin passive line (at 17.64 -6.35 180) (length 2.54)
          (name "RIGHT")
          (number "39"))
        (pin passive line (at 17.64 -8.89 180) (length 2.54)
          (name "AGND1")
          (number "40"))
        (pin passive line (at 17.64 -11.43 180) (length 2.54)
          (name "AGND2")
          (number "41"))
        (pin passive line (at 17.64 -13.97 180) (length 2.54)
          (name "GBUF")
          (number "42"))
        (pin passive line (at 17.64 -16.51 180) (length 2.54)
          (name "AVDD1")
          (number "43"))
        (pin passive line (at 17.64 -19.05 180) (length 2.54)
          (name "RCAP")
          (number "44"))
        (pin passive line (at 17.64 -21.59 180) (length 2.54)
          (name "AVDD2")
          (number "45"))
        (pin passive line (at 17.64 -24.13 180) (length 2.54)
          (name "LEFT")
          (number "46"))
        (pin passive line (at 17.64 -26.67 180) (length 2.54)
          (name "AGND3")
          (number "47"))
        (pin passive line (at 17.64 -29.21 180) (length 2.54)
          (name "LINE2")
          (number "48"))
      )
    )
  (symbol "wm8960" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 23.59 0))
      (property "Value" "WM8960 Stereo Audio Codec" (at 0 -26.13 0))
        (property "Footprint" "PartReel:wm8960"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://wiki.geekworm.com/images/5/58/WM8960-Datasheet.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cirrus/Wolfson WM8960 stereo CODEC with 1W class-D speaker drivers and headphone amp, I2S audio + 2-wire control (write-only, addr 0x1A), QFN-32 5x5. Raspberry Pi / ESP32 audio HAT staple. EP = analogue GND."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "wm8960 wolfson cirrus codec audio i2s class-d qfn"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/wm8960/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "wm8960_1_1"
        (pin passive line (at -12.69 19.05 0) (length 2.54)
          (name "MICBIAS")
          (number "1"))
        (pin passive line (at -12.69 16.51 0) (length 2.54)
          (name "LINPUT3/JD2")
          (number "2"))
        (pin passive line (at -12.69 13.97 0) (length 2.54)
          (name "LINPUT2")
          (number "3"))
        (pin passive line (at -12.69 11.43 0) (length 2.54)
          (name "LINPUT1")
          (number "4"))
        (pin passive line (at -12.69 8.89 0) (length 2.54)
          (name "RINPUT1")
          (number "5"))
        (pin passive line (at -12.69 6.35 0) (length 2.54)
          (name "RINPUT2")
          (number "6"))
        (pin passive line (at -12.69 3.81 0) (length 2.54)
          (name "RINPUT3/JD3")
          (number "7"))
        (pin passive line (at -12.69 1.27 0) (length 2.54)
          (name "DCVDD")
          (number "8"))
        (pin passive line (at -12.69 -1.27 0) (length 2.54)
          (name "DGND")
          (number "9"))
        (pin passive line (at -12.69 -3.81 0) (length 2.54)
          (name "DBVDD")
          (number "10"))
        (pin passive line (at -12.69 -6.35 0) (length 2.54)
          (name "MCLK")
          (number "11"))
        (pin passive line (at -12.69 -8.89 0) (length 2.54)
          (name "BCLK")
          (number "12"))
        (pin passive line (at -12.69 -11.43 0) (length 2.54)
          (name "DACLRC")
          (number "13"))
        (pin passive line (at -12.69 -13.97 0) (length 2.54)
          (name "DACDAT")
          (number "14"))
        (pin passive line (at -12.69 -16.51 0) (length 2.54)
          (name "ADCLRC/GPIO1")
          (number "15"))
        (pin passive line (at -12.69 -19.05 0) (length 2.54)
          (name "ADCDAT")
          (number "16"))
        (pin passive line (at 12.69 19.05 180) (length 2.54)
          (name "SCLK")
          (number "17"))
        (pin passive line (at 12.69 16.51 180) (length 2.54)
          (name "SDIN")
          (number "18"))
        (pin passive line (at 12.69 13.97 180) (length 2.54)
          (name "SPK_RN")
          (number "19"))
        (pin passive line (at 12.69 11.43 180) (length 2.54)
          (name "SPKGND2")
          (number "20"))
        (pin passive line (at 12.69 8.89 180) (length 2.54)
          (name "SPKVDD2")
          (number "21"))
        (pin passive line (at 12.69 6.35 180) (length 2.54)
          (name "SPK_RP")
          (number "22"))
        (pin passive line (at 12.69 3.81 180) (length 2.54)
          (name "SPK_LN")
          (number "23"))
        (pin passive line (at 12.69 1.27 180) (length 2.54)
          (name "SPKGND1")
          (number "24"))
        (pin passive line (at 12.69 -1.27 180) (length 2.54)
          (name "SPK_LP")
          (number "25"))
        (pin passive line (at 12.69 -3.81 180) (length 2.54)
          (name "SPKVDD1")
          (number "26"))
        (pin passive line (at 12.69 -6.35 180) (length 2.54)
          (name "VMID")
          (number "27"))
        (pin passive line (at 12.69 -8.89 180) (length 2.54)
          (name "AGND")
          (number "28"))
        (pin passive line (at 12.69 -11.43 180) (length 2.54)
          (name "HP_R")
          (number "29"))
        (pin passive line (at 12.69 -13.97 180) (length 2.54)
          (name "OUT3")
          (number "30"))
        (pin passive line (at 12.69 -16.51 180) (length 2.54)
          (name "HP_L")
          (number "31"))
        (pin passive line (at 12.69 -19.05 180) (length 2.54)
          (name "AVDD")
          (number "32"))
        (pin passive line (at 0.00 -26.67 90) (length 2.54)
          (name "EP/AGND")
          (number "33"))
      )
    )
  (symbol "a4988" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 21.05 0))
      (property "Value" "A4988 Microstepping Motor Driver" (at 0 -23.59 0))
        (property "Footprint" "PartReel:a4988"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.allegromicro.com/-/media/files/datasheets/a4988-datasheet.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Allegro A4988 DMOS microstepping driver with translator, up to 2A / 35V, 1/16 microstepping, QFN-28 5x5mm (ET). GND pins tie via exposed PAD ground plane."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "a4988 allegro stepper driver microstepping qfn-28"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/a4988/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "a4988_1_1"
        (pin passive line (at -11.43 16.51 0) (length 2.54)
          (name "OUT2B")
          (number "1"))
        (pin passive line (at -11.43 13.97 0) (length 2.54)
          (name "~ENABLE")
          (number "2"))
        (pin passive line (at -11.43 11.43 0) (length 2.54)
          (name "GND")
          (number "3"))
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "CP1")
          (number "4"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "CP2")
          (number "5"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "VCP")
          (number "6"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "NC")
          (number "7"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "VREG")
          (number "8"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "MS1")
          (number "9"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "MS2")
          (number "10"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "MS3")
          (number "11"))
        (pin passive line (at -11.43 -11.43 0) (length 2.54)
          (name "~RESET")
          (number "12"))
        (pin passive line (at -11.43 -13.97 0) (length 2.54)
          (name "ROSC")
          (number "13"))
        (pin passive line (at -11.43 -16.51 0) (length 2.54)
          (name "~SLEEP")
          (number "14"))
        (pin passive line (at 11.43 16.51 180) (length 2.54)
          (name "VDD")
          (number "15"))
        (pin passive line (at 11.43 13.97 180) (length 2.54)
          (name "STEP")
          (number "16"))
        (pin passive line (at 11.43 11.43 180) (length 2.54)
          (name "REF")
          (number "17"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "GND")
          (number "18"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "DIR")
          (number "19"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "NC")
          (number "20"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "OUT1B")
          (number "21"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "VBB1")
          (number "22"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "SENSE1")
          (number "23"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "OUT1A")
          (number "24"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "NC")
          (number "25"))
        (pin passive line (at 11.43 -11.43 180) (length 2.54)
          (name "OUT2A")
          (number "26"))
        (pin passive line (at 11.43 -13.97 180) (length 2.54)
          (name "SENSE2")
          (number "27"))
        (pin passive line (at 11.43 -16.51 180) (length 2.54)
          (name "VBB2")
          (number "28"))
        (pin passive line (at 0.00 -24.13 90) (length 2.54)
          (name "PAD")
          (number "29"))
      )
    )
  (symbol "drv8825" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 21.05 0))
      (property "Value" "DRV8825 Stepper Motor Driver" (at 0 -23.59 0))
        (property "Footprint" "PartReel:drv8825"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/drv8825.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "TI DRV8825 stepper motor driver, up to 2.5A / 45V, 1/32 microstepping, HTSSOP-28 with PowerPAD (PPAD = GND, must be soldered)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "drv8825 ti stepper driver microstepping htssop-28"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/drv8825/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "drv8825_1_1"
        (pin passive line (at -11.43 16.51 0) (length 2.54)
          (name "CP1")
          (number "1"))
        (pin passive line (at -11.43 13.97 0) (length 2.54)
          (name "CP2")
          (number "2"))
        (pin passive line (at -11.43 11.43 0) (length 2.54)
          (name "VCP")
          (number "3"))
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "VMA")
          (number "4"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "AOUT1")
          (number "5"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "ISENA")
          (number "6"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "AOUT2")
          (number "7"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "BOUT2")
          (number "8"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "ISENB")
          (number "9"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "BOUT1")
          (number "10"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "VMB")
          (number "11"))
        (pin passive line (at -11.43 -11.43 0) (length 2.54)
          (name "AVREF")
          (number "12"))
        (pin passive line (at -11.43 -13.97 0) (length 2.54)
          (name "BVREF")
          (number "13"))
        (pin passive line (at -11.43 -16.51 0) (length 2.54)
          (name "GND")
          (number "14"))
        (pin passive line (at 11.43 16.51 180) (length 2.54)
          (name "V3P3OUT")
          (number "15"))
        (pin passive line (at 11.43 13.97 180) (length 2.54)
          (name "nRESET")
          (number "16"))
        (pin passive line (at 11.43 11.43 180) (length 2.54)
          (name "nSLEEP")
          (number "17"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "nFAULT")
          (number "18"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "DECAY")
          (number "19"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "DIR")
          (number "20"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "nENBL")
          (number "21"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "STEP")
          (number "22"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "NC")
          (number "23"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "MODE0")
          (number "24"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "MODE1")
          (number "25"))
        (pin passive line (at 11.43 -11.43 180) (length 2.54)
          (name "MODE2")
          (number "26"))
        (pin passive line (at 11.43 -13.97 180) (length 2.54)
          (name "nHOME")
          (number "27"))
        (pin passive line (at 11.43 -16.51 180) (length 2.54)
          (name "GND")
          (number "28"))
        (pin passive line (at 0.00 -24.13 90) (length 2.54)
          (name "PPAD")
          (number "29"))
      )
    )
  (symbol "tm1637" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 15.97 0))
      (property "Value" "TM1637 LED Display Driver" (at 0 -15.97 0))
        (property "Footprint" "PartReel:tm1637"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://m5stack.oss-cn-shenzhen.aliyuncs.com/resource/docs/datasheet/unit/digi_clock/TM1637.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Titan Micro TM1637 6-digit LED display driver with keyscan, proprietary 2-wire interface (CLK/DIO, not I2C), 4.5-5.5V, SOP-20. The chip behind ubiquitous 4-digit clock display modules."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "tm1637 led display driver 7-segment sop-20"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/tm1637/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "tm1637_1_1"
        (pin passive line (at -11.43 11.43 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "SG1")
          (number "2"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "SG2")
          (number "3"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "SG3")
          (number "4"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SG4")
          (number "5"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "SG5")
          (number "6"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SG6")
          (number "7"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "SG7")
          (number "8"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "SG8")
          (number "9"))
        (pin passive line (at -11.43 -11.43 0) (length 2.54)
          (name "GRID6")
          (number "10"))
        (pin passive line (at 11.43 11.43 180) (length 2.54)
          (name "GRID5")
          (number "11"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "GRID4")
          (number "12"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "GRID3")
          (number "13"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "GRID2")
          (number "14"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "GRID1")
          (number "15"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "VDD")
          (number "16"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "DIO")
          (number "17"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "CLK")
          (number "18"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "K1")
          (number "19"))
        (pin passive line (at 11.43 -11.43 180) (length 2.54)
          (name "K2")
          (number "20"))
      )
    )
  (symbol "tm1638" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 21.05 0))
      (property "Value" "TM1638 LED Driver with Key Scan" (at 0 -21.05 0))
        (property "Footprint" "PartReel:tm1638"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.handsontec.com/dataspecs/display/TM1638.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Titan Micro TM1638 LED display driver (10 segments x 8 grids) with 8x3 key scan, 3-wire serial (STB/CLK/DIO), 5V, SOP-28. The chip on LED&KEY modules."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "tm1638 led driver keyscan 7-segment sop-28"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/tm1638/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "tm1638_1_1"
        (pin passive line (at -11.43 16.51 0) (length 2.54)
          (name "K1")
          (number "1"))
        (pin passive line (at -11.43 13.97 0) (length 2.54)
          (name "K2")
          (number "2"))
        (pin passive line (at -11.43 11.43 0) (length 2.54)
          (name "K3")
          (number "3"))
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "VDD")
          (number "4"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "SEG1/KS1")
          (number "5"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "SEG2/KS2")
          (number "6"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SEG3/KS3")
          (number "7"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "SEG4/KS4")
          (number "8"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SEG5/KS5")
          (number "9"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "SEG6/KS6")
          (number "10"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "SEG7/KS7")
          (number "11"))
        (pin passive line (at -11.43 -11.43 0) (length 2.54)
          (name "SEG8/KS8")
          (number "12"))
        (pin passive line (at -11.43 -13.97 0) (length 2.54)
          (name "SEG9")
          (number "13"))
        (pin passive line (at -11.43 -16.51 0) (length 2.54)
          (name "SEG10")
          (number "14"))
        (pin passive line (at 11.43 16.51 180) (length 2.54)
          (name "VDD")
          (number "15"))
        (pin passive line (at 11.43 13.97 180) (length 2.54)
          (name "GRID8")
          (number "16"))
        (pin passive line (at 11.43 11.43 180) (length 2.54)
          (name "GRID7")
          (number "17"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "GND")
          (number "18"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "GRID6")
          (number "19"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "GRID5")
          (number "20"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "GRID4")
          (number "21"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "GRID3")
          (number "22"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "GRID2")
          (number "23"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "GRID1")
          (number "24"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "GND")
          (number "25"))
        (pin passive line (at 11.43 -11.43 180) (length 2.54)
          (name "DIO")
          (number "26"))
        (pin passive line (at 11.43 -13.97 180) (length 2.54)
          (name "CLK")
          (number "27"))
        (pin passive line (at 11.43 -16.51 180) (length 2.54)
          (name "STB")
          (number "28"))
      )
    )
  (symbol "w25q64jv" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "W25Q64JV 64Mbit SPI Flash (SOIC-8 208mil)" (at 0 -8.35 0))
        (property "Footprint" "PartReel:w25q64jv"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.winbond.com/resource-files/w25q64jv%20revj%2003272018%20plus.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Winbond W25Q64JV 64Mbit (8MB) serial NOR flash, SPI/Dual/Quad, 2.7-3.6V, wide-body SOIC-8 208mil (not the 150mil narrow body)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "w25q64 winbond spi flash nor memory soic-8 208mil"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/w25q64jv/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "w25q64jv_1_1"
        (pin passive line (at -12.24 3.81 0) (length 2.54)
          (name "~CS")
          (number "1"))
        (pin passive line (at -12.24 1.27 0) (length 2.54)
          (name "DO(IO1)")
          (number "2"))
        (pin passive line (at -12.24 -1.27 0) (length 2.54)
          (name "~WP(IO2)")
          (number "3"))
        (pin passive line (at -12.24 -3.81 0) (length 2.54)
          (name "GND")
          (number "4"))
        (pin passive line (at 12.24 3.81 180) (length 2.54)
          (name "DI(IO0)")
          (number "5"))
        (pin passive line (at 12.24 1.27 180) (length 2.54)
          (name "CLK")
          (number "6"))
        (pin passive line (at 12.24 -1.27 180) (length 2.54)
          (name "~HOLD(IO3)")
          (number "7"))
        (pin passive line (at 12.24 -3.81 180) (length 2.54)
          (name "VCC")
          (number "8"))
      )
    )
  (symbol "cn3791" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 9.62 0))
      (property "Value" "CN3791 MPPT Solar Li-Ion Charger" (at 0 -9.62 0))
        (property "Footprint" "PartReel:cn3791"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/datasheet/pdf/6c2f62f31126495186741f6e77130abd.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Consonance CN3791 PWM switch-mode Li-ion charger with MPPT for solar panels, 4.5-28V input, 4.2V CV, up to 4A, SSOP-10."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cn3791 consonance mppt solar charger li-ion ssop-10"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/cn3791/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "cn3791_1_1"
        (pin passive line (at -11.43 5.08 0) (length 2.54)
          (name "VG")
          (number "1"))
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "~CHRG")
          (number "3"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "~DONE")
          (number "4"))
        (pin passive line (at -11.43 -5.08 0) (length 2.54)
          (name "COM")
          (number "5"))
        (pin passive line (at 11.43 5.08 180) (length 2.54)
          (name "MPPT")
          (number "6"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "BAT")
          (number "7"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "CSP")
          (number "8"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "VCC")
          (number "9"))
        (pin passive line (at 11.43 -5.08 180) (length 2.54)
          (name "DRV")
          (number "10"))
      )
    )
  (symbol "ip5306" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "IP5306 Power Bank SoC" (at 0 -10.89 0))
        (property "Footprint" "PartReel:ip5306"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet.lcsc.com/datasheet/pdf/309666add984eaea02a8f06d99102496.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Injoinic IP5306 fully-integrated power bank system-on-chip: 2.1A charger + 2.4A 5V boost output + battery indicator LEDs + key control, eSOP8 (EP = GND)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ip5306 injoinic power bank charger boost battery esop-8"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ip5306/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ip5306_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "VIN")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "LED1")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "LED2")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "LED3")
          (number "4"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "KEY")
          (number "5"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "BAT")
          (number "6"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "SW")
          (number "7"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "VOUT")
          (number "8"))
        (pin passive line (at 0.00 -11.43 90) (length 2.54)
          (name "EP/GND")
          (number "9"))
      )
    )
  (symbol "max17048" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "MAX17048 LiPo Fuel Gauge (1-cell)" (at 0 -10.89 0))
        (property "Footprint" "PartReel:max17048"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/5/2/7/6/6/MAX17048-MAX17049.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Maxim MAX17048 1-cell Li-ion fuel gauge with ModelGauge, I2C 0x36 fixed, 2.5-4.5V, TDFN-8 2x2 (EP=GND). The battery-percentage chip on modern ESP32 dev boards."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "max17048 maxim fuel gauge lipo battery i2c tdfn"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/max17048/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "max17048_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "CTG")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "CELL")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "VDD")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "GND")
          (number "4"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "ALRT")
          (number "5"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "QSTRT")
          (number "6"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "SCL")
          (number "7"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "SDA")
          (number "8"))
        (pin passive line (at 0.00 -11.43 90) (length 2.54)
          (name "EP/GND")
          (number "9"))
      )
    )
  (symbol "max17049" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "MAX17049 LiPo Fuel Gauge (2-cell)" (at 0 -10.89 0))
        (property "Footprint" "PartReel:max17049"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/5/2/7/6/6/MAX17048-MAX17049.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Maxim MAX17049 2-cell Li-ion fuel gauge with ModelGauge, I2C 0x36 fixed, 2.5-4.5V, TDFN-8 2x2 (EP=GND). CELL pin senses the 2-cell stack."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "max17049 maxim fuel gauge lipo battery i2c tdfn"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/max17049/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "max17049_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "CTG")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "CELL")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "VDD")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "GND")
          (number "4"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "ALRT")
          (number "5"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "QSTRT")
          (number "6"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "SCL")
          (number "7"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "SDA")
          (number "8"))
        (pin passive line (at 0.00 -11.43 90) (length 2.54)
          (name "EP/GND")
          (number "9"))
      )
    )
  (symbol "tp4054" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "TP4054 500mA Li-Ion Charger" (at 0 -7.08 0))
        (property "Footprint" "PartReel:tp4054"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/UTD%20Semi%20PDFs/TP4054.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "TP4054 single-cell Li-ion linear charger, 4.2V CV, up to 500mA (Ichg=1000V/Rprog), VCC 4.25-6.5V, SOT23-5. The tiny-charger staple."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "tp4054 charger li-ion lipo battery sot23-5"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/tp4054/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "tp4054_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "~CHRG")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "BAT")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "VCC")
          (number "4"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "PROG")
          (number "5"))
      )
    )
  (symbol "tp5100" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "TP5100 1/2-Cell Switching Charger" (at 0 -15.97 0))
        (property "Footprint" "PartReel:tp5100"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.toppwr.com/uploadfile/file/20240913/66e3a293b3c42.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "TopPower TP5100 switch-mode Li-ion charger, single-cell 4.2V or 2-cell 8.4V (CS pin select), 0.1-2A, VIN 4.5-12V, QFN16 4x4mm (EP = heatsink, ground only)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "tp5100 toppower charger li-ion 2-cell 8.4v qfn"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/tp5100/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "tp5100_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "VIN")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "LX")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "LX")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VIN")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "VIN")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "PWR_ON-")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "GND")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "VS")
          (number "8"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "BAT")
          (number "9"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "VREG")
          (number "10"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "TS")
          (number "11"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "RTRICK")
          (number "12"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "CS")
          (number "13"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "STDBY")
          (number "14"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "CHRG")
          (number "15"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "VIN")
          (number "16"))
        (pin passive line (at 0.00 -16.51 90) (length 2.54)
          (name "EP/GND")
          (number "17"))
      )
    )
  (symbol "ht7318" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.81 0))
      (property "Value" "HT7318-A Low-Power LDO 1.8V" (at 0 -5.81 0))
        (property "Footprint" "PartReel:ht7318"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.holtek.com/webapi/116711/HT73xxv180.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Holtek HT7318-A ultra-low-power LDO, 1.8V 250mA output, 2.5uA quiescent, VIN up to 12V, SOT-89. Battery-project staple."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ht7318 holtek ldo regulator 1.8v low quiescent sot-89"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ht7318/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ht7318_1_1"
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VIN")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "VOUT")
          (number "3"))
      )
    )
  (symbol "ht7330" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.81 0))
      (property "Value" "HT7330-A Low-Power LDO 3.0V" (at 0 -5.81 0))
        (property "Footprint" "PartReel:ht7330"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.holtek.com/webapi/116711/HT73xxv180.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Holtek HT7330-A ultra-low-power LDO, 3.0V 250mA output, 2.5uA quiescent, VIN up to 12V, SOT-89. Battery-project staple."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ht7330 holtek ldo regulator 3.0v low quiescent sot-89"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ht7330/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ht7330_1_1"
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VIN")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "VOUT")
          (number "3"))
      )
    )
  (symbol "ht7333" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.81 0))
      (property "Value" "HT7333-A Low-Power LDO 3.3V" (at 0 -5.81 0))
        (property "Footprint" "PartReel:ht7333"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.holtek.com/webapi/116711/HT73xxv180.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Holtek HT7333-A ultra-low-power LDO, 3.3V 250mA output, 2.5uA quiescent, VIN up to 12V, SOT-89. Battery-project staple."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ht7333 holtek ldo regulator 3.3v low quiescent sot-89"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ht7333/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ht7333_1_1"
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VIN")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "VOUT")
          (number "3"))
      )
    )
  (symbol "ht7335" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.81 0))
      (property "Value" "HT7335-A Low-Power LDO 3.5V" (at 0 -5.81 0))
        (property "Footprint" "PartReel:ht7335"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.holtek.com/webapi/116711/HT73xxv180.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Holtek HT7335-A ultra-low-power LDO, 3.5V 250mA output, 2.5uA quiescent, VIN up to 12V, SOT-89. Battery-project staple."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ht7335 holtek ldo regulator 3.5v low quiescent sot-89"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ht7335/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ht7335_1_1"
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VIN")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "VOUT")
          (number "3"))
      )
    )
  (symbol "ht7350" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.81 0))
      (property "Value" "HT7350-A Low-Power LDO 5.0V" (at 0 -5.81 0))
        (property "Footprint" "PartReel:ht7350"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.holtek.com/webapi/116711/HT73xxv180.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Holtek HT7350-A ultra-low-power LDO, 5.0V 250mA output, 2.5uA quiescent, VIN up to 12V, SOT-89. Battery-project staple."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ht7350 holtek ldo regulator 5.0v low quiescent sot-89"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ht7350/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ht7350_1_1"
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VIN")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "VOUT")
          (number "3"))
      )
    )
  (symbol "ht7833" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.81 0))
      (property "Value" "HT7833 500mA LDO 3.3V" (at 0 -5.81 0))
        (property "Footprint" "PartReel:ht7833"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.singsun.com/datasheet/en/HT78XX.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Holtek HT7833 TinyPower LDO, 3.3V 500mA output, 4uA quiescent, VIN up to 8V, SOT-89."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ht7833 holtek ldo regulator 3.3v 500ma sot-89"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ht7833/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ht7833_1_1"
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VIN")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "VOUT")
          (number "3"))
      )
    )
  (symbol "mp1584" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "MP1584EN 3A Buck Converter" (at 0 -8.35 0))
        (property "Footprint" "PartReel:mp1584"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://datasheet4u.com/pdf/1471577/MP1584.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "MPS MP1584EN 3A 1.5MHz step-down converter, 4.5-28V input, SOIC-8E with exposed pad (EP = GND, same net as pin 5). NOTE: MPS marks MP1584 NRND (successor MP2338) but it remains ubiquitous on buck modules."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "mp1584 mps buck step-down dc-dc regulator soic-8"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/mp1584/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "mp1584_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "SW")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "EN")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "COMP")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "FB")
          (number "4"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "GND")
          (number "5"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "FREQ")
          (number "6"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "VIN")
          (number "7"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "BST")
          (number "8"))
      )
    )
  (symbol "sy8008" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "SY8008B 1A Buck Converter" (at 0 -7.08 0))
        (property "Footprint" "PartReel:sy8008"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://mangopi.org/_media/sy8008.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Silergy SY8008B 1A 1.5MHz synchronous step-down regulator, 2.5-5.5V input, 0.6V reference, SOT23-5."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sy8008 silergy buck step-down dc-dc sot23-5"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sy8008/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "sy8008_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "EN")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "LX")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "IN")
          (number "4"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "FB")
          (number "5"))
      )
    )
  (symbol "sy8008a" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "SY8008A 0.6A Buck Converter" (at 0 -7.08 0))
        (property "Footprint" "PartReel:sy8008a"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://mangopi.org/_media/sy8008.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Silergy SY8008A 0.6A 1.5MHz synchronous step-down regulator, 2.5-5.5V input, 0.6V reference, SOT23-5."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sy8008a silergy buck step-down dc-dc sot23-5"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sy8008a/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "sy8008a_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "EN")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "LX")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "IN")
          (number "4"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "FB")
          (number "5"))
      )
    )
  (symbol "sy8089" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "SY8089A 2A Buck Converter" (at 0 -7.08 0))
        (property "Footprint" "PartReel:sy8089"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.olimex.com/Products/Components/IC/SY8009A/resources/SY8089AAAC.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Silergy SY8089A 2A (3A peak) 1MHz synchronous step-down regulator, 2.7-5.5V input, 0.6V reference, SOT23-5."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sy8089 silergy buck step-down dc-dc sot23-5 esp32 power"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sy8089/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "sy8089_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "EN")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "LX")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "IN")
          (number "4"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "FB")
          (number "5"))
      )
    )
  (symbol "xl6009" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "XL6009 4A Boost Converter" (at 0 -7.08 0))
        (property "Footprint" "PartReel:xl6009"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://components101.com/sites/default/files/component_datasheet/XL6009-Datasheet_0.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "XLSEMI XL6009 400kHz 4A step-up (boost) DC-DC converter, 5-32V input, TO-263-5. WARNING: the metal tab is the SW switch node, not GND - do not pour ground under it."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "xl6009 xlsemi boost step-up dc-dc to-263"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/xl6009/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "xl6009_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "VIN")
          (number "4"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "EN")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "SW")
          (number "3"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "FB")
          (number "5"))
      )
    )
  (symbol "as5600" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "AS5600 Magnetic Angle Sensor" (at 0 -8.35 0))
        (property "Footprint" "PartReel:as5600"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://look.ams-osram.com/m/7059eac7531a86fd/original/AS5600-DS000365.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ams AS5600 12-bit contactless magnetic rotary position sensor (on-axis), I2C 0x36 + analog/PWM out, 3.3V or 5V mode, SOIC-8. SimpleFOC/robotics encoder staple."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "as5600 ams magnetic encoder rotary angle i2c soic-8"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/as5600/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "as5600_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "VDD5V")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VDD3V3")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "OUT")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "GND")
          (number "4"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "PGO")
          (number "5"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "SDA")
          (number "6"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "SCL")
          (number "7"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "DIR")
          (number "8"))
      )
    )
  (symbol "bh1750" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "BH1750FVI Ambient Light Sensor" (at 0 -7.08 0))
        (property "Footprint" "PartReel:bh1750"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/1811081611_ROHM-Semicon-BH1750FVI-TR_C78960.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Rohm BH1750FVI digital 16-bit ambient light sensor (1-65535 lx), I2C (ADDR H=0x5C / L=0x23), 2.4-3.6V, WSOF6I. DVI pin needs 1uS low reset after power-up. Exposed back pad: leave unconnected (no copper)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "bh1750 rohm light lux ambient i2c gy-302"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/bh1750/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "bh1750_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "ADDR")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "GND")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "SDA")
          (number "4"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "DVI")
          (number "5"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "SCL")
          (number "6"))
      )
    )
  (symbol "max6675" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "MAX6675 Thermocouple-to-Digital Converter" (at 0 -8.35 0))
        (property "Footprint" "PartReel:max6675"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/MAX6675.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Maxim MAX6675 cold-junction-compensated K-thermocouple to digital converter, 12-bit SPI read-only, 3.0-5.5V, SOIC-8. The entry-level thermocouple interface on K-type breakouts (MAX31855 is 3.3V-only, not a drop-in)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "max6675 thermocouple k-type spi temperature soic-8"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/max6675/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "max6675_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "T-")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "T+")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "VCC")
          (number "4"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "SCK")
          (number "5"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "~CS")
          (number "6"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "SO")
          (number "7"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "N.C.")
          (number "8"))
      )
    )
  (symbol "stm32g431cbtx" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -27.94 26.04 0))
      (property "Value" "STM32G431CBTx (Cortex-M4 170MHz, LQFP-48)" (at 0 -9.94 0))
        (property "Footprint" "PartReel:stm32g431cbtx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.st.com/en/microcontrollers-microprocessors/stm32g431cb.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "STM32G431 Cortex-M4F MCU 170MHz, 128KB flash, LQFP-48 7x7mm 0.5mm pitch. 4-side physical symbol (pin order). Temperature-grade wildcard (x = 6/7)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "stm32 g431 cortex-m4 mcu lqfp-48"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/stm32g431cbtx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "stm32g431cbtx_1_1"
        (pin power_in line (at -27.94 13.97 0) (length 5.08)
          (name "VBAT")
          (number "1"))
        (pin bidirectional line (at -27.94 11.43 0) (length 5.08)
          (name "PC13")
          (number "2"))
        (pin bidirectional line (at -27.94 8.89 0) (length 5.08)
          (name "PC14-OSC32_IN")
          (number "3"))
        (pin bidirectional line (at -27.94 6.35 0) (length 5.08)
          (name "PC15-OSC32_OUT")
          (number "4"))
        (pin bidirectional line (at -27.94 3.81 0) (length 5.08)
          (name "PF0-OSC_IN")
          (number "5"))
        (pin bidirectional line (at -27.94 1.27 0) (length 5.08)
          (name "PF1-OSC_OUT")
          (number "6"))
        (pin bidirectional line (at -27.94 -1.27 0) (length 5.08)
          (name "PG10-NRST")
          (number "7"))
        (pin bidirectional line (at -27.94 -3.81 0) (length 5.08)
          (name "PA0")
          (number "8"))
        (pin bidirectional line (at -27.94 -6.35 0) (length 5.08)
          (name "PA1")
          (number "9"))
        (pin bidirectional line (at -27.94 -8.89 0) (length 5.08)
          (name "PA2")
          (number "10"))
        (pin bidirectional line (at -27.94 -11.43 0) (length 5.08)
          (name "PA3")
          (number "11"))
        (pin bidirectional line (at -27.94 -13.97 0) (length 5.08)
          (name "PA4")
          (number "12"))
        (pin bidirectional line (at -13.97 -27.94 90) (length 5.08)
          (name "PA5")
          (number "13"))
        (pin bidirectional line (at -11.43 -27.94 90) (length 5.08)
          (name "PA6")
          (number "14"))
        (pin bidirectional line (at -8.89 -27.94 90) (length 5.08)
          (name "PA7")
          (number "15"))
        (pin bidirectional line (at -6.35 -27.94 90) (length 5.08)
          (name "PB0")
          (number "16"))
        (pin bidirectional line (at -3.81 -27.94 90) (length 5.08)
          (name "PB1")
          (number "17"))
        (pin bidirectional line (at -1.27 -27.94 90) (length 5.08)
          (name "PB2")
          (number "18"))
        (pin power_in line (at 1.27 -27.94 90) (length 5.08)
          (name "VSSA")
          (number "19"))
        (pin power_in line (at 3.81 -27.94 90) (length 5.08)
          (name "VREF+")
          (number "20"))
        (pin power_in line (at 6.35 -27.94 90) (length 5.08)
          (name "VDDA")
          (number "21"))
        (pin bidirectional line (at 8.89 -27.94 90) (length 5.08)
          (name "PB10")
          (number "22"))
        (pin power_in line (at 11.43 -27.94 90) (length 5.08)
          (name "VSS")
          (number "23"))
        (pin power_in line (at 13.97 -27.94 90) (length 5.08)
          (name "VDD")
          (number "24"))
        (pin bidirectional line (at 27.94 -13.97 180) (length 5.08)
          (name "PB11")
          (number "25"))
        (pin bidirectional line (at 27.94 -11.43 180) (length 5.08)
          (name "PB12")
          (number "26"))
        (pin bidirectional line (at 27.94 -8.89 180) (length 5.08)
          (name "PB13")
          (number "27"))
        (pin bidirectional line (at 27.94 -6.35 180) (length 5.08)
          (name "PB14")
          (number "28"))
        (pin bidirectional line (at 27.94 -3.81 180) (length 5.08)
          (name "PB15")
          (number "29"))
        (pin bidirectional line (at 27.94 -1.27 180) (length 5.08)
          (name "PA8")
          (number "30"))
        (pin bidirectional line (at 27.94 1.27 180) (length 5.08)
          (name "PA9")
          (number "31"))
        (pin bidirectional line (at 27.94 3.81 180) (length 5.08)
          (name "PA10")
          (number "32"))
        (pin bidirectional line (at 27.94 6.35 180) (length 5.08)
          (name "PA11")
          (number "33"))
        (pin bidirectional line (at 27.94 8.89 180) (length 5.08)
          (name "PA12")
          (number "34"))
        (pin power_in line (at 27.94 11.43 180) (length 5.08)
          (name "VSS")
          (number "35"))
        (pin power_in line (at 27.94 13.97 180) (length 5.08)
          (name "VDD")
          (number "36"))
        (pin bidirectional line (at 13.97 27.94 270) (length 5.08)
          (name "PA13")
          (number "37"))
        (pin bidirectional line (at 11.43 27.94 270) (length 5.08)
          (name "PA14")
          (number "38"))
        (pin bidirectional line (at 8.89 27.94 270) (length 5.08)
          (name "PA15")
          (number "39"))
        (pin bidirectional line (at 6.35 27.94 270) (length 5.08)
          (name "PB3")
          (number "40"))
        (pin bidirectional line (at 3.81 27.94 270) (length 5.08)
          (name "PB4")
          (number "41"))
        (pin bidirectional line (at 1.27 27.94 270) (length 5.08)
          (name "PB5")
          (number "42"))
        (pin bidirectional line (at -1.27 27.94 270) (length 5.08)
          (name "PB6")
          (number "43"))
        (pin bidirectional line (at -3.81 27.94 270) (length 5.08)
          (name "PB7")
          (number "44"))
        (pin bidirectional line (at -6.35 27.94 270) (length 5.08)
          (name "PB8-BOOT0")
          (number "45"))
        (pin bidirectional line (at -8.89 27.94 270) (length 5.08)
          (name "PB9")
          (number "46"))
        (pin power_in line (at -11.43 27.94 270) (length 5.08)
          (name "VSS")
          (number "47"))
        (pin power_in line (at -13.97 27.94 270) (length 5.08)
          (name "VDD")
          (number "48"))
      ))
  (symbol "stm32g431rbtx" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -33.02 31.12 0))
      (property "Value" "STM32G431RBTx (Cortex-M4 170MHz, LQFP-64)" (at 0 -12.15 0))
        (property "Footprint" "PartReel:stm32g431rbtx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.st.com/en/microcontrollers-microprocessors/stm32g431rb.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "STM32G431 Cortex-M4F MCU 170MHz, 128KB flash, LQFP-64 10x10mm 0.5mm pitch. 4-side physical symbol (pin order). Temperature-grade wildcard (x = 6/7)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "stm32 g431 cortex-m4 mcu lqfp-64"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/stm32g431rbtx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "stm32g431rbtx_1_1"
        (pin power_in line (at -33.02 19.05 0) (length 5.08)
          (name "VBAT")
          (number "1"))
        (pin bidirectional line (at -33.02 16.51 0) (length 5.08)
          (name "PC13")
          (number "2"))
        (pin bidirectional line (at -33.02 13.97 0) (length 5.08)
          (name "PC14-OSC32_IN")
          (number "3"))
        (pin bidirectional line (at -33.02 11.43 0) (length 5.08)
          (name "PC15-OSC32_OUT")
          (number "4"))
        (pin bidirectional line (at -33.02 8.89 0) (length 5.08)
          (name "PF0-OSC_IN")
          (number "5"))
        (pin bidirectional line (at -33.02 6.35 0) (length 5.08)
          (name "PF1-OSC_OUT")
          (number "6"))
        (pin bidirectional line (at -33.02 3.81 0) (length 5.08)
          (name "PG10-NRST")
          (number "7"))
        (pin bidirectional line (at -33.02 1.27 0) (length 5.08)
          (name "PC0")
          (number "8"))
        (pin bidirectional line (at -33.02 -1.27 0) (length 5.08)
          (name "PC1")
          (number "9"))
        (pin bidirectional line (at -33.02 -3.81 0) (length 5.08)
          (name "PC2")
          (number "10"))
        (pin bidirectional line (at -33.02 -6.35 0) (length 5.08)
          (name "PC3")
          (number "11"))
        (pin bidirectional line (at -33.02 -8.89 0) (length 5.08)
          (name "PA0")
          (number "12"))
        (pin bidirectional line (at -33.02 -11.43 0) (length 5.08)
          (name "PA1")
          (number "13"))
        (pin bidirectional line (at -33.02 -13.97 0) (length 5.08)
          (name "PA2")
          (number "14"))
        (pin power_in line (at -33.02 -16.51 0) (length 5.08)
          (name "VSS")
          (number "15"))
        (pin power_in line (at -33.02 -19.05 0) (length 5.08)
          (name "VDD")
          (number "16"))
        (pin bidirectional line (at -19.05 -33.02 90) (length 5.08)
          (name "PA3")
          (number "17"))
        (pin bidirectional line (at -16.51 -33.02 90) (length 5.08)
          (name "PA4")
          (number "18"))
        (pin bidirectional line (at -13.97 -33.02 90) (length 5.08)
          (name "PA5")
          (number "19"))
        (pin bidirectional line (at -11.43 -33.02 90) (length 5.08)
          (name "PA6")
          (number "20"))
        (pin bidirectional line (at -8.89 -33.02 90) (length 5.08)
          (name "PA7")
          (number "21"))
        (pin bidirectional line (at -6.35 -33.02 90) (length 5.08)
          (name "PC4")
          (number "22"))
        (pin bidirectional line (at -3.81 -33.02 90) (length 5.08)
          (name "PC5")
          (number "23"))
        (pin bidirectional line (at -1.27 -33.02 90) (length 5.08)
          (name "PB0")
          (number "24"))
        (pin bidirectional line (at 1.27 -33.02 90) (length 5.08)
          (name "PB1")
          (number "25"))
        (pin bidirectional line (at 3.81 -33.02 90) (length 5.08)
          (name "PB2")
          (number "26"))
        (pin power_in line (at 6.35 -33.02 90) (length 5.08)
          (name "VSSA")
          (number "27"))
        (pin power_in line (at 8.89 -33.02 90) (length 5.08)
          (name "VREF+")
          (number "28"))
        (pin power_in line (at 11.43 -33.02 90) (length 5.08)
          (name "VDDA")
          (number "29"))
        (pin bidirectional line (at 13.97 -33.02 90) (length 5.08)
          (name "PB10")
          (number "30"))
        (pin power_in line (at 16.51 -33.02 90) (length 5.08)
          (name "VSS")
          (number "31"))
        (pin power_in line (at 19.05 -33.02 90) (length 5.08)
          (name "VDD")
          (number "32"))
        (pin bidirectional line (at 33.02 -19.05 180) (length 5.08)
          (name "PB11")
          (number "33"))
        (pin bidirectional line (at 33.02 -16.51 180) (length 5.08)
          (name "PB12")
          (number "34"))
        (pin bidirectional line (at 33.02 -13.97 180) (length 5.08)
          (name "PB13")
          (number "35"))
        (pin bidirectional line (at 33.02 -11.43 180) (length 5.08)
          (name "PB14")
          (number "36"))
        (pin bidirectional line (at 33.02 -8.89 180) (length 5.08)
          (name "PB15")
          (number "37"))
        (pin bidirectional line (at 33.02 -6.35 180) (length 5.08)
          (name "PC6")
          (number "38"))
        (pin bidirectional line (at 33.02 -3.81 180) (length 5.08)
          (name "PC7")
          (number "39"))
        (pin bidirectional line (at 33.02 -1.27 180) (length 5.08)
          (name "PC8")
          (number "40"))
        (pin bidirectional line (at 33.02 1.27 180) (length 5.08)
          (name "PC9")
          (number "41"))
        (pin bidirectional line (at 33.02 3.81 180) (length 5.08)
          (name "PA8")
          (number "42"))
        (pin bidirectional line (at 33.02 6.35 180) (length 5.08)
          (name "PA9")
          (number "43"))
        (pin bidirectional line (at 33.02 8.89 180) (length 5.08)
          (name "PA10")
          (number "44"))
        (pin bidirectional line (at 33.02 11.43 180) (length 5.08)
          (name "PA11")
          (number "45"))
        (pin bidirectional line (at 33.02 13.97 180) (length 5.08)
          (name "PA12")
          (number "46"))
        (pin power_in line (at 33.02 16.51 180) (length 5.08)
          (name "VSS")
          (number "47"))
        (pin power_in line (at 33.02 19.05 180) (length 5.08)
          (name "VDD")
          (number "48"))
        (pin bidirectional line (at 19.05 33.02 270) (length 5.08)
          (name "PA13")
          (number "49"))
        (pin bidirectional line (at 16.51 33.02 270) (length 5.08)
          (name "PA14")
          (number "50"))
        (pin bidirectional line (at 13.97 33.02 270) (length 5.08)
          (name "PA15")
          (number "51"))
        (pin bidirectional line (at 11.43 33.02 270) (length 5.08)
          (name "PC10")
          (number "52"))
        (pin bidirectional line (at 8.89 33.02 270) (length 5.08)
          (name "PC11")
          (number "53"))
        (pin bidirectional line (at 6.35 33.02 270) (length 5.08)
          (name "PC12")
          (number "54"))
        (pin bidirectional line (at 3.81 33.02 270) (length 5.08)
          (name "PD2")
          (number "55"))
        (pin bidirectional line (at 1.27 33.02 270) (length 5.08)
          (name "PB3")
          (number "56"))
        (pin bidirectional line (at -1.27 33.02 270) (length 5.08)
          (name "PB4")
          (number "57"))
        (pin bidirectional line (at -3.81 33.02 270) (length 5.08)
          (name "PB5")
          (number "58"))
        (pin bidirectional line (at -6.35 33.02 270) (length 5.08)
          (name "PB6")
          (number "59"))
        (pin bidirectional line (at -8.89 33.02 270) (length 5.08)
          (name "PB7")
          (number "60"))
        (pin bidirectional line (at -11.43 33.02 270) (length 5.08)
          (name "PB8-BOOT0")
          (number "61"))
        (pin bidirectional line (at -13.97 33.02 270) (length 5.08)
          (name "PB9")
          (number "62"))
        (pin power_in line (at -16.51 33.02 270) (length 5.08)
          (name "VSS")
          (number "63"))
        (pin power_in line (at -19.05 33.02 270) (length 5.08)
          (name "VDD")
          (number "64"))
      ))
  (symbol "cst816s" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 15.97 0))
      (property "Value" "CST816S Capacitive Touch Controller" (at 0 -18.51 0))
        (property "Footprint" "PartReel:cst816s"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.waveshare.com/w/upload/5/51/CST816S_Datasheet_EN.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hynitron CST816S self-capacitance touch controller - the touch chip paired with GC9A01 round LCDs in smartwatch projects. I2C 0x15, 2.7-3.6V, QFN-20 3x3. CMOD needs 1-5.6nF C0G cap."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "cst816s hynitron touch capacitive smartwatch gc9a01 qfn"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/cst816s/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "cst816s_1_1"
        (pin passive line (at -11.43 11.43 0) (length 2.54)
          (name "CMOD0")
          (number "1"))
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "S1L")
          (number "2"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "S2L")
          (number "3"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "S3L")
          (number "4"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "S4L")
          (number "5"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "S5L")
          (number "6"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "S6L")
          (number "7"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "S7R")
          (number "8"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "S8R")
          (number "9"))
        (pin passive line (at -11.43 -11.43 0) (length 2.54)
          (name "S9R")
          (number "10"))
        (pin passive line (at 11.43 11.43 180) (length 2.54)
          (name "S10R")
          (number "11"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "S11R")
          (number "12"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "S12R")
          (number "13"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "S13R")
          (number "14"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "CMOD1/S14")
          (number "15"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "VDDA")
          (number "16"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "RST")
          (number "17"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "SCL")
          (number "18"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "SDA")
          (number "19"))
        (pin passive line (at 11.43 -11.43 180) (length 2.54)
          (name "IRQ")
          (number "20"))
        (pin passive line (at 0.00 -19.05 90) (length 2.54)
          (name "EP/GND")
          (number "21"))
      )
    )
  (symbol "ttp223" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "TTP223-BA6 Touch Key IC" (at 0 -7.08 0))
        (property "Footprint" "PartReel:ttp223"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://vakits.com/sites/default/files/TTP223B%20Touch%20Switch.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Tontek TTP223-BA6 single-key capacitive touch detector, 2.0-5.5V, direct/toggle output modes, SOT-23-6."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ttp223 tontek touch capacitive key sot-23-6"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ttp223/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ttp223_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "Q")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "VSS")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "I")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "AHLB")
          (number "4"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "VDD")
          (number "5"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "TOG")
          (number "6"))
      )
    )
  (symbol "ttp224" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "TTP224N-BSB 4-Key Touch IC" (at 0 -13.43 0))
        (property "Footprint" "PartReel:ttp224"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcsc.com/product-detail/Touch-Screen-Controller-ICs_TTP224N-BSB_C90399.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Tontek TTP224N 4-key capacitive touch detector with direct outputs (TPQ0-3), option straps for output mode, 2.4-5.5V, SSOP-16."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ttp224 tontek touch capacitive 4-key ssop-16"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ttp224/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ttp224_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "TP0")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "TP1")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "TP2")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "TP3")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "AHLB")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "VDD")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "TOG")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "LPMB")
          (number "8"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "MOT0")
          (number "9"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "VSS")
          (number "10"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "OD")
          (number "11"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "SM")
          (number "12"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "TPQ3")
          (number "13"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "TPQ2")
          (number "14"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "TPQ1")
          (number "15"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "TPQ0")
          (number "16"))
      )
    )
  (symbol "ttp226" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 21.05 0))
      (property "Value" "TTP226-809SN 8-Key Touch IC" (at 0 -21.05 0))
        (property "Footprint" "PartReel:ttp226"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcsc.com/product-detail/Touch-Screen-Controller-ICs_TTP226-809SN_C183531.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Tontek TTP226 8-key capacitive touch detector with direct outputs (Q0-7), 2.4-5.5V, SSOP-28."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ttp226 tontek touch capacitive 8-key ssop-28"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ttp226/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ttp226_1_1"
        (pin passive line (at -11.43 16.51 0) (length 2.54)
          (name "OSC2/TOPAD")
          (number "1"))
        (pin passive line (at -11.43 13.97 0) (length 2.54)
          (name "I7")
          (number "2"))
        (pin passive line (at -11.43 11.43 0) (length 2.54)
          (name "I6")
          (number "3"))
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "I5")
          (number "4"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "I4")
          (number "5"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "I3")
          (number "6"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "I2")
          (number "7"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "I1")
          (number "8"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "I0")
          (number "9"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "OSC1")
          (number "10"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "VSS")
          (number "11"))
        (pin passive line (at -11.43 -11.43 0) (length 2.54)
          (name "VDD")
          (number "12"))
        (pin passive line (at -11.43 -13.97 0) (length 2.54)
          (name "OPS1")
          (number "13"))
        (pin passive line (at -11.43 -16.51 0) (length 2.54)
          (name "OPS0")
          (number "14"))
        (pin passive line (at 11.43 16.51 180) (length 2.54)
          (name "AHL")
          (number "15"))
        (pin passive line (at 11.43 13.97 180) (length 2.54)
          (name "Q0")
          (number "16"))
        (pin passive line (at 11.43 11.43 180) (length 2.54)
          (name "Q1")
          (number "17"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "Q2")
          (number "18"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "Q3")
          (number "19"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "Q4")
          (number "20"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "Q5")
          (number "21"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "Q6")
          (number "22"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "Q7")
          (number "23"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "DV")
          (number "24"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "SLSE1")
          (number "25"))
        (pin passive line (at 11.43 -11.43 180) (length 2.54)
          (name "SLSE2")
          (number "26"))
        (pin passive line (at 11.43 -13.97 180) (length 2.54)
          (name "SLSE3")
          (number "27"))
        (pin passive line (at 11.43 -16.51 180) (length 2.54)
          (name "SLSE4")
          (number "28"))
      )
    )
  (symbol "ttp229" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 21.05 0))
      (property "Value" "TTP229-BSF 16-Key Touch IC" (at 0 -21.05 0))
        (property "Footprint" "PartReel:ttp229"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.tontek.com.tw/uploads/product/97/TTP229-BSF_V1.1_EN.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Tontek TTP229-BSF 16-key capacitive touch detector with serial output, 2.4-5.5V, SSOP-28 150mil."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ttp229 tontek touch capacitive 16-key keypad ssop-28"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ttp229/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ttp229_1_1"
        (pin passive line (at -11.43 16.51 0) (length 2.54)
          (name "TP3")
          (number "1"))
        (pin passive line (at -11.43 13.97 0) (length 2.54)
          (name "TP2")
          (number "2"))
        (pin passive line (at -11.43 11.43 0) (length 2.54)
          (name "NC")
          (number "3"))
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "SENADJ0")
          (number "4"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "TP1")
          (number "5"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "TP0")
          (number "6"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "TP15")
          (number "7"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "TP14")
          (number "8"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SENADJ3")
          (number "9"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "TP13")
          (number "10"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "TP12")
          (number "11"))
        (pin passive line (at -11.43 -11.43 0) (length 2.54)
          (name "SDO")
          (number "12"))
        (pin passive line (at -11.43 -13.97 0) (length 2.54)
          (name "SCL")
          (number "13"))
        (pin passive line (at -11.43 -16.51 0) (length 2.54)
          (name "SLPSENB")
          (number "14"))
        (pin passive line (at 11.43 16.51 180) (length 2.54)
          (name "TP11")
          (number "15"))
        (pin passive line (at 11.43 13.97 180) (length 2.54)
          (name "TP10")
          (number "16"))
        (pin passive line (at 11.43 11.43 180) (length 2.54)
          (name "SENADJ2")
          (number "17"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "TP9")
          (number "18"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "TP8")
          (number "19"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "TEST")
          (number "20"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "TP7")
          (number "21"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "TP6")
          (number "22"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "SENADJ1")
          (number "23"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "TP5")
          (number "24"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "TP4")
          (number "25"))
        (pin passive line (at 11.43 -11.43 180) (length 2.54)
          (name "VDD")
          (number "26"))
        (pin passive line (at 11.43 -13.97 180) (length 2.54)
          (name "VSS")
          (number "27"))
        (pin passive line (at 11.43 -16.51 180) (length 2.54)
          (name "SLPSENA")
          (number "28"))
      )
    )
  (symbol "esp32_wroom32" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 27.40 0))
      (property "Value" "ESP32-WROOM-32 Module" (at 0 -29.94 0))
        (property "Footprint" "PartReel:esp32_wroom32"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Espressif ESP32-WROOM-32 Wi-Fi + Bluetooth module, SMD castellated, 38 pads + thermal. Land pattern per Espressif datasheet."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "esp32 wroom wroom-32 module wifi bluetooth espressif"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/esp32_wroom32/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "esp32_wroom32_1_1"
        (pin passive line (at -11.79 22.86 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.79 20.32 0) (length 2.54)
          (name "3V3")
          (number "2"))
        (pin passive line (at -11.79 17.78 0) (length 2.54)
          (name "EN")
          (number "3"))
        (pin passive line (at -11.79 15.24 0) (length 2.54)
          (name "SENSOR_VP")
          (number "4"))
        (pin passive line (at -11.79 12.70 0) (length 2.54)
          (name "SENSOR_VN")
          (number "5"))
        (pin passive line (at -11.79 10.16 0) (length 2.54)
          (name "IO34")
          (number "6"))
        (pin passive line (at -11.79 7.62 0) (length 2.54)
          (name "IO35")
          (number "7"))
        (pin passive line (at -11.79 5.08 0) (length 2.54)
          (name "IO32")
          (number "8"))
        (pin passive line (at -11.79 2.54 0) (length 2.54)
          (name "IO33")
          (number "9"))
        (pin passive line (at -11.79 0.00 0) (length 2.54)
          (name "IO25")
          (number "10"))
        (pin passive line (at -11.79 -2.54 0) (length 2.54)
          (name "IO26")
          (number "11"))
        (pin passive line (at -11.79 -5.08 0) (length 2.54)
          (name "IO27")
          (number "12"))
        (pin passive line (at -11.79 -7.62 0) (length 2.54)
          (name "IO14")
          (number "13"))
        (pin passive line (at -11.79 -10.16 0) (length 2.54)
          (name "IO12")
          (number "14"))
        (pin passive line (at -11.79 -12.70 0) (length 2.54)
          (name "GND")
          (number "15"))
        (pin passive line (at -11.79 -15.24 0) (length 2.54)
          (name "IO13")
          (number "16"))
        (pin passive line (at -11.79 -17.78 0) (length 2.54)
          (name "SHD/SD2")
          (number "17"))
        (pin passive line (at -11.79 -20.32 0) (length 2.54)
          (name "SWP/SD3")
          (number "18"))
        (pin passive line (at -11.79 -22.86 0) (length 2.54)
          (name "SCS/CMD")
          (number "19"))
        (pin passive line (at 11.79 22.86 180) (length 2.54)
          (name "SCK/CLK")
          (number "20"))
        (pin passive line (at 11.79 20.32 180) (length 2.54)
          (name "SDO/SD0")
          (number "21"))
        (pin passive line (at 11.79 17.78 180) (length 2.54)
          (name "SDI/SD1")
          (number "22"))
        (pin passive line (at 11.79 15.24 180) (length 2.54)
          (name "IO15")
          (number "23"))
        (pin passive line (at 11.79 12.70 180) (length 2.54)
          (name "IO2")
          (number "24"))
        (pin passive line (at 11.79 10.16 180) (length 2.54)
          (name "IO0")
          (number "25"))
        (pin passive line (at 11.79 7.62 180) (length 2.54)
          (name "IO4")
          (number "26"))
        (pin passive line (at 11.79 5.08 180) (length 2.54)
          (name "IO16")
          (number "27"))
        (pin passive line (at 11.79 2.54 180) (length 2.54)
          (name "IO17")
          (number "28"))
        (pin passive line (at 11.79 0.00 180) (length 2.54)
          (name "IO5")
          (number "29"))
        (pin passive line (at 11.79 -2.54 180) (length 2.54)
          (name "IO18")
          (number "30"))
        (pin passive line (at 11.79 -5.08 180) (length 2.54)
          (name "IO19")
          (number "31"))
        (pin passive line (at 11.79 -7.62 180) (length 2.54)
          (name "NC")
          (number "32"))
        (pin passive line (at 11.79 -10.16 180) (length 2.54)
          (name "IO21")
          (number "33"))
        (pin passive line (at 11.79 -12.70 180) (length 2.54)
          (name "RXD0/IO3")
          (number "34"))
        (pin passive line (at 11.79 -15.24 180) (length 2.54)
          (name "TXD0/IO1")
          (number "35"))
        (pin passive line (at 11.79 -17.78 180) (length 2.54)
          (name "IO22")
          (number "36"))
        (pin passive line (at 11.79 -20.32 180) (length 2.54)
          (name "IO23")
          (number "37"))
        (pin passive line (at 11.79 -22.86 180) (length 2.54)
          (name "GND")
          (number "38"))
        (pin passive line (at 0.00 -30.48 90) (length 2.54)
          (name "GND")
          (number "39"))
      )
    )
  (symbol "nordic_e73_2g4m08s1c"
        (property "Footprint" "PartReel:nordic_e73_2g4m08s1c"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ebyte.com/en/downpdf.aspx?id=445"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF52840 BT LE module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless Bluetooth LE nRF nordic"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_e73_2g4m08s1c/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 13.97 41.91 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "E73-2G4M08S1C"
  				(at 26.67 39.37 0)
  				(do_not_autoplace)
  			)
  			(property "LCSC" "C356849"
  				(at 0 0 0)
  			)
  			(property "ki_fp_filters" "E73*2G4M08S1C*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_e73_2g4m08s1c_0_0"
  				(pin bidirectional line
  					(at 22.86 -27.94 180)
  					(length 2.54)
  					(name "P1.11")
  					(number "1")
  				)
  				(pin power_in line
  					(at 22.86 15.24 180)
  					(length 2.54)
  					(name "P0.30/AIN6")
  					(number "10")
  				)
  				(pin bidirectional line
  					(at 22.86 7.62 180)
  					(length 2.54)
  					(name "P0.00/XL1")
  					(number "11")
  				)
  				(pin bidirectional line
  					(at -22.86 -30.48 0)
  					(length 2.54)
  					(name "P0.26")
  					(number "12")
  				)
  				(pin bidirectional line
  					(at 22.86 5.08 180)
  					(length 2.54)
  					(name "P0.01/XL2")
  					(number "13")
  				)
  				(pin bidirectional line
  					(at -22.86 -5.08 0)
  					(length 2.54)
  					(name "P0.06")
  					(number "14")
  				)
  				(pin bidirectional line
  					(at 22.86 22.86 180)
  					(length 2.54)
  					(name "P0.05/AIN3")
  					(number "15")
  				)
  				(pin bidirectional line
  					(at -22.86 -10.16 0)
  					(length 2.54)
  					(name "P0.08")
  					(number "16")
  				)
  				(pin bidirectional line
  					(at 22.86 -22.86 180)
  					(length 2.54)
  					(name "P1.09")
  					(number "17")
  				)
  				(pin bidirectional line
  					(at 22.86 25.4 180)
  					(length 2.54)
  					(name "P0.04/AIN2")
  					(number "18")
  				)
  				(pin bidirectional line
  					(at -2.54 40.64 270)
  					(length 2.54)
  					(name "VDD")
  					(number "19")
  				)
  				(pin bidirectional line
  					(at 22.86 -25.4 180)
  					(length 2.54)
  					(name "P1.10")
  					(number "2")
  				)
  				(pin bidirectional line
  					(at -22.86 -12.7 0)
  					(length 2.54)
  					(name "P0.12")
  					(number "20")
  				)
  				(pin bidirectional line
  					(at -22.86 -7.62 0)
  					(length 2.54)
  					(name "P0.07")
  					(number "22")
  				)
  				(pin bidirectional line
  					(at 2.54 40.64 270)
  					(length 2.54)
  					(name "VDDH")
  					(number "23")
  				)
  				(pin bidirectional line
  					(at 5.08 40.64 270)
  					(length 2.54)
  					(name "DCCH")
  					(number "25")
  				)
  				(pin input line
  					(at -22.86 17.78 0)
  					(length 2.54)
  					(name "VBUS")
  					(number "27")
  				)
  				(pin bidirectional line
  					(at -22.86 -17.78 0)
  					(length 2.54)
  					(name "P0.15")
  					(number "28")
  				)
  				(pin bidirectional line
  					(at -22.86 15.24 0)
  					(length 2.54)
  					(name "D-")
  					(number "29")
  				)
  				(pin bidirectional line
  					(at 22.86 27.94 180)
  					(length 2.54)
  					(name "P0.03/AIN1")
  					(number "3")
  				)
  				(pin bidirectional line
  					(at -22.86 -20.32 0)
  					(length 2.54)
  					(name "P0.17")
  					(number "30")
  				)
  				(pin bidirectional line
  					(at -22.86 12.7 0)
  					(length 2.54)
  					(name "D+")
  					(number "31")
  				)
  				(pin bidirectional line
  					(at -22.86 -22.86 0)
  					(length 2.54)
  					(name "P0.20")
  					(number "32")
  				)
  				(pin bidirectional line
  					(at -22.86 -15.24 0)
  					(length 2.54)
  					(name "P0.13")
  					(number "33")
  				)
  				(pin bidirectional line
  					(at -22.86 -25.4 0)
  					(length 2.54)
  					(name "P0.22")
  					(number "34")
  				)
  				(pin bidirectional line
  					(at -22.86 -27.94 0)
  					(length 2.54)
  					(name "P0.24")
  					(number "35")
  				)
  				(pin bidirectional line
  					(at 22.86 -12.7 180)
  					(length 2.54)
  					(name "P1.00")
  					(number "36")
  				)
  				(pin bidirectional line
  					(at -22.86 27.94 0)
  					(length 2.54)
  					(name "SWDIO")
  					(number "37")
  				)
  				(pin bidirectional line
  					(at 22.86 -15.24 180)
  					(length 2.54)
  					(name "P1.02")
  					(number "38")
  				)
  				(pin power_in line
  					(at -22.86 30.48 0)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "39")
  				)
  				(pin bidirectional line
  					(at 22.86 20.32 180)
  					(length 2.54)
  					(name "P0.28/AIN4")
  					(number "4")
  				)
  				(pin bidirectional line
  					(at 22.86 -17.78 180)
  					(length 2.54)
  					(name "P1.04")
  					(number "40")
  				)
  				(pin bidirectional line
  					(at 22.86 0 180)
  					(length 2.54)
  					(name "P0.09/NFC1")
  					(number "41")
  				)
  				(pin power_in line
  					(at 22.86 -20.32 180)
  					(length 2.54)
  					(name "P1.06")
  					(number "42")
  				)
  				(pin power_in line
  					(at 22.86 -2.54 180)
  					(length 2.54)
  					(name "P0.10/NFC2")
  					(number "43")
  				)
  				(pin bidirectional line
  					(at 22.86 -30.48 180)
  					(length 2.54)
  					(name "P1.13")
  					(number "6")
  				)
  				(pin bidirectional line
  					(at 22.86 30.48 180)
  					(length 2.54)
  					(name "P0.02/AIN0")
  					(number "7")
  				)
  				(pin bidirectional line
  					(at 22.86 17.78 180)
  					(length 2.54)
  					(name "P0.29/AIN5")
  					(number "8")
  				)
  				(pin power_in line
  					(at 22.86 12.7 180)
  					(length 2.54)
  					(name "P0.31/AIN7")
  					(number "9")
  				)
  			)
  			(symbol "nordic_e73_2g4m08s1c_0_1")
  			(symbol "nordic_e73_2g4m08s1c_1_0"
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "21")
  				)
  				(pin passive line
  					(at 0 -40.64 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "24")
  				)
  				(pin bidirectional line
  					(at -22.86 35.56 0)
  					(length 2.54)
  					(name "P0.18/~{RESET}")
  					(number "26")
  				)
  				(pin power_in line
  					(at 0 -40.64 90)
  					(length 2.54)
  					(name "GND")
  					(number "5")
  				)
  			)
  		)
  (symbol "nordic_isp1907_ll"
        (property "Footprint" "PartReel:nordic_isp1907_ll"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.insightsip.com/fichiers_insightsip/pdf/ble/ISP1907/isp_ble_DS1907.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ISP1907-LL."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_isp1907_ll/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "ISP1907-LL"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "LCSC" "C5657563"
  				(at 0 0 0)
  			)
  			(property "ki_fp_filters" "ISP1907*8x8mm*LGA*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_isp1907_ll_0_0"
  				(pin power_in line
  					(at 0 -22.86 90)
  					(length 2.54)
  					(name "VSS")
  					(number "1")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "10")
  				)
  				(pin no_connect line
  					(at -7.62 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "11")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "12")
  				)
  				(pin bidirectional line
  					(at -20.32 12.7 0)
  					(length 2.54)
  					(name "P0.21/~{RESET}")
  					(number "13")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "14")
  				)
  				(pin no_connect line
  					(at -10.16 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "15")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "16")
  				)
  				(pin no_connect line
  					(at -12.7 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "17")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "18")
  				)
  				(pin bidirectional line
  					(at 20.32 -15.24 180)
  					(length 2.54)
  					(name "P0.20")
  					(number "19")
  				)
  				(pin bidirectional line
  					(at 20.32 0 180)
  					(length 2.54)
  					(name "P0.12")
  					(number "2")
  				)
  				(pin input line
  					(at -20.32 -7.62 0)
  					(length 2.54)
  					(name "OUT_ANT")
  					(number "20")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "21")
  				)
  				(pin output line
  					(at -20.32 -5.08 0)
  					(length 2.54)
  					(name "OUT_MOD")
  					(number "22")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "23")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "24")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "25")
  				)
  				(pin power_in line
  					(at 0 22.86 270)
  					(length 2.54)
  					(name "VCC")
  					(number "26")
  				)
  				(pin no_connect line
  					(at -15.24 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "27")
  				)
  				(pin bidirectional line
  					(at -20.32 5.08 0)
  					(length 2.54)
  					(name "SWDIO")
  					(number "28")
  				)
  				(pin no_connect line
  					(at -17.78 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "29")
  				)
  				(pin no_connect line
  					(at -2.54 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "3")
  				)
  				(pin input line
  					(at -20.32 7.62 0)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "30")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "31")
  				)
  				(pin bidirectional line
  					(at 20.32 5.08 180)
  					(length 2.54)
  					(name "P0.08")
  					(number "32")
  				)
  				(pin no_connect line
  					(at 2.54 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "33")
  				)
  				(pin bidirectional line
  					(at 20.32 -10.16 180)
  					(length 2.54)
  					(name "P0.17")
  					(number "34")
  				)
  				(pin no_connect line
  					(at 15.24 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "35")
  				)
  				(pin bidirectional line
  					(at 20.32 7.62 180)
  					(length 2.54)
  					(name "P0.05/AIN3")
  					(number "36")
  				)
  				(pin no_connect line
  					(at 12.7 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "37")
  				)
  				(pin bidirectional line
  					(at 20.32 12.7 180)
  					(length 2.54)
  					(name "P0.03")
  					(number "38")
  				)
  				(pin no_connect line
  					(at 7.62 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "39")
  				)
  				(pin bidirectional line
  					(at 20.32 -2.54 180)
  					(length 2.54)
  					(name "P0.14")
  					(number "4")
  				)
  				(pin no_connect line
  					(at 5.08 20.32 270)
  					(length 2.54) hide
  					(name "P0.01/XL2")
  					(number "40")
  				)
  				(pin no_connect line
  					(at 17.78 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "41")
  				)
  				(pin no_connect line
  					(at 2.54 -20.32 90)
  					(length 2.54) hide
  					(name "P0.00/XL1")
  					(number "42")
  				)
  				(pin no_connect line
  					(at -17.78 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "43")
  				)
  				(pin bidirectional line
  					(at 20.32 -5.08 180)
  					(length 2.54)
  					(name "P0.15")
  					(number "44")
  				)
  				(pin no_connect line
  					(at 10.16 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "45")
  				)
  				(pin bidirectional line
  					(at 20.32 10.16 180)
  					(length 2.54)
  					(name "P0.04")
  					(number "46")
  				)
  				(pin no_connect line
  					(at -15.24 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "47")
  				)
  				(pin bidirectional line
  					(at 20.32 2.54 180)
  					(length 2.54)
  					(name "P0.11")
  					(number "48")
  				)
  				(pin no_connect line
  					(at -12.7 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "49")
  				)
  				(pin no_connect line
  					(at -5.08 20.32 270)
  					(length 2.54) hide
  					(name "NC")
  					(number "5")
  				)
  				(pin no_connect line
  					(at -10.16 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "50")
  				)
  				(pin no_connect line
  					(at -7.62 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "51")
  				)
  				(pin no_connect line
  					(at -5.08 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "52")
  				)
  				(pin no_connect line
  					(at -2.54 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "53")
  				)
  				(pin no_connect line
  					(at 5.08 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "54")
  				)
  				(pin no_connect line
  					(at 7.62 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "55")
  				)
  				(pin no_connect line
  					(at 10.16 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "56")
  				)
  				(pin no_connect line
  					(at 12.7 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "57")
  				)
  				(pin no_connect line
  					(at 15.24 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "58")
  				)
  				(pin no_connect line
  					(at 17.78 -20.32 90)
  					(length 2.54) hide
  					(name "NC")
  					(number "59")
  				)
  				(pin bidirectional line
  					(at 20.32 -12.7 180)
  					(length 2.54)
  					(name "P0.18")
  					(number "6")
  				)
  				(pin no_connect line
  					(at -17.78 -12.7 0)
  					(length 2.54) hide
  					(name "NC")
  					(number "60")
  				)
  				(pin no_connect line
  					(at -17.78 -15.24 0)
  					(length 2.54) hide
  					(name "NC")
  					(number "61")
  				)
  				(pin no_connect line
  					(at -17.78 -17.78 0)
  					(length 2.54) hide
  					(name "NC")
  					(number "62")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "7")
  				)
  				(pin passive line
  					(at 0 -22.86 90)
  					(length 2.54) hide
  					(name "VSS")
  					(number "8")
  				)
  				(pin bidirectional line
  					(at 20.32 -7.62 180)
  					(length 2.54)
  					(name "P0.16")
  					(number "9")
  				)
  			)
  			(symbol "nordic_isp1907_ll_1_1")
  		)
  (symbol "nordic_e83_2g4m03s"
        (property "Footprint" "PartReel:nordic_e83_2g4m03s"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.cdebyte.com/products/E83-2G4M03S"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF5340 Module External Antenna."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless nRF5340 Module External Antenna"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_e83_2g4m03s/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  			)
  			(property "Value" "E83-2G4M03S"
  				(at 0 -2.54 0)
  			)
  			(property "LCSC" "C5333991"
  				(at 0 0 0)
  			)
  			(property "ki_fp_filters" "E83*2G4M03S*16x16mm*LGA*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_e83_2g4m03s_0_0"
  				(pin input line
  					(at 22.86 -5.08 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "1")
  				)
  				(pin power_in line
  					(at 22.86 46.99 180)
  					(length 2.54)
  					(name "VBUS")
  					(number "10")
  				)
  				(pin bidirectional line
  					(at 22.86 2.54 180)
  					(length 2.54)
  					(name "P0.28/AIN7")
  					(number "11")
  				)
  				(pin power_in line
  					(at 0 -57.15 90)
  					(length 2.54)
  					(name "GND")
  					(number "12")
  				)
  				(pin bidirectional line
  					(at -22.86 33.02 0)
  					(length 2.54)
  					(name "P0.29")
  					(number "13")
  				)
  				(pin bidirectional line
  					(at -22.86 30.48 0)
  					(length 2.54)
  					(name "P0.30")
  					(number "14")
  				)
  				(pin bidirectional line
  					(at -22.86 2.54 0)
  					(length 2.54)
  					(name "P1.11")
  					(number "15")
  				)
  				(pin bidirectional line
  					(at -22.86 -2.54 0)
  					(length 2.54)
  					(name "P1.13")
  					(number "16")
  				)
  				(pin bidirectional line
  					(at -22.86 -7.62 0)
  					(length 2.54)
  					(name "P1.15")
  					(number "17")
  				)
  				(pin bidirectional line
  					(at 22.86 41.91 180)
  					(length 2.54)
  					(name "D-")
  					(number "18")
  				)
  				(pin passive line
  					(at 0 -57.15 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "19")
  				)
  				(pin bidirectional line
  					(at 22.86 -2.54 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "2")
  				)
  				(pin passive line
  					(at 0 -57.15 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "20")
  				)
  				(pin passive line
  					(at 0 -57.15 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "22")
  				)
  				(pin power_in line
  					(at 2.54 57.15 270)
  					(length 2.54)
  					(name "VDD")
  					(number "23")
  				)
  				(pin passive line
  					(at 0 -57.15 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "24")
  				)
  				(pin bidirectional line
  					(at 22.86 36.83 180)
  					(length 2.54)
  					(name "P0.00/XL1")
  					(number "25")
  				)
  				(pin bidirectional line
  					(at 22.86 31.75 180)
  					(length 2.54)
  					(name "P0.01/XL2")
  					(number "26")
  				)
  				(pin bidirectional line
  					(at 22.86 27.94 180)
  					(length 2.54)
  					(name "P0.02/NFC1")
  					(number "27")
  				)
  				(pin bidirectional line
  					(at 22.86 25.4 180)
  					(length 2.54)
  					(name "P0.03/NFC2")
  					(number "28")
  				)
  				(pin bidirectional line
  					(at -22.86 22.86 0)
  					(length 2.54)
  					(name "P1.01")
  					(number "29")
  				)
  				(pin bidirectional line
  					(at -22.86 25.4 0)
  					(length 2.54)
  					(name "P1.00")
  					(number "30")
  				)
  				(pin bidirectional line
  					(at 22.86 17.78 180)
  					(length 2.54)
  					(name "P0.05/AIN1")
  					(number "31")
  				)
  				(pin bidirectional line
  					(at 22.86 15.24 180)
  					(length 2.54)
  					(name "P0.06/AIN2")
  					(number "32")
  				)
  				(pin bidirectional line
  					(at 22.86 12.7 180)
  					(length 2.54)
  					(name "P0.07/AIN3")
  					(number "33")
  				)
  				(pin bidirectional line
  					(at -22.86 -45.72 0)
  					(length 2.54)
  					(name "P1.03/I2C")
  					(number "34")
  				)
  				(pin bidirectional line
  					(at -22.86 -43.18 0)
  					(length 2.54)
  					(name "P1.02/I2C")
  					(number "35")
  				)
  				(pin bidirectional line
  					(at -22.86 5.08 0)
  					(length 2.54)
  					(name "P1.10")
  					(number "4")
  				)
  				(pin bidirectional line
  					(at -22.86 -16.51 0)
  					(length 2.54)
  					(name "P0.13/QSPI0")
  					(number "40")
  				)
  				(pin bidirectional line
  					(at -22.86 48.26 0)
  					(length 2.54)
  					(name "P0.19")
  					(number "41")
  				)
  				(pin bidirectional line
  					(at -22.86 20.32 0)
  					(length 2.54)
  					(name "P1.04")
  					(number "42")
  				)
  				(pin bidirectional line
  					(at -22.86 10.16 0)
  					(length 2.54)
  					(name "P1.08")
  					(number "43")
  				)
  				(pin bidirectional line
  					(at -22.86 45.72 0)
  					(length 2.54)
  					(name "P0.20")
  					(number "44")
  				)
  				(pin bidirectional line
  					(at 22.86 7.62 180)
  					(length 2.54)
  					(name "P0.26/AIN5")
  					(number "45")
  				)
  				(pin passive line
  					(at 0 -57.15 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "46")
  				)
  				(pin passive line
  					(at 0 -57.15 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "47")
  				)
  				(pin bidirectional line
  					(at -22.86 -24.13 0)
  					(length 2.54)
  					(name "P0.16/QSPI3")
  					(number "49")
  				)
  				(pin bidirectional line
  					(at -22.86 27.94 0)
  					(length 2.54)
  					(name "P0.31")
  					(number "5")
  				)
  				(pin bidirectional line
  					(at -22.86 43.18 0)
  					(length 2.54)
  					(name "P0.21")
  					(number "50")
  				)
  				(pin bidirectional line
  					(at -22.86 15.24 0)
  					(length 2.54)
  					(name "P1.06")
  					(number "51")
  				)
  				(pin bidirectional line
  					(at -22.86 -19.05 0)
  					(length 2.54)
  					(name "P0.14/QSPI1")
  					(number "52")
  				)
  				(pin bidirectional line
  					(at -22.86 35.56 0)
  					(length 2.54)
  					(name "P0.24")
  					(number "53")
  				)
  				(pin bidirectional line
  					(at -22.86 40.64 0)
  					(length 2.54)
  					(name "P0.22")
  					(number "54")
  				)
  				(pin passive line
  					(at 0 -57.15 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "55")
  				)
  				(pin passive line
  					(at 0 -57.15 90)
  					(length 2.54) hide
  					(name "GND")
  					(number "56")
  				)
  				(pin bidirectional line
  					(at -22.86 38.1 0)
  					(length 2.54)
  					(name "P0.23")
  					(number "57")
  				)
  				(pin bidirectional line
  					(at -22.86 17.78 0)
  					(length 2.54)
  					(name "P1.05")
  					(number "58")
  				)
  				(pin bidirectional line
  					(at 22.86 10.16 180)
  					(length 2.54)
  					(name "P0.25/AIN4")
  					(number "59")
  				)
  				(pin bidirectional line
  					(at -22.86 0 0)
  					(length 2.54)
  					(name "P1.12")
  					(number "6")
  				)
  				(pin bidirectional line
  					(at 22.86 5.08 180)
  					(length 2.54)
  					(name "P0.27/AIN6")
  					(number "60")
  				)
  				(pin bidirectional line
  					(at -22.86 -13.97 0)
  					(length 2.54)
  					(name "P0.17/QSPI_CLK")
  					(number "61")
  				)
  				(pin bidirectional line
  					(at -22.86 -21.59 0)
  					(length 2.54)
  					(name "P0.15/QSPI2")
  					(number "62")
  				)
  				(pin bidirectional line
  					(at -22.86 -11.43 0)
  					(length 2.54)
  					(name "P0.18/QSPI_~{CS}")
  					(number "63")
  				)
  				(pin bidirectional line
  					(at -22.86 7.62 0)
  					(length 2.54)
  					(name "P1.09")
  					(number "64")
  				)
  				(pin bidirectional line
  					(at -22.86 12.7 0)
  					(length 2.54)
  					(name "P1.07")
  					(number "65")
  				)
  				(pin bidirectional line
  					(at -22.86 -5.08 0)
  					(length 2.54)
  					(name "P1.14")
  					(number "7")
  				)
  				(pin bidirectional line
  					(at 22.86 20.32 180)
  					(length 2.54)
  					(name "P0.04/AIN0")
  					(number "8")
  				)
  				(pin bidirectional line
  					(at 22.86 44.45 180)
  					(length 2.54)
  					(name "D+")
  					(number "9")
  				)
  			)
  			(symbol "nordic_e83_2g4m03s_1_0"
  				(pin power_in line
  					(at 0 57.15 270)
  					(length 2.54)
  					(name "VDDH")
  					(number "21")
  				)
  				(pin input line
  					(at 22.86 -7.62 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "3")
  				)
  				(pin bidirectional line
  					(at -22.86 -36.83 0)
  					(length 2.54)
  					(name "P0.08/TD3/SCK")
  					(number "36")
  				)
  				(pin bidirectional line
  					(at -22.86 -34.29 0)
  					(length 2.54)
  					(name "P0.09/TD2/MOSI")
  					(number "37")
  				)
  				(pin bidirectional line
  					(at -22.86 -31.75 0)
  					(length 2.54)
  					(name "P0.10/TD1/MISO")
  					(number "38")
  				)
  				(pin bidirectional line
  					(at -22.86 -29.21 0)
  					(length 2.54)
  					(name "P0.11/TD0/~{CS}")
  					(number "39")
  				)
  				(pin bidirectional line
  					(at -22.86 -39.37 0)
  					(length 2.54)
  					(name "P0.12/TC/DCX")
  					(number "48")
  				)
  			)
  			(symbol "nordic_e83_2g4m03s_1_1")
  		)
  (symbol "nordic_isp2053_ax"
        (property "Footprint" "PartReel:nordic_isp2053_ax"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/nordic_isp2053_ax/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ISP2053-AX."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_isp2053_ax/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "ISP2053-AX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "ISP2053*8x8mm*LGA*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_isp2053_ax_0_0"
  				(pin unspecified line
  					(at 30.48 55.88 180)
  					(length 5.08)
  					(name "VBUS")
  					(number "A2")
  				)
  				(pin unspecified line
  					(at -30.48 -48.26 0)
  					(length 5.08)
  					(name "P1.03/I2C")
  					(number "A3")
  				)
  				(pin unspecified line
  					(at 30.48 53.34 180)
  					(length 5.08)
  					(name "D+")
  					(number "A4")
  				)
  				(pin unspecified line
  					(at 30.48 50.8 180)
  					(length 5.08)
  					(name "D-")
  					(number "A5")
  				)
  				(pin unspecified line
  					(at 0 71.12 270)
  					(length 5.08)
  					(name "VDDH")
  					(number "A6")
  				)
  				(pin unspecified line
  					(at -2.54 71.12 270)
  					(length 5.08)
  					(name "DCCH")
  					(number "A7")
  				)
  				(pin unspecified line
  					(at -30.48 -53.34 0)
  					(length 5.08)
  					(name "P0.02/NFC1")
  					(number "A8")
  				)
  				(pin unspecified line
  					(at -30.48 -55.88 0)
  					(length 5.08)
  					(name "P0.03/NFC2")
  					(number "A9")
  				)
  				(pin unspecified line
  					(at -30.48 -45.72 0)
  					(length 5.08)
  					(name "P1.02/I2C")
  					(number "B10")
  				)
  				(pin unspecified line
  					(at -30.48 55.88 0)
  					(length 5.08)
  					(name "P1.15")
  					(number "B2")
  				)
  				(pin unspecified line
  					(at -30.48 -10.16 0)
  					(length 5.08)
  					(name "P0.06/AIN2")
  					(number "B3")
  				)
  				(pin unspecified line
  					(at -30.48 -5.08 0)
  					(length 5.08)
  					(name "P0.04/AIN0")
  					(number "B4")
  				)
  				(pin unspecified line
  					(at -30.48 53.34 0)
  					(length 5.08)
  					(name "P1.01")
  					(number "B5")
  				)
  				(pin unspecified line
  					(at -30.48 -12.7 0)
  					(length 5.08)
  					(name "P0.07/AIN3")
  					(number "B6")
  				)
  				(pin unspecified line
  					(at -30.48 50.8 0)
  					(length 5.08)
  					(name "P1.00")
  					(number "B7")
  				)
  				(pin unspecified line
  					(at -30.48 -7.62 0)
  					(length 5.08)
  					(name "P0.05/AIN1")
  					(number "B8")
  				)
  				(pin unspecified line
  					(at 30.48 20.32 180)
  					(length 5.08)
  					(name "P0.08/TD3")
  					(number "B9")
  				)
  				(pin unspecified line
  					(at 2.54 71.12 270)
  					(length 5.08)
  					(name "VDD")
  					(number "C1")
  				)
  				(pin unspecified line
  					(at -30.48 43.18 0)
  					(length 5.08)
  					(name "P1.05")
  					(number "C10")
  				)
  				(pin unspecified line
  					(at 30.48 38.1 180)
  					(length 5.08)
  					(name "SWDIO")
  					(number "C11")
  				)
  				(pin unspecified line
  					(at -30.48 -27.94 0)
  					(length 5.08)
  					(name "P0.13/QSPI0")
  					(number "C2")
  				)
  				(pin unspecified line
  					(at -30.48 48.26 0)
  					(length 5.08)
  					(name "P0.19")
  					(number "C3")
  				)
  				(pin unspecified line
  					(at -30.48 -33.02 0)
  					(length 5.08)
  					(name "P0.15/QSPI2")
  					(number "C4")
  				)
  				(pin unspecified line
  					(at -30.48 -30.48 0)
  					(length 5.08)
  					(name "P0.14/QSPI1")
  					(number "C5")
  				)
  				(pin unspecified line
  					(at -30.48 45.72 0)
  					(length 5.08)
  					(name "P0.16")
  					(number "C6")
  				)
  				(pin unspecified line
  					(at 30.48 22.86 180)
  					(length 5.08)
  					(name "P0.09/TD2")
  					(number "C7")
  				)
  				(pin unspecified line
  					(at 30.48 27.94 180)
  					(length 5.08)
  					(name "P0.11/TD0")
  					(number "C8")
  				)
  				(pin unspecified line
  					(at -30.48 -38.1 0)
  					(length 5.08)
  					(name "P0.17/QSPI_CLK")
  					(number "C9")
  				)
  				(pin unspecified line
  					(at -30.48 40.64 0)
  					(length 5.08)
  					(name "P1.13")
  					(number "D1")
  				)
  				(pin unspecified line
  					(at -30.48 22.86 0)
  					(length 5.08)
  					(name "P0.24")
  					(number "D10")
  				)
  				(pin unspecified line
  					(at 30.48 35.56 180)
  					(length 5.08)
  					(name "SWDCLK")
  					(number "D11")
  				)
  				(pin unspecified line
  					(at -30.48 38.1 0)
  					(length 5.08)
  					(name "P0.21")
  					(number "D3")
  				)
  				(pin unspecified line
  					(at -30.48 35.56 0)
  					(length 5.08)
  					(name "P0.22")
  					(number "D5")
  				)
  				(pin unspecified line
  					(at -30.48 33.02 0)
  					(length 5.08)
  					(name "P0.20")
  					(number "D6")
  				)
  				(pin unspecified line
  					(at -30.48 30.48 0)
  					(length 5.08)
  					(name "P1.08")
  					(number "D7")
  				)
  				(pin unspecified line
  					(at -30.48 27.94 0)
  					(length 5.08)
  					(name "P1.09")
  					(number "D8")
  				)
  				(pin unspecified line
  					(at -30.48 25.4 0)
  					(length 5.08)
  					(name "P1.04")
  					(number "D9")
  				)
  				(pin unspecified line
  					(at -30.48 20.32 0)
  					(length 5.08)
  					(name "P1.14")
  					(number "E1")
  				)
  				(pin unspecified line
  					(at -30.48 -17.78 0)
  					(length 5.08)
  					(name "P0.26/AIN5")
  					(number "E10")
  				)
  				(pin unspecified line
  					(at -30.48 17.78 0)
  					(length 5.08)
  					(name "P0.30")
  					(number "E2")
  				)
  				(pin unspecified line
  					(at -30.48 15.24 0)
  					(length 5.08)
  					(name "P0.31")
  					(number "E3")
  				)
  				(pin unspecified line
  					(at -30.48 12.7 0)
  					(length 5.08)
  					(name "P1.12")
  					(number "E4")
  				)
  				(pin unspecified line
  					(at -30.48 10.16 0)
  					(length 5.08)
  					(name "P1.11")
  					(number "E5")
  				)
  				(pin unspecified line
  					(at -30.48 -22.86 0)
  					(length 5.08)
  					(name "P0.28/AIN7")
  					(number "E6")
  				)
  				(pin unspecified line
  					(at -30.48 7.62 0)
  					(length 5.08)
  					(name "P0.29")
  					(number "E8")
  				)
  				(pin unspecified line
  					(at -30.48 -20.32 0)
  					(length 5.08)
  					(name "P0.27/AIN6")
  					(number "E9")
  				)
  				(pin unspecified line
  					(at -30.48 -15.24 0)
  					(length 5.08)
  					(name "P0.25/AIN4")
  					(number "F10")
  				)
  				(pin unspecified line
  					(at -30.48 5.08 0)
  					(length 5.08)
  					(name "P0.23")
  					(number "F3")
  				)
  				(pin unspecified line
  					(at -30.48 2.54 0)
  					(length 5.08)
  					(name "P1.07")
  					(number "F4")
  				)
  				(pin unspecified line
  					(at -30.48 0 0)
  					(length 5.08)
  					(name "P1.10")
  					(number "F5")
  				)
  			)
  			(symbol "nordic_isp2053_ax_1_0"
  				(pin passive line
  					(at 0 -71.12 90)
  					(length 5.08)
  					(name "VSS")
  					(number "A1")
  				)
  				(pin unspecified line
  					(at 30.48 25.4 180)
  					(length 5.08)
  					(name "P0.10/TD1")
  					(number "A10")
  				)
  				(pin passive line
  					(at 0 -71.12 90)
  					(length 5.08) hide
  					(name "VSS")
  					(number "A11")
  				)
  				(pin unspecified line
  					(at 30.48 17.78 180)
  					(length 5.08)
  					(name "P0.12/TC")
  					(number "D2")
  				)
  				(pin unspecified line
  					(at -30.48 -40.64 0)
  					(length 5.08)
  					(name "P0.18/QSPI_~{CS}")
  					(number "D4")
  				)
  				(pin unspecified line
  					(at 30.48 33.02 180)
  					(length 5.08)
  					(name "~{RST}")
  					(number "E11")
  				)
  				(pin passive line
  					(at 0 -71.12 90)
  					(length 5.08) hide
  					(name "VSS")
  					(number "E7")
  				)
  				(pin passive line
  					(at 0 -71.12 90)
  					(length 5.08) hide
  					(name "VSS")
  					(number "F1")
  				)
  				(pin passive line
  					(at 0 -71.12 90)
  					(length 5.08) hide
  					(name "VSS")
  					(number "F11")
  				)
  				(pin unspecified line
  					(at -30.48 -35.56 0)
  					(length 5.08)
  					(name "P1.06/QSPI3")
  					(number "F2")
  				)
  				(pin passive line
  					(at 0 -71.12 90)
  					(length 5.08) hide
  					(name "VSS")
  					(number "F6")
  				)
  				(pin output line
  					(at 30.48 45.72 180)
  					(length 5.08)
  					(name "OUT_ANT")
  					(number "F7")
  				)
  				(pin input line
  					(at 30.48 43.18 180)
  					(length 5.08)
  					(name "OUT_MOD")
  					(number "F8")
  				)
  				(pin passive line
  					(at 0 -71.12 90)
  					(length 5.08) hide
  					(name "VSS")
  					(number "F9")
  				)
  				(pin no_connect line
  					(at 25.4 -20.32 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "H1")
  				)
  				(pin no_connect line
  					(at 25.4 -22.86 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "H11")
  				)
  				(pin no_connect line
  					(at 25.4 -25.4 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "K1")
  				)
  				(pin no_connect line
  					(at 25.4 -27.94 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "K11")
  				)
  				(pin no_connect line
  					(at 25.4 -30.48 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "L1")
  				)
  				(pin no_connect line
  					(at 25.4 -33.02 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "L11")
  				)
  				(pin no_connect line
  					(at 25.4 -35.56 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "L3")
  				)
  				(pin no_connect line
  					(at 25.4 -15.24 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "L5")
  				)
  				(pin no_connect line
  					(at 25.4 -38.1 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "L7")
  				)
  				(pin no_connect line
  					(at 25.4 -17.78 180)
  					(length 5.08) hide
  					(name "NC")
  					(number "L9")
  				)
  			)
  			(symbol "nordic_isp2053_ax_1_1")
  		)
  (symbol "nordic_bl54l15_453_000xxx"
        (property "Footprint" "PartReel:nordic_bl54l15_453_000xxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_nrf54L15"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nRF54L Dual Core Multiprotocol BLE SoC."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless BLE SoC nRF"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_bl54l15_453_000xxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "BL54L15-453-000xxx"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BL54L*LGA*39*14x10mm"
  				(at 0 0 0)
  			)
  			(symbol "nordic_bl54l15_453_000xxx_1_0"
  				(pin bidirectional line
  					(at -27.94 38.1 0)
  					(length 2.54)
  					(name "P1.00")
  					(number "25")
  					(alternate "XL1" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 33.02 0)
  					(length 2.54)
  					(name "P1.01")
  					(number "24")
  					(alternate "XL2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 25.4 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "17")
  				)
  				(pin bidirectional line
  					(at -27.94 22.86 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "18")
  				)
  				(pin bidirectional line
  					(at -27.94 20.32 0)
  					(length 2.54)
  					(name "P0.02")
  					(number "19")
  				)
  				(pin bidirectional line
  					(at -27.94 17.78 0)
  					(length 2.54)
  					(name "P0.03")
  					(number "36")
  					(alternate "GRTCPWM" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 15.24 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "31")
  					(alternate "GRTCLFCLKOUT" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 10.16 0)
  					(length 2.54)
  					(name "P1.02")
  					(number "15")
  					(alternate "NFC1" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 7.62 0)
  					(length 2.54)
  					(name "P1.03")
  					(number "14")
  					(alternate "NFC2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 5.08 0)
  					(length 2.54)
  					(name "P1.04")
  					(number "23")
  					(alternate "AIN0" input line)
  					(alternate "ASO[0]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 2.54 0)
  					(length 2.54)
  					(name "P1.05")
  					(number "22")
  					(alternate "AIN1" bidirectional line)
  					(alternate "ASI[0]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 0 0)
  					(length 2.54)
  					(name "P1.06")
  					(number "21")
  					(alternate "AIN2" input line)
  					(alternate "ASO[1]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -2.54 0)
  					(length 2.54)
  					(name "P1.07")
  					(number "20")
  					(alternate "AIN3" input line)
  					(alternate "ASI[1]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -5.08 0)
  					(length 2.54)
  					(name "P1.08")
  					(number "30")
  					(alternate "EXTREF" input line)
  					(alternate "GRTCHFOUT" output line)
  					(alternate "TAMPC.EXT" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 -7.62 0)
  					(length 2.54)
  					(name "P1.09")
  					(number "29")
  					(alternate "ASO[2]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -10.16 0)
  					(length 2.54)
  					(name "P1.10")
  					(number "28")
  					(alternate "ASI[2]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -12.7 0)
  					(length 2.54)
  					(name "P1.11")
  					(number "35")
  					(alternate "AIN4" input line)
  					(alternate "ASO[3]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -15.24 0)
  					(length 2.54)
  					(name "P1.12")
  					(number "34")
  					(alternate "AIN5" input line)
  					(alternate "ASI[3]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -17.78 0)
  					(length 2.54)
  					(name "P1.13")
  					(number "33")
  					(alternate "AIN6" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -20.32 0)
  					(length 2.54)
  					(name "P1.14")
  					(number "32")
  					(alternate "AIN7" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -25.4 0)
  					(length 2.54)
  					(name "P2.00")
  					(number "9")
  					(alternate "QSPI_D3" bidirectional line)
  					(alternate "SPIM_DCX" output line)
  					(alternate "UARTE_RXD" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -27.94 0)
  					(length 2.54)
  					(name "P2.01")
  					(number "10")
  					(alternate "QSPI_SCK" output line)
  					(alternate "SPIM_SCK" output line)
  					(alternate "SPIS_SCK" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -30.48 0)
  					(length 2.54)
  					(name "P2.02")
  					(number "8")
  					(alternate "QSPI_D0" bidirectional line)
  					(alternate "SPIM_MOSI" output line)
  					(alternate "SPIS_MISO" output line)
  					(alternate "SWO" output line)
  					(alternate "UARTE_TXD" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -33.02 0)
  					(length 2.54)
  					(name "P2.03")
  					(number "13")
  					(alternate "QSPI_D2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 -35.56 0)
  					(length 2.54)
  					(name "P2.04")
  					(number "11")
  					(alternate "QSPI_D1" bidirectional line)
  					(alternate "SPIM_MISO" input line)
  					(alternate "SPIS_MOSI" input line)
  					(alternate "UARTE_CTS" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -38.1 0)
  					(length 2.54)
  					(name "P2.05")
  					(number "12")
  					(alternate "QSPI_CS" output line)
  					(alternate "SPIM_CS" output line)
  					(alternate "UARTE_RTS" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -40.64 0)
  					(length 2.54)
  					(name "P2.06")
  					(number "38")
  					(alternate "SPIM_SCK" output line)
  					(alternate "SPIS_SCK" input line)
  					(alternate "TRACE_CLK" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -43.18 0)
  					(length 2.54)
  					(name "P2.07")
  					(number "4")
  					(alternate "SPIM_DCX" output line)
  					(alternate "SWO" output line)
  					(alternate "TRACEDATA[0]" output line)
  					(alternate "UARTE_RXD" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -45.72 0)
  					(length 2.54)
  					(name "P2.08")
  					(number "3")
  					(alternate "SPIM_MOSI" output line)
  					(alternate "SPIS_MISO" input line)
  					(alternate "TRACEDATA[1]" output line)
  					(alternate "UARTE_TXD" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -48.26 0)
  					(length 2.54)
  					(name "P2.09")
  					(number "2")
  					(alternate "SPIM_MISO" input line)
  					(alternate "SPIS_MOSI" input line)
  					(alternate "TRACEDATA[2]" output line)
  					(alternate "UARTE_CTS" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -50.8 0)
  					(length 2.54)
  					(name "P2.10")
  					(number "37")
  					(alternate "SPIM_CS" output line)
  					(alternate "TRACEDATA[3]" output line)
  					(alternate "UARTE_RTS" output line)
  				)
  				(pin power_in line
  					(at 0 58.42 270)
  					(length 2.54)
  					(name "VDD")
  					(number "26")
  				)
  				(pin power_in line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(name "VSS")
  					(number "1")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "16")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "27")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "VSS")
  					(number "39")
  				)
  				(pin input line
  					(at 27.94 -43.18 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "7")
  				)
  				(pin input line
  					(at 27.94 -48.26 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "6")
  				)
  				(pin bidirectional line
  					(at 27.94 -50.8 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "5")
  				)
  			)
  			(symbol "nordic_bl54l15_453_000xxx_1_1"
  				(text "CLK"
  					(at -15.24 17.78 0)
  				)
  				(text "CLK"
  					(at -15.24 15.24 0)
  				)
  				(text "CLK"
  					(at -15.24 7.62 0)
  				)
  				(text "CLK"
  					(at -15.24 5.08 0)
  				)
  				(text "CLK"
  					(at -15.24 -5.08 0)
  				)
  				(text "CLK"
  					(at -15.24 -12.7 0)
  				)
  				(text "CLK"
  					(at -15.24 -15.24 0)
  				)
  				(text "CLK"
  					(at -15.24 -27.94 0)
  				)
  				(text "CLK"
  					(at -15.24 -40.64 0)
  				)
  			)
  			(embedded_fonts no)
  		)
  (symbol "nordic_bm15x"
        (property "Footprint" "PartReel:nordic_bm15x"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://static1.squarespace.com/static/561459a2e4b0b39f5cefa12e/t/66c3d7591cc204465c3f6e4f/1724110684125/BM15C+Product+Specifications.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "BM15x."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless nRF54L15"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_bm15x/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "BM15x"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BM15*-LGA-45*15.8x10mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_bm15x_0_0"
  				(pin passive line
  					(at 0 58.42 270)
  					(length 2.54)
  					(hide yes)
  					(name "VDD")
  					(number "C8")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "A9")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "B1")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "B7")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "B9")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "D1")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "E1")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "F1")
  				)
  				(pin passive line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "H8")
  				)
  				(pin input line
  					(at 27.94 -43.18 180)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "G2")
  				)
  				(pin input line
  					(at 27.94 -48.26 180)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "K3")
  				)
  				(pin bidirectional line
  					(at 27.94 -50.8 180)
  					(length 2.54)
  					(name "SWDIO")
  					(number "J3")
  				)
  			)
  			(symbol "nordic_bm15x_1_0"
  				(pin bidirectional line
  					(at -27.94 38.1 0)
  					(length 2.54)
  					(name "P1.00")
  					(number "D8")
  					(alternate "XL1" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 33.02 0)
  					(length 2.54)
  					(name "P1.01")
  					(number "C9")
  					(alternate "XL2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 25.4 0)
  					(length 2.54)
  					(name "P0.00")
  					(number "J4")
  				)
  				(pin bidirectional line
  					(at -27.94 22.86 0)
  					(length 2.54)
  					(name "P0.01")
  					(number "K4")
  				)
  				(pin bidirectional line
  					(at -27.94 20.32 0)
  					(length 2.54)
  					(name "P0.02")
  					(number "K2")
  				)
  				(pin bidirectional line
  					(at -27.94 17.78 0)
  					(length 2.54)
  					(name "P0.03")
  					(number "J2")
  					(alternate "GRTCPWM" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 15.24 0)
  					(length 2.54)
  					(name "P0.04")
  					(number "H2")
  					(alternate "GRTCLFCLKOUT" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 10.16 0)
  					(length 2.54)
  					(name "P1.02")
  					(number "D9")
  					(alternate "NFC1" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 7.62 0)
  					(length 2.54)
  					(name "P1.03")
  					(number "E8")
  					(alternate "NFC2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 5.08 0)
  					(length 2.54)
  					(name "P1.04")
  					(number "E9")
  					(alternate "AIN0" input line)
  					(alternate "ASO[0]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 2.54 0)
  					(length 2.54)
  					(name "P1.05")
  					(number "F8")
  					(alternate "AIN1" bidirectional line)
  					(alternate "ASI[0]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 0 0)
  					(length 2.54)
  					(name "P1.06")
  					(number "F9")
  					(alternate "AIN2" input line)
  					(alternate "ASO[1]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -2.54 0)
  					(length 2.54)
  					(name "P1.07")
  					(number "G9")
  					(alternate "AIN3" input line)
  					(alternate "ASI[1]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -5.08 0)
  					(length 2.54)
  					(name "P1.08")
  					(number "G8")
  					(alternate "EXTREF" input line)
  					(alternate "GRTCHFOUT" output line)
  					(alternate "TAMPC.EXT" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 -7.62 0)
  					(length 2.54)
  					(name "P1.09")
  					(number "A3")
  					(alternate "ASO[2]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -10.16 0)
  					(length 2.54)
  					(name "P1.10")
  					(number "B2")
  					(alternate "ASI[2]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -12.7 0)
  					(length 2.54)
  					(name "P1.11")
  					(number "B3")
  					(alternate "AIN4" input line)
  					(alternate "ASO[3]" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -15.24 0)
  					(length 2.54)
  					(name "P1.12")
  					(number "B4")
  					(alternate "AIN5" input line)
  					(alternate "ASI[3]" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -17.78 0)
  					(length 2.54)
  					(name "P1.13")
  					(number "B5")
  					(alternate "AIN6" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -20.32 0)
  					(length 2.54)
  					(name "P1.14")
  					(number "B6")
  					(alternate "AIN7" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -25.4 0)
  					(length 2.54)
  					(name "P2.00")
  					(number "H9")
  					(alternate "QSPI_D3" bidirectional line)
  					(alternate "SPIM_DCX" output line)
  					(alternate "UARTE_RXD" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -27.94 0)
  					(length 2.54)
  					(name "P2.01")
  					(number "J9")
  					(alternate "QSPI_SCK" output line)
  					(alternate "SPIM_SCK" output line)
  					(alternate "SPIS_SCK" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -30.48 0)
  					(length 2.54)
  					(name "P2.02")
  					(number "J8")
  					(alternate "QSPI_D0" bidirectional line)
  					(alternate "SPIM_MOSI" output line)
  					(alternate "SPIS_MISO" output line)
  					(alternate "SWO" output line)
  					(alternate "UARTE_TXD" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -33.02 0)
  					(length 2.54)
  					(name "P2.03")
  					(number "J7")
  					(alternate "QSPI_D2" bidirectional line)
  				)
  				(pin bidirectional line
  					(at -27.94 -35.56 0)
  					(length 2.54)
  					(name "P2.04")
  					(number "K9")
  					(alternate "QSPI_D1" bidirectional line)
  					(alternate "SPIM_MISO" input line)
  					(alternate "SPIS_MOSI" input line)
  					(alternate "UARTE_CTS" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -38.1 0)
  					(length 2.54)
  					(name "K8")
  					(number "16")
  					(alternate "QSPI_CS" output line)
  					(alternate "SPIM_CS" output line)
  					(alternate "UARTE_RTS" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -40.64 0)
  					(length 2.54)
  					(name "P2.06")
  					(number "K7")
  					(alternate "SPIM_SCK" output line)
  					(alternate "SPIS_SCK" input line)
  					(alternate "TRACE_CLK" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -43.18 0)
  					(length 2.54)
  					(name "J6")
  					(number "18")
  					(alternate "SPIM_DCX" output line)
  					(alternate "SWO" output line)
  					(alternate "TRACEDATA[0]" output line)
  					(alternate "UARTE_RXD" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -45.72 0)
  					(length 2.54)
  					(name "P2.08")
  					(number "K6")
  					(alternate "SPIM_MOSI" output line)
  					(alternate "SPIS_MISO" input line)
  					(alternate "TRACEDATA[1]" output line)
  					(alternate "UARTE_TXD" output line)
  				)
  				(pin bidirectional line
  					(at -27.94 -48.26 0)
  					(length 2.54)
  					(name "P2.09")
  					(number "J5")
  					(alternate "SPIM_MISO" input line)
  					(alternate "SPIS_MOSI" input line)
  					(alternate "TRACEDATA[2]" output line)
  					(alternate "UARTE_CTS" input line)
  				)
  				(pin bidirectional line
  					(at -27.94 -50.8 0)
  					(length 2.54)
  					(name "P2.10")
  					(number "K5")
  					(alternate "SPIM_CS" output line)
  					(alternate "TRACEDATA[3]" output line)
  					(alternate "UARTE_RTS" output line)
  				)
  				(pin power_in line
  					(at 0 58.42 270)
  					(length 2.54)
  					(name "VDD")
  					(number "B8")
  				)
  				(pin power_in line
  					(at 0 -58.42 90)
  					(length 2.54)
  					(name "GND")
  					(number "A1")
  				)
  			)
  			(symbol "nordic_bm15x_1_1"
  				(text "CLK"
  					(at -15.24 17.78 0)
  				)
  				(text "CLK"
  					(at -15.24 15.24 0)
  				)
  				(text "CLK"
  					(at -15.24 7.62 0)
  				)
  				(text "CLK"
  					(at -15.24 5.08 0)
  				)
  				(text "CLK"
  					(at -15.24 -5.08 0)
  				)
  				(text "CLK"
  					(at -15.24 -12.7 0)
  				)
  				(text "CLK"
  					(at -15.24 -15.24 0)
  				)
  				(text "CLK"
  					(at -15.24 -27.94 0)
  				)
  				(text "CLK"
  					(at -15.24 -40.64 0)
  				)
  			)
  			(embedded_fonts no)
  		)
  (symbol "nordic_bm20x"
        (property "Footprint" "PartReel:nordic_bm20x"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/nordic_bm20x/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "BM20x."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_bm20x/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "BM20x"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BM20*-LGA-90*15.8x10mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_bm20x_0_0"
  				(pin power_in line
  					(at -22.86 48.26 0)
  					(length 2.54)
  					(name "VBUS")
  					(number "H7")
  				)
  				(pin bidirectional line
  					(at -22.86 38.1 0)
  					(length 2.54)
  					(name "P6.00")
  					(number "J9")
  				)
  				(pin bidirectional line
  					(at -22.86 35.56 0)
  					(length 2.54)
  					(name "P6.01")
  					(number "J6")
  				)
  				(pin bidirectional line
  					(at -22.86 33.02 0)
  					(length 2.54)
  					(name "P6.02/RWDS")
  					(number "D7")
  				)
  				(pin bidirectional line
  					(at -22.86 30.48 0)
  					(length 2.54)
  					(name "P6.03/CS0")
  					(number "E8")
  				)
  				(pin bidirectional line
  					(at -22.86 27.94 0)
  					(length 2.54)
  					(name "P6.04/DQ7")
  					(number "E9")
  				)
  				(pin bidirectional line
  					(at -22.86 25.4 0)
  					(length 2.54)
  					(name "P6.05")
  					(number "K9")
  				)
  				(pin bidirectional line
  					(at -22.86 22.86 0)
  					(length 2.54)
  					(name "P6.06/DQ6")
  					(number "F9")
  				)
  				(pin bidirectional line
  					(at -22.86 20.32 0)
  					(length 2.54)
  					(name "P6.07")
  					(number "J8")
  				)
  				(pin bidirectional line
  					(at -22.86 17.78 0)
  					(length 2.54)
  					(name "P6.08/DQ5")
  					(number "F8")
  				)
  				(pin bidirectional line
  					(at -22.86 15.24 0)
  					(length 2.54)
  					(name "P6.09/DQ3")
  					(number "H9")
  				)
  				(pin bidirectional line
  					(at -22.86 12.7 0)
  					(length 2.54)
  					(name "P6.10")
  					(number "J7")
  				)
  				(pin bidirectional line
  					(at -22.86 10.16 0)
  					(length 2.54)
  					(name "P6.11")
  					(number "A5")
  				)
  				(pin bidirectional line
  					(at -22.86 5.08 0)
  					(length 2.54)
  					(name "P6.13")
  					(number "K8")
  				)
  				(pin bidirectional line
  					(at -22.86 0 0)
  					(length 2.54)
  					(name "P7.00")
  					(number "J5")
  				)
  				(pin bidirectional line
  					(at -22.86 -2.54 0)
  					(length 2.54)
  					(name "P7.01")
  					(number "K7")
  				)
  				(pin bidirectional line
  					(at -22.86 -5.08 0)
  					(length 2.54)
  					(name "P7.02")
  					(number "K5")
  				)
  				(pin bidirectional line
  					(at -22.86 -7.62 0)
  					(length 2.54)
  					(name "P7.03")
  					(number "K6")
  				)
  				(pin bidirectional line
  					(at -22.86 -10.16 0)
  					(length 2.54)
  					(name "P7.04")
  					(number "K4")
  				)
  				(pin bidirectional line
  					(at -22.86 -12.7 0)
  					(length 2.54)
  					(name "P7.05")
  					(number "A7")
  				)
  				(pin bidirectional line
  					(at -22.86 -15.24 0)
  					(length 2.54)
  					(name "P7.06")
  					(number "A6")
  				)
  				(pin bidirectional line
  					(at -22.86 -17.78 0)
  					(length 2.54)
  					(name "P7.07")
  					(number "A8")
  				)
  				(pin bidirectional line
  					(at -22.86 -22.86 0)
  					(length 2.54)
  					(name "P9.00")
  					(number "C9")
  				)
  				(pin bidirectional line
  					(at -22.86 -25.4 0)
  					(length 2.54)
  					(name "P9.01")
  					(number "D8")
  				)
  				(pin bidirectional line
  					(at -22.86 -27.94 0)
  					(length 2.54)
  					(name "P9.02")
  					(number "H4")
  				)
  				(pin bidirectional line
  					(at -22.86 -30.48 0)
  					(length 2.54)
  					(name "P9.03")
  					(number "H5")
  				)
  				(pin bidirectional line
  					(at -22.86 -33.02 0)
  					(length 2.54)
  					(name "P9.04")
  					(number "H6")
  				)
  				(pin bidirectional line
  					(at -22.86 -35.56 0)
  					(length 2.54)
  					(name "P9.05")
  					(number "D4")
  				)
  				(pin input line
  					(at -22.86 -40.64 0)
  					(length 2.54)
  					(name "~{RESET}")
  					(number "G2")
  				)
  				(pin input line
  					(at -22.86 -45.72 0)
  					(length 2.54)
  					(name "SWDCLK")
  					(number "K3")
  				)
  				(pin bidirectional line
  					(at -22.86 -48.26 0)
  					(length 2.54)
  					(name "SWDIO")
  					(number "J3")
  				)
  				(pin no_connect line
  					(at -15.24 50.8 270)
  					(length 2.54)
  					(hide yes)
  					(name "NC")
  					(number "A4")
  				)
  				(pin no_connect line
  					(at -10.16 50.8 270)
  					(length 2.54)
  					(hide yes)
  					(name "NC")
  					(number "C6")
  				)
  				(pin power_in line
  					(at -2.54 53.34 270)
  					(length 2.54)
  					(name "VDD")
  					(number "B8")
  				)
  				(pin power_in line
  					(at 0 53.34 270)
  					(length 2.54)
  					(name "VDD_HV")
  					(number "C8")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "A9")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "B1")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "B7")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "B9")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "C1")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "D1")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "E1")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "F1")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "G1")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "H1")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "H8")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "J1")
  				)
  				(pin passive line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(hide yes)
  					(name "GND")
  					(number "K1")
  				)
  				(pin power_in line
  					(at 2.54 53.34 270)
  					(length 2.54)
  					(name "VDD_P9")
  					(number "C7")
  				)
  				(pin bidirectional line
  					(at 22.86 48.26 180)
  					(length 2.54)
  					(name "P0.00")
  					(number "F5")
  				)
  				(pin bidirectional line
  					(at 22.86 45.72 180)
  					(length 2.54)
  					(name "P0.01")
  					(number "D6")
  				)
  				(pin bidirectional line
  					(at 22.86 43.18 180)
  					(length 2.54)
  					(name "P0.02")
  					(number "K2")
  				)
  				(pin bidirectional line
  					(at 22.86 40.64 180)
  					(length 2.54)
  					(name "P0.03")
  					(number "J2")
  				)
  				(pin bidirectional line
  					(at 22.86 38.1 180)
  					(length 2.54)
  					(name "P0.04")
  					(number "H2")
  				)
  				(pin bidirectional line
  					(at 22.86 35.56 180)
  					(length 2.54)
  					(name "P0.05")
  					(number "D9")
  				)
  				(pin bidirectional line
  					(at 22.86 33.02 180)
  					(length 2.54)
  					(name "P0.06")
  					(number "D5")
  				)
  				(pin bidirectional line
  					(at 22.86 30.48 180)
  					(length 2.54)
  					(name "P0.07")
  					(number "E3")
  				)
  				(pin bidirectional line
  					(at 22.86 27.94 180)
  					(length 2.54)
  					(name "P0.08")
  					(number "E5")
  				)
  				(pin bidirectional line
  					(at 22.86 25.4 180)
  					(length 2.54)
  					(name "P0.09")
  					(number "E4")
  				)
  				(pin bidirectional line
  					(at 22.86 22.86 180)
  					(length 2.54)
  					(name "P0.10")
  					(number "E6")
  				)
  				(pin bidirectional line
  					(at 22.86 20.32 180)
  					(length 2.54)
  					(name "P0.11")
  					(number "E7")
  				)
  				(pin bidirectional line
  					(at 22.86 15.24 180)
  					(length 2.54)
  					(name "P1.00")
  					(number "G3")
  				)
  				(pin bidirectional line
  					(at 22.86 12.7 180)
  					(length 2.54)
  					(name "P1.01")
  					(number "F3")
  				)
  				(pin bidirectional line
  					(at 22.86 10.16 180)
  					(length 2.54)
  					(name "P1.02")
  					(number "F2")
  				)
  				(pin bidirectional line
  					(at 22.86 7.62 180)
  					(length 2.54)
  					(name "P1.03")
  					(number "D3")
  				)
  				(pin bidirectional line
  					(at 22.86 5.08 180)
  					(length 2.54)
  					(name "P1.04")
  					(number "F4")
  				)
  				(pin bidirectional line
  					(at 22.86 2.54 180)
  					(length 2.54)
  					(name "P1.05")
  					(number "F6")
  				)
  				(pin bidirectional line
  					(at 22.86 0 180)
  					(length 2.54)
  					(name "P1.06")
  					(number "F7")
  				)
  				(pin bidirectional line
  					(at 22.86 -5.08 180)
  					(length 2.54)
  					(name "P1.08")
  					(number "G8")
  				)
  				(pin bidirectional line
  					(at 22.86 -7.62 180)
  					(length 2.54)
  					(name "P1.09")
  					(number "H3")
  				)
  				(pin bidirectional line
  					(at 22.86 -10.16 180)
  					(length 2.54)
  					(name "P1.10")
  					(number "G5")
  				)
  				(pin bidirectional line
  					(at 22.86 -12.7 180)
  					(length 2.54)
  					(name "P1.11")
  					(number "G4")
  				)
  				(pin bidirectional line
  					(at 22.86 -17.78 180)
  					(length 2.54)
  					(name "P2.00")
  					(number "B3")
  				)
  				(pin bidirectional line
  					(at 22.86 -20.32 180)
  					(length 2.54)
  					(name "P2.01")
  					(number "B2")
  				)
  				(pin bidirectional line
  					(at 22.86 -22.86 180)
  					(length 2.54)
  					(name "P2.02")
  					(number "E2")
  				)
  				(pin bidirectional line
  					(at 22.86 -25.4 180)
  					(length 2.54)
  					(name "P2.03")
  					(number "B4")
  				)
  				(pin bidirectional line
  					(at 22.86 -27.94 180)
  					(length 2.54)
  					(name "P2.04")
  					(number "B5")
  				)
  				(pin bidirectional line
  					(at 22.86 -30.48 180)
  					(length 2.54)
  					(name "P2.05")
  					(number "B6")
  				)
  				(pin bidirectional line
  					(at 22.86 -33.02 180)
  					(length 2.54)
  					(name "P2.06")
  					(number "A3")
  				)
  				(pin bidirectional line
  					(at 22.86 -35.56 180)
  					(length 2.54)
  					(name "P2.07")
  					(number "C4")
  				)
  				(pin bidirectional line
  					(at 22.86 -38.1 180)
  					(length 2.54)
  					(name "P2.08")
  					(number "C5")
  				)
  				(pin bidirectional line
  					(at 22.86 -40.64 180)
  					(length 2.54)
  					(name "P2.09")
  					(number "C3")
  				)
  			)
  			(symbol "nordic_bm20x_1_0"
  				(pin bidirectional line
  					(at -22.86 45.72 0)
  					(length 2.54)
  					(name "D+")
  					(number "G7")
  				)
  				(pin bidirectional line
  					(at -22.86 43.18 0)
  					(length 2.54)
  					(name "D-")
  					(number "G6")
  				)
  				(pin bidirectional line
  					(at -22.86 7.62 0)
  					(length 2.54)
  					(name "P6.12")
  					(number "J4")
  				)
  				(pin no_connect line
  					(at -12.7 50.8 270)
  					(length 2.54)
  					(hide yes)
  					(name "NC")
  					(number "A2")
  				)
  				(pin power_in line
  					(at 0 -53.34 90)
  					(length 2.54)
  					(name "GND")
  					(number "A1")
  				)
  				(pin bidirectional line
  					(at 22.86 -2.54 180)
  					(length 2.54)
  					(name "P1.07")
  					(number "G9")
  				)
  				(pin bidirectional line
  					(at 22.86 -43.18 180)
  					(length 2.54)
  					(name "P2.10/NFC1")
  					(number "D2")
  				)
  				(pin bidirectional line
  					(at 22.86 -45.72 180)
  					(length 2.54)
  					(name "P2.11/NFC2")
  					(number "C2")
  				)
  			)
  			(symbol "nordic_bm20x_1_1")
  			(embedded_fonts no)
  		)
  (symbol "sparkfun_dan_f10n"
        (property "Footprint" "PartReel:sparkfun_dan_f10n"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_dan_f10n/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "u-blox Dualband L1/L5 GNSS Receiver."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun GNSS GPS L1/L5 Receiver"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_dan_f10n/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -10.16 13.97 0)
    		)
    		(property "Value" "DAN-F10N (SparkFun)"
    			(at -7.62 -15.24 0)
    		)
    		(property "PROD_ID" "IC-25933"
    			(at 2.54 -20.32 0)
    		)
    		(symbol "sparkfun_dan_f10n_1_1"
    			(pin power_in line
    				(at -13.97 11.43 0)
    				(length 2.54)
    				(name "VCC")
    				(number "52")
    			)
    			(pin power_in line
    				(at -13.97 11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "VCC")
    				(number "53")
    			)
    			(pin power_in line
    				(at -13.97 8.89 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "55")
    			)
    			(pin input line
    				(at -13.97 6.35 0)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "16")
    			)
    			(pin input line
    				(at -13.97 1.27 0)
    				(length 2.54)
    				(name "EXT_RF_IN")
    				(number "34")
    			)
    			(pin output line
    				(at -13.97 -1.27 0)
    				(length 2.54)
    				(name "VCC_RF")
    				(number "31")
    			)
    			(pin input line
    				(at -13.97 -3.81 0)
    				(length 2.54)
    				(name "ANT_CTRL")
    				(number "32")
    			)
    			(pin output line
    				(at -13.97 -6.35 0)
    				(length 2.54)
    				(name "LNA_EN")
    				(number "39")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "13")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "14")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "15")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "19")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "2")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "21")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "22")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "23")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "26")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "27")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "28")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "29")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "30")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "33")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "35")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "37")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "38")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "4")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "40")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "41")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "42")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "43")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "44")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "47")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "48")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "5")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "50")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "51")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "54")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "56")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "57")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "6")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "7")
    			)
    			(pin power_in line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "8")
    			)
    			(pin output line
    				(at 13.97 11.43 180)
    				(length 2.54)
    				(name "TXD")
    				(number "10")
    			)
    			(pin input line
    				(at 13.97 8.89 180)
    				(length 2.54)
    				(name "RXD")
    				(number "9")
    			)
    			(pin input line
    				(at 13.97 -7.62 180)
    				(length 2.54)
    				(name "~{SAFEBOOT}")
    				(number "18")
    			)
    			(pin input line
    				(at 13.97 -10.16 180)
    				(length 2.54)
    				(name "EXTINT")
    				(number "17")
    			)
    			(pin output line
    				(at 13.97 -12.7 180)
    				(length 2.54)
    				(name "TIMEPULSE")
    				(number "20")
    			)
    			(pin no_connect line
    				(at 29.21 3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "11")
    			)
    			(pin no_connect line
    				(at 29.21 1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "12")
    			)
    			(pin no_connect line
    				(at 29.21 -1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "24")
    			)
    			(pin no_connect line
    				(at 29.21 -3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "25")
    			)
    			(pin no_connect line
    				(at 29.21 -6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "36")
    			)
    			(pin no_connect line
    				(at 29.21 -8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "45")
    			)
    			(pin no_connect line
    				(at 29.21 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "46")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_gnss_flex_carrier_left"
        (property "Footprint" "PartReel:sparkfun_gnss_flex_carrier_left"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.4uconnector.com/online/object/4udrawing/22817.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2x10 2.0mm Header with pegs that connect to the socket on a Flex module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_gnss_flex_carrier_left/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -10.16 12.7 0)
    		)
    		(property "Value" "GNSS_Flex_Carrier_Left (SparkFun)"
    			(at -5.08 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-25207"
    			(at 0 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_gnss_flex_carrier_left_1_1"
    			(text_box "3V3"
    				(at -8.89 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "GND"
    				(at -8.89 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "VBACKUP"
    				(at -8.89 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "RTK LED"
    				(at -8.89 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "PVT LED"
    				(at -8.89 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "I2C SDA"
    				(at -8.89 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 108 183 90 1)
    				)
    			)
    			(text_box "I2C SCL"
    				(at -8.89 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 108 183 90 1)
    				)
    			)
    			(text_box "USB D-"
    				(at -8.89 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 136 181 1)
    				)
    			)
    			(text_box "USB D+"
    				(at -8.89 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 136 181 1)
    				)
    			)
    			(text_box "VUSB"
    				(at -8.89 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "PPS1"
    				(at 0 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "PPS2"
    				(at 0 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "EVENTA"
    				(at 0 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "EVENTB"
    				(at 0 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "SD CMD"
    				(at 0 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 67 61 255 1)
    				)
    			)
    			(text_box "SD CLK"
    				(at 0 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 67 61 255 1)
    				)
    			)
    			(text_box "SD DAT0"
    				(at 0 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 67 61 255 1)
    				)
    			)
    			(text_box "SD DAT3"
    				(at 0 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 67 61 255 1)
    				)
    			)
    			(text_box "GND"
    				(at 0 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at 0 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(pin passive line
    				(at -13.97 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -13.97 7.62 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -13.97 5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -13.97 2.54 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -13.97 0 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -13.97 -2.54 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -13.97 -5.08 0)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at -13.97 -7.62 0)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at -13.97 -10.16 0)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at -13.97 -12.7 0)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    			(pin passive line
    				(at 13.97 10.16 180)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at 13.97 7.62 180)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at 13.97 5.08 180)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at 13.97 2.54 180)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at 13.97 0 180)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at 13.97 -2.54 180)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at 13.97 -5.08 180)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at 13.97 -7.62 180)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at 13.97 -10.16 180)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at 13.97 -12.7 180)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_gnss_flex_carrier_mid"
        (property "Footprint" "PartReel:sparkfun_gnss_flex_carrier_mid"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.4uconnector.com/online/object/4udrawing/22817.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2x10 2.0mm Header with pegs that connect to the socket on a Flex module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_gnss_flex_carrier_mid/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -10.16 12.7 0)
    		)
    		(property "Value" "GNSS_Flex_Carrier_Mid (SparkFun)"
    			(at -5.08 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-25207"
    			(at 0 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_gnss_flex_carrier_mid_1_1"
    			(text_box "3V3"
    				(at -8.89 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "GND"
    				(at -8.89 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "MDC"
    				(at -8.89 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII RXD0"
    				(at -8.89 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII RXER"
    				(at -8.89 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "GND"
    				(at -8.89 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "RMII TXD0"
    				(at -8.89 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "nRST LAN"
    				(at -8.89 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "ON OFF"
    				(at -8.89 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "READY"
    				(at -8.89 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RMII CLK"
    				(at 0 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "MDIO"
    				(at 0 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII RXD1"
    				(at 0 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII CRSDV"
    				(at 0 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "GND"
    				(at 0 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "RMII TXEN"
    				(at 0 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII TXD1"
    				(at 0 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "PMIC ON"
    				(at 0 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "GND"
    				(at 0 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at 0 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(pin passive line
    				(at -13.97 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -13.97 7.62 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -13.97 5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -13.97 2.54 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -13.97 0 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -13.97 -2.54 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -13.97 -5.08 0)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at -13.97 -7.62 0)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at -13.97 -10.16 0)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at -13.97 -12.7 0)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    			(pin passive line
    				(at 13.97 10.16 180)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at 13.97 7.62 180)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at 13.97 5.08 180)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at 13.97 2.54 180)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at 13.97 0 180)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at 13.97 -2.54 180)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at 13.97 -5.08 180)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at 13.97 -7.62 180)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at 13.97 -10.16 180)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at 13.97 -12.7 180)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_gnss_flex_carrier_right"
        (property "Footprint" "PartReel:sparkfun_gnss_flex_carrier_right"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.4uconnector.com/online/object/4udrawing/22817.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2x10 2.0mm Header with pegs that connect to the socket on a Flex module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_gnss_flex_carrier_right/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -10.16 12.7 0)
    		)
    		(property "Value" "GNSS_Flex_Carrier_Right (SparkFun)"
    			(at -5.08 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-25207"
    			(at 0 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_gnss_flex_carrier_right_1_1"
    			(text_box "3V3"
    				(at -8.89 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "GND"
    				(at -8.89 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "RTS3"
    				(at -8.89 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "CTS2"
    				(at -8.89 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "RTS2"
    				(at -8.89 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "TXD4"
    				(at -8.89 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RXD4"
    				(at -8.89 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "TXD1"
    				(at -8.89 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RTS1"
    				(at -8.89 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RXD1"
    				(at -8.89 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "ID"
    				(at 0 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 99 96 99 1)
    				)
    			)
    			(text_box "CTS3"
    				(at 0 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "TXD3"
    				(at 0 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RXD3"
    				(at 0 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "TXD2"
    				(at 0 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RXD2"
    				(at 0 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "CTS1"
    				(at 0 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "~{RESET}"
    				(at 0 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 176 171 176 1)
    				)
    			)
    			(text_box "GND"
    				(at 0 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at 0 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(pin passive line
    				(at -13.97 10.16 0)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at -13.97 7.62 0)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at -13.97 5.08 0)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at -13.97 2.54 0)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at -13.97 0 0)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at -13.97 -2.54 0)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at -13.97 -5.08 0)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at -13.97 -7.62 0)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at -13.97 -10.16 0)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at -13.97 -12.7 0)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    			(pin passive line
    				(at 13.97 10.16 180)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at 13.97 7.62 180)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at 13.97 5.08 180)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at 13.97 2.54 180)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at 13.97 0 180)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at 13.97 -2.54 180)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at 13.97 -5.08 180)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at 13.97 -7.62 180)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at 13.97 -10.16 180)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at 13.97 -12.7 180)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_gnss_flex_module_left"
        (property "Footprint" "PartReel:sparkfun_gnss_flex_module_left"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.4uconnector.com/online/object/4udrawing/22815.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2x10 2.0mm Socket with pegs used to connect to Flex carrier header pins."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun GNSS Flex Module connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_gnss_flex_module_left/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -10.16 12.7 0)
    		)
    		(property "Value" "GNSS_Flex_Module_Left (SparkFun)"
    			(at -5.08 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-25206"
    			(at 0 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_gnss_flex_module_left_1_1"
    			(text_box "PPS1"
    				(at -8.89 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "PPS2"
    				(at -8.89 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "EVENTA"
    				(at -8.89 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "EVENTB"
    				(at -8.89 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "SD CMD"
    				(at -8.89 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 67 61 255 1)
    				)
    			)
    			(text_box "SD CLK"
    				(at -8.89 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 67 61 255 1)
    				)
    			)
    			(text_box "SD DAT0"
    				(at -8.89 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 67 61 255 1)
    				)
    			)
    			(text_box "SD DAT3"
    				(at -8.89 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 67 61 255 1)
    				)
    			)
    			(text_box "GND"
    				(at -8.89 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at -8.89 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at 0 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "GND"
    				(at 0 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "VBACKUP"
    				(at 0 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "RTK LED"
    				(at 0 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "PVT LED"
    				(at 0 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "I2C SDA"
    				(at 0 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 108 183 90 1)
    				)
    			)
    			(text_box "I2C SCL"
    				(at 0 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 108 183 90 1)
    				)
    			)
    			(text_box "USB D-"
    				(at 0 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 136 181 1)
    				)
    			)
    			(text_box "USB D+"
    				(at 0 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 136 181 1)
    				)
    			)
    			(text_box "VUSB"
    				(at 0 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(pin passive line
    				(at -13.97 10.16 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -13.97 7.62 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -13.97 5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -13.97 2.54 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -13.97 0 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -13.97 -2.54 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at -13.97 -5.08 0)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at -13.97 -7.62 0)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at -13.97 -10.16 0)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at -13.97 -12.7 0)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    			(pin passive line
    				(at 13.97 10.16 180)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at 13.97 7.62 180)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at 13.97 5.08 180)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at 13.97 2.54 180)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at 13.97 0 180)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at 13.97 -2.54 180)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at 13.97 -5.08 180)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at 13.97 -7.62 180)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at 13.97 -10.16 180)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at 13.97 -12.7 180)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_gnss_flex_module_mid"
        (property "Footprint" "PartReel:sparkfun_gnss_flex_module_mid"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.4uconnector.com/online/object/4udrawing/22815.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2x10 2.0mm Socket with pegs used to connect to Flex carrier header pins."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Flex Module connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_gnss_flex_module_mid/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -10.16 12.7 0)
    		)
    		(property "Value" "GNSS_Flex_Module_Mid (SparkFun)"
    			(at -5.08 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-25206"
    			(at 0 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_gnss_flex_module_mid_1_1"
    			(text_box "RMII CLK"
    				(at -8.89 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "MDIO"
    				(at -8.89 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII RXD1"
    				(at -8.89 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII CRSDV"
    				(at -8.89 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "GND"
    				(at -8.89 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "RMII TXEN"
    				(at -8.89 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII TXD1"
    				(at -8.89 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "PMIC ON"
    				(at -8.89 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "GND"
    				(at -8.89 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at -8.89 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at 0 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "GND"
    				(at 0 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "MDC"
    				(at 0 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII RXD0"
    				(at 0 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "RMII RXER"
    				(at 0 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "GND"
    				(at 0 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "RMII TXD0"
    				(at 0 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "nRST LAN"
    				(at 0 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.6096 0.6096 0.6096 0.6096)
    				(fill
    					(type color)
    					(color 209 9 255 1)
    				)
    			)
    			(text_box "ON OFF"
    				(at 0 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "READY"
    				(at 0 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(pin passive line
    				(at -13.97 10.16 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -13.97 7.62 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -13.97 5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -13.97 2.54 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -13.97 0 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -13.97 -2.54 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at -13.97 -5.08 0)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at -13.97 -7.62 0)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at -13.97 -10.16 0)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at -13.97 -12.7 0)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    			(pin passive line
    				(at 13.97 10.16 180)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at 13.97 7.62 180)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at 13.97 5.08 180)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at 13.97 2.54 180)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at 13.97 0 180)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at 13.97 -2.54 180)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at 13.97 -5.08 180)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at 13.97 -7.62 180)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at 13.97 -10.16 180)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at 13.97 -12.7 180)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_gnss_flex_module_right"
        (property "Footprint" "PartReel:sparkfun_gnss_flex_module_right"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "http://www.4uconnector.com/online/object/4udrawing/22815.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "2x10 2.0mm Socket with pegs used to connect to Flex carrier header pins."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun connector"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_gnss_flex_module_right/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    			(hide yes)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "J"
    			(at -10.16 12.7 0)
    		)
    		(property "Value" "GNSS_Flex_Module_Right (SparkFun)"
    			(at -5.08 -15.24 0)
    		)
    		(property "PROD_ID" "CONN-25206"
    			(at 0 -25.4 0)
    		)
    		(property "ki_fp_filters" "Connector*:*_1x??_*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_gnss_flex_module_right_1_1"
    			(text_box "ID"
    				(at -8.89 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 99 96 99 1)
    				)
    			)
    			(text_box "CTS3"
    				(at -8.89 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "TXD3"
    				(at -8.89 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RXD3"
    				(at -8.89 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "TXD2"
    				(at -8.89 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RXD2"
    				(at -8.89 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "CTS1"
    				(at -8.89 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "~{RESET}"
    				(at -8.89 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 176 171 176 1)
    				)
    			)
    			(text_box "GND"
    				(at -8.89 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at -8.89 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "3V3"
    				(at 0 11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 0 0 1)
    				)
    			)
    			(text_box "GND"
    				(at 0 8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 0 0 0 1)
    				)
    			)
    			(text_box "RTS3"
    				(at 0 6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "CTS2"
    				(at 0 3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "RTS2"
    				(at 0 1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "TXD4"
    				(at 0 -1.27 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RXD4"
    				(at 0 -3.81 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(text_box "TXD1"
    				(at 0 -6.35 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RTS1"
    				(at 0 -8.89 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 248 32 1)
    				)
    			)
    			(text_box "RXD1"
    				(at 0 -11.43 0)
    				(size 8.89 -2.54)
    				(margins 0.8128 0.8128 0.8128 0.8128)
    				(fill
    					(type color)
    					(color 255 178 23 1)
    				)
    			)
    			(pin passive line
    				(at -13.97 10.16 0)
    				(length 3.81)
    				(name "Pin_2")
    				(number "2")
    			)
    			(pin passive line
    				(at -13.97 7.62 0)
    				(length 3.81)
    				(name "Pin_4")
    				(number "4")
    			)
    			(pin passive line
    				(at -13.97 5.08 0)
    				(length 3.81)
    				(name "Pin_6")
    				(number "6")
    			)
    			(pin passive line
    				(at -13.97 2.54 0)
    				(length 3.81)
    				(name "Pin_8")
    				(number "8")
    			)
    			(pin passive line
    				(at -13.97 0 0)
    				(length 3.81)
    				(name "Pin_10")
    				(number "10")
    			)
    			(pin passive line
    				(at -13.97 -2.54 0)
    				(length 3.81)
    				(name "Pin_12")
    				(number "12")
    			)
    			(pin passive line
    				(at -13.97 -5.08 0)
    				(length 3.81)
    				(name "Pin_14")
    				(number "14")
    			)
    			(pin passive line
    				(at -13.97 -7.62 0)
    				(length 3.81)
    				(name "Pin_16")
    				(number "16")
    			)
    			(pin passive line
    				(at -13.97 -10.16 0)
    				(length 3.81)
    				(name "Pin_18")
    				(number "18")
    			)
    			(pin passive line
    				(at -13.97 -12.7 0)
    				(length 3.81)
    				(name "Pin_20")
    				(number "20")
    			)
    			(pin passive line
    				(at 13.97 10.16 180)
    				(length 3.81)
    				(name "Pin_1")
    				(number "1")
    			)
    			(pin passive line
    				(at 13.97 7.62 180)
    				(length 3.81)
    				(name "Pin_3")
    				(number "3")
    			)
    			(pin passive line
    				(at 13.97 5.08 180)
    				(length 3.81)
    				(name "Pin_5")
    				(number "5")
    			)
    			(pin passive line
    				(at 13.97 2.54 180)
    				(length 3.81)
    				(name "Pin_7")
    				(number "7")
    			)
    			(pin passive line
    				(at 13.97 0 180)
    				(length 3.81)
    				(name "Pin_9")
    				(number "9")
    			)
    			(pin passive line
    				(at 13.97 -2.54 180)
    				(length 3.81)
    				(name "Pin_11")
    				(number "11")
    			)
    			(pin passive line
    				(at 13.97 -5.08 180)
    				(length 3.81)
    				(name "Pin_13")
    				(number "13")
    			)
    			(pin passive line
    				(at 13.97 -7.62 180)
    				(length 3.81)
    				(name "Pin_15")
    				(number "15")
    			)
    			(pin passive line
    				(at 13.97 -10.16 180)
    				(length 3.81)
    				(name "Pin_17")
    				(number "17")
    			)
    			(pin passive line
    				(at 13.97 -12.7 180)
    				(length 3.81)
    				(name "Pin_19")
    				(number "19")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_lc762z"
        (property "Footprint" "PartReel:sparkfun_lc762z"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_lc762z/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Quectel GPS BeiDou GNSS Module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Quectel GPS GNSS module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_lc762z/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -6.35 12.7 0)
    		)
    		(property "Value" "LC762Z (SparkFun)"
    			(at 5.08 12.7 0)
    		)
    		(property "PROD_ID" "IC-27030"
    			(at 1.27 -15.24 0)
    		)
    		(property "ki_fp_filters" "Quectel*L70*R*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_lc762z_0_1")
    		(symbol "sparkfun_lc762z_1_1"
    			(pin power_in line
    				(at -10.16 10.16 0)
    				(length 2.54)
    				(name "VCC")
    				(number "8")
    			)
    			(pin input line
    				(at -10.16 7.62 0)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "9")
    			)
    			(pin power_in line
    				(at -10.16 5.08 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "6")
    			)
    			(pin input line
    				(at -10.16 2.54 0)
    				(length 2.54)
    				(name "RF_IN")
    				(number "11")
    			)
    			(pin power_out line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "VDD_RF")
    				(number "14")
    			)
    			(pin output line
    				(at -10.16 -7.62 0)
    				(length 2.54)
    				(name "ANT_ON")
    				(number "13")
    			)
    			(pin power_in line
    				(at -10.16 -10.16 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin passive line
    				(at -10.16 -10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "10")
    			)
    			(pin passive line
    				(at -10.16 -10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "12")
    			)
    			(pin output line
    				(at 10.16 10.16 180)
    				(length 2.54)
    				(name "TXD1")
    				(number "2")
    			)
    			(pin input line
    				(at 10.16 7.62 180)
    				(length 2.54)
    				(name "RXD1")
    				(number "3")
    			)
    			(pin bidirectional line
    				(at 10.16 3.81 180)
    				(length 2.54)
    				(name "SCL")
    				(number "17")
    			)
    			(pin bidirectional line
    				(at 10.16 1.27 180)
    				(length 2.54)
    				(name "SDA")
    				(number "16")
    			)
    			(pin output line
    				(at 10.16 -3.81 180)
    				(length 2.54)
    				(name "PPS")
    				(number "4")
    			)
    			(pin no_connect line
    				(at 24.13 5.08 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "5")
    			)
    			(pin no_connect line
    				(at 24.13 2.54 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "7")
    			)
    			(pin no_connect line
    				(at 24.13 0 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "15")
    			)
    			(pin no_connect line
    				(at 24.13 -2.54 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "18")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_lg290p"
        (property "Footprint" "PartReel:sparkfun_lg290p"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/4/1/a/7/e/Quectel_LG290P_03__Hardware_Design_V1.0.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Quectel Quadband GNSS Receiver."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun GNSS GPS Receiver"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_lg290p/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -10.16 16.51 0)
    		)
    		(property "Value" "LG290P (SparkFun)"
    			(at -7.62 -17.78 0)
    		)
    		(property "PROD_ID" "GPS-23025"
    			(at 0 -22.86 0)
    		)
    		(symbol "sparkfun_lg290p_1_1"
    			(pin power_in line
    				(at -13.97 13.97 0)
    				(length 2.54)
    				(name "VCC")
    				(number "23")
    			)
    			(pin power_in line
    				(at -13.97 11.43 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "22")
    			)
    			(pin input line
    				(at -13.97 8.89 0)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "8")
    			)
    			(pin input line
    				(at -13.97 2.54 0)
    				(length 2.54)
    				(name "RF_IN")
    				(number "11")
    			)
    			(pin power_out line
    				(at -13.97 -2.54 0)
    				(length 2.54)
    				(name "VCC_RF")
    				(number "9")
    			)
    			(pin no_connect line
    				(at -13.97 -5.08 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "2")
    			)
    			(pin no_connect line
    				(at -13.97 -6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "1")
    			)
    			(pin no_connect line
    				(at -13.97 -7.62 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "17")
    			)
    			(pin no_connect line
    				(at -13.97 -8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "5")
    			)
    			(pin power_in line
    				(at -13.97 -15.24 0)
    				(length 2.54)
    				(name "GND")
    				(number "10")
    			)
    			(pin power_in line
    				(at -13.97 -15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "12")
    			)
    			(pin power_in line
    				(at -13.97 -15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "13")
    			)
    			(pin power_in line
    				(at -13.97 -15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "24")
    			)
    			(pin power_in line
    				(at -13.97 -15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "25")
    			)
    			(pin output line
    				(at 13.97 13.97 180)
    				(length 2.54)
    				(name "TXD1")
    				(number "20")
    			)
    			(pin input line
    				(at 13.97 11.43 180)
    				(length 2.54)
    				(name "RXD1")
    				(number "21")
    			)
    			(pin output line
    				(at 13.97 8.89 180)
    				(length 2.54)
    				(name "TXD2")
    				(number "6")
    			)
    			(pin input line
    				(at 13.97 6.35 180)
    				(length 2.54)
    				(name "RXD2")
    				(number "7")
    			)
    			(pin output line
    				(at 13.97 3.81 180)
    				(length 2.54)
    				(name "TXD3")
    				(number "16")
    			)
    			(pin input line
    				(at 13.97 1.27 180)
    				(length 2.54)
    				(name "RXD3")
    				(number "15")
    			)
    			(pin bidirectional line
    				(at 13.97 -2.54 180)
    				(length 2.54)
    				(name "SCL")
    				(number "19")
    			)
    			(pin bidirectional line
    				(at 13.97 -5.08 180)
    				(length 2.54)
    				(name "SDA")
    				(number "18")
    			)
    			(pin output line
    				(at 13.97 -8.89 180)
    				(length 2.54)
    				(name "RTK_STAT")
    				(number "14")
    			)
    			(pin output line
    				(at 13.97 -12.7 180)
    				(length 2.54)
    				(name "PPS")
    				(number "3")
    			)
    			(pin input line
    				(at 13.97 -15.24 180)
    				(length 2.54)
    				(name "EVENT")
    				(number "4")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_lg580p"
        (property "Footprint" "PartReel:sparkfun_lg580p"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/1/8/d/6/6/Quectel_LG580P_03__Hardware_Design_V1.0.0_Preliminary_20241012.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Quectel Quadband GNSS Receiver with Heading."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun GNSS GPS RTK Receiver with Heading"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_lg580p/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -10.16 30.48 0)
    		)
    		(property "Value" "LG580P (SparkFun)"
    			(at -7.62 -29.21 0)
    		)
    		(property "PROD_ID" "GPS-25039"
    			(at 2.54 -34.29 0)
    		)
    		(symbol "sparkfun_lg580p_1_1"
    			(pin power_in line
    				(at -13.97 27.94 0)
    				(length 2.54)
    				(name "VCC")
    				(number "23")
    			)
    			(pin power_in line
    				(at -13.97 27.94 0)
    				(length 2.54)
    				(hide yes)
    				(name "VCC")
    				(number "24")
    			)
    			(pin power_in line
    				(at -13.97 25.4 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "5")
    			)
    			(pin input line
    				(at -13.97 22.86 0)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "33")
    			)
    			(pin input line
    				(at -13.97 16.51 0)
    				(length 2.54)
    				(name "RF_IN1")
    				(number "2")
    			)
    			(pin input line
    				(at -13.97 11.43 0)
    				(length 2.54)
    				(name "RF_IN2")
    				(number "36")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    				(alternate "PowerPins" input line)
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "34")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "35")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "37")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "4")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "41")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "43")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "45")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49")
    			)
    			(pin output line
    				(at 13.97 27.94 180)
    				(length 2.54)
    				(name "TXD1")
    				(number "18")
    			)
    			(pin input line
    				(at 13.97 25.4 180)
    				(length 2.54)
    				(name "RXD1")
    				(number "17")
    			)
    			(pin output line
    				(at 13.97 22.86 180)
    				(length 2.54)
    				(name "TXD2")
    				(number "20")
    			)
    			(pin input line
    				(at 13.97 20.32 180)
    				(length 2.54)
    				(name "RXD2")
    				(number "19")
    			)
    			(pin output line
    				(at 13.97 17.78 180)
    				(length 2.54)
    				(name "TXD3")
    				(number "27")
    			)
    			(pin input line
    				(at 13.97 15.24 180)
    				(length 2.54)
    				(name "RXD3")
    				(number "28")
    			)
    			(pin bidirectional line
    				(at 13.97 11.43 180)
    				(length 2.54)
    				(name "SCL")
    				(number "21")
    			)
    			(pin bidirectional line
    				(at 13.97 8.89 180)
    				(length 2.54)
    				(name "SDA")
    				(number "22")
    			)
    			(pin input line
    				(at 13.97 3.81 180)
    				(length 2.54)
    				(name "~{CS}")
    				(number "6")
    			)
    			(pin input line
    				(at 13.97 1.27 180)
    				(length 2.54)
    				(name "CLK")
    				(number "8")
    			)
    			(pin output line
    				(at 13.97 -1.27 180)
    				(length 2.54)
    				(name "MISO")
    				(number "9")
    			)
    			(pin input line
    				(at 13.97 -3.81 180)
    				(length 2.54)
    				(name "MOSI")
    				(number "7")
    			)
    			(pin output line
    				(at 13.97 -6.35 180)
    				(length 2.54)
    				(name "~{SDRY}")
    				(number "10")
    			)
    			(pin output line
    				(at 13.97 -11.43 180)
    				(length 2.54)
    				(name "HEADING_STAT")
    				(number "11")
    			)
    			(pin output line
    				(at 13.97 -13.97 180)
    				(length 2.54)
    				(name "~{ERR}_STAT")
    				(number "14")
    			)
    			(pin output line
    				(at 13.97 -16.51 180)
    				(length 2.54)
    				(name "PVT_STAT")
    				(number "15")
    			)
    			(pin output line
    				(at 13.97 -19.05 180)
    				(length 2.54)
    				(name "RTK_STAT")
    				(number "16")
    			)
    			(pin output line
    				(at 13.97 -21.59 180)
    				(length 2.54)
    				(name "PPS")
    				(number "30")
    			)
    			(pin input line
    				(at 13.97 -26.67 180)
    				(length 2.54)
    				(name "EVENT")
    				(number "32")
    			)
    			(pin no_connect line
    				(at 31.75 15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "12")
    			)
    			(pin no_connect line
    				(at 31.75 12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "13")
    			)
    			(pin no_connect line
    				(at 31.75 10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "25")
    			)
    			(pin no_connect line
    				(at 31.75 7.62 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "26")
    			)
    			(pin no_connect line
    				(at 31.75 5.08 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "29")
    			)
    			(pin no_connect line
    				(at 31.75 2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "31")
    			)
    			(pin no_connect line
    				(at 31.75 0 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "38")
    			)
    			(pin no_connect line
    				(at 31.75 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "39")
    			)
    			(pin no_connect line
    				(at 31.75 -5.08 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "42")
    			)
    			(pin no_connect line
    				(at 31.75 -7.62 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "40")
    			)
    			(pin no_connect line
    				(at 31.75 -10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "44")
    			)
    			(pin no_connect line
    				(at 31.75 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "46")
    			)
    			(pin no_connect line
    				(at 31.75 -15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "47")
    			)
    			(pin no_connect line
    				(at 31.75 -17.78 0)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "48")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_mosaic_g5_p3"
        (property "Footprint" "PartReel:sparkfun_mosaic_g5_p3"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_mosaic_g5_p3/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Septentrio’s mosaic-G5 modules are low-power multi-band multi-constellation GNSSreceiver packaged in a 22.8x16.4 mm LGA module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun mosaic-G5 P3 LGA GNSS"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_mosaic_g5_p3/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 0.254)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -9.652 22.606 0)
    		)
    		(property "Value" "mosaic-G5_P3 (SparkFun)"
    			(at -3.302 -25.4 0)
    		)
    		(property "PROD_ID" "IC-26406"
    			(at 0 -34.036 0)
    		)
    		(property "ki_fp_filters" "LGA54_MOSAIC-MINI_SEP"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_mosaic_g5_p3_1_0"
    			(pin no_connect line
    				(at 29.21 20.32 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "8")
    			)
    			(pin no_connect line
    				(at 29.21 19.05 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "15")
    			)
    			(pin no_connect line
    				(at 29.21 17.78 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "16")
    			)
    			(pin no_connect line
    				(at 29.21 16.51 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "18")
    			)
    			(pin no_connect line
    				(at 29.21 15.24 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "19")
    			)
    			(pin no_connect line
    				(at 29.21 13.97 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "20")
    			)
    			(pin no_connect line
    				(at 29.21 12.7 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "22")
    			)
    			(pin no_connect line
    				(at 29.21 11.43 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "23")
    			)
    			(pin no_connect line
    				(at 29.21 10.16 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "24")
    			)
    			(pin no_connect line
    				(at 29.21 8.89 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "30")
    			)
    			(pin no_connect line
    				(at 29.21 7.62 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "31")
    			)
    			(pin no_connect line
    				(at 29.21 6.35 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "32")
    			)
    			(pin no_connect line
    				(at 29.21 5.08 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "33")
    			)
    			(pin no_connect line
    				(at 29.21 3.81 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "35")
    			)
    			(pin no_connect line
    				(at 29.21 2.54 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "36")
    			)
    			(pin no_connect line
    				(at 29.21 1.27 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "37")
    			)
    			(pin no_connect line
    				(at 29.21 0 180)
    				(length 2.54)
    				(hide yes)
    				(name "Reserved")
    				(number "38")
    			)
    		)
    		(symbol "sparkfun_mosaic_g5_p3_1_1"
    			(pin power_in line
    				(at -12.7 20.32 0)
    				(length 2.54)
    				(name "VDD_3V3")
    				(number "44")
    			)
    			(pin power_in line
    				(at -12.7 20.32 0)
    				(length 2.54)
    				(hide yes)
    				(name "VDD_3V3")
    				(number "45")
    			)
    			(pin input line
    				(at -12.7 17.78 0)
    				(length 2.54)
    				(name "~{RST_IN}")
    				(number "7")
    			)
    			(pin input line
    				(at -12.7 12.7 0)
    				(length 2.54)
    				(name "ANT_1")
    				(number "2")
    			)
    			(pin no_connect line
    				(at -12.7 10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "ANT_2")
    				(number "5")
    			)
    			(pin power_in line
    				(at -12.7 7.62 0)
    				(length 2.54)
    				(name "VANT")
    				(number "54")
    			)
    			(pin power_in line
    				(at -12.7 2.54 0)
    				(length 2.54)
    				(name "USB_VBUS")
    				(number "14")
    			)
    			(pin bidirectional line
    				(at -12.7 0 0)
    				(length 2.54)
    				(name "USB_DP")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at -12.7 -2.54 0)
    				(length 2.54)
    				(name "USB_DN")
    				(number "13")
    			)
    			(pin input line
    				(at -12.7 -7.62 0)
    				(length 2.54)
    				(name "REF_I")
    				(number "48")
    			)
    			(pin output line
    				(at -12.7 -10.16 0)
    				(length 2.54)
    				(name "REF_O")
    				(number "47")
    			)
    			(pin power_in line
    				(at -12.7 -15.24 0)
    				(length 2.54)
    				(name "VREF_I")
    				(number "50")
    			)
    			(pin power_out line
    				(at -12.7 -17.78 0)
    				(length 2.54)
    				(name "VREF_O")
    				(number "51")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "11")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "17")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "21")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "27")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "34")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "4")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "41")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "46")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "55")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "56")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "57")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "58")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "59")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "6")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "60")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "61")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "62")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "63")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "64")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "65")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "66")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "67")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "68")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "69")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "70")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "71")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "72")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "73")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "74")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "75")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "76")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "77")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "78")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "79")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "80")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "81")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "82")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "83")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "84")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "85")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "86")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "87")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "88")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "89")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "90")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "91")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "92")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "93")
    			)
    			(pin power_in line
    				(at -12.7 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "94")
    			)
    			(pin output line
    				(at 12.7 17.78 180)
    				(length 2.54)
    				(name "TXD1")
    				(number "10")
    			)
    			(pin input line
    				(at 12.7 15.24 180)
    				(length 2.54)
    				(name "RXD1")
    				(number "9")
    			)
    			(pin output line
    				(at 12.7 10.16 180)
    				(length 2.54)
    				(name "TXD2")
    				(number "25")
    			)
    			(pin input line
    				(at 12.7 7.62 180)
    				(length 2.54)
    				(name "RXD2")
    				(number "29")
    			)
    			(pin output line
    				(at 12.7 5.08 180)
    				(length 2.54)
    				(name "RTS2")
    				(number "26")
    			)
    			(pin input line
    				(at 12.7 2.54 180)
    				(length 2.54)
    				(name "CTS2")
    				(number "28")
    			)
    			(pin output line
    				(at 12.7 -2.54 180)
    				(length 2.54)
    				(name "PPS1")
    				(number "42")
    			)
    			(pin output line
    				(at 12.7 -5.08 180)
    				(length 2.54)
    				(name "PPS2")
    				(number "43")
    			)
    			(pin input line
    				(at 12.7 -10.16 180)
    				(length 2.54)
    				(name "EVENTA")
    				(number "39")
    			)
    			(pin input line
    				(at 12.7 -12.7 180)
    				(length 2.54)
    				(name "EVENTB")
    				(number "40")
    			)
    			(pin bidirectional line
    				(at 12.7 -17.78 180)
    				(length 2.54)
    				(name "GPIO1")
    				(number "52")
    			)
    			(pin bidirectional line
    				(at 12.7 -20.32 180)
    				(length 2.54)
    				(name "GPIO2")
    				(number "53")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_neo_d9s"
        (property "Footprint" "PartReel:sparkfun_neo_d9s"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/learn_tutorials/2/3/5/2/NEO-D9S-00B_DataSheet_UBX-18012996.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "u-blox GNSS Receiver L-Band."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun NEO-D9S GNSS correction service L band L-band"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_neo_d9s/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -10.16 20.32 0)
    		)
    		(property "Value" "NEO-D9S (SparkFun)"
    			(at -6.35 -20.32 0)
    		)
    		(property "PROD_ID" "IC-16579"
    			(at 0 -25.4 0)
    		)
    		(symbol "sparkfun_neo_d9s_1_0"
    			(pin input line
    				(at 13.97 -12.7 180)
    				(length 2.54)
    				(name "EXTINT")
    				(number "17")
    			)
    			(pin input line
    				(at 13.97 -15.24 180)
    				(length 2.54)
    				(name "D_SEL")
    				(number "2")
    			)
    			(pin input line
    				(at 13.97 -17.78 180)
    				(length 2.54)
    				(name "~{SAFEBOOT}")
    				(number "1")
    			)
    		)
    		(symbol "sparkfun_neo_d9s_1_1"
    			(pin power_in line
    				(at -13.97 17.78 0)
    				(length 2.54)
    				(name "VCC")
    				(number "23")
    			)
    			(pin power_in line
    				(at -13.97 15.24 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "22")
    			)
    			(pin input line
    				(at -13.97 10.16 0)
    				(length 2.54)
    				(name "RF_IN")
    				(number "11")
    			)
    			(pin power_out line
    				(at -13.97 7.62 0)
    				(length 2.54)
    				(name "VCC_RF")
    				(number "9")
    			)
    			(pin output line
    				(at -13.97 2.54 0)
    				(length 2.54)
    				(name "ANT_OFF")
    				(number "14")
    			)
    			(pin input line
    				(at -13.97 0 0)
    				(length 2.54)
    				(name "ANT_DETECT")
    				(number "15")
    			)
    			(pin output line
    				(at -13.97 -2.54 0)
    				(length 2.54)
    				(name "~{ANT_SHORT}")
    				(number "16")
    			)
    			(pin power_in line
    				(at -13.97 -7.62 0)
    				(length 2.54)
    				(name "V_USB")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at -13.97 -10.16 0)
    				(length 2.54)
    				(name "USB_D+")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(name "USB_D-")
    				(number "5")
    			)
    			(pin power_in line
    				(at -13.97 -17.78 0)
    				(length 2.54)
    				(name "GND")
    				(number "10")
    			)
    			(pin power_in line
    				(at -13.97 -17.78 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "12")
    			)
    			(pin power_in line
    				(at -13.97 -17.78 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "13")
    			)
    			(pin power_in line
    				(at -13.97 -17.78 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "24")
    			)
    			(pin input line
    				(at 13.97 17.78 180)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at 13.97 12.7 180)
    				(length 2.54)
    				(name "SDA/~{CS}")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at 13.97 10.16 180)
    				(length 2.54)
    				(name "SCL/SCK")
    				(number "19")
    			)
    			(pin output line
    				(at 13.97 5.08 180)
    				(length 2.54)
    				(name "TX2")
    				(number "3")
    			)
    			(pin input line
    				(at 13.97 2.54 180)
    				(length 2.54)
    				(name "RX2")
    				(number "4")
    			)
    			(pin output line
    				(at 13.97 -2.54 180)
    				(length 2.54)
    				(name "TX1/POCI")
    				(number "20")
    			)
    			(pin input line
    				(at 13.97 -5.08 180)
    				(length 2.54)
    				(name "RX1/PICO")
    				(number "21")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_neo_f10n"
        (property "Footprint" "PartReel:sparkfun_neo_f10n"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://content.u-blox.com/sites/default/files/documents/NEO-F10N_ProductSummary_UBX-22038758.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "NEO-F10N."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_neo_f10n/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -8.89 12.7 0)
    		)
    		(property "Value" "NEO-F10N (SparkFun)"
    			(at -5.08 -12.7 0)
    		)
    		(property "PROD_ID" "IC-20627"
    			(at 0 -19.05 0)
    		)
    		(symbol "sparkfun_neo_f10n_1_0"
    			(pin input line
    				(at 12.7 -5.08 180)
    				(length 2.54)
    				(name "~{SAFEBOOT}")
    				(number "1")
    			)
    			(pin input line
    				(at 12.7 -7.62 180)
    				(length 2.54)
    				(name "EXTINT")
    				(number "4")
    			)
    			(pin no_connect line
    				(at 30.48 7.62 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "5")
    			)
    			(pin no_connect line
    				(at 30.48 5.08 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "6")
    			)
    			(pin no_connect line
    				(at 30.48 2.54 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "7")
    			)
    			(pin no_connect line
    				(at 30.48 0 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "15")
    			)
    			(pin no_connect line
    				(at 30.48 -2.54 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "16")
    			)
    			(pin no_connect line
    				(at 30.48 -5.08 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "17")
    			)
    			(pin no_connect line
    				(at 30.48 -7.62 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "18")
    			)
    			(pin no_connect line
    				(at 30.48 -10.16 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "19")
    			)
    		)
    		(symbol "sparkfun_neo_f10n_1_1"
    			(pin power_in line
    				(at -12.7 10.16 0)
    				(length 2.54)
    				(name "VCC")
    				(number "23")
    			)
    			(pin power_in line
    				(at -12.7 7.62 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "22")
    			)
    			(pin input line
    				(at -12.7 5.08 0)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "8")
    			)
    			(pin input line
    				(at -12.7 0 0)
    				(length 2.54)
    				(name "RF_IN")
    				(number "11")
    			)
    			(pin power_out line
    				(at -12.7 -2.54 0)
    				(length 2.54)
    				(name "VCC_RF")
    				(number "9")
    			)
    			(pin output line
    				(at -12.7 -5.08 0)
    				(length 2.54)
    				(name "LNA_EN")
    				(number "14")
    			)
    			(pin power_in line
    				(at -12.7 -10.16 0)
    				(length 2.54)
    				(name "GND")
    				(number "10")
    			)
    			(pin power_in line
    				(at -12.7 -10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "12")
    			)
    			(pin power_in line
    				(at -12.7 -10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "13")
    			)
    			(pin power_in line
    				(at -12.7 -10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "24")
    			)
    			(pin output line
    				(at 12.7 10.16 180)
    				(length 2.54)
    				(name "TXD")
    				(number "20")
    			)
    			(pin input line
    				(at 12.7 7.62 180)
    				(length 2.54)
    				(name "RXD")
    				(number "21")
    			)
    			(pin output line
    				(at 12.7 -10.16 180)
    				(length 2.54)
    				(name "TIMEPULSE")
    				(number "3")
    			)
    			(pin no_connect line
    				(at 30.48 10.16 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_p23m"
        (property "Footprint" "PartReel:sparkfun_p23m"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/9/d/a/7/3/P23M_Datasheet_1.3.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Tri-band high percision RTK GNSS receiver with HAS capabilities."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun GNSS Receiver"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_p23m/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -8.89 13.97 0)
    		)
    		(property "Value" "P23M (SparkFun)"
    			(at 7.62 13.97 0)
    		)
    		(property "PROD_ID" "IC-28074"
    			(at 0 -16.51 0)
    		)
    		(symbol "sparkfun_p23m_1_0"
    			(pin output line
    				(at 12.7 6.35 180)
    				(length 2.54)
    				(name "TXD2")
    				(number "6")
    			)
    			(pin input line
    				(at 12.7 3.81 180)
    				(length 2.54)
    				(name "RXD2")
    				(number "7")
    			)
    			(pin output line
    				(at 12.7 1.27 180)
    				(length 2.54)
    				(name "TXD3")
    				(number "16")
    			)
    			(pin input line
    				(at 12.7 -1.27 180)
    				(length 2.54)
    				(name "RXD3")
    				(number "15")
    			)
    			(pin bidirectional line
    				(at 12.7 -3.81 180)
    				(length 2.54)
    				(name "SDA")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at 12.7 -6.35 180)
    				(length 2.54)
    				(name "SCL")
    				(number "19")
    			)
    			(pin input line
    				(at 12.7 -8.89 180)
    				(length 2.54)
    				(name "EXTINT")
    				(number "4")
    			)
    			(pin no_connect line
    				(at 21.59 7.62 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "1")
    			)
    			(pin no_connect line
    				(at 21.59 2.54 180)
    				(length 2.54)
    				(hide yes)
    				(name "PICO")
    				(number "17")
    			)
    			(pin no_connect line
    				(at 21.59 0 180)
    				(length 2.54)
    				(hide yes)
    				(name "POCI")
    				(number "5")
    			)
    		)
    		(symbol "sparkfun_p23m_1_1"
    			(pin power_in line
    				(at -12.7 11.43 0)
    				(length 2.54)
    				(name "VCC")
    				(number "23")
    			)
    			(pin power_in line
    				(at -12.7 8.89 0)
    				(length 2.54)
    				(name "VBAT")
    				(number "22")
    			)
    			(pin input line
    				(at -12.7 6.35 0)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "8")
    			)
    			(pin input line
    				(at -12.7 1.27 0)
    				(length 2.54)
    				(name "RF_IN")
    				(number "11")
    			)
    			(pin power_out line
    				(at -12.7 -1.27 0)
    				(length 2.54)
    				(name "VCC_RF")
    				(number "9")
    			)
    			(pin output line
    				(at -12.7 -3.81 0)
    				(length 2.54)
    				(name "RTK_STAT")
    				(number "14")
    			)
    			(pin power_in line
    				(at -12.7 -11.43 0)
    				(length 2.54)
    				(name "GND")
    				(number "10")
    			)
    			(pin power_in line
    				(at -12.7 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "12")
    			)
    			(pin power_in line
    				(at -12.7 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "13")
    			)
    			(pin power_in line
    				(at -12.7 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "24")
    			)
    			(pin power_in line
    				(at -12.7 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "25")
    			)
    			(pin output line
    				(at 12.7 11.43 180)
    				(length 2.54)
    				(name "TXD1")
    				(number "20")
    			)
    			(pin input line
    				(at 12.7 8.89 180)
    				(length 2.54)
    				(name "RXD1")
    				(number "21")
    			)
    			(pin output line
    				(at 12.7 -11.43 180)
    				(length 2.54)
    				(name "TIMEPULSE")
    				(number "3")
    			)
    			(pin no_connect line
    				(at 21.59 5.08 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESERVED")
    				(number "2")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_zed_f9p"
        (property "Footprint" "PartReel:sparkfun_zed_f9p"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/f/8/d/6/d/ZED-F9P-02B_DataSheet_UBX-21023276.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "u-blox Dual-Band RTK GNSS Receiver."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun u-blox ZED F9P RTK GNSS dual band"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_zed_f9p/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -10.16 25.4 0)
    		)
    		(property "Value" "ZED-F9P (SparkFun)"
    			(at -6.35 -25.4 0)
    		)
    		(property "PROD_ID" "IC-16923"
    			(at 0 -30.48 0)
    		)
    		(symbol "sparkfun_zed_f9p_1_0"
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "100")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "101")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "102")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "12")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "14")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "32")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "37")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "41")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "48")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "55")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "56")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "57")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "58")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "59")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "60")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "61")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "62")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "63")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "64")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "65")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "66")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "67")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "68")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "69")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "70")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "71")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "72")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "73")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "74")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "75")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "76")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "77")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "78")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "79")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "80")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "81")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "82")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "83")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "84")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "85")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "86")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "87")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "88")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "89")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "90")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "91")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "92")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "93")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "94")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "95")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "96")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "97")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "98")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "99")
    			)
    			(pin input line
    				(at 13.97 -17.78 180)
    				(length 2.54)
    				(name "EXTINT")
    				(number "51")
    			)
    			(pin input line
    				(at 13.97 -20.32 180)
    				(length 2.54)
    				(name "D_SEL")
    				(number "47")
    			)
    			(pin input line
    				(at 13.97 -22.86 180)
    				(length 2.54)
    				(name "~{SAFEBOOT}")
    				(number "50")
    			)
    			(pin no_connect line
    				(at 31.75 26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "8")
    			)
    			(pin no_connect line
    				(at 31.75 24.13 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "9")
    			)
    			(pin no_connect line
    				(at 31.75 21.59 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "10")
    			)
    			(pin no_connect line
    				(at 31.75 19.05 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "11")
    			)
    			(pin no_connect line
    				(at 31.75 16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "13")
    			)
    			(pin no_connect line
    				(at 31.75 13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "15")
    			)
    			(pin no_connect line
    				(at 31.75 11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "16")
    			)
    			(pin no_connect line
    				(at 31.75 8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "17")
    			)
    			(pin no_connect line
    				(at 31.75 6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "18")
    			)
    			(pin no_connect line
    				(at 31.75 3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "21")
    			)
    			(pin no_connect line
    				(at 31.75 1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "22")
    			)
    			(pin no_connect line
    				(at 31.75 -1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "23")
    			)
    			(pin no_connect line
    				(at 31.75 -3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "24")
    			)
    			(pin no_connect line
    				(at 31.75 -6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "25")
    			)
    			(pin no_connect line
    				(at 31.75 -8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "28")
    			)
    			(pin no_connect line
    				(at 31.75 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "29")
    			)
    			(pin no_connect line
    				(at 31.75 -13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "30")
    			)
    			(pin no_connect line
    				(at 31.75 -16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "31")
    			)
    			(pin no_connect line
    				(at 31.75 -19.05 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "35")
    			)
    			(pin no_connect line
    				(at 31.75 -21.59 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "52")
    			)
    			(pin no_connect line
    				(at 31.75 -24.13 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "54")
    			)
    		)
    		(symbol "sparkfun_zed_f9p_1_1"
    			(pin power_in line
    				(at -13.97 22.86 0)
    				(length 2.54)
    				(name "VCC")
    				(number "33")
    			)
    			(pin power_in line
    				(at -13.97 22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "VCC")
    				(number "34")
    			)
    			(pin power_in line
    				(at -13.97 20.32 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "36")
    			)
    			(pin input line
    				(at -13.97 12.7 0)
    				(length 2.54)
    				(name "RF_IN")
    				(number "2")
    			)
    			(pin power_out line
    				(at -13.97 10.16 0)
    				(length 2.54)
    				(name "VCC_RF")
    				(number "7")
    			)
    			(pin input line
    				(at -13.97 5.08 0)
    				(length 2.54)
    				(name "ANT_DETECT")
    				(number "4")
    			)
    			(pin output line
    				(at -13.97 2.54 0)
    				(length 2.54)
    				(name "ANT_OFF")
    				(number "5")
    			)
    			(pin output line
    				(at -13.97 0 0)
    				(length 2.54)
    				(name "~{ANT_SHORT}")
    				(number "6")
    			)
    			(pin power_in line
    				(at -13.97 -7.62 0)
    				(length 2.54)
    				(name "V_USB")
    				(number "38")
    			)
    			(pin bidirectional line
    				(at -13.97 -10.16 0)
    				(length 2.54)
    				(name "USB_D+")
    				(number "40")
    			)
    			(pin bidirectional line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(name "USB_D-")
    				(number "39")
    			)
    			(pin input line
    				(at 13.97 22.86 180)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "49")
    			)
    			(pin bidirectional line
    				(at 13.97 17.78 180)
    				(length 2.54)
    				(name "SDA/~{CS}")
    				(number "44")
    			)
    			(pin bidirectional line
    				(at 13.97 15.24 180)
    				(length 2.54)
    				(name "SCL/SCK")
    				(number "45")
    			)
    			(pin output line
    				(at 13.97 10.16 180)
    				(length 2.54)
    				(name "TX1/POCI")
    				(number "42")
    			)
    			(pin input line
    				(at 13.97 7.62 180)
    				(length 2.54)
    				(name "RX1/PICO")
    				(number "43")
    			)
    			(pin output line
    				(at 13.97 2.54 180)
    				(length 2.54)
    				(name "TX2")
    				(number "27")
    			)
    			(pin input line
    				(at 13.97 0 180)
    				(length 2.54)
    				(name "RX2")
    				(number "26")
    			)
    			(pin output line
    				(at 13.97 -5.08 180)
    				(length 2.54)
    				(name "TX_READY")
    				(number "46")
    			)
    			(pin output line
    				(at 13.97 -7.62 180)
    				(length 2.54)
    				(name "RTK_STAT")
    				(number "20")
    			)
    			(pin output line
    				(at 13.97 -10.16 180)
    				(length 2.54)
    				(name "GEO_STAT")
    				(number "19")
    			)
    			(pin output line
    				(at 13.97 -12.7 180)
    				(length 2.54)
    				(name "TIMEPULSE")
    				(number "53")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_zed_f9t"
        (property "Footprint" "PartReel:sparkfun_zed_f9t"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/7/a/e/d/3/ZED-F9T-00B_DataSheet_UBX-18053713.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "u-blox Dual-Band GNSS Timing Receiver."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun u-blox ZED F9T Disciplined Oscillator dual band"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_zed_f9t/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -10.16 25.4 0)
    		)
    		(property "Value" "ZED-F9T (SparkFun)"
    			(at -6.35 -25.4 0)
    		)
    		(property "PROD_ID" "IC-16292"
    			(at 0 -30.48 0)
    		)
    		(symbol "sparkfun_zed_f9t_1_0"
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "100")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "101")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "102")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "12")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "14")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "32")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "37")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "41")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "48")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "55")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "56")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "57")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "58")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "59")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "60")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "61")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "62")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "63")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "64")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "65")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "66")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "67")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "68")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "69")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "70")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "71")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "72")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "73")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "74")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "75")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "76")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "77")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "78")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "79")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "80")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "81")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "82")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "83")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "84")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "85")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "86")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "87")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "88")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "89")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "90")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "91")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "92")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "93")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "94")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "95")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "96")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "97")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "98")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "99")
    			)
    			(pin input line
    				(at 13.97 -15.24 180)
    				(length 2.54)
    				(name "EXTINT")
    				(number "51")
    			)
    			(pin input line
    				(at 13.97 -17.78 180)
    				(length 2.54)
    				(name "EXTINT2")
    				(number "52")
    			)
    			(pin input line
    				(at 13.97 -20.32 180)
    				(length 2.54)
    				(name "D_SEL")
    				(number "47")
    			)
    			(pin input line
    				(at 13.97 -22.86 180)
    				(length 2.54)
    				(name "~{SAFEBOOT}")
    				(number "50")
    			)
    		)
    		(symbol "sparkfun_zed_f9t_1_1"
    			(pin power_in line
    				(at -13.97 22.86 0)
    				(length 2.54)
    				(name "VCC")
    				(number "33")
    			)
    			(pin power_in line
    				(at -13.97 22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "VCC")
    				(number "34")
    			)
    			(pin power_in line
    				(at -13.97 20.32 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "36")
    			)
    			(pin input line
    				(at -13.97 12.7 0)
    				(length 2.54)
    				(name "RF_IN")
    				(number "2")
    			)
    			(pin power_out line
    				(at -13.97 10.16 0)
    				(length 2.54)
    				(name "VCC_RF")
    				(number "7")
    			)
    			(pin input line
    				(at -13.97 5.08 0)
    				(length 2.54)
    				(name "ANT_DETECT")
    				(number "4")
    			)
    			(pin output line
    				(at -13.97 2.54 0)
    				(length 2.54)
    				(name "ANT_OFF")
    				(number "5")
    			)
    			(pin output line
    				(at -13.97 0 0)
    				(length 2.54)
    				(name "~{ANT_SHORT}")
    				(number "6")
    			)
    			(pin power_in line
    				(at -13.97 -7.62 0)
    				(length 2.54)
    				(name "V_USB")
    				(number "38")
    			)
    			(pin bidirectional line
    				(at -13.97 -10.16 0)
    				(length 2.54)
    				(name "USB_D+")
    				(number "40")
    			)
    			(pin bidirectional line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(name "USB_D-")
    				(number "39")
    			)
    			(pin input line
    				(at 13.97 22.86 180)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "49")
    			)
    			(pin bidirectional line
    				(at 13.97 17.78 180)
    				(length 2.54)
    				(name "SDA/~{CS}")
    				(number "44")
    			)
    			(pin bidirectional line
    				(at 13.97 15.24 180)
    				(length 2.54)
    				(name "SCL/SCK")
    				(number "45")
    			)
    			(pin output line
    				(at 13.97 10.16 180)
    				(length 2.54)
    				(name "TX1/POCI")
    				(number "42")
    			)
    			(pin input line
    				(at 13.97 7.62 180)
    				(length 2.54)
    				(name "RX1/PICO")
    				(number "43")
    			)
    			(pin output line
    				(at 13.97 2.54 180)
    				(length 2.54)
    				(name "TX2")
    				(number "27")
    			)
    			(pin input line
    				(at 13.97 0 180)
    				(length 2.54)
    				(name "RX2")
    				(number "26")
    			)
    			(pin output line
    				(at 13.97 -5.08 180)
    				(length 2.54)
    				(name "TX_READY")
    				(number "46")
    			)
    			(pin output line
    				(at 13.97 -7.62 180)
    				(length 2.54)
    				(name "GEO_STAT")
    				(number "19")
    			)
    			(pin output line
    				(at 13.97 -10.16 180)
    				(length 2.54)
    				(name "TIMEPULSE")
    				(number "53")
    			)
    			(pin output line
    				(at 13.97 -12.7 180)
    				(length 2.54)
    				(name "TIMEPULSE2")
    				(number "54")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_zed_x20p"
        (property "Footprint" "PartReel:sparkfun_zed_x20p"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.u-blox.com/sites/default/files/documents/ZED-X20P_ProductSummary_UBXDOC-304424225-18238.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "u-blox All-Band RTK GNSS Receiver."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun u-blox ZED X20P RTK GNSS all band"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_zed_x20p/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -10.16 25.4 0)
    		)
    		(property "Value" "ZED-X20P (SparkFun)"
    			(at -6.35 -25.4 0)
    		)
    		(property "PROD_ID" "IC-26061"
    			(at 0 -30.48 0)
    		)
    		(symbol "sparkfun_zed_x20p_1_0"
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "100")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "101")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "102")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "12")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "14")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "32")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "37")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "41")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "48")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "55")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "56")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "57")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "58")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "59")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "60")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "61")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "62")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "63")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "64")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "65")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "66")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "67")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "68")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "69")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "70")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "71")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "72")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "73")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "74")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "75")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "76")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "77")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "78")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "79")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "80")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "81")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "82")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "83")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "84")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "85")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "86")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "87")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "88")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "89")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "90")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "91")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "92")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "93")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "94")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "95")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "96")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "97")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "98")
    			)
    			(pin power_in line
    				(at -13.97 -22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "99")
    			)
    			(pin input line
    				(at 13.97 -17.78 180)
    				(length 2.54)
    				(name "EXTINT")
    				(number "51")
    			)
    			(pin input line
    				(at 13.97 -20.32 180)
    				(length 2.54)
    				(name "D_SEL")
    				(number "47")
    			)
    			(pin input line
    				(at 13.97 -22.86 180)
    				(length 2.54)
    				(name "~{SAFEBOOT}")
    				(number "50")
    			)
    			(pin no_connect line
    				(at 33.02 24.13 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "8")
    			)
    			(pin no_connect line
    				(at 33.02 21.59 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "9")
    			)
    			(pin no_connect line
    				(at 33.02 19.05 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "10")
    			)
    			(pin no_connect line
    				(at 33.02 16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "11")
    			)
    			(pin no_connect line
    				(at 33.02 13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "13")
    			)
    			(pin no_connect line
    				(at 33.02 11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "15")
    			)
    			(pin no_connect line
    				(at 33.02 8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "16")
    			)
    			(pin no_connect line
    				(at 33.02 6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "17")
    			)
    			(pin no_connect line
    				(at 33.02 3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "18")
    			)
    			(pin no_connect line
    				(at 33.02 1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "21")
    			)
    			(pin no_connect line
    				(at 33.02 -1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "22")
    			)
    			(pin no_connect line
    				(at 33.02 -3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "23")
    			)
    			(pin no_connect line
    				(at 33.02 -6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "24")
    			)
    			(pin no_connect line
    				(at 33.02 -8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "25")
    			)
    			(pin no_connect line
    				(at 33.02 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "28")
    			)
    			(pin no_connect line
    				(at 33.02 -13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "29")
    			)
    			(pin no_connect line
    				(at 33.02 -16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "30")
    			)
    			(pin no_connect line
    				(at 33.02 -19.05 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "31")
    			)
    			(pin no_connect line
    				(at 33.02 -21.59 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "35")
    			)
    			(pin no_connect line
    				(at 33.02 -24.13 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "52")
    			)
    			(pin no_connect line
    				(at 33.02 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "54")
    			)
    		)
    		(symbol "sparkfun_zed_x20p_1_1"
    			(pin power_in line
    				(at -13.97 22.86 0)
    				(length 2.54)
    				(name "VCC")
    				(number "33")
    			)
    			(pin power_in line
    				(at -13.97 22.86 0)
    				(length 2.54)
    				(hide yes)
    				(name "VCC")
    				(number "34")
    			)
    			(pin power_in line
    				(at -13.97 20.32 0)
    				(length 2.54)
    				(name "V_BCKP")
    				(number "36")
    			)
    			(pin input line
    				(at -13.97 12.7 0)
    				(length 2.54)
    				(name "RF_IN")
    				(number "2")
    			)
    			(pin power_out line
    				(at -13.97 10.16 0)
    				(length 2.54)
    				(name "VCC_RF")
    				(number "7")
    			)
    			(pin input line
    				(at -13.97 5.08 0)
    				(length 2.54)
    				(name "ANT_DETECT")
    				(number "4")
    			)
    			(pin output line
    				(at -13.97 2.54 0)
    				(length 2.54)
    				(name "ANT_OFF")
    				(number "5")
    			)
    			(pin output line
    				(at -13.97 0 0)
    				(length 2.54)
    				(name "~{ANT_SHORT}")
    				(number "6")
    			)
    			(pin power_in line
    				(at -13.97 -7.62 0)
    				(length 2.54)
    				(name "V_USB")
    				(number "38")
    			)
    			(pin bidirectional line
    				(at -13.97 -10.16 0)
    				(length 2.54)
    				(name "USB_D+")
    				(number "40")
    			)
    			(pin bidirectional line
    				(at -13.97 -12.7 0)
    				(length 2.54)
    				(name "USB_D-")
    				(number "39")
    			)
    			(pin input line
    				(at 13.97 22.86 180)
    				(length 2.54)
    				(name "~{RESET}")
    				(number "49")
    			)
    			(pin bidirectional line
    				(at 13.97 17.78 180)
    				(length 2.54)
    				(name "SDA/~{CS}")
    				(number "44")
    			)
    			(pin bidirectional line
    				(at 13.97 15.24 180)
    				(length 2.54)
    				(name "SCL/SCK")
    				(number "45")
    			)
    			(pin output line
    				(at 13.97 10.16 180)
    				(length 2.54)
    				(name "TX1/POCI")
    				(number "42")
    			)
    			(pin input line
    				(at 13.97 7.62 180)
    				(length 2.54)
    				(name "RX1/PICO")
    				(number "43")
    			)
    			(pin output line
    				(at 13.97 2.54 180)
    				(length 2.54)
    				(name "TX2")
    				(number "27")
    			)
    			(pin input line
    				(at 13.97 0 180)
    				(length 2.54)
    				(name "RX2")
    				(number "26")
    			)
    			(pin output line
    				(at 13.97 -5.08 180)
    				(length 2.54)
    				(name "TX_READY")
    				(number "46")
    			)
    			(pin output line
    				(at 13.97 -7.62 180)
    				(length 2.54)
    				(name "RTK_STAT")
    				(number "20")
    			)
    			(pin output line
    				(at 13.97 -10.16 180)
    				(length 2.54)
    				(name "GEO_STAT")
    				(number "19")
    			)
    			(pin output line
    				(at 13.97 -12.7 180)
    				(length 2.54)
    				(name "TIMEPULSE")
    				(number "53")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_esp32_c5_wroom_1"
        (property "Footprint" "PartReel:sparkfun_esp32_c5_wroom_1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://documentation.espressif.com/esp32-c5-wroom-1_wroom-1u_datasheet_en.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Dual-band 2.4GHz and 5GHz WiFi, BLE, Zigbee, and Thread ESP32 Module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun ESP32 C6 WROOM 2.4GHz 5GHz WiFi BLE"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_esp32_c5_wroom_1/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 31.75 0)
    		)
    		(property "Value" "ESP32-C5-WROOM-1 (SparkFun)"
    			(at 0 29.21 0)
    		)
    		(property "PROD_ID" "IC-27645"
    			(at -1.27 -36.83 0)
    		)
    		(symbol "sparkfun_esp32_c5_wroom_1_0_1")
    		(symbol "sparkfun_esp32_c5_wroom_1_1_1"
    			(text "IO15 can't be\nused if module\nhas PSRAM."
    				(at 1.905 -12.065 0)
    			)
    			(text "Caution!\nIO27 and IO28\nset boot mode,\nsee datasheet."
    				(at 1.905 -25.4 0)
    			)
    			(pin power_in line
    				(at -13.97 26.67 0)
    				(length 2.54)
    				(name "3V3")
    				(number "2")
    			)
    			(pin input line
    				(at -13.97 16.51 0)
    				(length 2.54)
    				(name "EN")
    				(number "3")
    			)
    			(pin no_connect line
    				(at -13.97 -21.59 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "20")
    			)
    			(pin no_connect line
    				(at -13.97 -24.13 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "22")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "28")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "EPAD")
    			)
    			(pin bidirectional line
    				(at 13.97 26.67 180)
    				(length 2.54)
    				(name "XTAL_32K_P/IO0")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 13.97 24.13 180)
    				(length 2.54)
    				(name "XTAL_32K_N/IOA1")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 13.97 21.59 180)
    				(length 2.54)
    				(name "MTMS/IOA2")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at 13.97 19.05 180)
    				(length 2.54)
    				(name "MTDI/IOA3")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 13.97 16.51 180)
    				(length 2.54)
    				(name "MTCK/IOA4")
    				(number "17")
    			)
    			(pin bidirectional line
    				(at 13.97 13.97 180)
    				(length 2.54)
    				(name "MTDO/IOA5")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at 13.97 11.43 180)
    				(length 2.54)
    				(name "IOA6")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at 13.97 8.89 180)
    				(length 2.54)
    				(name "IO7")
    				(number "9")
    			)
    			(pin bidirectional line
    				(at 13.97 6.35 180)
    				(length 2.54)
    				(name "IO8")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at 13.97 3.81 180)
    				(length 2.54)
    				(name "IO9")
    				(number "11")
    			)
    			(pin bidirectional line
    				(at 13.97 1.27 180)
    				(length 2.54)
    				(name "IO10")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at 13.97 -1.27 180)
    				(length 2.54)
    				(name "UART0_TX/IO11")
    				(number "25")
    			)
    			(pin bidirectional line
    				(at 13.97 -3.81 180)
    				(length 2.54)
    				(name "UART0_RX/IO12")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 13.97 -6.35 180)
    				(length 2.54)
    				(name "USB_DN/IO13")
    				(number "13")
    			)
    			(pin bidirectional line
    				(at 13.97 -8.89 180)
    				(length 2.54)
    				(name "USB_DP/IO14")
    				(number "14")
    			)
    			(pin bidirectional line
    				(at 13.97 -11.43 180)
    				(length 2.54)
    				(name "IO15")
    				(number "19")
    			)
    			(pin bidirectional line
    				(at 13.97 -13.97 180)
    				(length 2.54)
    				(name "IO23")
    				(number "21")
    			)
    			(pin bidirectional line
    				(at 13.97 -16.51 180)
    				(length 2.54)
    				(name "IO24")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 13.97 -19.05 180)
    				(length 2.54)
    				(name "IO25")
    				(number "26")
    			)
    			(pin bidirectional line
    				(at 13.97 -21.59 180)
    				(length 2.54)
    				(name "IO26")
    				(number "27")
    			)
    			(pin bidirectional line
    				(at 13.97 -24.13 180)
    				(length 2.54)
    				(name "IO27")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at 13.97 -26.67 180)
    				(length 2.54)
    				(name "IO28")
    				(number "15")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_esp32_c5_wroom_1_narrow"
        (property "Footprint" "PartReel:sparkfun_esp32_c5_wroom_1_narrow"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://documentation.espressif.com/esp32-c5-wroom-1_wroom-1u_datasheet_en.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Dual-band 2.4GHz and 5GHz WiFi, BLE, Zigbee, and Thread ESP32 Module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun ESP32 C6 WROOM 2.4GHz 5GHz WiFi BLE"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_esp32_c5_wroom_1_narrow/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 31.75 0)
    		)
    		(property "Value" "ESP32-C5-WROOM-1-NARROW (SparkFun)"
    			(at 0 29.21 0)
    		)
    		(property "PROD_ID" "IC-27645"
    			(at -1.27 -36.83 0)
    		)
    		(symbol "sparkfun_esp32_c5_wroom_1_narrow_0_1")
    		(symbol "sparkfun_esp32_c5_wroom_1_narrow_1_1"
    			(text "IO15 can't be\nused if module\nhas PSRAM."
    				(at 1.905 -12.065 0)
    			)
    			(text "Caution!\nIO27 and IO28\nset boot mode,\nsee datasheet."
    				(at 1.905 -25.4 0)
    			)
    			(pin power_in line
    				(at -13.97 26.67 0)
    				(length 2.54)
    				(name "3V3")
    				(number "2")
    			)
    			(pin input line
    				(at -13.97 16.51 0)
    				(length 2.54)
    				(name "EN")
    				(number "3")
    			)
    			(pin no_connect line
    				(at -13.97 -21.59 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "20")
    			)
    			(pin no_connect line
    				(at -13.97 -24.13 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "22")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "28")
    			)
    			(pin power_in line
    				(at -13.97 -26.67 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "EPAD")
    			)
    			(pin bidirectional line
    				(at 13.97 26.67 180)
    				(length 2.54)
    				(name "XTAL_32K_P/IO0")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 13.97 24.13 180)
    				(length 2.54)
    				(name "XTAL_32K_N/IOA1")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 13.97 21.59 180)
    				(length 2.54)
    				(name "MTMS/IOA2")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at 13.97 19.05 180)
    				(length 2.54)
    				(name "MTDI/IOA3")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 13.97 16.51 180)
    				(length 2.54)
    				(name "MTCK/IOA4")
    				(number "17")
    			)
    			(pin bidirectional line
    				(at 13.97 13.97 180)
    				(length 2.54)
    				(name "MTDO/IOA5")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at 13.97 11.43 180)
    				(length 2.54)
    				(name "IOA6")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at 13.97 8.89 180)
    				(length 2.54)
    				(name "IO7")
    				(number "9")
    			)
    			(pin bidirectional line
    				(at 13.97 6.35 180)
    				(length 2.54)
    				(name "IO8")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at 13.97 3.81 180)
    				(length 2.54)
    				(name "IO9")
    				(number "11")
    			)
    			(pin bidirectional line
    				(at 13.97 1.27 180)
    				(length 2.54)
    				(name "IO10")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at 13.97 -1.27 180)
    				(length 2.54)
    				(name "UART0_TX/IO11")
    				(number "25")
    			)
    			(pin bidirectional line
    				(at 13.97 -3.81 180)
    				(length 2.54)
    				(name "UART0_RX/IO12")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 13.97 -6.35 180)
    				(length 2.54)
    				(name "USB_DN/IO13")
    				(number "13")
    			)
    			(pin bidirectional line
    				(at 13.97 -8.89 180)
    				(length 2.54)
    				(name "USB_DP/IO14")
    				(number "14")
    			)
    			(pin bidirectional line
    				(at 13.97 -11.43 180)
    				(length 2.54)
    				(name "IO15")
    				(number "19")
    			)
    			(pin bidirectional line
    				(at 13.97 -13.97 180)
    				(length 2.54)
    				(name "IO23")
    				(number "21")
    			)
    			(pin bidirectional line
    				(at 13.97 -16.51 180)
    				(length 2.54)
    				(name "IO24")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 13.97 -19.05 180)
    				(length 2.54)
    				(name "IO25")
    				(number "26")
    			)
    			(pin bidirectional line
    				(at 13.97 -21.59 180)
    				(length 2.54)
    				(name "IO26")
    				(number "27")
    			)
    			(pin bidirectional line
    				(at 13.97 -24.13 180)
    				(length 2.54)
    				(name "IO27")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at 13.97 -26.67 180)
    				(length 2.54)
    				(name "IO28")
    				(number "15")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_esp32_pico_v3_02"
        (property "Footprint" "PartReel:sparkfun_esp32_pico_v3_02"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-pico-mini-02_datasheet_en.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ESP32 Small Formfactor."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun RF Radio BT ESP ESP32 Espressif onboard"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_esp32_pico_v3_02/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -12.7 33.02 0)
    		)
    		(property "Value" "ESP32-PICO-V3-02 (SparkFun)"
    			(at 1.27 33.02 0)
    		)
    		(property "PROD_ID" "IC-19692"
    			(at -1.27 -59.69 0)
    		)
    		(property "ki_fp_filters" "ESP32?WROOM?32*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_esp32_pico_v3_02_1_1"
    			(text "Boot\nControl"
    				(at 2.54 19.05 900)
    			)
    			(pin input line
    				(at -15.24 29.21 0)
    				(length 2.54)
    				(name "EN")
    				(number "8")
    			)
    			(pin no_connect line
    				(at -12.7 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "25")
    			)
    			(pin no_connect line
    				(at -12.7 -13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "32")
    			)
    			(pin power_in line
    				(at 0 34.29 270)
    				(length 2.54)
    				(name "VDD")
    				(number "3")
    			)
    			(pin power_in line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "11")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "14")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "2")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "36")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "37")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "38")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "39")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "40")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "41")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "42")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "43")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "44")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "45")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "46")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "47")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "48")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.1")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.2")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.3")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.4")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.5")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.6")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.7")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.8")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.9")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "50")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "51")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "52")
    			)
    			(pin passive line
    				(at 0 -41.91 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "53")
    			)
    			(pin bidirectional line
    				(at 15.24 30.48 180)
    				(length 2.54)
    				(name "TXD0/IO1")
    				(number "31")
    			)
    			(pin bidirectional line
    				(at 15.24 27.94 180)
    				(length 2.54)
    				(name "RXD0/IO3")
    				(number "30")
    			)
    			(pin bidirectional line
    				(at 15.24 24.13 180)
    				(length 2.54)
    				(name "IOA0")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 15.24 21.59 180)
    				(length 2.54)
    				(name "IOA2")
    				(number "22")
    			)
    			(pin bidirectional line
    				(at 15.24 19.05 180)
    				(length 2.54)
    				(name "IO5")
    				(number "29")
    			)
    			(pin bidirectional line
    				(at 15.24 16.51 180)
    				(length 2.54)
    				(name "IOA12")
    				(number "19")
    			)
    			(pin bidirectional line
    				(at 15.24 13.97 180)
    				(length 2.54)
    				(name "IOA15")
    				(number "21")
    			)
    			(pin bidirectional line
    				(at 15.24 10.16 180)
    				(length 2.54)
    				(name "IOA4")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 15.24 7.62 180)
    				(length 2.54)
    				(name "IO7")
    				(number "27")
    			)
    			(pin bidirectional line
    				(at 15.24 5.08 180)
    				(length 2.54)
    				(name "IO8")
    				(number "28")
    			)
    			(pin bidirectional line
    				(at 15.24 2.54 180)
    				(length 2.54)
    				(name "IOA13")
    				(number "20")
    			)
    			(pin bidirectional line
    				(at 15.24 0 180)
    				(length 2.54)
    				(name "IOA14")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at 15.24 -2.54 180)
    				(length 2.54)
    				(name "IO19")
    				(number "33")
    			)
    			(pin bidirectional line
    				(at 15.24 -5.08 180)
    				(length 2.54)
    				(name "IO20")
    				(number "26")
    			)
    			(pin bidirectional line
    				(at 15.24 -7.62 180)
    				(length 2.54)
    				(name "IO21")
    				(number "35")
    			)
    			(pin bidirectional line
    				(at 15.24 -10.16 180)
    				(length 2.54)
    				(name "IO22")
    				(number "34")
    			)
    			(pin bidirectional line
    				(at 15.24 -12.7 180)
    				(length 2.54)
    				(name "IOA25")
    				(number "15")
    			)
    			(pin bidirectional line
    				(at 15.24 -15.24 180)
    				(length 2.54)
    				(name "IOA26")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at 15.24 -17.78 180)
    				(length 2.54)
    				(name "IOA27")
    				(number "17")
    			)
    			(pin bidirectional line
    				(at 15.24 -20.32 180)
    				(length 2.54)
    				(name "IOA32")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at 15.24 -22.86 180)
    				(length 2.54)
    				(name "IOA33")
    				(number "13")
    			)
    			(pin input line
    				(at 15.24 -25.4 180)
    				(length 2.54)
    				(name "IA34")
    				(number "9")
    			)
    			(pin input line
    				(at 15.24 -27.94 180)
    				(length 2.54)
    				(name "IA35")
    				(number "10")
    			)
    			(pin input line
    				(at 15.24 -30.48 180)
    				(length 2.54)
    				(name "IA36")
    				(number "4")
    			)
    			(pin input line
    				(at 15.24 -33.02 180)
    				(length 2.54)
    				(name "IA37")
    				(number "5")
    			)
    			(pin input line
    				(at 15.24 -35.56 180)
    				(length 2.54)
    				(name "IA38")
    				(number "6")
    			)
    			(pin input line
    				(at 15.24 -38.1 180)
    				(length 2.54)
    				(name "IA39")
    				(number "7")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_esp32_s3_mini"
        (property "Footprint" "PartReel:sparkfun_esp32_s3_mini"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3-mini-1_mini-1u_datasheet_en.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ESP32-S3-MINI."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun RF Radio Bluetooth BT ESP ESP32 Espressif"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_esp32_s3_mini/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -12.7 48.26 0)
    		)
    		(property "Value" "ESP32-S3-MINI (SparkFun)"
    			(at 1.27 48.26 0)
    		)
    		(property "PROD_ID" "IC-20979"
    			(at 0 -72.39 0)
    		)
    		(property "ki_fp_filters" "ESP32?WROOM?32*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_esp32_s3_mini_1_1"
    			(text "Boot\nControl"
    				(at 2.54 35.56 900)
    			)
    			(pin input line
    				(at -15.24 44.45 0)
    				(length 2.54)
    				(name "EN")
    				(number "45")
    			)
    			(pin power_in line
    				(at 0 49.53 270)
    				(length 2.54)
    				(name "3V3")
    				(number "3")
    			)
    			(pin power_in line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "2")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "42")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "43")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "46")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "47")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "48")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "50")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "51")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "52")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "53")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "54")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "55")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "56")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "57")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "58")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "59")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "60")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "61")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "62")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "63")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "64")
    			)
    			(pin passive line
    				(at 0 -57.15 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "65")
    			)
    			(pin bidirectional line
    				(at 15.24 45.72 180)
    				(length 2.54)
    				(name "TXD0/IO43")
    				(number "39")
    			)
    			(pin bidirectional line
    				(at 15.24 43.18 180)
    				(length 2.54)
    				(name "RXD0/IO44")
    				(number "40")
    			)
    			(pin bidirectional line
    				(at 15.24 39.37 180)
    				(length 2.54)
    				(name "IO0")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at 15.24 36.83 180)
    				(length 2.54)
    				(name "IOA3")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 15.24 34.29 180)
    				(length 2.54)
    				(name "IO45")
    				(number "41")
    			)
    			(pin bidirectional line
    				(at 15.24 31.75 180)
    				(length 2.54)
    				(name "IO46")
    				(number "44")
    			)
    			(pin bidirectional line
    				(at 15.24 27.94 180)
    				(length 2.54)
    				(name "IOA1")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 15.24 25.4 180)
    				(length 2.54)
    				(name "IOA2")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 15.24 22.86 180)
    				(length 2.54)
    				(name "IOA4")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at 15.24 20.32 180)
    				(length 2.54)
    				(name "IOA5")
    				(number "9")
    			)
    			(pin bidirectional line
    				(at 15.24 17.78 180)
    				(length 2.54)
    				(name "IOA6")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at 15.24 15.24 180)
    				(length 2.54)
    				(name "IOA7")
    				(number "11")
    			)
    			(pin bidirectional line
    				(at 15.24 12.7 180)
    				(length 2.54)
    				(name "IOA8")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at 15.24 10.16 180)
    				(length 2.54)
    				(name "IOA9")
    				(number "13")
    			)
    			(pin bidirectional line
    				(at 15.24 7.62 180)
    				(length 2.54)
    				(name "IOA10")
    				(number "14")
    			)
    			(pin bidirectional line
    				(at 15.24 5.08 180)
    				(length 2.54)
    				(name "IOA11")
    				(number "15")
    			)
    			(pin bidirectional line
    				(at 15.24 2.54 180)
    				(length 2.54)
    				(name "IOA12")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at 15.24 0 180)
    				(length 2.54)
    				(name "IOA13")
    				(number "17")
    			)
    			(pin bidirectional line
    				(at 15.24 -2.54 180)
    				(length 2.54)
    				(name "IOA14")
    				(number "18")
    			)
    			(pin bidirectional line
    				(at 15.24 -5.08 180)
    				(length 2.54)
    				(name "IOA15")
    				(number "19")
    			)
    			(pin bidirectional line
    				(at 15.24 -7.62 180)
    				(length 2.54)
    				(name "IOA16")
    				(number "20")
    			)
    			(pin bidirectional line
    				(at 15.24 -10.16 180)
    				(length 2.54)
    				(name "IOA17")
    				(number "21")
    			)
    			(pin bidirectional line
    				(at 15.24 -12.7 180)
    				(length 2.54)
    				(name "IOA18")
    				(number "22")
    			)
    			(pin bidirectional line
    				(at 15.24 -15.24 180)
    				(length 2.54)
    				(name "IOA19")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 15.24 -17.78 180)
    				(length 2.54)
    				(name "IOA20")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 15.24 -20.32 180)
    				(length 2.54)
    				(name "IO21")
    				(number "25")
    			)
    			(pin no_connect line
    				(at 15.24 -22.86 180)
    				(length 2.54)
    				(name "IO26")
    				(number "26")
    			)
    			(pin bidirectional line
    				(at 15.24 -25.4 180)
    				(length 2.54)
    				(name "IO33")
    				(number "28")
    			)
    			(pin bidirectional line
    				(at 15.24 -27.94 180)
    				(length 2.54)
    				(name "IO34")
    				(number "29")
    			)
    			(pin bidirectional line
    				(at 15.24 -30.48 180)
    				(length 2.54)
    				(name "IO35")
    				(number "31")
    			)
    			(pin bidirectional line
    				(at 15.24 -33.02 180)
    				(length 2.54)
    				(name "IO36")
    				(number "32")
    			)
    			(pin bidirectional line
    				(at 15.24 -35.56 180)
    				(length 2.54)
    				(name "IO37")
    				(number "33")
    			)
    			(pin bidirectional line
    				(at 15.24 -38.1 180)
    				(length 2.54)
    				(name "IO38")
    				(number "34")
    			)
    			(pin bidirectional line
    				(at 15.24 -40.64 180)
    				(length 2.54)
    				(name "IO39")
    				(number "35")
    			)
    			(pin bidirectional line
    				(at 15.24 -43.18 180)
    				(length 2.54)
    				(name "IO40")
    				(number "36")
    			)
    			(pin bidirectional line
    				(at 15.24 -45.72 180)
    				(length 2.54)
    				(name "IO41")
    				(number "37")
    			)
    			(pin bidirectional line
    				(at 15.24 -48.26 180)
    				(length 2.54)
    				(name "IO42")
    				(number "38")
    			)
    			(pin bidirectional line
    				(at 15.24 -50.8 180)
    				(length 2.54)
    				(name "IO47")
    				(number "27")
    			)
    			(pin bidirectional line
    				(at 15.24 -53.34 180)
    				(length 2.54)
    				(name "IO48")
    				(number "30")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_esp32_wroom"
        (property "Footprint" "PartReel:sparkfun_esp32_wroom"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.mouser.com/datasheet/2/891/esp32_wroom_32e_esp32_wroom_32ue_datasheet_en-1855879.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ESP32-WROOM."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun RF Radio Bluetooth BT ESP ESP32 Espressif"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_esp32_wroom/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -12.7 33.02 0)
    		)
    		(property "Value" "ESP32-WROOM (SparkFun)"
    			(at 1.27 33.02 0)
    		)
    		(property "PROD_ID" "IC-15676"
    			(at -1.27 -57.15 0)
    		)
    		(property "ki_fp_filters" "ESP32?WROOM?32*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_esp32_wroom_1_1"
    			(text "Boot\nControl"
    				(at 2.54 19.05 900)
    			)
    			(pin input line
    				(at -15.24 29.21 0)
    				(length 2.54)
    				(name "EN")
    				(number "3")
    			)
    			(pin no_connect line
    				(at -12.7 1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "17")
    			)
    			(pin no_connect line
    				(at -12.7 -1.27 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "18")
    			)
    			(pin no_connect line
    				(at -12.7 -3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "19")
    			)
    			(pin no_connect line
    				(at -12.7 -6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "20")
    			)
    			(pin no_connect line
    				(at -12.7 -8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "21")
    			)
    			(pin no_connect line
    				(at -12.7 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "22")
    			)
    			(pin no_connect line
    				(at -12.7 -13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "32")
    			)
    			(pin power_in line
    				(at 0 34.29 270)
    				(length 2.54)
    				(name "VDD")
    				(number "2")
    			)
    			(pin power_in line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "15")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "38")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.1")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.2")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.3")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.4")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.5")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.6")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.7")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.8")
    			)
    			(pin passive line
    				(at 0 -39.37 90)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "49.9")
    			)
    			(pin bidirectional line
    				(at 15.24 30.48 180)
    				(length 2.54)
    				(name "TXD0/IO1")
    				(number "35")
    			)
    			(pin bidirectional line
    				(at 15.24 27.94 180)
    				(length 2.54)
    				(name "RXD0/IO3")
    				(number "34")
    			)
    			(pin bidirectional line
    				(at 15.24 24.13 180)
    				(length 2.54)
    				(name "IOA0")
    				(number "25")
    			)
    			(pin bidirectional line
    				(at 15.24 21.59 180)
    				(length 2.54)
    				(name "IOA2")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 15.24 19.05 180)
    				(length 2.54)
    				(name "IO5")
    				(number "29")
    			)
    			(pin bidirectional line
    				(at 15.24 16.51 180)
    				(length 2.54)
    				(name "IOA12")
    				(number "14")
    			)
    			(pin bidirectional line
    				(at 15.24 13.97 180)
    				(length 2.54)
    				(name "IOA15")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 15.24 10.16 180)
    				(length 2.54)
    				(name "IOA4")
    				(number "26")
    			)
    			(pin bidirectional line
    				(at 15.24 7.62 180)
    				(length 2.54)
    				(name "IOA13")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at 15.24 5.08 180)
    				(length 2.54)
    				(name "IOA14")
    				(number "13")
    			)
    			(pin bidirectional line
    				(at 15.24 2.54 180)
    				(length 2.54)
    				(name "IO16")
    				(number "27")
    			)
    			(pin bidirectional line
    				(at 15.24 0 180)
    				(length 2.54)
    				(name "IO17")
    				(number "28")
    			)
    			(pin bidirectional line
    				(at 15.24 -2.54 180)
    				(length 2.54)
    				(name "IO19")
    				(number "31")
    			)
    			(pin bidirectional line
    				(at 15.24 -5.08 180)
    				(length 2.54)
    				(name "IO18")
    				(number "30")
    			)
    			(pin bidirectional line
    				(at 15.24 -7.62 180)
    				(length 2.54)
    				(name "IO21")
    				(number "33")
    			)
    			(pin bidirectional line
    				(at 15.24 -10.16 180)
    				(length 2.54)
    				(name "IO22")
    				(number "36")
    			)
    			(pin bidirectional line
    				(at 15.24 -12.7 180)
    				(length 2.54)
    				(name "IO23")
    				(number "37")
    			)
    			(pin bidirectional line
    				(at 15.24 -15.24 180)
    				(length 2.54)
    				(name "IOA25")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at 15.24 -17.78 180)
    				(length 2.54)
    				(name "IOA26")
    				(number "11")
    			)
    			(pin bidirectional line
    				(at 15.24 -20.32 180)
    				(length 2.54)
    				(name "IOA27")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at 15.24 -22.86 180)
    				(length 2.54)
    				(name "IOA32")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at 15.24 -25.4 180)
    				(length 2.54)
    				(name "IOA33")
    				(number "9")
    			)
    			(pin input line
    				(at 15.24 -27.94 180)
    				(length 2.54)
    				(name "IA34")
    				(number "6")
    			)
    			(pin input line
    				(at 15.24 -30.48 180)
    				(length 2.54)
    				(name "IA35")
    				(number "7")
    			)
    			(pin input line
    				(at 15.24 -33.02 180)
    				(length 2.54)
    				(name "IA36")
    				(number "4")
    			)
    			(pin input line
    				(at 15.24 -35.56 180)
    				(length 2.54)
    				(name "IA39")
    				(number "5")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_power_divider_bp2g1"
        (property "Footprint" "PartReel:sparkfun_power_divider_bp2g1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.minicircuits.com/pdfs/BP2G1+.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "RF Antenna Splitter."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun 2 Ways MMIC DC Pass Power Splitter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_power_divider_bp2g1/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -7.62 5.08 0)
    		)
    		(property "Value" "Power_Divider_BP2G1+ (SparkFun)"
    			(at -6.35 -5.08 0)
    		)
    		(property "PROD_ID" "IC-17198"
    			(at 0 -12.7 0)
    		)
    		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_power_divider_bp2g1_0_1")
    		(symbol "sparkfun_power_divider_bp2g1_1_1"
    			(pin input line
    				(at -10.16 2.54 0)
    				(length 2.54)
    				(name "INPUT")
    				(number "2")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "4")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "6")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "7")
    			)
    			(pin output line
    				(at 11.43 2.54 180)
    				(length 2.54)
    				(name "OUTPUT1")
    				(number "8")
    			)
    			(pin output line
    				(at 11.43 -2.54 180)
    				(length 2.54)
    				(name "OUTPUT2")
    				(number "5")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_power_divider_bp2g1_bypass1"
        (property "Footprint" "PartReel:sparkfun_power_divider_bp2g1_bypass1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.minicircuits.com/pdfs/BP2G1+.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "RF Antenna Splitter."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun 2 Ways MMIC DC Pass Power Splitter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_power_divider_bp2g1_bypass1/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -7.62 5.08 0)
    		)
    		(property "Value" "Power_Divider_BP2G1+_Bypass1 (SparkFun)"
    			(at -6.35 -5.08 0)
    		)
    		(property "PROD_ID" "IC-17198"
    			(at 0 -12.7 0)
    		)
    		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_power_divider_bp2g1_bypass1_0_1")
    		(symbol "sparkfun_power_divider_bp2g1_bypass1_1_1"
    			(pin input line
    				(at -10.16 2.54 0)
    				(length 2.54)
    				(name "INPUT")
    				(number "2")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "4")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "6")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "7")
    			)
    			(pin output line
    				(at 11.43 2.54 180)
    				(length 2.54)
    				(name "OUTPUT1")
    				(number "8")
    			)
    			(pin output line
    				(at 11.43 -2.54 180)
    				(length 2.54)
    				(name "OUTPUT2")
    				(number "5")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_power_divider_bp2g1_bypass2"
        (property "Footprint" "PartReel:sparkfun_power_divider_bp2g1_bypass2"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.minicircuits.com/pdfs/BP2G1+.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "RF Antenna Splitter."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun 2 Ways MMIC DC Pass Power Splitter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_power_divider_bp2g1_bypass2/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -7.62 5.08 0)
    		)
    		(property "Value" "Power_Divider_BP2G1+_Bypass2 (SparkFun)"
    			(at -6.35 -5.08 0)
    		)
    		(property "PROD_ID" "IC-17198"
    			(at 0 -12.7 0)
    		)
    		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_power_divider_bp2g1_bypass2_0_1")
    		(symbol "sparkfun_power_divider_bp2g1_bypass2_1_1"
    			(pin input line
    				(at -10.16 2.54 0)
    				(length 2.54)
    				(name "INPUT")
    				(number "2")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "4")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "6")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "7")
    			)
    			(pin output line
    				(at 11.43 2.54 180)
    				(length 2.54)
    				(name "OUTPUT1")
    				(number "8")
    			)
    			(pin output line
    				(at 11.43 -2.54 180)
    				(length 2.54)
    				(name "OUTPUT2")
    				(number "5")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_power_splitter_jps_3_1"
        (property "Footprint" "PartReel:sparkfun_power_splitter_jps_3_1"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.minicircuits.com/pdfs/JPS-3-1+.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Power splitter / combiner 3-Way 50Ohm 5 to 300MHz."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun power splitter combiner"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_power_splitter_jps_3_1/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -5.715 5.08 0)
    		)
    		(property "Value" "Power_Splitter_JPS-3-1+ (SparkFun)"
    			(at 0 -5.08 0)
    		)
    		(property "PROD_ID" "COMP-24906"
    			(at 0 -15.24 0)
    		)
    		(symbol "sparkfun_power_splitter_jps_3_1_1_1"
    			(pin passive line
    				(at -8.89 0 0)
    				(length 2.54)
    				(name "SUM")
    				(number "1")
    			)
    			(pin power_in line
    				(at -8.89 -2.54 0)
    				(length 2.54)
    				(name "GND")
    				(number "2")
    			)
    			(pin power_in line
    				(at -8.89 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "5")
    			)
    			(pin passive line
    				(at 8.89 2.54 180)
    				(length 2.54)
    				(name "PORT1")
    				(number "6")
    			)
    			(pin passive line
    				(at 8.89 0 180)
    				(length 2.54)
    				(name "PORT2")
    				(number "4")
    			)
    			(pin passive line
    				(at 8.89 -2.54 180)
    				(length 2.54)
    				(name "PORT3")
    				(number "3")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_rc522"
        (property "Footprint" "PartReel:sparkfun_rc522"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MFRC522.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "13.65MHz RFID Reader IC."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun ISO 14443 MIFARE I2C/SPI/UART"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_rc522/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -13.97 20.32 0)
    		)
    		(property "Value" "RC522 (SparkFun)"
    			(at 11.43 20.32 0)
    		)
    		(property "PROD_ID" "IC-TBD"
    			(at 0 -20.32 0)
    		)
    		(property "ki_fp_filters" "SOT?23*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_rc522_0_1")
    		(symbol "sparkfun_rc522_1_1"
    			(pin power_in line
    				(at -17.78 17.78 0)
    				(length 2.54)
    				(hide yes)
    				(name "TVDD")
    				(number "12")
    			)
    			(pin power_in line
    				(at -17.78 17.78 0)
    				(length 2.54)
    				(hide yes)
    				(name "AVDD")
    				(number "15")
    			)
    			(pin power_in line
    				(at -17.78 17.78 0)
    				(length 2.54)
    				(name "VDD")
    				(number "2")
    			)
    			(pin power_in line
    				(at -17.78 17.78 0)
    				(length 2.54)
    				(hide yes)
    				(name "DVDD")
    				(number "3")
    			)
    			(pin power_in line
    				(at -17.78 17.78 0)
    				(length 2.54)
    				(hide yes)
    				(name "SVDD")
    				(number "9")
    			)
    			(pin input line
    				(at -17.78 15.24 0)
    				(length 2.54)
    				(name "~{RST}")
    				(number "6")
    			)
    			(pin output line
    				(at -17.78 10.16 0)
    				(length 2.54)
    				(name "TX1")
    				(number "11")
    			)
    			(pin output line
    				(at -17.78 7.62 0)
    				(length 2.54)
    				(name "TX2")
    				(number "13")
    			)
    			(pin input line
    				(at -17.78 5.08 0)
    				(length 2.54)
    				(name "RX")
    				(number "17")
    			)
    			(pin power_out line
    				(at -17.78 2.54 0)
    				(length 2.54)
    				(name "VMID")
    				(number "16")
    			)
    			(pin input line
    				(at -17.78 -2.54 0)
    				(length 2.54)
    				(name "OSCIN")
    				(number "21")
    			)
    			(pin output line
    				(at -17.78 -5.08 0)
    				(length 2.54)
    				(name "OSCOUT")
    				(number "22")
    			)
    			(pin output line
    				(at -17.78 -10.16 0)
    				(length 2.54)
    				(name "MFOUT")
    				(number "8")
    			)
    			(pin input line
    				(at -17.78 -12.7 0)
    				(length 2.54)
    				(name "MFIN")
    				(number "7")
    			)
    			(pin power_out line
    				(at -17.78 -16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "TVSS")
    				(number "10")
    			)
    			(pin power_out line
    				(at -17.78 -16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "TVSS")
    				(number "14")
    			)
    			(pin power_out line
    				(at -17.78 -16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "AVSS")
    				(number "18")
    			)
    			(pin power_out line
    				(at -17.78 -16.51 0)
    				(length 2.54)
    				(name "VSS")
    				(number "4")
    			)
    			(pin power_out line
    				(at -17.78 -16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "PVSS")
    				(number "5")
    			)
    			(pin no_connect line
    				(at -3.81 -13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "AUX1")
    				(number "19")
    			)
    			(pin no_connect line
    				(at -3.81 -16.51 0)
    				(length 2.54)
    				(hide yes)
    				(name "AUX2")
    				(number "20")
    			)
    			(pin input line
    				(at 17.78 17.78 180)
    				(length 2.54)
    				(name "I2C")
    				(number "1")
    			)
    			(pin input line
    				(at 17.78 15.24 180)
    				(length 2.54)
    				(name "EA")
    				(number "32")
    			)
    			(pin bidirectional line
    				(at 17.78 10.16 180)
    				(length 2.54)
    				(name "SDA/~{CS}/RX")
    				(number "24")
    			)
    			(pin bidirectional line
    				(at 17.78 7.62 180)
    				(length 2.54)
    				(name "SCL/MISO/TX")
    				(number "31")
    			)
    			(pin output line
    				(at 17.78 5.08 180)
    				(length 2.54)
    				(name "IRQ")
    				(number "23")
    			)
    			(pin bidirectional line
    				(at 17.78 0 180)
    				(length 2.54)
    				(name "ADR0/MOSI/MX")
    				(number "30")
    			)
    			(pin bidirectional line
    				(at 17.78 -2.54 180)
    				(length 2.54)
    				(name "ADR1/SCK/DTR")
    				(number "29")
    			)
    			(pin input line
    				(at 17.78 -5.08 180)
    				(length 2.54)
    				(name "ADR2")
    				(number "28")
    			)
    			(pin input line
    				(at 17.78 -7.62 180)
    				(length 2.54)
    				(name "ADR3")
    				(number "27")
    			)
    			(pin input line
    				(at 17.78 -10.16 180)
    				(length 2.54)
    				(name "ADR4")
    				(number "26")
    			)
    			(pin input line
    				(at 17.78 -12.7 180)
    				(length 2.54)
    				(name "ADR5")
    				(number "25")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_rm2"
        (property "Footprint" "PartReel:sparkfun_rm2"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_rm2/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Radio module from Raspberry Pi using the CYW43 supporting WiFi and Bluetooth/BLE."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Raspberry Pi RPi RM2 WiFi Bluetooth BLE"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_rm2/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 16.51 0)
    		)
    		(property "Value" "RM2 (SparkFun)"
    			(at 0 13.97 0)
    		)
    		(property "PROD_ID" "IC-21607"
    			(at 0 -16.51 0)
    		)
    		(property "ki_fp_filters" "ESP32?WROOM?32*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_rm2_1_0"
    			(pin bidirectional line
    				(at -10.16 11.43 0)
    				(length 2.54)
    				(name "VDDBAT")
    				(number "C2")
    			)
    			(pin bidirectional line
    				(at -10.16 8.89 0)
    				(length 2.54)
    				(name "VDDIO")
    				(number "B7")
    			)
    			(pin bidirectional line
    				(at -10.16 3.81 0)
    				(length 2.54)
    				(name "WLON")
    				(number "B5")
    			)
    			(pin bidirectional line
    				(at -10.16 1.27 0)
    				(length 2.54)
    				(name "BTON")
    				(number "B6")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(name "GND")
    				(number "A1")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "A4")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "A7")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "B4")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "C1")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "C7")
    			)
    			(pin no_connect line
    				(at -7.62 -3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC1")
    				(number "A2")
    			)
    			(pin no_connect line
    				(at -7.62 -6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC2")
    				(number "C5")
    			)
    			(pin no_connect line
    				(at -7.62 -8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC3")
    				(number "C6")
    			)
    			(pin bidirectional line
    				(at 10.16 11.43 180)
    				(length 2.54)
    				(name "~{CS}")
    				(number "B2")
    			)
    			(pin bidirectional line
    				(at 10.16 8.89 180)
    				(length 2.54)
    				(name "SCLK")
    				(number "A3")
    			)
    			(pin bidirectional line
    				(at 10.16 6.35 180)
    				(length 2.54)
    				(name "PICO")
    				(number "A5")
    			)
    			(pin bidirectional line
    				(at 10.16 3.81 180)
    				(length 2.54)
    				(name "POCI")
    				(number "A6")
    			)
    			(pin bidirectional line
    				(at 10.16 -1.27 180)
    				(length 2.54)
    				(name "IRQ")
    				(number "B3")
    			)
    			(pin bidirectional line
    				(at 10.16 -6.35 180)
    				(length 2.54)
    				(name "GPIO0")
    				(number "B1")
    			)
    			(pin bidirectional line
    				(at 10.16 -8.89 180)
    				(length 2.54)
    				(name "GPIO1")
    				(number "C4")
    			)
    			(pin bidirectional line
    				(at 10.16 -11.43 180)
    				(length 2.54)
    				(name "GPIO2")
    				(number "C3")
    			)
    		)
    		(symbol "sparkfun_rm2_1_1")
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_rm2_tight"
        (property "Footprint" "PartReel:sparkfun_rm2_tight"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/sparkfun_rm2_tight/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Radio module from Raspberry Pi using the CYW43 supporting WiFi and Bluetooth/BLE."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Raspberry Pi RPi RM2 WiFi Bluetooth BLE"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_rm2_tight/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 16.51 0)
    		)
    		(property "Value" "RM2_Tight (SparkFun)"
    			(at 0 13.97 0)
    		)
    		(property "PROD_ID" "IC-21607"
    			(at 0 -16.51 0)
    		)
    		(property "ki_fp_filters" "ESP32?WROOM?32*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_rm2_tight_1_0"
    			(pin bidirectional line
    				(at -10.16 11.43 0)
    				(length 2.54)
    				(name "VDDBAT")
    				(number "C2")
    			)
    			(pin bidirectional line
    				(at -10.16 8.89 0)
    				(length 2.54)
    				(name "VDDIO")
    				(number "B7")
    			)
    			(pin bidirectional line
    				(at -10.16 3.81 0)
    				(length 2.54)
    				(name "WLON")
    				(number "B5")
    			)
    			(pin bidirectional line
    				(at -10.16 1.27 0)
    				(length 2.54)
    				(name "BTON")
    				(number "B6")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(name "GND")
    				(number "A1")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "A4")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "A7")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "B4")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "C1")
    			)
    			(pin bidirectional line
    				(at -10.16 -11.43 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "C7")
    			)
    			(pin no_connect line
    				(at -7.62 -3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC1")
    				(number "A2")
    			)
    			(pin no_connect line
    				(at -7.62 -6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC2")
    				(number "C5")
    			)
    			(pin no_connect line
    				(at -7.62 -8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC3")
    				(number "C6")
    			)
    			(pin bidirectional line
    				(at 10.16 11.43 180)
    				(length 2.54)
    				(name "~{CS}")
    				(number "B2")
    			)
    			(pin bidirectional line
    				(at 10.16 8.89 180)
    				(length 2.54)
    				(name "SCLK")
    				(number "A3")
    			)
    			(pin bidirectional line
    				(at 10.16 6.35 180)
    				(length 2.54)
    				(name "PICO")
    				(number "A5")
    			)
    			(pin bidirectional line
    				(at 10.16 3.81 180)
    				(length 2.54)
    				(name "POCI")
    				(number "A6")
    			)
    			(pin bidirectional line
    				(at 10.16 -1.27 180)
    				(length 2.54)
    				(name "IRQ")
    				(number "B3")
    			)
    			(pin bidirectional line
    				(at 10.16 -6.35 180)
    				(length 2.54)
    				(name "GPIO0")
    				(number "B1")
    			)
    			(pin bidirectional line
    				(at 10.16 -8.89 180)
    				(length 2.54)
    				(name "GPIO1")
    				(number "C4")
    			)
    			(pin bidirectional line
    				(at 10.16 -11.43 180)
    				(length 2.54)
    				(name "GPIO2")
    				(number "C3")
    			)
    		)
    		(symbol "sparkfun_rm2_tight_1_1")
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_saw_filter_1575mhz"
        (property "Footprint" "PartReel:sparkfun_saw_filter_1575mhz"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.murata.com/en/products/productdata/8797683712030/DS-SAFFB1G56KB0F0A.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Murata 1575.42/1602MHz SAW filter, SMD 1109."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun SAW filter GNSS GPS GLONAS BeiDou"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_saw_filter_1575mhz/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(pin_names
    			(offset 1.016)
    		)
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "FL"
    			(at 2.54 -6.35 0)
    		)
    		(property "Value" "SAW_Filter_1575MHz (SparkFun)"
    			(at 0 6.35 0)
    		)
    		(property "PROD_ID" "IC-27031"
    			(at 0 -16.51 0)
    		)
    		(property "ki_fp_filters" "Filter*1109*1.1x0.9mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_saw_filter_1575mhz_0_1")
    		(symbol "sparkfun_saw_filter_1575mhz_1_1"
    			(pin passive line
    				(at -7.62 2.54 0)
    				(length 2.54)
    				(name "~")
    				(number "1")
    			)
    			(pin passive line
    				(at -7.62 -2.54 0)
    				(length 2.54)
    				(name "~")
    				(number "2")
    			)
    			(pin passive line
    				(at -7.62 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "~")
    				(number "3")
    			)
    			(pin passive line
    				(at -7.62 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "~")
    				(number "5")
    			)
    			(pin passive line
    				(at 7.62 2.54 180)
    				(length 2.54)
    				(name "~")
    				(number "4")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "dfplayer_mini" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "DFPlayer Mini MP3 Player Module" (at 0 -13.43 0))
        (property "Footprint" "PartReel:dfplayer_mini"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://wiki.dfrobot.com/DFPlayer_Mini_SKU_DFR0299"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "DFRobot DFPlayer Mini serial MP3 player module with microSD slot and 3W amp, 3.2-5V, UART control. Clones (MP3-TF-16P) share the identical footprint. Row spacing is 18.03mm per the official drawing."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "dfplayer mp3 audio module dfrobot microsd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/dfplayer_mini/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "dfplayer_mini_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "RX")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "TX")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "DAC_R")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "DAC_L")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SPK_1")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "GND")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "SPK_2")
          (number "8"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "BUSY")
          (number "16"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "USB-")
          (number "15"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "USB+")
          (number "14"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "ADKEY_2")
          (number "13"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "ADKEY_1")
          (number "12"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "IO_2")
          (number "11"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "GND")
          (number "10"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "IO_1")
          (number "9"))
      )
    )
  (symbol "esp32_devkitc_v4" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 27.40 0))
      (property "Value" "ESP32-DevKitC V4 Development Board" (at 0 -27.40 0))
        (property "Footprint" "PartReel:esp32_devkitc_v4"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.espressif.com/projects/esp-dev-kits/en/latest/esp32/esp32-devkitc/user_guide.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Espressif ESP32-DevKitC V4 dev board (ESP32-WROOM-32E), 38-pin 2.54 headers at 25.4mm row spacing - drop it onto a carrier PCB with two 1x19 sockets. WROOM antenna overhangs the board edge by 6mm: keep that zone copper-free."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "esp32 devkitc devboard wroom-32 espressif development"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/esp32_devkitc_v4/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "esp32_devkitc_v4_1_1"
        (pin passive line (at -11.43 22.86 0) (length 2.54)
          (name "3V3")
          (number "1"))
        (pin passive line (at -11.43 20.32 0) (length 2.54)
          (name "EN")
          (number "2"))
        (pin passive line (at -11.43 17.78 0) (length 2.54)
          (name "VP")
          (number "3"))
        (pin passive line (at -11.43 15.24 0) (length 2.54)
          (name "VN")
          (number "4"))
        (pin passive line (at -11.43 12.70 0) (length 2.54)
          (name "IO34")
          (number "5"))
        (pin passive line (at -11.43 10.16 0) (length 2.54)
          (name "IO35")
          (number "6"))
        (pin passive line (at -11.43 7.62 0) (length 2.54)
          (name "IO32")
          (number "7"))
        (pin passive line (at -11.43 5.08 0) (length 2.54)
          (name "IO33")
          (number "8"))
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "IO25")
          (number "9"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "IO26")
          (number "10"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "IO27")
          (number "11"))
        (pin passive line (at -11.43 -5.08 0) (length 2.54)
          (name "IO14")
          (number "12"))
        (pin passive line (at -11.43 -7.62 0) (length 2.54)
          (name "IO12")
          (number "13"))
        (pin passive line (at -11.43 -10.16 0) (length 2.54)
          (name "GND")
          (number "14"))
        (pin passive line (at -11.43 -12.70 0) (length 2.54)
          (name "IO13")
          (number "15"))
        (pin passive line (at -11.43 -15.24 0) (length 2.54)
          (name "D2")
          (number "16"))
        (pin passive line (at -11.43 -17.78 0) (length 2.54)
          (name "D3")
          (number "17"))
        (pin passive line (at -11.43 -20.32 0) (length 2.54)
          (name "CMD")
          (number "18"))
        (pin passive line (at -11.43 -22.86 0) (length 2.54)
          (name "5V")
          (number "19"))
        (pin passive line (at 11.43 22.86 180) (length 2.54)
          (name "GND")
          (number "20"))
        (pin passive line (at 11.43 20.32 180) (length 2.54)
          (name "IO23")
          (number "21"))
        (pin passive line (at 11.43 17.78 180) (length 2.54)
          (name "IO22")
          (number "22"))
        (pin passive line (at 11.43 15.24 180) (length 2.54)
          (name "TX")
          (number "23"))
        (pin passive line (at 11.43 12.70 180) (length 2.54)
          (name "RX")
          (number "24"))
        (pin passive line (at 11.43 10.16 180) (length 2.54)
          (name "IO21")
          (number "25"))
        (pin passive line (at 11.43 7.62 180) (length 2.54)
          (name "GND")
          (number "26"))
        (pin passive line (at 11.43 5.08 180) (length 2.54)
          (name "IO19")
          (number "27"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "IO18")
          (number "28"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "IO5")
          (number "29"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "IO17")
          (number "30"))
        (pin passive line (at 11.43 -5.08 180) (length 2.54)
          (name "IO16")
          (number "31"))
        (pin passive line (at 11.43 -7.62 180) (length 2.54)
          (name "IO4")
          (number "32"))
        (pin passive line (at 11.43 -10.16 180) (length 2.54)
          (name "IO0")
          (number "33"))
        (pin passive line (at 11.43 -12.70 180) (length 2.54)
          (name "IO2")
          (number "34"))
        (pin passive line (at 11.43 -15.24 180) (length 2.54)
          (name "IO15")
          (number "35"))
        (pin passive line (at 11.43 -17.78 180) (length 2.54)
          (name "D1")
          (number "36"))
        (pin passive line (at 11.43 -20.32 180) (length 2.54)
          (name "D0")
          (number "37"))
        (pin passive line (at 11.43 -22.86 180) (length 2.54)
          (name "CLK")
          (number "38"))
      )
    )
  (symbol "gc9a01_module_128" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "1.28\" GC9A01 Round LCD Module (240x240, SPI)" (at 0 -13.43 0))
        (property "Footprint" "PartReel:gc9a01_module_128"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/res/MSP1281/MSP1281_Size.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Common 1.28 inch round IPS LCD module with GC9A01 controller, 240x240, SPI 8-pin header (BLK CS DC RES SDA SCL VCC GND), round PCB D38 with 23mm bottom tab. Smartwatch-project staple; pairs with CST816S touch variants. Verify against your vendor - clones vary."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "gc9a01 round lcd 1.28 240x240 spi module smartwatch"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/gc9a01_module_128/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "gc9a01_module_128_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "BLK")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "CS")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "DC")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "RES")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "SDA")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SCL")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "VCC")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "GND")
          (number "8"))
      )
    )
  (symbol "max7219_matrix_module" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 9.62 0))
      (property "Value" "MAX7219 8x8 LED Matrix Module (FC-16)" (at 0 -9.62 0))
        (property "Footprint" "PartReel:max7219_matrix_module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://components101.com/sites/default/files/component_datasheet/MAX7219%208x8%20LED%20Matrix%20Module%20Datasheet.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cascadable 8x8 LED dot matrix module driven by MAX7219, SPI-like 3-wire, 5V, IN/OUT headers for daisy-chaining, 32x32mm. The bare MAX7219 chip is in the official KiCad library; this is the module board."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "max7219 led matrix 8x8 module fc-16 cascadable"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/max7219_matrix_module/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "max7219_matrix_module_1_1"
        (pin passive line (at -11.43 5.08 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "DIN")
          (number "3"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "CS")
          (number "4"))
        (pin passive line (at -11.43 -5.08 0) (length 2.54)
          (name "CLK")
          (number "5"))
        (pin passive line (at 11.43 5.08 180) (length 2.54)
          (name "VCC")
          (number "6"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "GND")
          (number "7"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "DOUT")
          (number "8"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "CS")
          (number "9"))
        (pin passive line (at 11.43 -5.08 180) (length 2.54)
          (name "CLK")
          (number "10"))
      )
    )
  (symbol "mc01506" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "1.5\" OLED Module (128x128, I2C, MC01506)" (at 0 -8.35 0))
        (property "Footprint" "PartReel:mc01506"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/1.5inch_OLED_Module_SKU:MC01506"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Generic 1.5 inch 128x128 OLED module (SH1107-class controller per lcdwiki; lcdwiki MC01506), I2C 4-pin header (GND VCC SCL SDA), 34x47mm board, four 2.2mm holes."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sh1107 oled 1.5 128x128 i2c module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/mc01506/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "mc01506_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VCC")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SDA")
          (number "4"))
      )
    )
  (symbol "mc091gx" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "0.91\" SSD1306 I2C OLED Module (128x32, MC091GX)" (at 0 -8.35 0))
        (property "Footprint" "PartReel:mc091gx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/res/MC091GX/0.91inch_IIC_OLED_Module_MC091GX_User_Manual_EN.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Generic 0.91 inch 128x32 I2C OLED module (SSD1306, lcdwiki MC091GX), 4-pin header (GND VCC SCL SDA), 38x12mm board, no mounting holes. NOTE: different board from the official library ER_OLEDM0.91 bare glass."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ssd1306 oled 0.91 128x32 i2c module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/mc091gx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "mc091gx_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VCC")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SDA")
          (number "4"))
      )
    )
  (symbol "msp0961" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "0.96\" ST7735S IPS Module (80x160, SPI, MSP0961)" (at 0 -13.43 0))
        (property "Footprint" "PartReel:msp0961"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/0.96inch_IPS_Module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Generic 0.96 inch 80x160 IPS TFT module (ST7735S, lcdwiki MSP0961), SPI 8-pin header (GND VCC SCL SDA RES DC CS BLK), 30x24mm board, four 2.0mm holes."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "st7735 ips 0.96 80x160 spi module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/msp0961/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "msp0961_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "VCC")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SDA")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "RES")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "DC")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "CS")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "BLK")
          (number "8"))
      )
    )
  (symbol "msp1541" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "1.54\" ST7789 IPS Module (240x240, SPI, MSP1541)" (at 0 -13.43 0))
        (property "Footprint" "PartReel:msp1541"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/1.54inch_IPS_Module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Generic 1.54 inch 240x240 IPS TFT module (ST7789, lcdwiki MSP1541), SPI 8-pin header (GND VCC SCL SDA RES DC CS BLK), 32x43.7mm board, four 2.0mm holes."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "st7789 ips 1.54 240x240 spi module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/msp1541/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "msp1541_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "VCC")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SDA")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "RES")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "DC")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "CS")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "BLK")
          (number "8"))
      )
    )
  (symbol "msp1803" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "1.8\" ST7735 TFT Module (128x160, SPI, MSP1803)" (at 0 -13.43 0))
        (property "Footprint" "PartReel:msp1803"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/1.8inch_SPI_Module_ST7735S_SKU:MSP1803"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Generic 1.8 inch 128x160 TFT module (ST7735, lcdwiki MSP1803), SPI 8-pin main header + 4-pin SD header, 34.5x58mm board, four 3.2mm holes. Main header pin1=VCC is on the RIGHT in front view (vendor drawing is back-view)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "st7735 tft 1.8 128x160 spi sd module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/msp1803/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "msp1803_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "CS")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "RESET")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "AO")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SDA")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "SCK")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "LED")
          (number "8"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "SD_CS")
          (number "9"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "SD_MOSI")
          (number "10"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "SD_MISO")
          (number "11"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "SD_SCK")
          (number "12"))
      )
    )
  (symbol "msp2008" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "2.0\" ST7789V IPS Module (240x320, SPI, MSP2008)" (at 0 -13.43 0))
        (property "Footprint" "PartReel:msp2008"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/2.0inch_IPS_Module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Generic 2.0 inch 240x320 IPS TFT module (ST7789V, lcdwiki MSP2008-class), SPI 8-pin header (GND VCC SCL SDA RES DC CS BLK), 36.5x61mm board, four 2.0mm holes."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "st7789 ips 2.0 240x320 spi module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/msp2008/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "msp2008_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "VCC")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SDA")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "RES")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "DC")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "CS")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "BLK")
          (number "8"))
      )
    )
  (symbol "msp2807" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 21.05 0))
      (property "Value" "2.8\" ILI9341 TFT Module (240x320, SPI+Touch+SD, MSP2807)" (at 0 -21.05 0))
        (property "Footprint" "PartReel:msp2807"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/2.8inch_SPI_Module_ILI9341_SKU:MSP2807"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Classic 2.8 inch 240x320 TFT module (ILI9341V + resistive touch + microSD, lcdwiki MSP2807), 14-pin SPI/touch header + 4-pin SD header, 50x86mm board, four 3.2mm holes."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ili9341 tft 2.8 240x320 spi touch sd module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/msp2807/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "msp2807_1_1"
        (pin passive line (at -11.43 16.51 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 13.97 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 11.43 0) (length 2.54)
          (name "CS")
          (number "3"))
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "RESET")
          (number "4"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "DC")
          (number "5"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "SDI(MOSI)")
          (number "6"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SCK")
          (number "7"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "LED")
          (number "8"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SDO(MISO)")
          (number "9"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "T_CLK")
          (number "10"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "T_CS")
          (number "11"))
        (pin passive line (at -11.43 -11.43 0) (length 2.54)
          (name "T_DIN")
          (number "12"))
        (pin passive line (at -11.43 -13.97 0) (length 2.54)
          (name "T_DO")
          (number "13"))
        (pin passive line (at -11.43 -16.51 0) (length 2.54)
          (name "T_IRQ")
          (number "14"))
        (pin passive line (at 11.43 16.51 180) (length 2.54)
          (name "SD_CS")
          (number "15"))
        (pin passive line (at 11.43 13.97 180) (length 2.54)
          (name "SD_MOSI")
          (number "16"))
        (pin passive line (at 11.43 11.43 180) (length 2.54)
          (name "SD_MISO")
          (number "17"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "SD_SCK")
          (number "18"))
      )
    )
  (symbol "sh1106_module_13" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "1.3\" SH1106 I2C OLED Module (128x64)" (at 0 -8.35 0))
        (property "Footprint" "PartReel:sh1106_module_13"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/1.3inch_IIC_OLED_Module_SKU:MC130VX"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Common 1.3 inch 128x64 OLED display module with SH1106 controller, I2C 4-pin header (GND VCC SCL SDA - note order differs from 0.96\" module!), 35.4x33.5mm board, four 3.0mm mounting holes. Dimensions per LCDwiki vendor drawing - verify against your specific module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sh1106 oled display module 1.3 128x64 i2c"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sh1106_module_13/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "sh1106_module_13_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VCC")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SDA")
          (number "4"))
      )
    )
  (symbol "ssd1306_module_096" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "0.96\" SSD1306 I2C OLED Module (128x64)" (at 0 -8.35 0))
        (property "Footprint" "PartReel:ssd1306_module_096"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/0.96inch_OLED_Module_(IIC-4P_SKU:MC096VX)"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Common 0.96 inch 128x64 OLED display module with SSD1306 controller, I2C 4-pin header (VCC GND SCL SDA), 27.3x27.8mm board, four 2.0mm mounting holes. Dimensions per LCDwiki vendor drawing - verify against your specific module (Chinese modules vary slightly)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ssd1306 oled display module 0.96 128x64 i2c"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ssd1306_module_096/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ssd1306_module_096_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SDA")
          (number "4"))
      )
    )
  (symbol "ssd1331_module_095" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "0.95\" SSD1331 RGB OLED Module (96x64, SPI, Waveshare)" (at 0 -13.43 0))
        (property "Footprint" "PartReel:ssd1331_module_095"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.waveshare.com/wiki/0.95inch_RGB_OLED_(A)"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Waveshare 0.95 inch 96x64 RGB OLED module (SSD1331), SPI 8-pin header (pin 1 = VCC at the right per vendor numbering: VCC GND NC DIN CLK CS D/C RES), 31.7x37mm board, four 3.0mm holes. (A)=bent pins, (B)=straight - same PCB."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ssd1331 rgb oled 0.95 96x64 spi module waveshare"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ssd1331_module_095/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ssd1331_module_095_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "NC")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "DIN")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "CLK")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "CS")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "D/C")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "RES")
          (number "8"))
      )
    )
  (symbol "ssd1351_module_15" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 12.16 0))
      (property "Value" "1.5\" SSD1351 RGB OLED Module (128x128, SPI, Waveshare)" (at 0 -12.16 0))
        (property "Footprint" "PartReel:ssd1351_module_15"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.waveshare.com/wiki/1.5inch_RGB_OLED_Module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Waveshare 1.5 inch 128x128 RGB OLED module (SSD1351), SPI 7-pin vertical header on the left edge (VCC GND DIN CLK CS DC RST top to bottom), 44.5x37mm board, four 2.0mm holes. Second 1.25mm SMD wafer on back carries the same signals."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ssd1351 rgb oled 1.5 128x128 spi module waveshare"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ssd1351_module_15/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ssd1351_module_15_1_1"
        (pin passive line (at -11.43 7.62 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 5.08 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "DIN")
          (number "3"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "CLK")
          (number "4"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "CS")
          (number "5"))
        (pin passive line (at -11.43 -5.08 0) (length 2.54)
          (name "DC")
          (number "6"))
        (pin passive line (at -11.43 -7.62 0) (length 2.54)
          (name "RST")
          (number "7"))
      )
    )
  (symbol "st7789_module_13" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 12.16 0))
      (property "Value" "1.3\" ST7789 IPS TFT Module (240x240, SPI)" (at 0 -12.16 0))
        (property "Footprint" "PartReel:st7789_module_13"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.lcdwiki.com/1.3inch_IPS_Module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Common 1.3 inch 240x240 IPS TFT display module with ST7789 controller, SPI 7-pin header (GND VCC SCL SDA RES DC BLK), 27.78x39.22mm board, four 2.0mm mounting holes. Dimensions per LCDwiki vendor drawing - verify against your specific module."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "st7789 tft ips display module 1.3 240x240 spi"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/st7789_module_13/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "st7789_module_13_1_1"
        (pin passive line (at -11.43 7.62 0) (length 2.54)
          (name "GND")
          (number "1"))
        (pin passive line (at -11.43 5.08 0) (length 2.54)
          (name "VCC")
          (number "2"))
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "SDA")
          (number "4"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "RES")
          (number "5"))
        (pin passive line (at -11.43 -5.08 0) (length 2.54)
          (name "DC")
          (number "6"))
        (pin passive line (at -11.43 -7.62 0) (length 2.54)
          (name "BLK")
          (number "7"))
      )
    )
  (symbol "weact_epaper_213" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "2.13\" WeAct E-Paper Module (SSD1680, 122x250, SPI)" (at 0 -13.43 0))
        (property "Footprint" "PartReel:weact_epaper_213"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://github.com/WeActStudio/WeActStudio.EpaperModule"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "WeAct Studio 2.13 inch black/white e-paper module (SSD1680 driver, 122x250, YRD0213 panel), SPI via a 2x4 (dual-row!) 2.54 header near the left edge (1 BUSY 2 RES 3 D/C 4 CS 5 SCL 6 SDA 7 GND 8 VCC, odd pins in the edge-side column), 72x30mm board, four 3.2mm holes. The official KiCad library has no e-paper content at all."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ssd1680 epaper e-ink eink 2.13 weact spi module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/weact_epaper_213/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "weact_epaper_213_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "BUSY")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "RES")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "D/C")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "CS")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "SCL")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SDA")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "GND")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "VCC")
          (number "8"))
      )
    )
  (symbol "hc05" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 10.89 0))
      (property "Value" "HC-05 Bluetooth Module (ZS-040)" (at 0 -10.89 0))
        (property "Footprint" "PartReel:hc05"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://protosupplies.com/product/hc-05-bluetooth-module/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "HC-05 bluetooth serial (SPP) module on the common ZS-040 carrier board, 3.6-6V supply / 3.3V logic, 6-pin right-angle header. HC-06 ships on the same board (4 of 6 pins used)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "hc-05 hc-06 bluetooth serial module zs-040"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/hc05/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "hc05_1_1"
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "STATE")
          (number "1"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "RXD")
          (number "2"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "TXD")
          (number "3"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "4"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "VCC")
          (number "5"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "EN")
          (number "6"))
      )
    )
  (symbol "sim800l" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 10.89 0))
      (property "Value" "SIM800L GSM/GPRS Module (Red Breakout)" (at 0 -10.89 0))
        (property "Footprint" "PartReel:sim800l"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.haoyuelectronics.com/Attachment/SIM800L/SIM800L_Coreboard.jpg"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "SIM800L quad-band GSM/GPRS module on the common red coreboard, 3.4-4.4V (2A bursts!), UART, u.FL + solder antenna pads, micro-SIM on back. Do not confuse with the larger blue SIM800L EVB v2.0."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sim800l gsm gprs sms module simcom"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sim800l/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "sim800l_1_1"
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "NET")
          (number "1"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "VCC")
          (number "2"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "RST")
          (number "3"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "RXD")
          (number "4"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "TXD")
          (number "5"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "GND")
          (number "6"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "RING")
          (number "7"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "DTR")
          (number "8"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "MIC+")
          (number "9"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "MIC-")
          (number "10"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "SPK+")
          (number "11"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "SPK-")
          (number "12"))
      )
    )
  (symbol "hc_sr04" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "HC-SR04 Ultrasonic Distance Sensor Module" (at 0 -8.35 0))
        (property "Footprint" "PartReel:hc_sr04"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/datasheets/Sensors/Proximity/HCSR04.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Classic HC-SR04 ultrasonic ranging module (2-400cm), 5V, 4-pin header (VCC Trig Echo GND). Footprint is the module board with mounting holes; HC-SR04P (3.3-5.5V) and RCWL clones are mechanically identical. Some units have only 2 diagonal mounting holes."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "hc-sr04 ultrasonic distance sonar module arduino"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/hc_sr04/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "hc_sr04_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "VCC")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "Trig")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "Echo")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "GND")
          (number "4"))
      )
    )
  (symbol "ld2410c" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 9.62 0))
      (property "Value" "HLK-LD2410C 24GHz mmWave Presence Radar" (at 0 -9.62 0))
        (property "Footprint" "PartReel:ld2410c"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://d.hlktech.net/download/HLK-LD2410C/1/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hi-Link LD2410C 24GHz FMCW radar for human presence detection, UART + presence OUT pin (3.3V logic), 5-12V supply (5V advised, 200mA). ESPHome/Home Assistant staple. Antenna side must face the room."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "ld2410 mmwave radar presence human sensor hi-link esphome"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ld2410c/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "ld2410c_1_1"
        (pin passive line (at -11.43 5.08 0) (length 2.54)
          (name "TX")
          (number "1"))
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "RX")
          (number "2"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "OUT")
          (number "3"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "GND")
          (number "4"))
        (pin passive line (at -11.43 -5.08 0) (length 2.54)
          (name "VCC")
          (number "5"))
      )
    )
  (symbol "samsung_cl05a105ka5nnnc" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0 2.54 0))
      (property "Value" "1µF 10% 0402 MLCC (Samsung CL05A105KA5NNNC)" (at 0 -2.54 0))
        (property "Footprint" "PartReel:samsung_cl05a105ka5nnnc"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://weblib.samsungsem.com/mlcc/mlcc-ec-data-sheet.do?partNumber=CL05A105KA5NNNC"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "MLCC ceramic capacitor 1µF +-10% 0402 (1005 metric), X5R 25V. Generated for PartReel circuit blocks."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "capacitor 1µF 0402 chip smd x5r 25v"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/samsung_cl05a105ka5nnnc/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "samsung_cl05a105ka5nnnc_1_1"
        (pin passive line (at -3.81 0 0) (length 3.302)
          (name "~")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 3.302)
          (name "~")
          (number "2"))
      ))
  (symbol "kemet_c0805c222k1ractu" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0 2.54 0))
      (property "Value" "2.2nF 10% 0805 MLCC (KEMET C0805C222K1RACTU)" (at 0 -2.54 0))
        (property "Footprint" "PartReel:kemet_c0805c222k1ractu"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://content.kemet.com/datasheets/KEM_C1002_X7R_SMD.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "MLCC ceramic capacitor 2.2nF +-10% 0805 (2012 metric), X7R 100V. Generated for PartReel circuit blocks."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "capacitor 2.2nF 0805 chip smd x7r 100v"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/kemet_c0805c222k1ractu/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "kemet_c0805c222k1ractu_1_1"
        (pin passive line (at -3.81 0 0) (length 3.302)
          (name "~")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 3.302)
          (name "~")
          (number "2"))
      ))
  (symbol "vishay_crcw040210k0fked" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 0 2.54 0))
      (property "Value" "10kΩ 1% 0402 (Vishay CRCW040210K0FKED)" (at 0 -2.54 0))
        (property "Footprint" "PartReel:vishay_crcw040210k0fked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.vishay.com/docs/20035/dcrcwe3.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Thick film chip resistor 10kΩ +-1% 0402 (1/0/0/5mm metric), 0.063W. Generated for PartReel circuit blocks."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "resistor 10kΩ 0402 chip smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/vishay_crcw040210k0fked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "vishay_crcw040210k0fked_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "~")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "~")
          (number "2"))
      ))
  (symbol "vishay_crcw04025k10fked" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 0 2.54 0))
      (property "Value" "5.1k 1% 0402 (Vishay CRCW04025K10FKED)" (at 0 -2.54 0))
        (property "Footprint" "PartReel:vishay_crcw04025k10fked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.vishay.com/docs/20035/dcrcwe3.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Thick film chip resistor 5.1k +-1% 0402 (1/0/0/5mm metric), 0.063W. Generated for PartReel circuit blocks."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "resistor 5.1k 0402 chip smd"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/vishay_crcw04025k10fked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "vishay_crcw04025k10fked_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "~")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "~")
          (number "2"))
      ))
  (symbol "nordic_npm1100_caxx"
        (property "Footprint" "PartReel:nordic_npm1100_caxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs-be.nordicsemi.com/bundle/ps_npm1100/attach/nPM1100_PS_v1.4.pdf?_LANG=enus"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "PMIC and Battery Charger, BGA-25."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless PMIC Charger Regulator"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_npm1100_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nPM1100-CAXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA?*?*?2.075x2.075mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_npm1100_caxx_0_0"
  				(pin bidirectional line
  					(at -25.4 12.7 0)
  					(length 5.08)
  					(name "D+")
  					(number "A2")
  				)
  				(pin bidirectional line
  					(at -25.4 10.16 0)
  					(length 5.08)
  					(name "D-")
  					(number "A1")
  				)
  				(pin passive line
  					(at -25.4 2.54 0)
  					(length 5.08)
  					(name "NTC")
  					(number "E1")
  				)
  				(pin passive line
  					(at -25.4 -5.08 0)
  					(length 5.08)
  					(name "VTERMSET")
  					(number "C3")
  				)
  				(pin passive line
  					(at -25.4 -7.62 0)
  					(length 5.08)
  					(name "ICHG")
  					(number "E2")
  				)
  				(pin passive line
  					(at -25.4 -12.7 0)
  					(length 5.08)
  					(name "ERR")
  					(number "E3")
  				)
  				(pin passive line
  					(at -25.4 -15.24 0)
  					(length 5.08)
  					(name "CHG")
  					(number "E4")
  				)
  				(pin power_in line
  					(at -7.62 30.48 270)
  					(length 5.08)
  					(name "VBAT")
  					(number "D1")
  				)
  				(pin power_in line
  					(at 0 30.48 270)
  					(length 5.08)
  					(name "VBUS")
  					(number "B1")
  				)
  				(pin power_out line
  					(at 7.62 30.48 270)
  					(length 5.08)
  					(name "VSYS")
  					(number "C1")
  				)
  				(pin passive line
  					(at 25.4 12.7 180)
  					(length 5.08)
  					(name "DEC")
  					(number "A3")
  				)
  				(pin passive line
  					(at 25.4 7.62 180)
  					(length 5.08)
  					(name "VOUTBSET1")
  					(number "B3")
  				)
  				(pin power_out line
  					(at 25.4 5.08 180)
  					(length 5.08)
  					(name "VOUTB")
  					(number "B5")
  				)
  				(pin passive line
  					(at 25.4 0 180)
  					(length 5.08)
  					(name "SW")
  					(number "A4")
  				)
  				(pin passive line
  					(at 25.4 -5.08 180)
  					(length 5.08)
  					(name "MODE")
  					(number "E5")
  				)
  				(pin passive line
  					(at 25.4 -7.62 180)
  					(length 5.08)
  					(name "ISET")
  					(number "D5")
  				)
  				(pin input line
  					(at 25.4 -12.7 180)
  					(length 5.08)
  					(name "SHPACT")
  					(number "D4")
  				)
  				(pin input line
  					(at 25.4 -15.24 180)
  					(length 5.08)
  					(name "SHPHLD")
  					(number "D3")
  				)
  			)
  			(symbol "nordic_npm1100_caxx_1_0"
  				(pin passive line
  					(at -7.62 30.48 270)
  					(length 5.08)
  					(hide yes)
  					(name "VBAT")
  					(number "D2")
  				)
  				(pin passive line
  					(at 0 30.48 270)
  					(length 5.08)
  					(hide yes)
  					(name "VBUS")
  					(number "B2")
  				)
  				(pin power_in line
  					(at 0 -30.48 90)
  					(length 5.08)
  					(name "VSS")
  					(number "A5")
  				)
  				(pin passive line
  					(at 0 -30.48 90)
  					(length 5.08)
  					(hide yes)
  					(name "AVSS")
  					(number "C4")
  				)
  				(pin passive line
  					(at 0 -30.48 90)
  					(length 5.08)
  					(hide yes)
  					(name "AVSS")
  					(number "C5")
  				)
  				(pin passive line
  					(at 7.62 30.48 270)
  					(length 5.08)
  					(hide yes)
  					(name "VSYS")
  					(number "C2")
  				)
  				(pin passive line
  					(at 25.4 10.16 180)
  					(length 5.08)
  					(name "VOUTBSET0")
  					(number "B4")
  				)
  			)
  			(symbol "nordic_npm1100_caxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_npm1300_caxx"
        (property "Footprint" "PartReel:nordic_npm1300_caxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_npm1300"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "PMIC, LED Driver, Battery Charger, BGA-35."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless PMIC Regulator LED Driver Battery Charger"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_npm1300_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nPM1300-CAXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA*35*7x5*3.077x2.3775mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_npm1300_caxx_0_0"
  				(pin bidirectional line
  					(at -35.56 0 0)
  					(length 5.08)
  					(name "GPIO1")
  					(number "E6")
  				)
  				(pin bidirectional line
  					(at -35.56 -2.54 0)
  					(length 5.08)
  					(name "GPIO2")
  					(number "C5")
  				)
  				(pin bidirectional line
  					(at -35.56 -5.08 0)
  					(length 5.08)
  					(name "GPIO3")
  					(number "C4")
  				)
  			)
  			(symbol "nordic_npm1300_caxx_1_0"
  				(pin power_in line
  					(at -35.56 33.02 0)
  					(length 5.08)
  					(name "VBUS")
  					(number "B1")
  				)
  				(pin passive line
  					(at -35.56 33.02 0)
  					(length 5.08)
  					(hide yes)
  					(name "VBUS")
  					(number "B2")
  				)
  				(pin bidirectional line
  					(at -35.56 20.32 0)
  					(length 5.08)
  					(name "CC1")
  					(number "D5")
  				)
  				(pin bidirectional line
  					(at -35.56 17.78 0)
  					(length 5.08)
  					(name "CC2")
  					(number "B3")
  				)
  				(pin open_collector line
  					(at -35.56 12.7 0)
  					(length 5.08)
  					(name "LED0")
  					(number "A1")
  				)
  				(pin open_collector line
  					(at -35.56 10.16 0)
  					(length 5.08)
  					(name "LED1")
  					(number "A2")
  				)
  				(pin open_collector line
  					(at -35.56 7.62 0)
  					(length 5.08)
  					(name "LED2")
  					(number "A3")
  				)
  				(pin bidirectional line
  					(at -35.56 2.54 0)
  					(length 5.08)
  					(name "GPIO0")
  					(number "D6")
  				)
  				(pin bidirectional line
  					(at -35.56 -12.7 0)
  					(length 5.08)
  					(name "SDA")
  					(number "E5")
  				)
  				(pin bidirectional line
  					(at -35.56 -15.24 0)
  					(length 5.08)
  					(name "SCL")
  					(number "E3")
  				)
  				(pin passive line
  					(at -35.56 -20.32 0)
  					(length 5.08)
  					(name "VSET1")
  					(number "E2")
  				)
  				(pin passive line
  					(at -35.56 -22.86 0)
  					(length 5.08)
  					(name "VSET2")
  					(number "E1")
  				)
  				(pin passive line
  					(at -35.56 -27.94 0)
  					(length 5.08)
  					(name "SHPHLD")
  					(number "D4")
  				)
  				(pin power_in line
  					(at -2.54 40.64 270)
  					(length 5.08)
  					(name "VDDIO")
  					(number "E4")
  				)
  				(pin power_in line
  					(at 0 40.64 270)
  					(length 5.08)
  					(name "PVDD")
  					(number "C7")
  				)
  				(pin power_in line
  					(at 0 -40.64 90)
  					(length 5.08)
  					(name "VSS")
  					(number "A6")
  				)
  				(pin power_out line
  					(at 2.54 40.64 270)
  					(length 5.08)
  					(name "VSYS")
  					(number "C1")
  				)
  				(pin passive line
  					(at 2.54 40.64 270)
  					(length 5.08)
  					(hide yes)
  					(name "VSYS")
  					(number "C2")
  				)
  				(pin power_out line
  					(at 35.56 33.02 180)
  					(length 5.08)
  					(name "VBUSOUT")
  					(number "C3")
  				)
  				(pin power_out line
  					(at 35.56 17.78 180)
  					(length 5.08)
  					(name "VOUT1")
  					(number "B6")
  				)
  				(pin passive line
  					(at 35.56 12.7 180)
  					(length 5.08)
  					(name "SW1")
  					(number "B7")
  				)
  				(pin power_in line
  					(at 35.56 10.16 180)
  					(length 5.08)
  					(name "PVSS1")
  					(number "A7")
  				)
  				(pin power_out line
  					(at 35.56 5.08 180)
  					(length 5.08)
  					(name "VOUT2")
  					(number "C6")
  				)
  				(pin passive line
  					(at 35.56 0 180)
  					(length 5.08)
  					(name "SW2")
  					(number "D7")
  				)
  				(pin power_in line
  					(at 35.56 -2.54 180)
  					(length 5.08)
  					(name "PVSS2")
  					(number "E7")
  				)
  				(pin input line
  					(at 35.56 -7.62 180)
  					(length 5.08)
  					(name "LSIN1/VINLDO1")
  					(number "B4")
  				)
  				(pin output line
  					(at 35.56 -10.16 180)
  					(length 5.08)
  					(name "LSOUT1/VOUTLDO1")
  					(number "A4")
  				)
  				(pin input line
  					(at 35.56 -15.24 180)
  					(length 5.08)
  					(name "LSIN2/VINLDO2")
  					(number "B5")
  				)
  				(pin output line
  					(at 35.56 -17.78 180)
  					(length 5.08)
  					(name "LSOUT2/VOUTLDO2")
  					(number "A5")
  				)
  				(pin power_in line
  					(at 35.56 -30.48 180)
  					(length 5.08)
  					(name "VBAT")
  					(number "D1")
  				)
  				(pin passive line
  					(at 35.56 -30.48 180)
  					(length 5.08)
  					(hide yes)
  					(name "VBAT")
  					(number "D2")
  				)
  				(pin passive line
  					(at 35.56 -33.02 180)
  					(length 5.08)
  					(name "NTC")
  					(number "D3")
  				)
  			)
  			(symbol "nordic_npm1300_caxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_npm2100_caxx"
        (property "Footprint" "PartReel:nordic_npm2100_caxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/nordic_npm2100_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "nPM2100-CAXX."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_npm2100_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at -11.43 17.78 0)
  			)
  			(property "Value" "nPM2100-CAXX"
  				(at -5.08 15.24 0)
  			)
  			(property "ki_fp_filters" "BGA*16*4x4*1.9175x1.8975mm*"
  				(at -5.08 17.78 0)
  			)
  			(symbol "nordic_npm2100_caxx_0_0"
  				(pin power_in line
  					(at -15.24 10.16 0)
  					(length 2.54)
  					(name "VBAT")
  					(number "C4")
  				)
  				(pin passive line
  					(at -15.24 5.08 0)
  					(length 2.54)
  					(name "SW")
  					(number "B4")
  				)
  				(pin input line
  					(at -15.24 2.54 0)
  					(length 2.54)
  					(name "VSET")
  					(number "B3")
  				)
  				(pin bidirectional line
  					(at -15.24 -10.16 0)
  					(length 2.54)
  					(name "GPIO0")
  					(number "C3")
  				)
  				(pin power_in line
  					(at 0 -16.51 90)
  					(length 2.54)
  					(name "PVSS")
  					(number "A4")
  				)
  				(pin passive line
  					(at 0 -16.51 90)
  					(length 2.54)
  					(hide yes)
  					(name "AVSS1")
  					(number "B1")
  				)
  				(pin passive line
  					(at 0 -16.51 90)
  					(length 2.54)
  					(hide yes)
  					(name "AVSS2")
  					(number "B2")
  				)
  				(pin power_out line
  					(at 15.24 10.16 180)
  					(length 2.54)
  					(name "VOUT")
  					(number "A2")
  				)
  				(pin passive line
  					(at 15.24 0 180)
  					(length 2.54)
  					(name "VINT")
  					(number "A3")
  				)
  				(pin bidirectional line
  					(at 15.24 -7.62 180)
  					(length 2.54)
  					(name "PG/RESET")
  					(number "C1")
  				)
  				(pin input line
  					(at 15.24 -10.16 180)
  					(length 2.54)
  					(name "SYSGDEN")
  					(number "C2")
  				)
  			)
  			(symbol "nordic_npm2100_caxx_1_0"
  				(pin bidirectional line
  					(at -15.24 -2.54 0)
  					(length 2.54)
  					(name "SDA")
  					(number "D3")
  				)
  				(pin input line
  					(at -15.24 -5.08 0)
  					(length 2.54)
  					(name "SCL")
  					(number "D2")
  				)
  				(pin bidirectional line
  					(at -15.24 -12.7 0)
  					(length 2.54)
  					(name "GPIO1")
  					(number "D1")
  				)
  				(pin power_out line
  					(at 15.24 5.08 180)
  					(length 2.54)
  					(name "VOUTLDO")
  					(number "A1")
  					(alternate "LSOUT" power_out line)
  				)
  				(pin input line
  					(at 15.24 -5.08 180)
  					(length 2.54)
  					(name "SHPHLD")
  					(number "D4")
  				)
  			)
  			(symbol "nordic_npm2100_caxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "nordic_npm6001_caxx"
        (property "Footprint" "PartReel:nordic_npm6001_caxx"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://docs.nordicsemi.com/bundle/ps_npm6001"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "PMIC with Buck/LDO."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "nordic wireless PMIC Buck Regulator LDO"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/nordic_npm6001_caxx/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
  			(exclude_from_sim no)
  			(in_bom yes)
  			(on_board yes)
  			(property "Reference" "U"
  				(at 0 0 0)
  				(do_not_autoplace)
  			)
  			(property "Value" "nPM6001-CAXX"
  				(at 0 -2.54 0)
  				(do_not_autoplace)
  			)
  			(property "ki_fp_filters" "BGA*45*5x9*2.175x3.635mm*"
  				(at 0 0 0)
  			)
  			(symbol "nordic_npm6001_caxx_0_0"
  				(pin bidirectional line
  					(at -30.48 33.02 0)
  					(length 2.54)
  					(name "ENABLE")
  					(number "B2")
  				)
  				(pin bidirectional line
  					(at -30.48 27.94 0)
  					(length 2.54)
  					(name "READY")
  					(number "H4")
  				)
  				(pin bidirectional line
  					(at -30.48 22.86 0)
  					(length 2.54)
  					(name "BUCK_MODE0")
  					(number "G2")
  				)
  				(pin bidirectional line
  					(at -30.48 20.32 0)
  					(length 2.54)
  					(name "BUCK_MODE1")
  					(number "F5")
  				)
  				(pin bidirectional line
  					(at -30.48 17.78 0)
  					(length 2.54)
  					(name "BUCK_MODE2")
  					(number "G4")
  				)
  				(pin power_in line
  					(at -30.48 12.7 0)
  					(length 2.54)
  					(name "VIN_GPIO")
  					(number "E1")
  				)
  				(pin bidirectional line
  					(at -30.48 10.16 0)
  					(length 2.54)
  					(name "GPIO0")
  					(number "C2")
  				)
  				(pin bidirectional line
  					(at -30.48 7.62 0)
  					(length 2.54)
  					(name "GPIO1")
  					(number "D3")
  				)
  				(pin bidirectional line
  					(at -30.48 5.08 0)
  					(length 2.54)
  					(name "GPIO2")
  					(number "D2")
  				)
  				(pin power_in line
  					(at -30.48 0 0)
  					(length 2.54)
  					(name "VDD_TWI")
  					(number "C4")
  				)
  				(pin bidirectional line
  					(at -30.48 -2.54 0)
  					(length 2.54)
  					(name "SDA")
  					(number "E2")
  				)
  				(pin bidirectional line
  					(at -30.48 -5.08 0)
  					(length 2.54)
  					(name "SCL")
  					(number "E3")
  				)
  				(pin power_in line
  					(at 0 48.26 270)
  					(length 2.54)
  					(name "VIN")
  					(number "G1")
  				)
  				(pin power_in line
  					(at 5.08 48.26 270)
  					(length 2.54)
  					(name "VIN_BUCK0")
  					(number "J5")
  				)
  				(pin power_in line
  					(at 7.62 48.26 270)
  					(length 2.54)
  					(name "VIN_BUCK1")
  					(number "A5")
  				)
  				(pin power_in line
  					(at 10.16 48.26 270)
  					(length 2.54)
  					(name "VIN_BUCK2")
  					(number "A1")
  				)
  				(pin power_in line
  					(at 12.7 48.26 270)
  					(length 2.54)
  					(name "VIN_BUCK3")
  					(number "J1")
  				)
  				(pin passive line
  					(at 30.48 33.02 180)
  					(length 2.54)
  					(name "SW0")
  					(number "J4")
  				)
  				(pin passive line
  					(at 30.48 17.78 180)
  					(length 2.54)
  					(name "SW1")
  					(number "A4")
  				)
  				(pin power_out line
  					(at 30.48 12.7 180)
  					(length 2.54)
  					(name "VO1")
  					(number "B5")
  				)
  				(pin passive line
  					(at 30.48 2.54 180)
  					(length 2.54)
  					(name "SW2")
  					(number "A2")
  				)
  				(pin power_out line
  					(at 30.48 -2.54 180)
  					(length 2.54)
  					(name "VO2")
  					(number "B1")
  				)
  				(pin passive line
  					(at 30.48 -12.7 180)
  					(length 2.54)
  					(name "SW3")
  					(number "J2")
  				)
  				(pin passive line
  					(at 30.48 -17.78 180)
  					(length 2.54)
  					(name "VO3")
  					(number "H1")
  				)
  				(pin power_in line
  					(at 30.48 -27.94 180)
  					(length 2.54)
  					(name "VIN_LDO0")
  					(number "C1")
  				)
  				(pin power_out line
  					(at 30.48 -30.48 180)
  					(length 2.54)
  					(name "VLDO0")
  					(number "D1")
  				)
  				(pin power_in line
  					(at 30.48 -33.02 180)
  					(length 2.54)
  					(name "VIN_LDO1")
  					(number "D5")
  				)
  				(pin power_out line
  					(at 30.48 -35.56 180)
  					(length 2.54)
  					(name "VLDO1")
  					(number "C5")
  				)
  			)
  			(symbol "nordic_npm6001_caxx_1_0"
  				(pin output line
  					(at -30.48 30.48 0)
  					(length 2.54)
  					(name "~{INT}")
  					(number "D4")
  				)
  				(pin passive line
  					(at 0 48.26 270)
  					(length 2.54)
  					(hide yes)
  					(name "VIN_ANA")
  					(number "F3")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "AVSS1_2")
  					(number "A3")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "RESERVED")
  					(number "B3")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "RESERVED")
  					(number "E5")
  				)
  				(pin power_in line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(name "VSS")
  					(number "F1")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "AVSS_ANA")
  					(number "F2")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "RESERVED")
  					(number "F4")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "RESERVED")
  					(number "G3")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "RESERVED")
  					(number "H2")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "AVSS0")
  					(number "H3")
  				)
  				(pin passive line
  					(at 0 -48.26 90)
  					(length 2.54)
  					(hide yes)
  					(name "AVSS3")
  					(number "J3")
  				)
  				(pin passive line
  					(at 30.48 27.94 180)
  					(length 2.54)
  					(hide yes)
  					(name "RESERVED")
  					(number "B4")
  				)
  				(pin passive line
  					(at 30.48 27.94 180)
  					(length 2.54)
  					(hide yes)
  					(name "RESERVED")
  					(number "C3")
  				)
  				(pin passive line
  					(at 30.48 27.94 180)
  					(length 2.54)
  					(hide yes)
  					(name "RESERVED")
  					(number "E4")
  				)
  				(pin passive line
  					(at 30.48 27.94 180)
  					(length 2.54)
  					(hide yes)
  					(name "VO0_IN")
  					(number "G5")
  				)
  				(pin power_out line
  					(at 30.48 27.94 180)
  					(length 2.54)
  					(name "VO0")
  					(number "H5")
  				)
  			)
  			(symbol "nordic_npm6001_caxx_1_1")
  			(embedded_fonts no)
  		)
  (symbol "aht10" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "AHT10 Temperature and Humidity Sensor" (at 0 -7.08 0))
        (property "Footprint" "PartReel:aht10"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://components101.com/sites/default/files/component_datasheet/AHT10.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ASAIR AHT10 calibrated digital temperature and humidity sensor, I2C (address 0x38), SMD LGA-6 package 4x5x1.6mm. Land pattern per manufacturer technical manual. Note: 1.8-3.6V supply; single device per I2C bus."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "aht10 asair aosong humidity temperature sensor i2c lga 4x5mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/aht10/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "aht10_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "ADR")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "SDA")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "NC")
          (number "6"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "GND")
          (number "5"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "VDD")
          (number "4"))
      )
    )
  (symbol "aht20" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "AHT20 Humidity and Temperature Sensor" (at 0 -7.08 0))
        (property "Footprint" "PartReel:aht20"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://asairsensors.com/wp-content/uploads/2021/09/Data-Sheet-AHT20-Humidity-and-Temperature-Sensor-ASAIR-V1.0.03.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ASAIR AHT20 calibrated digital humidity and temperature sensor, I2C (address 0x38), SMD LGA-6 package 3x3x1.0mm. Land pattern per manufacturer datasheet."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "aht20 asair aosong humidity temperature sensor i2c lga 3x3mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/aht20/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "aht20_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "NC")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "VDD")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "NC")
          (number "6"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "GND")
          (number "5"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "SDA")
          (number "4"))
      )
    )
  (symbol "aht21" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "AHT21 Humidity and Temperature Sensor" (at 0 -7.08 0))
        (property "Footprint" "PartReel:aht21"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://asairsensors.com/wp-content/uploads/2021/09/Data-Sheet-AHT21-Humidity-and-Temperature-Sensor-ASAIR-V1.0.03.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ASAIR AHT21 calibrated digital humidity and temperature sensor, I2C (address 0x38), SMD LGA-6 package 3x3x0.8mm. Land pattern per manufacturer datasheet (identical to AHT20; 0.2mm lower body)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "aht21 asair aosong humidity temperature sensor i2c lga 3x3mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/aht21/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "aht21_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "NC")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "VDD")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "NC")
          (number "6"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "GND")
          (number "5"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "SDA")
          (number "4"))
      )
    )
  (symbol "aht30" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "AHT30 Humidity and Temperature Sensor" (at 0 -7.08 0))
        (property "Footprint" "PartReel:aht30"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://asairsensors.com/product/aht30-integrated-temperature-and-humidity-sensor/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ASAIR AHT30 calibrated digital humidity and temperature sensor (AHT20 successor), I2C (address 0x38), SMD 3x3x1.0mm. Footprint identical to AHT20 (verified against the AHT30 datasheet Fig.8)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "aht30 asair aosong humidity temperature sensor i2c lga 3x3mm"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/aht30/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "aht30_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "NC")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "VDD")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "SCL")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "NC")
          (number "6"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "GND")
          (number "5"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "SDA")
          (number "4"))
      )
    )
  (symbol "sparkfun_cap1203"
        (property "Footprint" "PartReel:sparkfun_cap1203"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/00001572B.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "3-Channel Capacitive Touch Sensor."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Capacitive Touch Sensor I2C CAP1203"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_cap1203/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 11.43 0)
    		)
    		(property "Value" "CAP1203 (SparkFun)"
    			(at 0 8.89 0)
    		)
    		(property "PROD_ID" "IC-14356"
    			(at 0 -15.24 0)
    		)
    		(symbol "sparkfun_cap1203_1_1"
    			(pin power_in line
    				(at -8.89 6.35 0)
    				(length 2.54)
    				(name "VDD")
    				(number "4")
    			)
    			(pin power_in line
    				(at -8.89 -6.35 0)
    				(length 2.54)
    				(name "GND")
    				(number "5")
    			)
    			(pin open_collector line
    				(at 8.89 6.35 180)
    				(length 2.54)
    				(name "~{ALERT}")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at 8.89 3.81 180)
    				(length 2.54)
    				(name "SDA")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at 8.89 1.27 180)
    				(length 2.54)
    				(name "SCL")
    				(number "3")
    			)
    			(pin passive line
    				(at 8.89 -1.27 180)
    				(length 2.54)
    				(name "CS1")
    				(number "8")
    			)
    			(pin passive line
    				(at 8.89 -3.81 180)
    				(length 2.54)
    				(name "CS2")
    				(number "7")
    			)
    			(pin passive line
    				(at 8.89 -6.35 180)
    				(length 2.54)
    				(name "CS3")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_cy8cmbr3102"
        (property "Footprint" "PartReel:sparkfun_cy8cmbr3102"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.infineon.com/assets/row/public/documents/30/49/infineon-cy8cmbr3002-cy8cmbr3102-cy8cmbr3106s-cy8cmbr3108-cy8cmbr3110-cy8cmbr3116-datasheet-en.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Capacitive Touch Sensor."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_cy8cmbr3102/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 8.89 0)
    		)
    		(property "Value" "CY8CMBR3102 (SparkFun)"
    			(at 0 6.35 0)
    		)
    		(property "PROD_ID" "IC-27515"
    			(at 0 -12.7 0)
    		)
    		(symbol "sparkfun_cy8cmbr3102_1_1"
    			(pin power_in line
    				(at -11.43 3.81 0)
    				(length 2.54)
    				(name "VDD")
    				(number "4")
    			)
    			(pin power_in line
    				(at -11.43 1.27 0)
    				(length 2.54)
    				(name "VCC")
    				(number "3")
    			)
    			(pin passive line
    				(at -11.43 -1.27 0)
    				(length 2.54)
    				(name "CMOD")
    				(number "2")
    			)
    			(pin power_in line
    				(at -11.43 -3.81 0)
    				(length 2.54)
    				(name "GND")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 11.43 3.81 180)
    				(length 2.54)
    				(name "SDA")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at 11.43 1.27 180)
    				(length 2.54)
    				(name "SCL")
    				(number "1")
    			)
    			(pin passive line
    				(at 11.43 -1.27 180)
    				(length 2.54)
    				(name "CS0")
    				(number "7")
    			)
    			(pin passive line
    				(at 11.43 -3.81 180)
    				(length 2.54)
    				(name "GPO0/CS1")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_fpc235x"
        (property "Footprint" "PartReel:sparkfun_fpc235x"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/6585/SPC27317-5%20FPC2530.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "FPC2530 Allkey Pro 100026223‎ Fingerprint Sensor."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Fingerprint Sensor"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_fpc235x/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -8.89 16.51 0)
    		)
    		(property "Value" "FPC235x (SparkFun)"
    			(at 8.89 16.51 0)
    		)
    		(property "PROD_ID" "IC-26955"
    			(at 0.254 -26.924 0)
    		)
    		(symbol "sparkfun_fpc235x_1_0"
    			(pin power_in line
    				(at -12.7 13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "3V3")
    				(number "A2")
    			)
    			(pin power_in line
    				(at -12.7 13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "3V3")
    				(number "A7")
    			)
    			(pin power_in line
    				(at -12.7 13.97 0)
    				(length 2.54)
    				(name "3V3")
    				(number "H2")
    			)
    			(pin power_in line
    				(at -12.7 13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "3V3")
    				(number "H7")
    			)
    			(pin input line
    				(at -12.7 11.43 0)
    				(length 2.54)
    				(name "~{RST}")
    				(number "B6")
    			)
    			(pin bidirectional line
    				(at -12.7 6.35 0)
    				(length 2.54)
    				(name "DP")
    				(number "G6")
    			)
    			(pin bidirectional line
    				(at -12.7 3.81 0)
    				(length 2.54)
    				(name "DM")
    				(number "G5")
    			)
    			(pin input line
    				(at -12.7 -2.54 0)
    				(length 2.54)
    				(name "IF_CFG_1")
    				(number "D7")
    			)
    			(pin input line
    				(at -12.7 -5.08 0)
    				(length 2.54)
    				(name "IF_CFG_2")
    				(number "C7")
    			)
    			(pin power_in line
    				(at -12.7 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "B1")
    			)
    			(pin power_in line
    				(at -12.7 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "B8")
    			)
    			(pin power_in line
    				(at -12.7 -12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "G1")
    			)
    			(pin power_in line
    				(at -12.7 -12.7 0)
    				(length 2.54)
    				(name "GND")
    				(number "G8")
    			)
    			(pin power_in line
    				(at -12.7 -15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "EGND")
    				(number "A1")
    			)
    			(pin power_in line
    				(at -12.7 -15.24 0)
    				(length 2.54)
    				(name "EGND")
    				(number "A8")
    			)
    			(pin power_in line
    				(at -12.7 -15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "EGND")
    				(number "H1")
    			)
    			(pin power_in line
    				(at -12.7 -15.24 0)
    				(length 2.54)
    				(hide yes)
    				(name "EGND")
    				(number "H8")
    			)
    			(pin output line
    				(at 12.7 13.97 180)
    				(length 2.54)
    				(name "IRQ")
    				(number "E7")
    			)
    			(pin output line
    				(at 12.7 11.43 180)
    				(length 2.54)
    				(name "TX")
    				(number "G3")
    			)
    			(pin input line
    				(at 12.7 8.89 180)
    				(length 2.54)
    				(name "RX")
    				(number "G4")
    			)
    			(pin bidirectional line
    				(at 12.7 3.81 180)
    				(length 2.54)
    				(name "SDA")
    				(number "B4")
    			)
    			(pin bidirectional line
    				(at 12.7 1.27 180)
    				(length 2.54)
    				(name "SCL")
    				(number "B5")
    			)
    			(pin input line
    				(at 12.7 -3.81 180)
    				(length 2.54)
    				(name "~{CS}")
    				(number "C2")
    			)
    			(pin input line
    				(at 12.7 -6.35 180)
    				(length 2.54)
    				(name "SCK")
    				(number "E2")
    			)
    			(pin output line
    				(at 12.7 -8.89 180)
    				(length 2.54)
    				(name "POCI")
    				(number "D2")
    			)
    			(pin input line
    				(at 12.7 -11.43 180)
    				(length 2.54)
    				(name "PICO")
    				(number "F2")
    			)
    			(pin bidirectional line
    				(at 12.7 -15.24 180)
    				(length 2.54)
    				(name "GPIO1")
    				(number "B7")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_hmc6343"
        (property "Footprint" "PartReel:sparkfun_hmc6343"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/694/HMC6343.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "HMC6343 is a fully integrated compass module that includes firmware for heading computation and calibration for magnetic distortions."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Digital Compass Qwiic three-axis MEMS"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_hmc6343/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -6.604 9.144 0)
    		)
    		(property "Value" "HMC6343 (SparkFun)"
    			(at -6.35 -9.652 0)
    		)
    		(property "PROD_ID" "IC-12117"
    			(at 0 -20.828 0)
    		)
    		(symbol "sparkfun_hmc6343_1_0"
    			(pin power_in line
    				(at -8.89 6.35 0)
    				(length 2.54)
    				(name "VDD")
    				(number "3")
    			)
    			(pin power_out line
    				(at -8.89 -6.35 0)
    				(length 2.54)
    				(name "GND")
    				(number "29")
    			)
    			(pin bidirectional line
    				(at 8.89 6.35 180)
    				(length 2.54)
    				(name "SCL")
    				(number "32")
    			)
    			(pin bidirectional line
    				(at 8.89 3.81 180)
    				(length 2.54)
    				(name "SDA")
    				(number "36")
    			)
    			(pin bidirectional line
    				(at 8.89 -6.35 180)
    				(length 2.54)
    				(name "DRDY")
    				(number "35")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_hx711"
        (property "Footprint" "PartReel:sparkfun_hx711"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/datasheets/Sensors/ForceFlex/hx711_english.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "24-Bit Analog-to-Digital Converter (ADC) for Weight Scales."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Load cell amplifier"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_hx711/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 5.08 21.59 0)
    		)
    		(property "Value" "HX711 (SparkFun)"
    			(at 7.62 19.05 0)
    		)
    		(property "PROD_ID" "IC-12445"
    			(at 0 -31.75 0)
    		)
    		(property "ki_fp_filters" "SOP*3.9x9.9mm*P1.27mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_hx711_0_1")
    		(symbol "sparkfun_hx711_1_1"
    			(pin passive line
    				(at -12.7 12.7 0)
    				(length 2.54)
    				(name "BASE")
    				(number "2")
    			)
    			(pin power_in line
    				(at -12.7 10.16 0)
    				(length 2.54)
    				(name "AVDD")
    				(number "3")
    			)
    			(pin input line
    				(at -12.7 7.62 0)
    				(length 2.54)
    				(name "VFB")
    				(number "4")
    			)
    			(pin input line
    				(at -12.7 0 0)
    				(length 2.54)
    				(name "INA+")
    				(number "8")
    			)
    			(pin input line
    				(at -12.7 -2.54 0)
    				(length 2.54)
    				(name "INA-")
    				(number "7")
    			)
    			(pin input line
    				(at -12.7 -7.62 0)
    				(length 2.54)
    				(name "INB+")
    				(number "10")
    			)
    			(pin input line
    				(at -12.7 -10.16 0)
    				(length 2.54)
    				(name "INB-")
    				(number "9")
    			)
    			(pin passive line
    				(at -12.7 -15.24 0)
    				(length 2.54)
    				(name "VBG")
    				(number "6")
    			)
    			(pin power_in line
    				(at -2.54 20.32 270)
    				(length 2.54)
    				(name "VSUP")
    				(number "1")
    			)
    			(pin power_in line
    				(at 0 -20.32 90)
    				(length 2.54)
    				(name "AGND")
    				(number "5")
    			)
    			(pin power_in line
    				(at 2.54 20.32 270)
    				(length 2.54)
    				(name "DVDD")
    				(number "16")
    			)
    			(pin output line
    				(at 12.7 7.62 180)
    				(length 2.54)
    				(name "DOUT")
    				(number "12")
    			)
    			(pin input line
    				(at 12.7 5.08 180)
    				(length 2.54)
    				(name "PD_SCK")
    				(number "11")
    			)
    			(pin passive line
    				(at 12.7 0 180)
    				(length 2.54)
    				(name "XO")
    				(number "13")
    			)
    			(pin passive line
    				(at 12.7 -2.54 180)
    				(length 2.54)
    				(name "XI")
    				(number "14")
    			)
    			(pin input line
    				(at 12.7 -10.16 180)
    				(length 2.54)
    				(name "RATE")
    				(number "15")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_im19"
        (property "Footprint" "PartReel:sparkfun_im19"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/6/c/c/a/0/IM19_Product_Integration_Guide_v1.4.1.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "GNSS capable IMU for tilt compensation."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun 9-DoF IMU accelerometer gyroscope magnetometer"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_im19/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 10.16 0)
    		)
    		(property "Value" "IM19 (SparkFun)"
    			(at 0 -10.16 0)
    		)
    		(property "PROD_ID" "IC-26590"
    			(at 0 -15.24 0)
    		)
    		(property "ki_fp_filters" "SOIC*5.23x5.23mm*P1.27mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_im19_0_1")
    		(symbol "sparkfun_im19_1_0"
    			(pin input line
    				(at -11.43 5.08 0)
    				(length 2.54)
    				(name "~{RST}")
    				(number "2")
    			)
    			(pin input line
    				(at -11.43 2.54 0)
    				(length 2.54)
    				(name "BOOT")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at -11.43 0 0)
    				(length 2.54)
    				(name "GPIO")
    				(number "5")
    			)
    			(pin no_connect line
    				(at -11.43 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "SWCLK")
    				(number "20")
    			)
    			(pin no_connect line
    				(at -11.43 -5.08 0)
    				(length 2.54)
    				(hide yes)
    				(name "SWDIO")
    				(number "19")
    			)
    			(pin no_connect line
    				(at 11.43 12.7 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "12")
    			)
    			(pin no_connect line
    				(at 11.43 10.16 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "11")
    			)
    			(pin input line
    				(at 11.43 7.62 180)
    				(length 2.54)
    				(name "1PPS")
    				(number "15")
    			)
    			(pin output line
    				(at 11.43 5.08 180)
    				(length 2.54)
    				(name "UART1_TX")
    				(number "16")
    			)
    			(pin input line
    				(at 11.43 2.54 180)
    				(length 2.54)
    				(name "UART1_RX")
    				(number "17")
    			)
    			(pin input line
    				(at 11.43 -2.54 180)
    				(length 2.54)
    				(name "UART2_RX")
    				(number "8")
    			)
    		)
    		(symbol "sparkfun_im19_1_1"
    			(pin power_in line
    				(at -11.43 7.62 0)
    				(length 2.54)
    				(name "VCC")
    				(number "10")
    			)
    			(pin power_in line
    				(at -11.43 7.62 0)
    				(length 2.54)
    				(hide yes)
    				(name "VCC")
    				(number "6")
    			)
    			(pin power_in line
    				(at -11.43 -7.62 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "18")
    			)
    			(pin power_in line
    				(at -11.43 -7.62 0)
    				(length 2.54)
    				(name "GND")
    				(number "21")
    			)
    			(pin power_in line
    				(at -11.43 -7.62 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "3")
    			)
    			(pin power_in line
    				(at -11.43 -7.62 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "4")
    			)
    			(pin power_in line
    				(at -11.43 -7.62 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "9")
    			)
    			(pin output line
    				(at 11.43 0 180)
    				(length 2.54)
    				(name "UART2_TX")
    				(number "7")
    			)
    			(pin no_connect line
    				(at 11.43 -5.08 180)
    				(length 2.54)
    				(name "NC")
    				(number "14")
    				(alternate "UART3_TX" output line)
    			)
    			(pin no_connect line
    				(at 11.43 -7.62 180)
    				(length 2.54)
    				(name "NC")
    				(number "13")
    				(alternate "UART3_RX" input line)
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_lis3dh"
        (property "Footprint" "PartReel:sparkfun_lis3dh"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.st.com/en/mems-and-sensors/lis3dh.html"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "The LIS3DH has dynamically user-selectable full scales of ±2g/±4g/±8g/±16g and is capable of measuring accelerations with output data rates from 1 Hz to 5.3 kHz."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Accelerometer Triple-Axis Temperature"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_lis3dh/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -10.414 13.462 0)
    		)
    		(property "Value" "LIS3DH (SparkFun)"
    			(at 3.556 14.986 0)
    		)
    		(property "PROD_ID" "IC-13419"
    			(at 0.254 -26.924 0)
    		)
    		(symbol "sparkfun_lis3dh_1_0"
    			(pin power_in line
    				(at -12.7 11.43 0)
    				(length 2.54)
    				(name "VDD")
    				(number "14")
    			)
    			(pin power_in line
    				(at -12.7 8.89 0)
    				(length 2.54)
    				(name "VDDIO")
    				(number "1")
    			)
    			(pin power_in line
    				(at -12.7 6.35 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC2")
    				(number "2")
    			)
    			(pin power_in line
    				(at -12.7 3.81 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC3")
    				(number "3")
    			)
    			(pin bidirectional line
    				(at -12.7 0 0)
    				(length 2.54)
    				(name "RES")
    				(number "10")
    			)
    			(pin power_out line
    				(at -12.7 -13.97 0)
    				(length 2.54)
    				(name "GND")
    				(number "12")
    			)
    			(pin power_out line
    				(at -12.7 -13.97 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 12.7 11.43 180)
    				(length 2.54)
    				(name "~{CS}/MODE")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at 12.7 8.89 180)
    				(length 2.54)
    				(name "SCL/SPC")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at 12.7 6.35 180)
    				(length 2.54)
    				(name "SDA/SDI")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at 12.7 3.81 180)
    				(length 2.54)
    				(name "SA0/SDO")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 12.7 -1.27 180)
    				(length 2.54)
    				(name "INT1")
    				(number "11")
    			)
    			(pin bidirectional line
    				(at 12.7 -3.81 180)
    				(length 2.54)
    				(name "INT2")
    				(number "9")
    			)
    			(pin bidirectional line
    				(at 12.7 -8.89 180)
    				(length 2.54)
    				(name "ADC1")
    				(number "16")
    			)
    			(pin bidirectional line
    				(at 12.7 -11.43 180)
    				(length 2.54)
    				(name "ADC2")
    				(number "15")
    			)
    			(pin bidirectional line
    				(at 12.7 -13.97 180)
    				(length 2.54)
    				(name "ADC3")
    				(number "13")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_lsm6dsox"
        (property "Footprint" "PartReel:sparkfun_lsm6dsox"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.st.com/resource/en/datasheet/lsm6dsox.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "6-DoF IMU."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun 6-DoF IMU accelerometer gyroscope"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_lsm6dsox/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 11.43 0)
    		)
    		(property "Value" "LSM6DSOX (SparkFun)"
    			(at 0 -11.43 0)
    		)
    		(property "PROD_ID" "IC-18009"
    			(at 0 -19.05 0)
    		)
    		(property "ki_fp_filters" "SOIC*5.23x5.23mm*P1.27mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_lsm6dsox_0_1")
    		(symbol "sparkfun_lsm6dsox_1_0"
    			(pin bidirectional line
    				(at 10.16 8.89 180)
    				(length 2.54)
    				(name "SDA")
    				(number "14")
    			)
    			(pin bidirectional line
    				(at 10.16 6.35 180)
    				(length 2.54)
    				(name "SCL")
    				(number "13")
    			)
    			(pin bidirectional line
    				(at 10.16 1.27 180)
    				(length 2.54)
    				(name "~{CS}")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at 10.16 -6.35 180)
    				(length 2.54)
    				(name "OCS_Aux")
    				(number "10")
    			)
    			(pin bidirectional line
    				(at 10.16 -8.89 180)
    				(length 2.54)
    				(name "SDO_Aux")
    				(number "11")
    			)
    		)
    		(symbol "sparkfun_lsm6dsox_1_1"
    			(pin power_in line
    				(at -10.16 8.89 0)
    				(length 2.54)
    				(name "VDD")
    				(number "8")
    			)
    			(pin power_in line
    				(at -10.16 6.35 0)
    				(length 2.54)
    				(name "VDDIO")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at -10.16 1.27 0)
    				(length 2.54)
    				(name "INT1")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at -10.16 -1.27 0)
    				(length 2.54)
    				(name "INT2")
    				(number "9")
    			)
    			(pin power_in line
    				(at -10.16 -8.89 0)
    				(length 2.54)
    				(name "GND")
    				(number "6")
    			)
    			(pin power_in line
    				(at -10.16 -8.89 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 10.16 3.81 180)
    				(length 2.54)
    				(name "SDO/SA0")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at 10.16 -1.27 180)
    				(length 2.54)
    				(name "SDx")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at 10.16 -3.81 180)
    				(length 2.54)
    				(name "SCx")
    				(number "3")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_mpr121qr2"
        (property "Footprint" "PartReel:sparkfun_mpr121qr2"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MPR121.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "The MPR121 is the second generation sensor controller after the release of the MPR03x series devices."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun Capacitive Sensor"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_mpr121qr2/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -9.398 19.05 0)
    		)
    		(property "Value" "MPR121QR2 (SparkFun)"
    			(at 6.604 19.304 0)
    		)
    		(property "PROD_ID" "IC-09490"
    			(at 0 -33.02 0)
    		)
    		(symbol "sparkfun_mpr121qr2_0_1")
    		(symbol "sparkfun_mpr121qr2_1_1"
    			(pin bidirectional line
    				(at -12.7 15.24 0)
    				(length 2.54)
    				(name "SDA")
    				(number "3")
    			)
    			(pin input line
    				(at -12.7 12.7 0)
    				(length 2.54)
    				(name "SCL")
    				(number "2")
    			)
    			(pin open_collector line
    				(at -12.7 10.16 0)
    				(length 2.54)
    				(name "~{IRQ}")
    				(number "1")
    			)
    			(pin input line
    				(at -12.7 -7.62 0)
    				(length 2.54)
    				(name "ADDR")
    				(number "4")
    			)
    			(pin passive line
    				(at -12.7 -10.16 0)
    				(length 2.54)
    				(name "VREG")
    				(number "5")
    			)
    			(pin passive line
    				(at -12.7 -12.7 0)
    				(length 2.54)
    				(name "REXT")
    				(number "7")
    			)
    			(pin power_in line
    				(at 0 20.955 270)
    				(length 2.54)
    				(name "VDD")
    				(number "20")
    			)
    			(pin power_in line
    				(at 0 -21.59 90)
    				(length 2.54)
    				(name "VSS")
    				(number "6")
    			)
    			(pin passive line
    				(at 12.7 15.24 180)
    				(length 2.54)
    				(name "ELE0")
    				(number "8")
    			)
    			(pin passive line
    				(at 12.7 12.7 180)
    				(length 2.54)
    				(name "ELE1")
    				(number "9")
    			)
    			(pin passive line
    				(at 12.7 10.16 180)
    				(length 2.54)
    				(name "ELE2")
    				(number "10")
    			)
    			(pin passive line
    				(at 12.7 7.62 180)
    				(length 2.54)
    				(name "ELE3")
    				(number "11")
    			)
    			(pin passive line
    				(at 12.7 5.08 180)
    				(length 2.54)
    				(name "LED0/ELE4")
    				(number "12")
    			)
    			(pin passive line
    				(at 12.7 2.54 180)
    				(length 2.54)
    				(name "LED1/ELE5")
    				(number "13")
    			)
    			(pin passive line
    				(at 12.7 0 180)
    				(length 2.54)
    				(name "LED2/ELE6")
    				(number "14")
    			)
    			(pin passive line
    				(at 12.7 -2.54 180)
    				(length 2.54)
    				(name "LED3/ELE7")
    				(number "15")
    			)
    			(pin passive line
    				(at 12.7 -5.08 180)
    				(length 2.54)
    				(name "LED4/ELE8")
    				(number "16")
    			)
    			(pin passive line
    				(at 12.7 -7.62 180)
    				(length 2.54)
    				(name "LED5/ELE9")
    				(number "17")
    			)
    			(pin passive line
    				(at 12.7 -10.16 180)
    				(length 2.54)
    				(name "LED6/ELE10")
    				(number "18")
    			)
    			(pin passive line
    				(at 12.7 -12.7 180)
    				(length 2.54)
    				(name "LED7/ELE11")
    				(number "19")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_mpu_6050"
        (property "Footprint" "PartReel:sparkfun_mpu_6050"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://invensense.tdk.com/wp-content/uploads/2015/02/MPU-6000-Datasheet1.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "InvenSense 6-Axis Motion Sensor, Gyroscope, Accelerometer, I2C."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun mems IMU"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_mpu_6050/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -11.43 15.24 0)
    		)
    		(property "Value" "MPU-6050 (SparkFun)"
    			(at 7.62 -15.24 0)
    		)
    		(property "PROD_ID" "IC-10756"
    			(at 0 -27.94 0)
    		)
    		(property "ki_fp_filters" "*QFN*4x4mm*P0.5mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_mpu_6050_0_0"
    			(text ""
    				(at 12.7 -2.54 0)
    			)
    		)
    		(symbol "sparkfun_mpu_6050_0_1")
    		(symbol "sparkfun_mpu_6050_1_1"
    			(pin bidirectional line
    				(at -17.78 7.62 0)
    				(length 5.08)
    				(name "SDA")
    				(number "24")
    			)
    			(pin input line
    				(at -17.78 5.08 0)
    				(length 5.08)
    				(name "SCL")
    				(number "23")
    			)
    			(pin input line
    				(at -17.78 2.54 0)
    				(length 5.08)
    				(name "AD0")
    				(number "9")
    			)
    			(pin input line
    				(at -17.78 -5.08 0)
    				(length 5.08)
    				(name "FSYNC")
    				(number "11")
    			)
    			(pin input clock
    				(at -17.78 -7.62 0)
    				(length 5.08)
    				(name "CLKIN")
    				(number "1")
    			)
    			(pin no_connect line
    				(at -12.7 12.7 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "2")
    			)
    			(pin no_connect line
    				(at -12.7 10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "3")
    			)
    			(pin no_connect line
    				(at -12.7 0 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "4")
    			)
    			(pin no_connect line
    				(at -12.7 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "5")
    			)
    			(pin no_connect line
    				(at -12.7 -10.16 0)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "14")
    			)
    			(pin power_in line
    				(at -2.54 17.78 270)
    				(length 3.81)
    				(name "VLOGIC")
    				(number "8")
    			)
    			(pin power_in line
    				(at 0 -17.78 90)
    				(length 3.81)
    				(name "GND")
    				(number "18")
    			)
    			(pin power_in line
    				(at 2.54 17.78 270)
    				(length 3.81)
    				(name "VDD")
    				(number "13")
    			)
    			(pin no_connect line
    				(at 12.7 12.7 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "15")
    			)
    			(pin no_connect line
    				(at 12.7 10.16 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "16")
    			)
    			(pin no_connect line
    				(at 12.7 5.08 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "17")
    			)
    			(pin no_connect line
    				(at 12.7 -2.54 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESV")
    				(number "21")
    			)
    			(pin no_connect line
    				(at 12.7 -10.16 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESV")
    				(number "19")
    			)
    			(pin no_connect line
    				(at 12.7 -12.7 180)
    				(length 2.54)
    				(hide yes)
    				(name "RESV")
    				(number "22")
    			)
    			(pin output line
    				(at 17.78 7.62 180)
    				(length 5.08)
    				(name "INT")
    				(number "12")
    			)
    			(pin bidirectional line
    				(at 17.78 2.54 180)
    				(length 5.08)
    				(name "AUX_DA")
    				(number "6")
    			)
    			(pin output clock
    				(at 17.78 0 180)
    				(length 5.08)
    				(name "AUX_CL")
    				(number "7")
    			)
    			(pin passive line
    				(at 17.78 -5.08 180)
    				(length 5.08)
    				(name "CPOUT")
    				(number "20")
    			)
    			(pin passive line
    				(at 17.78 -7.62 180)
    				(length 5.08)
    				(name "REGOUT")
    				(number "10")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_ms8607_02ba"
        (property "Footprint" "PartReel:sparkfun_ms8607_02ba"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=MS8607-02BA01&DocType=Data%20Sheet&DocLang=English&DocFormat=pdf&PartCntxt=CAT-BLPS0018"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "The MS8607 is a low power digital sensor providing 3 environmental physical measurements all-in-one: pressure, humidity and temperature (PHT)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun Pressure Temperrature Humidity I2C"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_ms8607_02ba/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -6.35 7.62 0)
    		)
    		(property "Value" "MS8607-02BA (SparkFun)"
    			(at 7.62 7.62 0)
    		)
    		(property "PROD_ID" "IC-15048"
    			(at 0 -27.94 0)
    		)
    		(property "ki_fp_filters" "LGA*3x5mm*P1.25mm*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_ms8607_02ba_0_1")
    		(symbol "sparkfun_ms8607_02ba_1_1"
    			(pin bidirectional line
    				(at -8.89 1.27 0)
    				(length 2.54)
    				(name "SDA")
    				(number "7")
    			)
    			(pin input line
    				(at -8.89 -1.27 0)
    				(length 2.54)
    				(name "SCL")
    				(number "8")
    			)
    			(pin power_in line
    				(at 0 8.89 270)
    				(length 2.54)
    				(name "VDD")
    				(number "1")
    			)
    			(pin power_in line
    				(at 0 -8.89 90)
    				(length 2.54)
    				(name "GND")
    				(number "3")
    			)
    			(pin no_connect line
    				(at 8.89 3.81 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "2")
    			)
    			(pin no_connect line
    				(at 8.89 1.27 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "4")
    			)
    			(pin no_connect line
    				(at 8.89 -1.27 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "5")
    			)
    			(pin no_connect line
    				(at 8.89 -3.81 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_scd41"
        (property "Footprint" "PartReel:sparkfun_scd41"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn.sparkfun.com/assets/d/4/9/a/d/Sensirion_CO2_Sensors_SCD4x_Datasheet.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Photoacoustic CO2 Sensor."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun I2C ±(40 ppm + 5 %)"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_scd41/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -6.35 5.715 0)
    		)
    		(property "Value" "SCD41 (SparkFun)"
    			(at -2.54 5.715 0)
    		)
    		(property "PROD_ID" "IC-16053"
    			(at 0 -6.35 0)
    		)
    		(property "ki_fp_filters" "SOT?23*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_scd41_0_1")
    		(symbol "sparkfun_scd41_1_1"
    			(pin power_in line
    				(at -8.89 2.54 0)
    				(length 2.54)
    				(name "VDD")
    				(number "7")
    			)
    			(pin power_in line
    				(at -8.89 0 0)
    				(length 2.54)
    				(name "VDDH")
    				(number "19")
    			)
    			(pin power_in line
    				(at -8.89 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "20")
    			)
    			(pin power_in line
    				(at -8.89 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "21")
    			)
    			(pin power_in line
    				(at -8.89 -2.54 0)
    				(length 2.54)
    				(name "GND")
    				(number "6")
    			)
    			(pin no_connect line
    				(at 8.89 39.37 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "18")
    			)
    			(pin no_connect line
    				(at 8.89 36.83 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "17")
    			)
    			(pin no_connect line
    				(at 8.89 34.29 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "16")
    			)
    			(pin no_connect line
    				(at 8.89 31.75 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "15")
    			)
    			(pin no_connect line
    				(at 8.89 29.21 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "14")
    			)
    			(pin no_connect line
    				(at 8.89 26.67 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "13")
    			)
    			(pin no_connect line
    				(at 8.89 24.13 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "12")
    			)
    			(pin no_connect line
    				(at 8.89 21.59 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "11")
    			)
    			(pin no_connect line
    				(at 8.89 19.05 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "8")
    			)
    			(pin no_connect line
    				(at 8.89 16.51 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "5")
    			)
    			(pin no_connect line
    				(at 8.89 13.97 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "4")
    			)
    			(pin no_connect line
    				(at 8.89 11.43 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "3")
    			)
    			(pin no_connect line
    				(at 8.89 8.89 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "2")
    			)
    			(pin no_connect line
    				(at 8.89 6.35 180)
    				(length 2.54)
    				(hide yes)
    				(name "NC")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at 8.89 2.54 180)
    				(length 2.54)
    				(name "SDA")
    				(number "10")
    			)
    			(pin input line
    				(at 8.89 0 180)
    				(length 2.54)
    				(name "SCL")
    				(number "9")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_sht40"
        (property "Footprint" "PartReel:sparkfun_sht40"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://sensirion.com/media/documents/33FD6951/624C4357/Datasheet_SHT4x.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Digital Humidity and Temperature Sensor, ±1%RH, ±0.1°C, I2C, 1.08-3.6V, 16bit, DFN-4."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun Sensirion environment environmental measurement digital SHT40 SHT41 SHT45"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_sht40/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -3.81 5.08 0)
    		)
    		(property "Value" "SHT40 (SparkFun)"
    			(at 2.54 5.08 0)
    		)
    		(property "PROD_ID" "IC-..."
    			(at 0 -13.97 0)
    		)
    		(property "ki_fp_filters" "Sensirion?DFN*1.5x1.5mm*P0.8mm*SHT4x*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_sht40_1_1"
    			(pin power_in line
    				(at -7.62 2.54 0)
    				(length 2.54)
    				(name "VDD")
    				(number "3")
    			)
    			(pin power_in line
    				(at -7.62 -2.54 0)
    				(length 2.54)
    				(name "VSS")
    				(number "4")
    			)
    			(pin input line
    				(at 7.62 2.54 180)
    				(length 2.54)
    				(name "SCL")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at 7.62 -2.54 180)
    				(length 2.54)
    				(name "SDA")
    				(number "1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_shtc3"
        (property "Footprint" "PartReel:sparkfun_shtc3"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://sensirion.com/media/documents/643F9C8E/63A5A436/Datasheet_SHTC3.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "The SHTC3 is a digital humidity and temperature sensor designed especially for battery-driven high-volume consumer electronics applications."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_shtc3/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -6.858 6.096 0)
    		)
    		(property "Value" "SHTC3 (SparkFun)"
    			(at 4.572 6.35 0)
    		)
    		(property "PROD_ID" "IC-14840"
    			(at 0 -19.812 0)
    		)
    		(symbol "sparkfun_shtc3_1_0"
    			(pin bidirectional line
    				(at -10.16 2.54 0)
    				(length 2.54)
    				(name "VDD")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "VSS")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at 10.16 2.54 180)
    				(length 2.54)
    				(name "SCL")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at 10.16 -2.54 180)
    				(length 2.54)
    				(name "SDA")
    				(number "3")
    			)
    		)
    		(symbol "sparkfun_shtc3_1_1")
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_stc31"
        (property "Footprint" "PartReel:sparkfun_stc31"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://sensirion.com/media/documents/7B1D0EA7/61652CD0/Sensirion_Thermal_Conductivity_Datasheet_STC31_D1_1.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "The STC3x sensor family is Sensirion’s series of Gas Concentration sensors designed for high-volume applications. The STC3x utilizes a revolutionized thermal conductivity measurement principle, which results in superior repeatability and long-term stability. This make the STC31 a perfect choice for applications where reliability is key."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun CO2 Sensor"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_stc31/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -6.604 6.096 0)
    		)
    		(property "Value" "STC31 (SparkFun)"
    			(at 4.826 6.096 0)
    		)
    		(property "PROD_ID" "IC-16076"
    			(at 0.254 -19.812 0)
    		)
    		(symbol "sparkfun_stc31_1_0"
    			(pin power_in line
    				(at -10.16 2.54 0)
    				(length 2.54)
    				(name "VDD")
    				(number "6")
    			)
    			(pin bidirectional line
    				(at -10.16 0 0)
    				(length 2.54)
    				(name "ADDR")
    				(number "3")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "11")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "5")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(hide yes)
    				(name "GND")
    				(number "9")
    			)
    			(pin bidirectional line
    				(at 10.16 2.54 180)
    				(length 2.54)
    				(name "SCL")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at 10.16 -2.54 180)
    				(length 2.54)
    				(name "SDA")
    				(number "7")
    			)
    		)
    		(symbol "sparkfun_stc31_1_1")
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_stcc4"
        (property "Footprint" "PartReel:sparkfun_stcc4"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://sensirion.com/media/documents/6AED4B15/684A889C/CD_DS_STCC4_D1_3.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "The STCC4 is Sensirion’s next generation miniature CO2 sensor for indoor air quality applications."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun CO2 Sensor"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_stcc4/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -6.604 4.826 0)
    		)
    		(property "Value" "STCC4 (SparkFun)"
    			(at 4.826 4.826 0)
    		)
    		(property "PROD_ID" "IC-..."
    			(at 0 -15.24 0)
    		)
    		(symbol "sparkfun_stcc4_1_0"
    			(pin power_in line
    				(at -10.16 2.54 0)
    				(length 2.54)
    				(name "VDD_IO")
    				(number "6")
    			)
    			(pin power_in line
    				(at -10.16 0 0)
    				(length 2.54)
    				(name "VDD")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "ADDR")
    				(number "3")
    			)
    			(pin power_in line
    				(at -10.16 -5.08 0)
    				(length 2.54)
    				(name "GND")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at 10.16 2.54 180)
    				(length 2.54)
    				(name "SCL")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at 10.16 0 180)
    				(length 2.54)
    				(name "SDA")
    				(number "5")
    			)
    			(pin bidirectional line
    				(at 10.16 -2.54 180)
    				(length 2.54)
    				(name "SCL_C")
    				(number "8")
    			)
    			(pin bidirectional line
    				(at 10.16 -5.08 180)
    				(length 2.54)
    				(name "SDA_C")
    				(number "2")
    			)
    		)
    		(symbol "sparkfun_stcc4_1_1")
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_tmp102"
        (property "Footprint" "PartReel:sparkfun_tmp102"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ti.com/lit/ds/symlink/tmp102.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Digital Temperature Sensor, ±3°C, low-Power, SMBus, 12 bit, Two-Wire Serial Interface, SOT-563."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun digital temperature sensor i2c smbus"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_tmp102/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at -2.54 10.795 0)
    		)
    		(property "Value" "TMP102 (SparkFun)"
    			(at -2.54 8.89 0)
    		)
    		(property "PROD_ID" "IC-09303"
    			(at 0 -20.32 0)
    		)
    		(property "ki_fp_filters" "SOT?563*"
    			(at 0 0 0)
    		)
    		(symbol "sparkfun_tmp102_0_1")
    		(symbol "sparkfun_tmp102_1_1"
    			(pin open_collector line
    				(at -10.16 5.08 0)
    				(length 2.54)
    				(name "ALERT")
    				(number "3")
    			)
    			(pin power_in line
    				(at 0 10.16 270)
    				(length 2.54)
    				(name "V+")
    				(number "5")
    			)
    			(pin power_in line
    				(at 0 -10.16 90)
    				(length 2.54)
    				(name "GND")
    				(number "2")
    			)
    			(pin bidirectional line
    				(at 10.16 5.08 180)
    				(length 2.54)
    				(name "SDA")
    				(number "6")
    			)
    			(pin input line
    				(at 10.16 2.54 180)
    				(length 2.54)
    				(name "SCL")
    				(number "1")
    			)
    			(pin input line
    				(at 10.16 -2.54 180)
    				(length 2.54)
    				(name "ADD0")
    				(number "4")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_vcnl4040"
        (property "Footprint" "PartReel:sparkfun_vcnl4040"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.vishay.com/docs/84274/vcnl4040.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Vishay VCNL4040 Human Presence sensor."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun SparkFun distance presence sensor"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_vcnl4040/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 10.16 0)
    		)
    		(property "Value" "VCNL4040 (SparkFun)"
    			(at 0 7.62 0)
    		)
    		(symbol "sparkfun_vcnl4040_1_0"
    			(pin power_in line
    				(at -12.7 5.08 0)
    				(length 2.54)
    				(name "VDD")
    				(number "3")
    			)
    			(pin bidirectional line
    				(at -12.7 2.54 0)
    				(length 2.54)
    				(name "ANODE")
    				(number "4")
    			)
    			(pin input line
    				(at -12.7 0 0)
    				(length 2.54)
    				(name "CATHODE_LED")
    				(number "5")
    			)
    			(pin output line
    				(at -12.7 -2.54 0)
    				(length 2.54)
    				(name "CATHODE_SEN")
    				(number "2")
    			)
    			(pin power_in line
    				(at -12.7 -5.08 0)
    				(length 2.54)
    				(name "GND")
    				(number "1")
    			)
    			(pin bidirectional line
    				(at 12.7 5.08 180)
    				(length 2.54)
    				(name "SDA")
    				(number "7")
    			)
    			(pin bidirectional line
    				(at 12.7 2.54 180)
    				(length 2.54)
    				(name "SCL")
    				(number "8")
    			)
    			(pin output line
    				(at 12.7 -2.54 180)
    				(length 2.54)
    				(name "~{INT}")
    				(number "6")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "sparkfun_veml7700_tt"
        (property "Footprint" "PartReel:sparkfun_veml7700_tt"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.vishay.com/docs/84286/veml7700.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "VEML7700 is a high accuracy ambient light digital 16-bit resolution sensor in a miniature transparent 6.8 mm x 2.35 mm x 3.0 mm package."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sparkfun Ambient Light Sensor"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sparkfun_veml7700_tt/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
    		(exclude_from_sim no)
    		(in_bom yes)
    		(on_board yes)
    		(property "Reference" "U"
    			(at 0 6.35 0)
    		)
    		(property "Value" "VEML7700-TT (SparkFun)"
    			(at 0 -7.112 0)
    		)
    		(property "PROD_ID" "IC-16311"
    			(at 0 -18.542 0)
    		)
    		(symbol "sparkfun_veml7700_tt_1_0"
    			(pin power_in line
    				(at -10.16 2.54 0)
    				(length 2.54)
    				(name "VDD")
    				(number "2")
    			)
    			(pin power_in line
    				(at -10.16 -2.54 0)
    				(length 2.54)
    				(name "GND")
    				(number "3")
    			)
    			(pin bidirectional line
    				(at 10.16 2.54 180)
    				(length 2.54)
    				(name "SDA")
    				(number "4")
    			)
    			(pin bidirectional line
    				(at 10.16 -2.54 180)
    				(length 2.54)
    				(name "SCL")
    				(number "1")
    			)
    		)
    		(embedded_fonts no)
    	)
  (symbol "adxl345" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 12.16 0))
      (property "Value" "ADXL345 3-Axis Accelerometer" (at 0 -12.16 0))
        (property "Footprint" "PartReel:adxl345"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://components101.com/sites/default/files/component_datasheet/ADXL345-Datasheet.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Analog Devices ADXL345 3-axis digital accelerometer, SPI/I2C (0x1D or 0x53), LGA-14 3x5x0.95mm. Land pattern per ADI datasheet. CS and ALT_ADDR must not float."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "adxl345 accelerometer 3-axis spi i2c adi gy-291 lga"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/adxl345/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "adxl345_1_1"
        (pin passive line (at -13.14 7.62 0) (length 2.54)
          (name "VDD_IO")
          (number "1"))
        (pin passive line (at -13.14 5.08 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -13.14 2.54 0) (length 2.54)
          (name "RESERVED")
          (number "3"))
        (pin passive line (at -13.14 0.00 0) (length 2.54)
          (name "GND")
          (number "4"))
        (pin passive line (at -13.14 -2.54 0) (length 2.54)
          (name "GND")
          (number "5"))
        (pin passive line (at -13.14 -5.08 0) (length 2.54)
          (name "VS")
          (number "6"))
        (pin passive line (at -13.14 -7.62 0) (length 2.54)
          (name "~CS")
          (number "7"))
        (pin passive line (at 13.14 7.62 180) (length 2.54)
          (name "INT1")
          (number "8"))
        (pin passive line (at 13.14 5.08 180) (length 2.54)
          (name "INT2")
          (number "9"))
        (pin passive line (at 13.14 2.54 180) (length 2.54)
          (name "NC")
          (number "10"))
        (pin passive line (at 13.14 0.00 180) (length 2.54)
          (name "RESERVED")
          (number "11"))
        (pin passive line (at 13.14 -2.54 180) (length 2.54)
          (name "SDO/ALT_ADDR")
          (number "12"))
        (pin passive line (at 13.14 -5.08 180) (length 2.54)
          (name "SDA/SDI/SDIO")
          (number "13"))
        (pin passive line (at 13.14 -7.62 180) (length 2.54)
          (name "SCL/SCLK")
          (number "14"))
      )
    )
  (symbol "sgp40" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "SGP40 VOC Air Quality Sensor" (at 0 -9.62 0))
        (property "Footprint" "PartReel:sgp40"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://sensirion.com/media/documents/296373BB/6203C5DF/Sensirion_Gas_Sensors_Datasheet_SGP40.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Sensirion SGP40 digital VOC sensor for air quality, I2C 0x59, 1.7-3.6V (VDD and VDDH must share one supply), DFN-6 with sensing opening on top (do not cover). Die pad = GND, soldering recommended."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "sgp40 sensirion voc gas air quality i2c dfn"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/sgp40/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "sgp40_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "VDD")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "VSS")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "SDA")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "n/a(GND)")
          (number "4"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "VDDH")
          (number "5"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "SCL")
          (number "6"))
        (pin passive line (at 0.00 -10.16 90) (length 2.54)
          (name "DIE/GND")
          (number "7"))
      )
    )
  (symbol "aht25" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "AHT25 Humidity and Temperature Sensor Module" (at 0 -8.35 0))
        (property "Footprint" "PartReel:aht25"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.aosong.com/userfiles/files/media/Data%20Sheet%20AHT25%20A2.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ASAIR AHT25 humidity/temperature sensor - a small dumbbell-shaped PCB module with 4 gold-finger solder tabs (not a molded IC). I2C 0x38, 2.2-5.5V."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "aht25 asair humidity temperature i2c module"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/aht25/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "aht25_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "VDD")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SDA")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SCL")
          (number "4"))
      )
    )
  (symbol "dht20" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 8.35 0))
      (property "Value" "DHT20 Temperature & Humidity Sensor (DHT Housing)" (at 0 -8.35 0))
        (property "Footprint" "PartReel:dht20"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://aqicn.org/air/sensor/spec/asair-dht20.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "ASAIR DHT20 - the AHT20 die in a classic DHT-style 4-pin housing. I2C interface (address 0x38), 2.2-5.5V. Drop-in mechanical replacement for DHT11/DHT22 boards but NOT protocol-compatible (I2C, not 1-wire)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "dht20 asair aht20 humidity temperature i2c dht22"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/dht20/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "dht20_1_1"
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "VDD")
          (number "1"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SDA")
          (number "2"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "GND")
          (number "3"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "SCL")
          (number "4"))
      )
    )
  (symbol "hmc5883l" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "HMC5883L 3-Axis Magnetometer" (at 0 -13.43 0))
        (property "Footprint" "PartReel:hmc5883l"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/HMC5883L_3-Axis_Digital_Compass_IC.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Honeywell HMC5883L 3-axis magnetic sensor (compass), I2C address 0x1E, LGA-16 3x3x0.9mm. Land pattern per manufacturer datasheet. S1 must tie to VDDIO; C1 reservoir capacitor required."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "hmc5883l honeywell magnetometer compass 3-axis i2c gy-273 lcc"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/hmc5883l/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "hmc5883l_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "SCL")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "VDD")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "NC")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "S1")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "NC")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "NC")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "NC")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "SETP")
          (number "8"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "GND")
          (number "9"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "C1")
          (number "10"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "GND")
          (number "11"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "SETC")
          (number "12"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "VDDIO")
          (number "13"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "NC")
          (number "14"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "DRDY")
          (number "15"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "SDA")
          (number "16"))
      )
    )
  (symbol "qmc5883l" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "QMC5883L 3-Axis Magnetometer" (at 0 -13.43 0))
        (property "Footprint" "PartReel:qmc5883l"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://nettigo.pl/attachments/440"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "QST QMC5883L 3-axis magnetic sensor (compass), I2C address 0x0D, LGA-16 3x3x0.9mm. Land pattern per manufacturer datasheet. S1 must tie to VDDIO; C1 reservoir capacitor required."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "qmc5883l qst magnetometer compass 3-axis i2c gy-271 lga"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/qmc5883l/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "qmc5883l_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "SCL")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "VDD")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "NC")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "S1")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "NC")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "NC")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "NC")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "SETP")
          (number "8"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "GND")
          (number "9"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "C1")
          (number "10"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "GND")
          (number "11"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "SETC")
          (number "12"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "VDDIO")
          (number "13"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "NC")
          (number "14"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "DRDY")
          (number "15"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "SDA")
          (number "16"))
      )
    )
  (symbol "qmc5883p" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 13.43 0))
      (property "Value" "QMC5883P 3-Axis Magnetometer" (at 0 -13.43 0))
        (property "Footprint" "PartReel:qmc5883p"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.qstcorp.com/upload/pdf/202202/%EF%BC%88%E5%B7%B2%E4%BC%A0%EF%BC%8913-52-19%20QMC5883P%20Datasheet%20Rev.C(1).pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "QST QMC5883P 3-axis magnetic sensor - the chip on NEW GY-271 boards, I2C address 0x2C, LGA-16 3x3x0.9mm. NOT register- or pinout-compatible with QMC5883L (only 6 active pads: SCK/VDD/GND/C1/GND/SDA). C1 4.7uF reservoir capacitor required."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "qmc5883p qst magnetometer compass i2c gy-271 lga"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/qmc5883p/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "qmc5883p_1_1"
        (pin passive line (at -11.43 8.89 0) (length 2.54)
          (name "SCK")
          (number "1"))
        (pin passive line (at -11.43 6.35 0) (length 2.54)
          (name "VDD")
          (number "2"))
        (pin passive line (at -11.43 3.81 0) (length 2.54)
          (name "NC")
          (number "3"))
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "NC")
          (number "4"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "NC")
          (number "5"))
        (pin passive line (at -11.43 -3.81 0) (length 2.54)
          (name "NC")
          (number "6"))
        (pin passive line (at -11.43 -6.35 0) (length 2.54)
          (name "NC")
          (number "7"))
        (pin passive line (at -11.43 -8.89 0) (length 2.54)
          (name "NC")
          (number "8"))
        (pin passive line (at 11.43 8.89 180) (length 2.54)
          (name "GND")
          (number "9"))
        (pin passive line (at 11.43 6.35 180) (length 2.54)
          (name "C1")
          (number "10"))
        (pin passive line (at 11.43 3.81 180) (length 2.54)
          (name "GND")
          (number "11"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "NC")
          (number "12"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "NC")
          (number "13"))
        (pin passive line (at 11.43 -3.81 180) (length 2.54)
          (name "NC")
          (number "14"))
        (pin passive line (at 11.43 -6.35 180) (length 2.54)
          (name "NC")
          (number "15"))
        (pin passive line (at 11.43 -8.89 180) (length 2.54)
          (name "SDA")
          (number "16"))
      )
    )
  (symbol "bno085" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 21.05 0))
      (property "Value" "BNO085 9-DOF Sensor Fusion IMU" (at 0 -21.05 0))
        (property "Footprint" "PartReel:bno085"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.ceva-ip.com/wp-content/uploads/BNO080_085-Datasheet.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "CEVA BNO085 9-DOF IMU with on-chip sensor fusion (quaternion output) - Adafruit/SparkFun flagship IMU. Host interface selected by PS1/PS0: I2C 0x4A/0x4B, SPI, or UART. VDD 2.4-3.6V, LGA-28 5.2x3.8. Needs 32.768kHz crystal or CLKSEL strap."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "bno085 bno080 ceva hillcrest imu 9-dof fusion quaternion lga"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/bno085/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "bno085_1_1"
        (pin passive line (at -14.49 16.51 0) (length 2.54)
          (name "RESV_NC")
          (number "1"))
        (pin passive line (at -14.49 13.97 0) (length 2.54)
          (name "GND")
          (number "2"))
        (pin passive line (at -14.49 11.43 0) (length 2.54)
          (name "VDD")
          (number "3"))
        (pin passive line (at -14.49 8.89 0) (length 2.54)
          (name "BOOTN")
          (number "4"))
        (pin passive line (at -14.49 6.35 0) (length 2.54)
          (name "PS1")
          (number "5"))
        (pin passive line (at -14.49 3.81 0) (length 2.54)
          (name "PS0/WAKE")
          (number "6"))
        (pin passive line (at -14.49 1.27 0) (length 2.54)
          (name "RESV_NC")
          (number "7"))
        (pin passive line (at -14.49 -1.27 0) (length 2.54)
          (name "RESV_NC")
          (number "8"))
        (pin passive line (at -14.49 -3.81 0) (length 2.54)
          (name "CAP")
          (number "9"))
        (pin passive line (at -14.49 -6.35 0) (length 2.54)
          (name "CLKSEL0")
          (number "10"))
        (pin passive line (at -14.49 -8.89 0) (length 2.54)
          (name "NRST")
          (number "11"))
        (pin passive line (at -14.49 -11.43 0) (length 2.54)
          (name "RESV_NC")
          (number "12"))
        (pin passive line (at -14.49 -13.97 0) (length 2.54)
          (name "RESV_NC")
          (number "13"))
        (pin passive line (at -14.49 -16.51 0) (length 2.54)
          (name "H_INTN")
          (number "14"))
        (pin passive line (at 14.49 16.51 180) (length 2.54)
          (name "ENV_SCL")
          (number "15"))
        (pin passive line (at 14.49 13.97 180) (length 2.54)
          (name "ENV_SDA")
          (number "16"))
        (pin passive line (at 14.49 11.43 180) (length 2.54)
          (name "SA0/H_MOSI")
          (number "17"))
        (pin passive line (at 14.49 8.89 180) (length 2.54)
          (name "H_CSN")
          (number "18"))
        (pin passive line (at 14.49 6.35 180) (length 2.54)
          (name "H_SCL/SCK/RX")
          (number "19"))
        (pin passive line (at 14.49 3.81 180) (length 2.54)
          (name "H_SDA/H_MISO/TX")
          (number "20"))
        (pin passive line (at 14.49 1.27 180) (length 2.54)
          (name "RESV_NC")
          (number "21"))
        (pin passive line (at 14.49 -1.27 180) (length 2.54)
          (name "RESV_NC")
          (number "22"))
        (pin passive line (at 14.49 -3.81 180) (length 2.54)
          (name "RESV_NC")
          (number "23"))
        (pin passive line (at 14.49 -6.35 180) (length 2.54)
          (name "RESV_NC")
          (number "24"))
        (pin passive line (at 14.49 -8.89 180) (length 2.54)
          (name "GND")
          (number "25"))
        (pin passive line (at 14.49 -11.43 180) (length 2.54)
          (name "XOUT32/CLKSEL1")
          (number "26"))
        (pin passive line (at 14.49 -13.97 180) (length 2.54)
          (name "XIN32")
          (number "27"))
        (pin passive line (at 14.49 -16.51 180) (length 2.54)
          (name "VDDIO")
          (number "28"))
      )
    )
  (symbol "icm42688" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 12.16 0))
      (property "Value" "ICM-42688-P 6-Axis IMU" (at 0 -12.16 0))
        (property "Footprint" "PartReel:icm42688"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.cdiweb.com/datasheets/invensense/ds-000347-icm-42688-p-v1.2.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "TDK InvenSense ICM-42688-P 6-axis gyroscope+accelerometer - the standard modern FPV flight-controller IMU (Betaflight/ArduPilot). SPI 24MHz / I2C 0x68-0x69 / I3C, 1.71-3.6V, LGA-14 2.5x3. Pin 7 RESV must connect to GND."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "icm-42688 icm42688 imu gyroscope accelerometer fpv betaflight spi tdk"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/icm42688/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "icm42688_1_1"
        (pin passive line (at -20.32 7.62 0) (length 2.54)
          (name "AP_SDO/AD0")
          (number "1"))
        (pin passive line (at -20.32 5.08 0) (length 2.54)
          (name "RESV")
          (number "2"))
        (pin passive line (at -20.32 2.54 0) (length 2.54)
          (name "RESV")
          (number "3"))
        (pin passive line (at -20.32 0.00 0) (length 2.54)
          (name "INT1")
          (number "4"))
        (pin passive line (at -20.32 -2.54 0) (length 2.54)
          (name "VDDIO")
          (number "5"))
        (pin passive line (at -20.32 -5.08 0) (length 2.54)
          (name "GND")
          (number "6"))
        (pin passive line (at -20.32 -7.62 0) (length 2.54)
          (name "RESV(GND!)")
          (number "7"))
        (pin passive line (at 20.32 7.62 180) (length 2.54)
          (name "VDD")
          (number "8"))
        (pin passive line (at 20.32 5.08 180) (length 2.54)
          (name "INT2/FSYNC/CLKIN")
          (number "9"))
        (pin passive line (at 20.32 2.54 180) (length 2.54)
          (name "RESV")
          (number "10"))
        (pin passive line (at 20.32 0.00 180) (length 2.54)
          (name "RESV")
          (number "11"))
        (pin passive line (at 20.32 -2.54 180) (length 2.54)
          (name "AP_CS")
          (number "12"))
        (pin passive line (at 20.32 -5.08 180) (length 2.54)
          (name "AP_SCL/SCLK")
          (number "13"))
        (pin passive line (at 20.32 -7.62 180) (length 2.54)
          (name "AP_SDA/SDIO/SDI")
          (number "14"))
      )
    )
  (symbol "tcs34725" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 7.08 0))
      (property "Value" "TCS34725 RGBC Color Sensor" (at 0 -7.08 0))
        (property "Footprint" "PartReel:tcs34725"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/TCS34725.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "TAOS/ams TCS34725 RGB+clear color sensor with IR blocking filter, I2C 0x29, 2.7-3.6V, clear DFN-6 2.0x2.4. The Adafruit color sensor (GY-33 boards). Pin 4 NC: do not connect."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "tcs34725 taos ams color rgb sensor i2c gy-33"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/tcs34725/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "tcs34725_1_1"
        (pin passive line (at -11.43 2.54 0) (length 2.54)
          (name "VDD")
          (number "1"))
        (pin passive line (at -11.43 0.00 0) (length 2.54)
          (name "SCL")
          (number "2"))
        (pin passive line (at -11.43 -2.54 0) (length 2.54)
          (name "GND")
          (number "3"))
        (pin passive line (at 11.43 2.54 180) (length 2.54)
          (name "NC")
          (number "4"))
        (pin passive line (at 11.43 0.00 180) (length 2.54)
          (name "INT")
          (number "5"))
        (pin passive line (at 11.43 -2.54 180) (length 2.54)
          (name "SDA")
          (number "6"))
      )
    )
  (symbol "veml7700" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.81 0))
      (property "Value" "VEML7700 Ambient Light Sensor" (at 0 -5.81 0))
        (property "Footprint" "PartReel:veml7700"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.vishay.com/docs/84286/veml7700.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Vishay VEML7700 high-accuracy 16-bit ambient light sensor, 0-140klx, I2C 0x10 fixed, 2.5-3.6V, transparent side-view SMD package."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "veml7700 vishay light lux ambient i2c"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/veml7700/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "veml7700_1_1"
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "SCL")
          (number "1"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "VDD")
          (number "2"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "GND")
          (number "3"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "SDA")
          (number "4"))
      )
    )
  (symbol "mlx90614" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 5.81 0))
      (property "Value" "MLX90614 IR Thermometer (TO-39)" (at 0 -5.81 0))
        (property "Footprint" "PartReel:mlx90614"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://www.melexis.com/-/media/files/documents/datasheets/mlx90614-datasheet-melexis.pdf"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Melexis MLX90614 contactless infrared thermometer, SMBus (default 0x5A) or PWM output, factory-calibrated, TO-39 metal can. GY-906 module chip. Metal can: no electrical connection except via VSS."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "mlx90614 melexis infrared thermometer contactless smbus gy-906 to-39"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/mlx90614/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "mlx90614_1_1"
        (pin passive line (at -11.43 1.27 0) (length 2.54)
          (name "VDD")
          (number "3"))
        (pin passive line (at -11.43 -1.27 0) (length 2.54)
          (name "VSS")
          (number "4"))
        (pin passive line (at 11.43 1.27 180) (length 2.54)
          (name "SCL/Vz")
          (number "1"))
        (pin passive line (at 11.43 -1.27 180) (length 2.54)
          (name "SDA/PWM")
          (number "2"))
      )
    )
  (symbol "alps_rkjxm1015004" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 0 10.16 0))
      (property "Value" "RKJXM1015004" (at 0 -10.16 0))
        (property "Footprint" "PartReel:alps_rkjxm1015004"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://tech.alpsalpine.com/e/products/detail/RKJXM1015004/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "8-directional stick switch with center push, single shaft, 11x11mm body, THT, automotive grade."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "alps rkjxm stick joystick switch 8-direction center push navigation"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/alps_rkjxm1015004/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "alps_rkjxm1015004_0_1")
      (symbol "alps_rkjxm1015004_1_1"
        (pin passive line (at -12.7 5.08 0) (length 5.08) (name "A") (number "1"))
        (pin passive line (at -12.7 2.54 0) (length 5.08) (name "B") (number "2"))
        (pin passive line (at -12.7 0.0 0) (length 5.08) (name "C") (number "3"))
        (pin passive line (at -12.7 -2.54 0) (length 5.08) (name "D") (number "4"))
        (pin passive line (at 12.7 5.08 180) (length 5.08) (name "COM") (number "5"))
        (pin passive line (at 12.7 2.54 180) (length 5.08) (name "PUSH") (number "6"))
        (pin passive line (at 12.7 0.0 180) (length 5.08) (name "PUSH") (number "7"))
        (pin passive line (at 12.7 -2.54 180) (length 5.08) (name "PUSH") (number "8"))
        (pin passive line (at 12.7 -5.08 180) (length 5.08) (name "GND") (number "9"))
      )
    )
  (symbol "alps_rkjxm2e13004" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 0 15.239999999999998 0))
      (property "Value" "RKJXM2E13004" (at 0 -15.239999999999998 0))
        (property "Footprint" "PartReel:alps_rkjxm2e13004"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://tech.alpsalpine.com/e/products/detail/RKJXM2E13004/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "8-directional stick switch with center push and outer-shaft rotary encoder (15 detent / 15 pulse), dual shaft, 19.5mm round body, THT, automotive grade."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "alps rkjxm stick joystick switch 8-direction center push navigation encoder dual shaft"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/alps_rkjxm2e13004/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "alps_rkjxm2e13004_0_1")
      (symbol "alps_rkjxm2e13004_1_1"
        (pin passive line (at -12.7 10.16 0) (length 5.08) (name "A") (number "1"))
        (pin passive line (at -12.7 7.62 0) (length 5.08) (name "B") (number "2"))
        (pin passive line (at -12.7 5.08 0) (length 5.08) (name "C") (number "3"))
        (pin passive line (at -12.7 2.54 0) (length 5.08) (name "D") (number "4"))
        (pin passive line (at -12.7 0.0 0) (length 5.08) (name "COM") (number "5"))
        (pin passive line (at -12.7 -2.54 0) (length 5.08) (name "PUSH") (number "6"))
        (pin passive line (at -12.7 -5.08 0) (length 5.08) (name "PUSH") (number "7"))
        (pin passive line (at -12.7 -7.62 0) (length 5.08) (name "PUSH") (number "8"))
        (pin passive line (at -12.7 -10.16 0) (length 5.08) (name "GND") (number "9"))
        (pin passive line (at 12.7 10.16 180) (length 5.08) (name "ENC_A") (number "10"))
        (pin passive line (at 12.7 7.62 180) (length 5.08) (name "ENC_B") (number "11"))
        (pin passive line (at 12.7 5.08 180) (length 5.08) (name "ENC_COM") (number "12"))
        (pin passive line (at 12.7 2.54 180) (length 5.08) (name "ENC_COM") (number "13"))
        (pin passive line (at 12.7 0.0 180) (length 5.08) (name "FIX") (number "14"))
        (pin passive line (at 12.7 -2.54 180) (length 5.08) (name "FIX") (number "15"))
        (pin passive line (at 12.7 -5.08 180) (length 5.08) (name "FIX") (number "16"))
        (pin passive line (at 12.7 -7.62 180) (length 5.08) (name "FIX") (number "17"))
      )
    )
  (symbol "alps_rkjxt1f42001" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (at 0 12.7 0))
      (property "Value" "RKJXT1F42001" (at 0 -12.7 0))
        (property "Footprint" "PartReel:alps_rkjxt1f42001"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://tech.alpsalpine.com/e/products/detail/RKJXT1F42001/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "4-directional stick switch with rotary encoder (30 detent / 15 pulse) and center push, 17x17mm round body, THT, automotive grade."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "alps rkjxt1f stick encoder joystick switch center push navigation"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/alps_rkjxt1f42001/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (symbol "alps_rkjxt1f42001_0_1")
      (symbol "alps_rkjxt1f42001_1_1"
        (pin passive line (at -12.7 7.62 0) (length 5.08) (name "A") (number "1"))
        (pin passive line (at -12.7 5.08 0) (length 5.08) (name "B") (number "2"))
        (pin passive line (at -12.7 2.54 0) (length 5.08) (name "C") (number "3"))
        (pin passive line (at -12.7 0.0 0) (length 5.08) (name "D") (number "4"))
        (pin passive line (at -12.7 -2.54 0) (length 5.08) (name "COM") (number "5"))
        (pin passive line (at -12.7 -5.08 0) (length 5.08) (name "PUSH") (number "6"))
        (pin passive line (at 12.7 7.62 180) (length 5.08) (name "ENC_A") (number "7"))
        (pin passive line (at 12.7 5.08 180) (length 5.08) (name "ENC_B") (number "8"))
        (pin passive line (at 12.7 2.54 180) (length 5.08) (name "ENC_COM") (number "9"))
        (pin passive line (at 12.7 0.0 180) (length 5.08) (name "GND") (number "10"))
      )
    )
  (symbol "ai03_alps_solderable_1_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_1_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 1.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-1.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_1_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_1_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_1_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 1.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-1.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_1_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_1_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_1_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 1.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-1.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_1_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_1u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 1u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-1U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_1u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_2_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_2_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 2.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-2.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_2_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_2_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_2_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 2.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-2.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_2_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_2u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-2U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_2u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_3u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_3u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_3u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 3u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 3u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_3u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-3U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_3u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_6_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_6_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 6.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-6.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_6_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_6_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_6_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_6_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 6.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_6_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-6.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_6_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_7u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered, 7u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable 7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-7U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_7u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_solderable_iso" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_solderable_iso"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_solderable_iso/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Alps SKCM/SKCL-type keyboard switch, soldered."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps solderable iso"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_solderable_iso/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Alps-Solderable-ISO (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_solderable_iso_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_1_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_1_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 1.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-1.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_1_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_1_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_1_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 1.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-1.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_1_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_1_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_1_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 1.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-1.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_1_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_1u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 1u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-1U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_1u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_2_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_2_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 2.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-2.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_2_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_2_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_2_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 2.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-2.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_2_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_2u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-2U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_2u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_6_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_6_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 6.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-6.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_6_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_hotswap_7u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_hotswap_7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_hotswap_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, hotswap socket, 7u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 hotswap 7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_hotswap_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Hotswap-7U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_hotswap_7u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_1_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_1_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 1.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-1.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_1_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_1_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_1_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 1.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-1.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_1_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_1_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_1_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 1.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-1.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_1_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_1u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 1u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-1U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_1u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_2_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_2_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 2.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-2.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_2_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_2_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_2_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 2.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-2.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_2_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_2u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-2U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_2u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_6_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_6_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 6.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-6.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_6_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_gateron_ks33_solderable_7u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_gateron_ks33_solderable_7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_gateron_ks33_solderable_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Gateron low-profile KS-27/KS-33 switch, soldered, 7u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 gateron ks33 solderable 7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_gateron_ks33_solderable_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Gateron-KS33-Solderable-7U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_gateron_ks33_solderable_7u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_1_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_1_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 1.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-1.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_1_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_1_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_1_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 1.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-1.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_1_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_1_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_1_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 1.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-1.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_1_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_1u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 1u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-1U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_1u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_2_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_2_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 2.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-2.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_2_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_2_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_2_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 2.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-2.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_2_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_2u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-2U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_2u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_6_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_6_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 6.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-6.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_6_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_hotswap_7u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_hotswap_7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, hotswap socket, 7u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 hotswap 7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_hotswap_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Hotswap-7U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_hotswap_7u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_1_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_1_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 1.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-1.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_1_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_1_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_1_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 1.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-1.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_1_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_1_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_1_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 1.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-1.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_1_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_1u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 1u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-1U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_1u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_2_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_2_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 2.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-2.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_2_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_2_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_2_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 2.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-2.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_2_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_2u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-2U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_2u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_6_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_6_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 6.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-6.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_6_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_kailh_pg1353_solderable_7u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_kailh_pg1353_solderable_7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_kailh_pg1353_solderable_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Kailh Choc V2 (PG1353) low-profile switch, soldered, 7u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 kailh pg1353 solderable 7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_kailh_pg1353_solderable_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "Kailh-PG1353-Solderable-7U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_kailh_pg1353_solderable_7u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_10u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_10u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_10u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 10u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 10u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_10u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-10U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_10u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_10u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_10u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_10u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 10u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 10u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_10u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-10U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_10u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_1_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_1_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 1.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-1.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_1_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_1_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_1_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 1.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-1.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_1_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_1_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_1_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 1.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-1.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_1_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_1u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 1u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-1U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_1u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_2_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_2_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 2.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-2.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_2_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_2_25u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_2_25u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_2_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 2.25u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 25u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_2_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-2.25U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_2_25u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_2_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_2_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 2.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-2.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_2_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_2_75u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_2_75u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_2_75u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 2.75u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 75u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_2_75u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-2.75U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_2_75u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_2u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-2U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_2u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_2u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_2u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_2u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 2u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 2u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_2u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-2U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_2u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_2u_vertical" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_2u_vertical"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_2u_vertical/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 2u vertical"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_2u_vertical/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-2U-Vertical (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_2u_vertical_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_2u_vertical_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_2u_vertical_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_2u_vertical_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 2u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 2u vertical reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_2u_vertical_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-2U-Vertical-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_2u_vertical_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_3u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_3u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_3u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 3u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 3u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_3u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-3U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_3u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_3u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_3u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_3u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 3u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 3u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_3u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-3U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_3u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_6_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_6_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 6.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-6.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_6_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_6_25u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_6_25u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_6_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 6.25u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 25u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_6_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-6.25U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_6_25u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_6u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_6u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_6u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 6u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 6u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_6u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-6U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_6u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_6u_offcenter" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_6u_offcenter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_6u_offcenter/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 6u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 6u offcenter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_6u_offcenter/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-6U-Offcenter (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_6u_offcenter_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_6u_offcenter_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_6u_offcenter_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_6u_offcenter_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 6u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 6u offcenter reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_6u_offcenter_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-6U-Offcenter-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_6u_offcenter_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_6u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_6u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_6u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 6u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 6u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_6u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-6U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_6u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_7u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 7u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-7U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_7u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_7u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_7u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_7u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 7u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 7u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_7u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-7U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_7u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_8u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_8u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_8u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 8u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 8u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_8u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-8U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_8u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_8u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_8u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_8u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 8u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 8u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_8u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-8U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_8u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_9u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_9u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_9u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 9u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 9u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_9u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-9U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_9u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_9u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_9u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_9u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket, 9u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap 9u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_9u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-9U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_9u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_iso" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_iso"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_iso/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap iso"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_iso/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-ISO (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_iso_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_iso_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_iso_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_iso_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap iso reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_iso_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-ISO-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_iso_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_iso_rotated" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_iso_rotated"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_iso_rotated/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap iso rotated"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_iso_rotated/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-ISO-Rotated (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_iso_rotated_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_hotswap_iso_rotated_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_hotswap_iso_rotated_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_hotswap_iso_rotated_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, Kailh hotswap socket (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx hotswap iso rotated reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_hotswap_iso_rotated_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Hotswap-ISO-Rotated-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_hotswap_iso_rotated_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_10u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_10u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_10u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 10u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 10u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_10u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-10U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_10u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_10u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_10u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_10u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 10u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 10u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_10u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-10U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_10u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_1_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_1_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 1.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-1.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_1_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_1_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_1_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 1.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-1.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_1_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_1_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_1_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 1.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-1.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_1_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_1u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 1u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-1U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_1u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_2_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_2_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 2.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-2.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_2_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_2_25u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_2_25u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_2_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 2.25u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 25u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_2_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-2.25U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_2_25u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_2_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_2_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 2.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-2.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_2_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_2_75u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_2_75u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_2_75u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 2.75u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 75u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_2_75u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-2.75U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_2_75u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_2u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-2U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_2u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_2u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_2u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_2u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 2u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 2u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_2u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-2U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_2u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_2u_vertical" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_2u_vertical"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_2u_vertical/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 2u vertical"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_2u_vertical/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-2U-Vertical (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_2u_vertical_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_2u_vertical_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_2u_vertical_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_2u_vertical_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 2u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 2u vertical reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_2u_vertical_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-2U-Vertical-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_2u_vertical_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_3u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_3u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_3u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 3u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 3u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_3u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-3U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_3u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_3u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_3u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_3u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 3u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 3u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_3u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-3U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_3u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_6_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_6_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 6.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-6.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_6_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_6_25u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_6_25u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_6_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 6.25u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 25u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_6_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-6.25U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_6_25u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_6u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_6u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_6u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 6u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 6u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_6u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-6U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_6u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_6u_offcenter" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_6u_offcenter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_6u_offcenter/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 6u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 6u offcenter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_6u_offcenter/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-6U-Offcenter (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_6u_offcenter_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_6u_offcenter_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_6u_offcenter_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_6u_offcenter_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 6u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 6u offcenter reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_6u_offcenter_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-6U-Offcenter-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_6u_offcenter_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_6u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_6u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_6u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 6u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 6u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_6u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-6U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_6u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_7u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 7u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-7U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_7u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_7u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_7u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_7u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 7u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 7u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_7u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-7U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_7u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_8u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_8u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_8u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 8u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 8u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_8u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-8U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_8u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_8u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_8u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_8u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 8u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 8u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_8u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-8U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_8u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_9u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_9u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_9u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 9u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 9u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_9u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-9U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_9u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_9u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_9u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_9u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered, 9u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable 9u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_9u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-9U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_9u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_iso" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_iso"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_iso/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable iso"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_iso/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-ISO (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_iso_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_iso_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_iso_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_iso_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable iso reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_iso_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-ISO-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_iso_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_iso_rotated" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_iso_rotated"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_iso_rotated/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable iso rotated"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_iso_rotated/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-ISO-Rotated (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_iso_rotated_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_solderable_iso_rotated_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_solderable_iso_rotated_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_solderable_iso_rotated_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Cherry MX-type mechanical keyboard switch, soldered (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx solderable iso rotated reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_solderable_iso_rotated_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Solderable-ISO-Rotated-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_solderable_iso_rotated_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_10u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_10u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_10u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 10u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 10u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_10u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-10U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_10u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_10u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_10u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_10u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 10u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 10u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_10u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-10U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_10u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_1_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_1_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 1.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_1_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-1.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_1_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_1_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_1_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 1.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_1_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-1.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_1_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_1_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_1_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 1.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_1_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-1.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_1_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_1u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 1u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 1u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_1u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-1U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_1u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_2_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_2_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 2.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_2_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-2.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_2_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_2_25u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_2_25u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_2_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 2.25u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 25u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_2_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-2.25U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_2_25u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_2_75u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_2_75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 2.75u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 75u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_2_75u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-2.75U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_2_75u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_2_75u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_2_75u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_2_75u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 2.75u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 75u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_2_75u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-2.75U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_2_75u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_2u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 2u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_2u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-2U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_2u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_2u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_2u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_2u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 2u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 2u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_2u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-2U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_2u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_2u_vertical" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_2u_vertical"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_2u_vertical/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 2u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 2u vertical"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_2u_vertical/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-2U-Vertical (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_2u_vertical_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_2u_vertical_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_2u_vertical_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_2u_vertical_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 2u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 2u vertical reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_2u_vertical_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-2U-Vertical-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_2u_vertical_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_3u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_3u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_3u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 3u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 3u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_3u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-3U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_3u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_3u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_3u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_3u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 3u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 3u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_3u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-3U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_3u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_6_25u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_6_25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 6.25u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 25u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_6_25u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-6.25U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_6_25u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_6_25u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_6_25u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_6_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 6.25u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 25u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_6_25u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-6.25U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_6_25u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_6_5u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_6_5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_6_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 6.5u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 5u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_6_5u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-6.5U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_6_5u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_6u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_6u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_6u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 6u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 6u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_6u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-6U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_6u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_6u_offcenter" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_6u_offcenter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_6u_offcenter/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 6u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 6u offcenter"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_6u_offcenter/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-6U-Offcenter (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_6u_offcenter_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_6u_offcenter_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_6u_offcenter_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_6u_offcenter_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 6u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 6u offcenter reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_6u_offcenter_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-6U-Offcenter-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_6u_offcenter_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_6u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_6u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_6u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 6u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 6u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_6u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-6U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_6u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_7u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 7u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 7u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_7u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-7U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_7u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_7u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_7u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_7u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 7u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 7u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_7u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-7U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_7u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_8u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_8u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_8u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 8u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 8u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_8u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-8U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_8u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_8u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_8u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_8u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 8u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 8u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_8u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-8U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_8u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_9u" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_9u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_9u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 9u keysize."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 9u"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_9u/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-9U (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_9u_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_9u_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_9u_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_9u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered, 9u keysize (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid 9u reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_9u_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-9U-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_9u_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_iso" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_iso"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_iso/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid iso"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_iso/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-ISO (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_iso_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_iso_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_iso_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_iso_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid iso reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_iso_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-ISO-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_iso_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_iso_rotated" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_iso_rotated"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_iso_rotated/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid iso rotated"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_iso_rotated/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-ISO-Rotated (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_iso_rotated_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_mx_alps_hybrid_iso_rotated_reversedstabilizers" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_alps_hybrid_iso_rotated_reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_alps_hybrid_iso_rotated_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "Hybrid MX+Alps compatible keyboard switch, soldered (reversed stabilizers)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx alps hybrid iso rotated reversedstabilizers"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_alps_hybrid_iso_rotated_reversedstabilizers/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "SW" (at 0 3.81 0))
      (property "Value" "MX-Alps-Hybrid-ISO-Rotated-ReversedStabilizers (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_alps_hybrid_iso_rotated_reversedstabilizers_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1"))
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2"))
      )
    )
  (symbol "ai03_alps_led" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_led"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_led/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "In-switch indicator LED aligned to the switch footprint."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps led"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_led/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "D" (at 0 3.81 0))
      (property "Value" "Alps-LED (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_led_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2"))
      )
    )
  (symbol "ai03_alps_led_polaritymarked" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_led_polaritymarked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_led_polaritymarked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "In-switch indicator LED aligned to the switch footprint (polarity marked)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps led polaritymarked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_led_polaritymarked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "D" (at 0 3.81 0))
      (property "Value" "Alps-LED-PolarityMarked (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_led_polaritymarked_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2"))
      )
    )
  (symbol "ai03_alps_led_reversed" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_led_reversed"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_led_reversed/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "In-switch indicator LED aligned to the switch footprint (reversed pin order)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps led reversed"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_led_reversed/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "D" (at 0 3.81 0))
      (property "Value" "Alps-LED-Reversed (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_led_reversed_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2"))
      )
    )
  (symbol "ai03_alps_led_reversed_polaritymarked" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_alps_led_reversed_polaritymarked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_alps_led_reversed_polaritymarked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "In-switch indicator LED aligned to the switch footprint (reversed pin order, polarity marked)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 alps led reversed polaritymarked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_alps_led_reversed_polaritymarked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "D" (at 0 3.81 0))
      (property "Value" "Alps-LED-Reversed-PolarityMarked (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_alps_led_reversed_polaritymarked_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2"))
      )
    )
  (symbol "ai03_mx_led" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_led"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_led/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "In-switch indicator LED aligned to the switch footprint."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx led"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_led/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "D" (at 0 3.81 0))
      (property "Value" "MX-LED (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_led_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2"))
      )
    )
  (symbol "ai03_mx_led_polaritymarked" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_led_polaritymarked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_led_polaritymarked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "In-switch indicator LED aligned to the switch footprint (polarity marked)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx led polaritymarked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_led_polaritymarked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "D" (at 0 3.81 0))
      (property "Value" "MX-LED-PolarityMarked (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_led_polaritymarked_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2"))
      )
    )
  (symbol "ai03_mx_led_reversed" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_led_reversed"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_led_reversed/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "In-switch indicator LED aligned to the switch footprint (reversed pin order)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx led reversed"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_led_reversed/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "D" (at 0 3.81 0))
      (property "Value" "MX-LED-Reversed (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_led_reversed_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2"))
      )
    )
  (symbol "ai03_mx_led_reversed_polaritymarked" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
        (property "Footprint" "PartReel:ai03_mx_led_reversed_polaritymarked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Datasheet" "https://partreel.com/p/ai03_mx_led_reversed_polaritymarked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "Description" "In-switch indicator LED aligned to the switch footprint (reversed pin order, polarity marked)."
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "ki_keywords" "keyboard switch ai03 mx led reversed polaritymarked"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
        (property "PartReel" "https://partreel.com/p/ai03_mx_led_reversed_polaritymarked/"
          (at 0 0 0)
          (show_name no)
          (do_not_autoplace no)
          (hide yes)
        )
      (property "Reference" "D" (at 0 3.81 0))
      (property "Value" "MX-LED-Reversed-PolarityMarked (ai03 MX_V2)" (at 0 -3.81 0))
      (symbol "ai03_mx_led_reversed_polaritymarked_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1"))
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "K")
          (number "2"))
      )
    )
)
