(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Molex_Mini-Fit-Jr_2x4_0455860005"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 26.67 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Molex_Mini-Fit-Jr_2x4_0455860005"
				(at 26.67 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Molex_Mini-Fit-Jr_2x4_0455860005"
				(at 26.67 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://tools.molex.com/pdm_docs/sd/455860005_sd.pdf"
				(at 26.67 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Connector Header Through Hole, Right Angle 8 position 0.165\" (4.20mm)"
				(at 26.67 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "0455860005"
				(at 26.67 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Molex"
				(at 26.67 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 26.67 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 26.67 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "VERTICAL, THT, HEADER, CONNECTOR, MALE, WIRE-BOARD, POWER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Molex_Mini-Fit-Jr_2x4_0455860005_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at 11.43 0 180)
					(length 2.54)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at 11.43 -2.54 180)
					(length 2.54)
					(name "6")
					(number "6")
				)
				(pin passive line
					(at 11.43 -5.08 180)
					(length 2.54)
					(name "7")
					(number "7")
				)
				(pin passive line
					(at 11.43 -7.62 180)
					(length 2.54)
					(name "8")
					(number "8")
				)
				(pin passive line
					(at 11.43 -10.16 180)
					(length 2.54)
					(name "MH")
					(number "MH")
				)
			)
			(embedded_fonts no)
		)
)
