(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "HDMI-A_Molex_476591100"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "HDMI-A_Molex_476591100"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "HDMI-A_Molex_476591100"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.molex.com/en-us/products/part-detail/0476591100"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "HDMI REC.VERTICAL SMT TYPE W/HEI"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "0476591100"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Molex"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HDMI, CONNECTOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "HDMI-A_Molex_476591100_0_0")
			(symbol "HDMI-A_Molex_476591100_0_1")
			(symbol "HDMI-A_Molex_476591100_1_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "D2+")
					(number "1")
				)
				(pin passive line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "D2S")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "D2-")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D1+")
					(number "4")
				)
				(pin passive line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "D1S")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D1-")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D0+")
					(number "7")
				)
				(pin passive line
					(at 25.4 -43.18 180)
					(length 2.54)
					(name "D0S")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "D0-")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "CK+")
					(number "10")
				)
				(pin passive line
					(at 25.4 -45.72 180)
					(length 2.54)
					(name "CKS")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "CK-")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "CEC")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "UTILITY/HEAC+")
					(number "14")
					(alternate "HEAC+" passive line)
					(alternate "UTILITY" passive line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SCL")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SDA")
					(number "16")
				)
				(pin power_in line
					(at 25.4 -48.26 180)
					(length 2.54)
					(name "GND")
					(number "17")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "+5V")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "HPD/HEAC-")
					(number "19")
					(alternate "HEAC-" passive line)
					(alternate "HPD" passive line)
				)
				(pin passive line
					(at 25.4 -50.8 180)
					(length 2.54)
					(name "SH")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
