(footprint "PCIe_x8_Molex_0755860007"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -7.3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "PCIe_x8_Molex_0755860007"
		(at 0 8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -42.1 15.526 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -42.1 16.726 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -42.1 17.926 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -14.4 2.88)
		(size 1.55 1.55)
		(drill 1.55)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 0.127)
		(solder_paste_margin -1518.485687)
	)
	(pad "" np_thru_hole circle
		(at 14.4 2.88)
		(size 1.55 1.55)
		(drill 1.55)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 0.127)
		(solder_paste_margin -1518.485687)
	)
	(pad "A1" smd rect
		(at 13.4 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A2" smd rect
		(at 12.6 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A3" smd rect
		(at 11.8 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A4" smd rect
		(at 11 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A5" smd rect
		(at 10.2 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A6" smd rect
		(at 9.4 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A7" smd rect
		(at 8.6 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A8" smd rect
		(at 7.8 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A9" smd rect
		(at 7 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A10" smd rect
		(at 6.2 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A11" smd rect
		(at 5.4 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A12" smd rect
		(at 4.6 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A13" smd rect
		(at 3.8 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A14" smd rect
		(at 3 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A15" smd rect
		(at 2.2 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A16" smd rect
		(at 1.4 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A17" smd rect
		(at 0.6 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A18" smd rect
		(at -0.2 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A19" smd rect
		(at -1 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A20" smd rect
		(at -1.8 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A21" smd rect
		(at -2.6 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A22" smd rect
		(at -3.4 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A23" smd rect
		(at -4.2 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A24" smd rect
		(at -5 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A25" smd rect
		(at -5.8 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A26" smd rect
		(at -6.6 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A27" smd rect
		(at -7.4 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A28" smd rect
		(at -8.2 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A29" smd rect
		(at -9 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A30" smd rect
		(at -9.8 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A31" smd rect
		(at -10.6 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A32" smd rect
		(at -11.4 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A33" smd rect
		(at -12.2 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "A34" smd rect
		(at -13 -2.3)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B1" smd rect
		(at 13 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B2" smd rect
		(at 12.2 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B3" smd rect
		(at 11.4 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B4" smd rect
		(at 10.6 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B5" smd rect
		(at 9.8 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B6" smd rect
		(at 9 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B7" smd rect
		(at 8.2 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B8" smd rect
		(at 7.4 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B9" smd rect
		(at 6.6 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B10" smd rect
		(at 5.8 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B11" smd rect
		(at 5 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B12" smd rect
		(at 4.2 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B13" smd rect
		(at 3.4 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B14" smd rect
		(at 2.6 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B15" smd rect
		(at 1.8 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B16" smd rect
		(at 1 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B17" smd rect
		(at 0.2 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B18" smd rect
		(at -0.6 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B19" smd rect
		(at -1.4 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B20" smd rect
		(at -2.2 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B21" smd rect
		(at -3 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B22" smd rect
		(at -3.8 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B23" smd rect
		(at -4.6 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B24" smd rect
		(at -5.4 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B25" smd rect
		(at -6.2 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B26" smd rect
		(at -7 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B27" smd rect
		(at -7.8 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B28" smd rect
		(at -8.6 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B29" smd rect
		(at -9.4 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B30" smd rect
		(at -10.2 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B31" smd rect
		(at -11 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B32" smd rect
		(at -11.8 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B33" smd rect
		(at -12.6 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "B34" smd rect
		(at -13.4 -4.81)
		(size 0.35 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(zone
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -15.32 4.571) (xy -15.32 6.031) (xy -13.48 6.031) (xy -13.48 4.571)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 13.48 4.571) (xy 13.48 6.031) (xy 15.32 6.031) (xy 15.32 4.571)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_0755860007.glb"
		(offset
			(xyz 13.5 -3.1 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 -180 -90)
		)
	)
)
