(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCIe_x8_Molex_0755860007"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 52.07 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCIe_x8_Molex_0755860007"
				(at 52.07 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCIe_x8_Molex_0755860007"
				(at 52.07 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://tools.molex.com/pdm_docs/sd/755860007_sd.pdf"
				(at 52.07 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "68 Position SAS, Mini Receptacle Connector Solder Surface Mount, Right Angle"
				(at 52.07 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Molex"
				(at 52.07 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "0755860007"
				(at 52.07 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 52.07 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 52.07 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "PCIE, CONNECTOR, RECEPTACLE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCIe_x8_Molex_0755860007_1_1"
				(pin power_in line
					(at 30.48 -71.12 180)
					(length 3.81)
					(name "GND")
					(number "A1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "PETP0")
					(number "A2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PETN0")
					(number "A3")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 0 -6.35 0)
					(length 3.81)
					(name "PETP1")
					(number "A5")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 3.81)
					(name "PETN1")
					(number "A6")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A7")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PETP2")
					(number "A8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PETN2")
					(number "A9")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A10")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 3.81)
					(name "PETP3")
					(number "A11")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 3.81)
					(name "PETN3")
					(number "A12")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A13")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "CREFCLKP")
					(number "A14")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "CREFCLKN")
					(number "A15")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A16")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "RSVD1")
					(number "A17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "RSVD2")
					(number "A18")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "SB_RTN")
					(number "A19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "CPRSNT#")
					(number "A20")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "CPWRON")
					(number "A21")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PETP4")
					(number "A23")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PETN4")
					(number "A24")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A25")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 3.81)
					(name "PETP5")
					(number "A26")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 3.81)
					(name "PETN5")
					(number "A27")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A28")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PETP6")
					(number "A29")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PETN6")
					(number "A30")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A31")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(name "PETP7")
					(number "A32")
				)
				(pin passive line
					(at 0 -46.99 0)
					(length 3.81)
					(name "PETN7")
					(number "A33")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A34")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B1")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(name "PERP0")
					(number "B2")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "PERN0")
					(number "B3")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 30.48 -6.35 180)
					(length 3.81)
					(name "PERP1")
					(number "B5")
				)
				(pin passive line
					(at 30.48 -8.89 180)
					(length 3.81)
					(name "PERN1")
					(number "B6")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "PERP2")
					(number "B8")
				)
				(pin passive line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "PERN2")
					(number "B9")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B10")
				)
				(pin passive line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "PERP3")
					(number "B11")
				)
				(pin passive line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "PERN3")
					(number "B12")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B13")
				)
				(pin power_in line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "PWR1")
					(number "B14")
				)
				(pin power_in line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "PWR2")
					(number "B15")
				)
				(pin power_in line
					(at 30.48 -55.88 180)
					(length 3.81)
					(name "PWR3")
					(number "B16")
				)
				(pin power_in line
					(at 30.48 -58.42 180)
					(length 3.81)
					(name "PWR_RTN1")
					(number "B17")
				)
				(pin power_in line
					(at 30.48 -60.96 180)
					(length 3.81)
					(name "PWR_RTN2")
					(number "B18")
				)
				(pin power_in line
					(at 30.48 -63.5 180)
					(length 3.81)
					(name "PWR_RTN3")
					(number "B19")
				)
				(pin passive line
					(at 30.48 -66.04 180)
					(length 3.81)
					(name "CWAKE#")
					(number "B20")
				)
				(pin passive line
					(at 30.48 -68.58 180)
					(length 3.81)
					(name "CPERST#")
					(number "B21")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B22")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 3.81)
					(name "PERP4")
					(number "B23")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 3.81)
					(name "PERN4")
					(number "B24")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B25")
				)
				(pin passive line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "PERP5")
					(number "B26")
				)
				(pin passive line
					(at 30.48 -34.29 180)
					(length 3.81)
					(name "PERN5")
					(number "B27")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B28")
				)
				(pin passive line
					(at 30.48 -38.1 180)
					(length 3.81)
					(name "PERP6")
					(number "B29")
				)
				(pin passive line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "PERN6")
					(number "B30")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B31")
				)
				(pin passive line
					(at 30.48 -44.45 180)
					(length 3.81)
					(name "PERP7")
					(number "B32")
				)
				(pin passive line
					(at 30.48 -46.99 180)
					(length 3.81)
					(name "PERN7")
					(number "B33")
				)
				(pin passive line
					(at 30.48 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B34")
				)
			)
			(embedded_fonts no)
		)
)
