(footprint "0895-2C1R-GVH"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -6.5 -28.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "0895-2C1R-GVH"
		(at 0 -2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -10.86 14.316 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -10.86 15.516 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -10.86 16.716 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -5.715 0)
		(size 3.2512 3.2512)
		(drill 3.2512)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 5.714 0)
		(size 3.2512 3.2512)
		(drill 3.2512)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1_1" thru_hole circle
		(at -3.302 -4.699)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1_2" thru_hole circle
		(at 3.301 -4.699)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2_1" thru_hole circle
		(at -2.032 -5.97)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2_2" thru_hole circle
		(at 2.031 -5.97)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3_1" thru_hole circle
		(at -3.302 -7.239)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3_2" thru_hole circle
		(at 3.301 -7.239)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4_1" thru_hole circle
		(at -2.032 -8.51)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4_2" thru_hole circle
		(at 2.031 -8.51)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5_1" thru_hole circle
		(at -3.302 -9.779)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5_2" thru_hole circle
		(at 3.301 -9.779)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6_1" thru_hole circle
		(at -2.032 -11.049)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6_2" thru_hole circle
		(at 2.031 -11.049)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7_1" thru_hole circle
		(at -3.302 -12.321)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7_2" thru_hole circle
		(at 3.301 -12.321)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8_1" thru_hole circle
		(at -2.032 -13.59)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8_2" thru_hole circle
		(at 2.031 -13.59)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9_1" thru_hole circle
		(at -3.302 -14.859)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9_2" thru_hole circle
		(at 3.301 -14.859)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10_1" thru_hole circle
		(at -2.032 -16.13)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10_2" thru_hole circle
		(at 2.031 -16.13)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11_1" thru_hole circle
		(at -3.302 -19.939)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11_2" thru_hole circle
		(at 3.301 -19.939)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12_1" thru_hole circle
		(at -2.032 -21.209)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12_2" thru_hole circle
		(at 2.031 -21.209)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13_1" thru_hole circle
		(at -3.302 -22.479)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13_2" thru_hole circle
		(at 3.301 -22.479)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14_1" thru_hole circle
		(at -2.032 -23.749)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14_2" thru_hole circle
		(at 2.031 -23.749)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15_1" thru_hole circle
		(at -6.986 2.894)
		(size 1.62 1.62)
		(drill 1.143)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15_2" thru_hole circle
		(at -6.986 -11.786)
		(size 1.7145 1.7145)
		(drill 1.143)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16_1" thru_hole circle
		(at -4.446 2.894)
		(size 1.62 1.62)
		(drill 1.143)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16_2" thru_hole circle
		(at -6.986 -5.436)
		(size 1.7145 1.7145)
		(drill 1.143)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17_1" thru_hole circle
		(at 4.445 2.894)
		(size 1.62 1.62)
		(drill 1.143)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17_2" thru_hole circle
		(at 6.985 -7.976)
		(size 1.7145 1.7145)
		(drill 1.143)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18_1" thru_hole circle
		(at 6.985 2.894)
		(size 1.62 1.62)
		(drill 1.143)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18_2" thru_hole circle
		(at 6.985 -5.436)
		(size 1.7145 1.7145)
		(drill 1.143)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -8.51 -25.781)
		(size 2.3622 2.3622)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -8.51 -15.494)
		(size 2.3622 2.3622)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -8.51 4.57)
		(size 2.3622 2.3622)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 8.509 -25.781)
		(size 2.3622 2.3622)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 8.509 -11.43)
		(size 2.3622 2.3622)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 8.509 4.57)
		(size 2.3622 2.3622)
		(drill 1.5748)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 0 -2.668) (xy 0 10.794) (xy -9.398 10.794) (xy -9.398 -27.601) (xy -5.588 -27.601) (xy -5.588 -2.668)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 0 -2.668) (xy 0 10.794) (xy 9.397 10.794) (xy 9.397 -27.601) (xy 5.586 -27.601) (xy 5.586 -2.668)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_0895_2c1r_gvh.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "antmicro_0895_2c1r_gvh.glb"
		(offset
			(xyz 0 0 17.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "antmicro_0895_2c1r_gvh.glb"
		(offset
			(xyz 0 0 8.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 -180 0)
		)
	)
)
