(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "0895-2C1R-GVH"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "0895-2C1R-GVH"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "0895-2C1R-GVH"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.belfuse.com/resources/drawings/magneticsolutions/dr-mag-0895-2c1r-gvh.pdf"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Modular connector with magnetics"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "0895-2C1R-GVH"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Bel Fuse"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "RJ45, HORIZONTAL, THT, ETHERNET, CONNECTOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "0895-2C1R-GVH_1_1"
				(text "LOWER"
					(at 14.605 -0.635 0)
				)
				(text "Y"
					(at 17.399 -4.826 0)
				)
				(text "Y"
					(at 17.399 -14.986 0)
				)
				(text "G"
					(at 21.082 -8.128 0)
				)
				(text "G"
					(at 21.082 -18.288 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "TRD1-_1")
					(number "1_1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "TRD1+_1")
					(number "2_1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "TRD2-_1")
					(number "3_1")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "TRD2+_1")
					(number "4_1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "TRD3-_1")
					(number "5_1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "TRD3+_1")
					(number "6_1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "TRD4-_1")
					(number "7_1")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "TRD4+_1")
					(number "8_1")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "TRDCT1/2/3/4_1")
					(number "9_1")
				)
				(pin power_in line
					(at 26.67 -33.02 180)
					(length 5.08)
					(name "GND_1")
					(number "10_1")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "VC36_1")
					(number "11_1")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VC45_1")
					(number "12_1")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VC78_1")
					(number "13_1")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "VC12_1")
					(number "14_1")
				)
				(pin passive line
					(at 26.67 -4.445 180)
					(length 5.08)
					(name "")
					(number "15_1")
				)
				(pin passive line
					(at 26.67 -8.89 180)
					(length 5.08)
					(name "")
					(number "16_1")
				)
				(pin passive line
					(at 26.67 -14.605 180)
					(length 5.08)
					(name "")
					(number "17_1")
				)
				(pin passive line
					(at 26.67 -19.05 180)
					(length 5.08)
					(name "")
					(number "18_1")
				)
				(pin passive line
					(at 26.67 -30.48 180)
					(length 5.08)
					(name "SHIELD")
					(number "SH")
				)
				(pin passive line
					(at 26.67 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "SHIELD")
					(number "SH")
				)
				(pin passive line
					(at 26.67 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "SHIELD")
					(number "SH")
				)
				(pin passive line
					(at 26.67 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "SHIELD")
					(number "SH")
				)
				(pin passive line
					(at 26.67 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "SHIELD")
					(number "SH")
				)
				(pin passive line
					(at 26.67 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "SHIELD")
					(number "SH")
				)
			)
			(symbol "0895-2C1R-GVH_2_1"
				(text "UPPER"
					(at 14.605 -0.635 0)
				)
				(text "Y"
					(at 17.399 -4.826 0)
				)
				(text "Y"
					(at 17.399 -14.986 0)
				)
				(text "G"
					(at 21.082 -8.128 0)
				)
				(text "G"
					(at 21.082 -18.288 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "TRD1-_2")
					(number "1_2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "TRD1+_2")
					(number "2_2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "TRD2-_2")
					(number "3_2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "TRD2+_2")
					(number "4_2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "TRD3-_2")
					(number "5_2")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "TRD3+_2")
					(number "6_2")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "TRD4-_2")
					(number "7_2")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "TRD4+_2")
					(number "8_2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "TRDCT1/2/3/4_2")
					(number "9_2")
				)
				(pin passive line
					(at 26.67 -33.02 180)
					(length 5.08)
					(name "GND_2")
					(number "10_2")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "VC36_2")
					(number "11_2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VC45_2")
					(number "12_2")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VC78_2")
					(number "13_2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "VC12_2")
					(number "14_2")
				)
				(pin passive line
					(at 26.67 -4.445 180)
					(length 5.08)
					(name "")
					(number "15_2")
				)
				(pin passive line
					(at 26.67 -8.89 180)
					(length 5.08)
					(name "")
					(number "16_2")
				)
				(pin passive line
					(at 26.67 -14.605 180)
					(length 5.08)
					(name "")
					(number "17_2")
				)
				(pin passive line
					(at 26.67 -19.05 180)
					(length 5.08)
					(name "")
					(number "18_2")
				)
			)
			(embedded_fonts no)
		)
)
