(footprint "Ethernet_Jack_Harting-09452812560"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -3.55 -12.7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Ethernet_Jack_Harting-09452812560"
		(at 0 -1.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.3 9.55 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.3 10.75 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.3 11.95 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole oval
		(at 0 -0.9)
		(size 1.2 1.6)
		(drill oval 1.35 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -3.375 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.875 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.375 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.875 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.375 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 1.375 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1.875 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.375 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 2.875 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 3.375 -9.8)
		(size 0.32 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "SH" thru_hole roundrect
		(at -4.2 -7.15)
		(size 1.4 2.5)
		(drill oval 0.8 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.3571428571)
	)
	(pad "SH" thru_hole roundrect
		(at -2.9 -1.4)
		(size 1.4 2.5)
		(drill oval 0.8 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.3571428571)
	)
	(pad "SH" thru_hole circle
		(at 0 -9.1)
		(size 2 2)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole roundrect
		(at 2.9 -1.4)
		(size 1.4 2.5)
		(drill oval 0.8 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.3571428571)
	)
	(pad "SH" thru_hole roundrect
		(at 4.2 -7.15)
		(size 1.4 2.5)
		(drill oval 0.8 1.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.3571428571)
	)
	(zone
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 4.9 -8.5) (xy 3.4 -8.5) (xy 3.4 -5.8) (xy 4.9 -5.8) (xy 4.9 -4.25) (xy 4.2 -4.25) (xy 4.2 0.35)
				(xy 3.7 0.35) (xy 3.7 -2.7) (xy 2.1 -2.7) (xy 2.1 0.35) (xy 0.7 0.35) (xy 0.7 -1.725) (xy -0.7 -1.725)
				(xy -0.7 0.35) (xy -2.1 0.35) (xy -2.1 -2.7) (xy -3.7 -2.7) (xy -3.7 0.35) (xy -4.2 0.35) (xy -4.2 -4.25)
				(xy -4.9 -4.25) (xy -4.9 -5.8) (xy -3.4 -5.8) (xy -3.4 -8.5) (xy -4.9 -8.5) (xy -4.9 -9) (xy -1.1 -9)
				(xy -1.1 -8) (xy 0 -8) (xy 1.1 -8) (xy 1.1 -9) (xy 4.9 -9)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_09452812560.glb"
		(offset
			(xyz 0 1.5 4.7)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
	(model "antmicro_09452812560.glb"
		(offset
			(xyz 0 2.65 5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 180 -90 90)
		)
	)
)
