(footprint "Ethernet_Jack_Harting-09452812561"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Based on: https://b2b.harting.com/files/download/PRD/PDF_TS/09452812561_100805702DRW000C.pdf")
	(property "Reference" "REF**"
		(at 0 -7.45 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Ethernet_Jack_Harting-09452812561"
		(at 0 7.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 3.65 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 3.65 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -8.5 8.6 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -8.5 9.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.5 11 0)
		(layer "F.Fab")
	)
	(dimension
		(type leader)
		(layer "Dwgs.User")
		(pts
			(xy -5.48 4.35) (xy -7 6.08)
		)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 0)
			(precision 4)
			(override_value "PCB end")
		)
		(style
			(thickness 0.1)
			(arrow_length 0.72)
			(text_position_mode 0)
			(text_frame 0)
			(extension_offset 0.5)
		)
		(gr_text "PCB end"
			(at -10.94 6.08 0)
			(layer "Dwgs.User")
		)
	)
	(pad "" np_thru_hole circle
		(at -2.1 -2.7)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.1 -2.7)
		(size 1.45 1.45)
		(drill 1.45)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -1.575 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.075 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.575 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.075 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.575 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.575 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 2.075 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.575 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 3.075 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 3.575 -5.8)
		(size 0.3 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" thru_hole roundrect
		(at -5.2 1.35)
		(size 1.6 3.05)
		(drill oval 1 2.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.375)
	)
	(pad "SH" thru_hole roundrect
		(at -4.5 -3.1)
		(size 1.6 3.05)
		(drill oval 1 2.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.375)
	)
	(pad "SH" thru_hole roundrect
		(at 4.5 -3.1)
		(size 1.6 3.05)
		(drill oval 1 2.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.375)
	)
	(pad "SH" thru_hole roundrect
		(at 5.2 1.35)
		(size 1.6 3.05)
		(drill oval 1 2.45)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.375)
	)
	(zone
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(keepout
			(tracks not_allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 5.3 -5.1) (xy 5.3 -4.6482) (xy 3.683 -4.6482) (xy 3.683 -1.5494) (xy 6 -1.5494) (xy 6 -0.175)
				(xy 4.4 -0.175) (xy 4.4 2.875) (xy 6 2.875) (xy 6 3.69) (xy -6 3.7) (xy -6 2.875) (xy -4.3688 2.875)
				(xy -4.3942 -0.175) (xy -6 -0.175) (xy -6 -1.5508) (xy -3.683 -1.5494) (xy -3.683 -4.6482) (xy -5.3254 -4.6482)
				(xy -5.3 -5.1)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_09452812561.glb"
		(offset
			(xyz 0.2 -2.05 2.64)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 90)
		)
	)
	(model "antmicro_09452812561.glb"
		(offset
			(xyz 0 -1.05 2.65)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
