(footprint "PCIe_x16_10025026-10103TLF"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -30.001 -15.85 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "PCIe_x16_10025026-10103TLF"
		(at -30.001 -14.35 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -49.401 0.149 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -49.401 1.35 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -49.401 2.55 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -46.299 -4.36 270)
		(size 2 2)
		(drill 2)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 46.301 -4.36 270)
		(size 2 2)
		(drill 2)
		(layers "*.Mask")
	)
	(pad "A1" smd rect
		(at 41.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at 40.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at 39.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at 38.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd rect
		(at 37.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd rect
		(at 36.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd rect
		(at 35.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd rect
		(at 34.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd rect
		(at 33.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd rect
		(at 32.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd rect
		(at 31.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd rect
		(at 28.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd rect
		(at 27.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd rect
		(at 26.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd rect
		(at 25.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd rect
		(at 24.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd rect
		(at 23.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd rect
		(at 22.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd rect
		(at 21.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd rect
		(at 20.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd rect
		(at 19.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd rect
		(at 18.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd rect
		(at 17.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A24" smd rect
		(at 16.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A25" smd rect
		(at 15.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A26" smd rect
		(at 14.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A27" smd rect
		(at 13.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A28" smd rect
		(at 12.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A29" smd rect
		(at 11.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A30" smd rect
		(at 10.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A31" smd rect
		(at 9.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A32" smd rect
		(at 8.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A33" smd rect
		(at 7.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A34" smd rect
		(at 6.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A35" smd rect
		(at 5.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A36" smd rect
		(at 4.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A37" smd rect
		(at 3.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A38" smd rect
		(at 2.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A39" smd rect
		(at 1.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A40" smd rect
		(at 0.501 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A41" smd rect
		(at -0.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A42" smd rect
		(at -1.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A43" smd rect
		(at -2.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A44" smd rect
		(at -3.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A45" smd rect
		(at -4.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A46" smd rect
		(at -5.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A47" smd rect
		(at -6.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A48" smd rect
		(at -7.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A49" smd rect
		(at -8.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A50" smd rect
		(at -9.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A51" smd rect
		(at -10.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A52" smd rect
		(at -11.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A53" smd rect
		(at -12.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A54" smd rect
		(at -13.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A55" smd rect
		(at -14.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A56" smd rect
		(at -15.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A57" smd rect
		(at -16.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A58" smd rect
		(at -17.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A59" smd rect
		(at -18.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A60" smd rect
		(at -19.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A61" smd rect
		(at -20.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A62" smd rect
		(at -21.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A63" smd rect
		(at -22.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A64" smd rect
		(at -23.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A65" smd rect
		(at -24.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A66" smd rect
		(at -25.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A67" smd rect
		(at -26.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A68" smd rect
		(at -27.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A69" smd rect
		(at -28.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A70" smd rect
		(at -29.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A71" smd rect
		(at -30.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A72" smd rect
		(at -31.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A73" smd rect
		(at -32.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A74" smd rect
		(at -33.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A75" smd rect
		(at -34.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A76" smd rect
		(at -35.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A77" smd rect
		(at -36.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A78" smd rect
		(at -37.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A79" smd rect
		(at -38.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A80" smd rect
		(at -39.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A81" smd rect
		(at -40.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A82" smd rect
		(at -41.499 -5.051 180)
		(size 0.7 3.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd rect
		(at 41.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B2" smd rect
		(at 40.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B3" smd rect
		(at 39.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B4" smd rect
		(at 38.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B5" smd rect
		(at 37.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B6" smd rect
		(at 36.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B7" smd rect
		(at 35.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B8" smd rect
		(at 34.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B9" smd rect
		(at 33.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B10" smd rect
		(at 32.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B11" smd rect
		(at 31.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B12" smd rect
		(at 28.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B13" smd rect
		(at 27.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B14" smd rect
		(at 26.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B15" smd rect
		(at 25.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B16" smd rect
		(at 24.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B17" smd rect
		(at 23.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B18" smd rect
		(at 22.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B19" smd rect
		(at 21.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B20" smd rect
		(at 20.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B21" smd rect
		(at 19.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B22" smd rect
		(at 18.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B23" smd rect
		(at 17.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B24" smd rect
		(at 16.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B25" smd rect
		(at 15.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B26" smd rect
		(at 14.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B27" smd rect
		(at 13.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B28" smd rect
		(at 12.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B29" smd rect
		(at 11.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B30" smd rect
		(at 10.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B31" smd rect
		(at 9.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B32" smd rect
		(at 8.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B33" smd rect
		(at 7.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B34" smd rect
		(at 6.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B35" smd rect
		(at 5.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B36" smd rect
		(at 4.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B37" smd rect
		(at 3.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B38" smd rect
		(at 2.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B39" smd rect
		(at 1.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B40" smd rect
		(at 0.501 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B41" smd rect
		(at -0.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B42" smd rect
		(at -1.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B43" smd rect
		(at -2.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B44" smd rect
		(at -3.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B45" smd rect
		(at -4.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B46" smd rect
		(at -5.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B47" smd rect
		(at -6.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B48" smd rect
		(at -7.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B49" smd rect
		(at -8.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B50" smd rect
		(at -9.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B51" smd rect
		(at -10.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B52" smd rect
		(at -11.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B53" smd rect
		(at -12.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B54" smd rect
		(at -13.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B55" smd rect
		(at -14.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B56" smd rect
		(at -15.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B57" smd rect
		(at -16.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B58" smd rect
		(at -17.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B59" smd rect
		(at -18.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B60" smd rect
		(at -19.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B61" smd rect
		(at -20.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B62" smd rect
		(at -21.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B63" smd rect
		(at -22.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B64" smd rect
		(at -23.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B65" smd rect
		(at -24.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B66" smd rect
		(at -25.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B67" smd rect
		(at -26.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B68" smd rect
		(at -27.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B69" smd rect
		(at -28.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B70" smd rect
		(at -29.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B71" smd rect
		(at -30.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B72" smd rect
		(at -31.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B73" smd rect
		(at -32.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B74" smd rect
		(at -33.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B75" smd rect
		(at -34.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B76" smd rect
		(at -35.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B77" smd rect
		(at -36.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B78" smd rect
		(at -37.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B79" smd rect
		(at -38.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B80" smd rect
		(at -39.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B81" smd rect
		(at -40.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(pad "B82" smd rect
		(at -41.499 -5.051)
		(size 0.7 3.6)
		(layers "B.Cu" "B.Mask" "B.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_10025026_10103tlf.glb"
		(offset
			(xyz -0.000001 1.85 -0.9)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 180 -180 0)
		)
	)
)
