(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCIe_x16_10025026-10103TLF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCIe_x16_10025026-10103TLF"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCIe_x16_10025026-10103TLF"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/10025026.pdf"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PCI Express Card Edge SKT 164 POS 1mm Solder ST Edge Mount Tray"
				(at 48.26 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "10025026-10103TLF"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, PCIE, EDGE, FEMALE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCIe_x16_10025026-10103TLF_0_1")
			(symbol "PCIe_x16_10025026-10103TLF_1_1"
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(name "~{PRSNT1}")
					(number "A1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "12V")
					(number "A2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "12V")
					(number "A3")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A4")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "TCK")
					(number "A5")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "TDI")
					(number "A6")
				)
				(pin output line
					(at 0 -24.13 0)
					(length 3.81)
					(name "TDO")
					(number "A7")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 3.81)
					(name "TMS")
					(number "A8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "A9")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "3V3")
					(number "A10")
				)
				(pin open_collector line
					(at 33.02 -27.94 180)
					(length 3.81)
					(name "~{PERST}")
					(number "A11")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "GND")
					(number "A12")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "REFCLK_p")
					(number "A13")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "REFCLK_n")
					(number "A14")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A15")
				)
				(pin output line
					(at 33.02 -48.26 180)
					(length 3.81)
					(name "HSI0_p")
					(number "A16")
				)
				(pin output line
					(at 33.02 -50.8 180)
					(length 3.81)
					(name "HSI0_n")
					(number "A17")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A18")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A19")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A20")
				)
				(pin output line
					(at 33.02 -55.88 180)
					(length 3.81)
					(name "HSI1_p")
					(number "A21")
				)
				(pin output line
					(at 33.02 -58.42 180)
					(length 3.81)
					(name "HSI1_n")
					(number "A22")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A23")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A24")
				)
				(pin output line
					(at 33.02 -63.5 180)
					(length 3.81)
					(name "HSI2_p")
					(number "A25")
				)
				(pin output line
					(at 33.02 -66.04 180)
					(length 3.81)
					(name "HSI2_n")
					(number "A26")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A27")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A28")
				)
				(pin output line
					(at 33.02 -71.12 180)
					(length 3.81)
					(name "HSI3_p")
					(number "A29")
				)
				(pin output line
					(at 33.02 -73.66 180)
					(length 3.81)
					(name "HSI3_n")
					(number "A30")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A31")
				)
				(pin no_connect line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A32")
				)
				(pin no_connect line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A33")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A34")
				)
				(pin output line
					(at 33.02 -78.74 180)
					(length 3.81)
					(name "HSI4_p")
					(number "A35")
				)
				(pin output line
					(at 33.02 -81.28 180)
					(length 3.81)
					(name "HSI4_n")
					(number "A36")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A37")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A38")
				)
				(pin output line
					(at 33.02 -86.36 180)
					(length 3.81)
					(name "HSI5_p")
					(number "A39")
				)
				(pin output line
					(at 33.02 -88.9 180)
					(length 3.81)
					(name "HSI5_n")
					(number "A40")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A41")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A42")
				)
				(pin output line
					(at 33.02 -93.98 180)
					(length 3.81)
					(name "HSI6_p")
					(number "A43")
				)
				(pin output line
					(at 33.02 -96.52 180)
					(length 3.81)
					(name "HSI6_n")
					(number "A44")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A45")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A46")
				)
				(pin output line
					(at 33.02 -101.6 180)
					(length 3.81)
					(name "HSI7_p")
					(number "A47")
				)
				(pin output line
					(at 33.02 -104.14 180)
					(length 3.81)
					(name "HSI7_n")
					(number "A48")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A49")
				)
				(pin no_connect line
					(at 3.81 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A50")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A51")
				)
				(pin output line
					(at 33.02 -109.22 180)
					(length 3.81)
					(name "HSI8_p")
					(number "A52")
				)
				(pin output line
					(at 33.02 -111.76 180)
					(length 3.81)
					(name "HSI8_n")
					(number "A53")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A54")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A55")
				)
				(pin output line
					(at 33.02 -116.84 180)
					(length 3.81)
					(name "HSI9_p")
					(number "A56")
				)
				(pin output line
					(at 33.02 -119.38 180)
					(length 3.81)
					(name "HSI9_n")
					(number "A57")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A58")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A59")
				)
				(pin output line
					(at 33.02 -124.46 180)
					(length 3.81)
					(name "HSI10_p")
					(number "A60")
				)
				(pin output line
					(at 33.02 -127 180)
					(length 3.81)
					(name "HSI10_n")
					(number "A61")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A62")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A63")
				)
				(pin output line
					(at 33.02 -132.08 180)
					(length 3.81)
					(name "HSI11_p")
					(number "A64")
				)
				(pin output line
					(at 33.02 -134.62 180)
					(length 3.81)
					(name "HSI11_n")
					(number "A65")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A66")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A67")
				)
				(pin output line
					(at 33.02 -139.7 180)
					(length 3.81)
					(name "HSI12_p")
					(number "A68")
				)
				(pin output line
					(at 33.02 -142.24 180)
					(length 3.81)
					(name "HSI12_n")
					(number "A69")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A70")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A71")
				)
				(pin output line
					(at 33.02 -147.32 180)
					(length 3.81)
					(name "HSI13_p")
					(number "A72")
				)
				(pin output line
					(at 33.02 -149.86 180)
					(length 3.81)
					(name "HSI13_n")
					(number "A73")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A74")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A75")
				)
				(pin output line
					(at 33.02 -154.94 180)
					(length 3.81)
					(name "HSI14_p")
					(number "A76")
				)
				(pin output line
					(at 33.02 -157.48 180)
					(length 3.81)
					(name "HSI14_n")
					(number "A77")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A78")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A79")
				)
				(pin output line
					(at 33.02 -162.56 180)
					(length 3.81)
					(name "HSI15_p")
					(number "A80")
				)
				(pin output line
					(at 33.02 -165.1 180)
					(length 3.81)
					(name "HSI15_n")
					(number "A81")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A82")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "12V")
					(number "B1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "12V")
					(number "B2")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "12V")
					(number "B3")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin open_collector line
					(at 33.02 -40.64 180)
					(length 3.81)
					(name "SMCLK")
					(number "B5")
				)
				(pin open_collector line
					(at 33.02 -43.18 180)
					(length 3.81)
					(name "SMDAT")
					(number "B6")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "B8")
				)
				(pin input line
					(at 33.02 -20.32 180)
					(length 3.81)
					(name "~{TRST}")
					(number "B9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "3V3AUX")
					(number "B10")
				)
				(pin open_collector line
					(at 33.02 -22.86 180)
					(length 3.81)
					(name "~{WAKE}")
					(number "B11")
				)
				(pin open_collector line
					(at 33.02 -25.4 180)
					(length 3.81)
					(name "~{CLKREQ}")
					(number "B12")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B13")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "HSO0_p")
					(number "B14")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 3.81)
					(name "HSO0_n")
					(number "B15")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B16")
				)
				(pin passive line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "~{PRSNT2_x1}")
					(number "B17")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B18")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 3.81)
					(name "HSO1_p")
					(number "B19")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 3.81)
					(name "HSO1_n")
					(number "B20")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B21")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B22")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 3.81)
					(name "HSO2_p")
					(number "B23")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 3.81)
					(name "HSO2_n")
					(number "B24")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B25")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B26")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 3.81)
					(name "HSO3_p")
					(number "B27")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(name "HSO3_n")
					(number "B28")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B29")
				)
				(pin open_collector line
					(at 33.02 -30.48 180)
					(length 3.81)
					(name "~{PWRBRK}")
					(number "B30")
				)
				(pin passive line
					(at 33.02 -5.08 180)
					(length 3.81)
					(name "~{PRSNT2_x4}")
					(number "B31")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B32")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 3.81)
					(name "HSO4_p")
					(number "B33")
				)
				(pin input line
					(at 0 -81.28 0)
					(length 3.81)
					(name "HSO4_n")
					(number "B34")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B35")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B36")
				)
				(pin input line
					(at 0 -86.36 0)
					(length 3.81)
					(name "HSO5_p")
					(number "B37")
				)
				(pin input line
					(at 0 -88.9 0)
					(length 3.81)
					(name "HSO5_n")
					(number "B38")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B39")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B40")
				)
				(pin input line
					(at 0 -93.98 0)
					(length 3.81)
					(name "HSO6_p")
					(number "B41")
				)
				(pin input line
					(at 0 -96.52 0)
					(length 3.81)
					(name "HSO6_n")
					(number "B42")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B43")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B44")
				)
				(pin input line
					(at 0 -101.6 0)
					(length 3.81)
					(name "HSO7_p")
					(number "B45")
				)
				(pin input line
					(at 0 -104.14 0)
					(length 3.81)
					(name "HSO7_n")
					(number "B46")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B47")
				)
				(pin passive line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "~{PRSNT2_x8}")
					(number "B48")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B49")
				)
				(pin input line
					(at 0 -109.22 0)
					(length 3.81)
					(name "HSO8_p")
					(number "B50")
				)
				(pin input line
					(at 0 -111.76 0)
					(length 3.81)
					(name "HSO8_n")
					(number "B51")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B52")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B53")
				)
				(pin input line
					(at 0 -116.84 0)
					(length 3.81)
					(name "HSO9_p")
					(number "B54")
				)
				(pin input line
					(at 0 -119.38 0)
					(length 3.81)
					(name "HSO9_n")
					(number "B55")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B56")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B57")
				)
				(pin input line
					(at 0 -124.46 0)
					(length 3.81)
					(name "HSO10_p")
					(number "B58")
				)
				(pin input line
					(at 0 -127 0)
					(length 3.81)
					(name "HSO10_n")
					(number "B59")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B60")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B61")
				)
				(pin input line
					(at 0 -132.08 0)
					(length 3.81)
					(name "HSO11_p")
					(number "B62")
				)
				(pin input line
					(at 0 -134.62 0)
					(length 3.81)
					(name "HSO11_n")
					(number "B63")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B64")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B65")
				)
				(pin input line
					(at 0 -139.7 0)
					(length 3.81)
					(name "HSO12_p")
					(number "B66")
				)
				(pin input line
					(at 0 -142.24 0)
					(length 3.81)
					(name "HSO12_n")
					(number "B67")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B68")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B69")
				)
				(pin input line
					(at 0 -147.32 0)
					(length 3.81)
					(name "HSO13_p")
					(number "B70")
				)
				(pin input line
					(at 0 -149.86 0)
					(length 3.81)
					(name "HSO13_n")
					(number "B71")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B72")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B73")
				)
				(pin input line
					(at 0 -154.94 0)
					(length 3.81)
					(name "HSO14_p")
					(number "B74")
				)
				(pin input line
					(at 0 -157.48 0)
					(length 3.81)
					(name "HSO14_n")
					(number "B75")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B76")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B77")
				)
				(pin input line
					(at 0 -162.56 0)
					(length 3.81)
					(name "HSO15_p")
					(number "B78")
				)
				(pin input line
					(at 0 -165.1 0)
					(length 3.81)
					(name "HSO15_n")
					(number "B79")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B80")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "~{PRSNT2_x16}")
					(number "B81")
				)
				(pin no_connect line
					(at 3.81 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B82")
				)
			)
			(embedded_fonts no)
		)
)
