(footprint "Conn_Amphenol_SATA_1x22_10034814-001LF"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -6.7 180)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Amphenol_SATA_1x22_10034814-001LF"
		(at 0 7.5 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -22.5 9.2 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -22.5 10.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -22.5 11.6 0)
		(layer "F.Fab")
	)
	(pad "" thru_hole circle
		(at -20 3.2 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "" np_thru_hole circle
		(at -18.51 5 180)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 18.02 5 180)
		(size 0.9 0.9)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" thru_hole circle
		(at 20 3.2 180)
		(size 3 3)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1A" smd rect
		(at -15.87 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1B" smd rect
		(at -1.92 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2A" smd rect
		(at -14.6 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2B" smd rect
		(at -0.65 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3A" smd rect
		(at -13.33 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3B" smd rect
		(at 0.62 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4A" smd rect
		(at -12.06 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4B" smd rect
		(at 1.89 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5A" smd rect
		(at -10.79 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5B" smd rect
		(at 3.16 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6A" smd rect
		(at -9.52 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6B" smd rect
		(at 4.43 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7A" smd rect
		(at -8.25 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7B" smd rect
		(at 5.7 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8B" smd rect
		(at 6.97 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9B" smd rect
		(at 8.24 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10B" smd rect
		(at 9.51 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11B" smd rect
		(at 10.78 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12B" smd rect
		(at 12.05 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13B" smd rect
		(at 13.32 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14B" smd rect
		(at 14.59 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15B" smd rect
		(at 15.86 5 180)
		(size 0.65 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_10034814_001lf.glb"
		(offset
			(xyz 0 -1.2 3.75)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 180)
		)
	)
)
