(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Amphenol_SATA_1x22_10034814-001LF"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 33.02 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Amphenol_SATA_1x22_10034814-001LF"
				(at 33.02 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Amphenol_SATA_1x22_10034814-001LF"
				(at 33.02 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/ProductDetail/Amphenol-FCI/10034814-001LF?qs=Lu3apKW7jUjFKgbXELt%252Btg%3D%3D"
				(at 33.02 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "22 Position SATA Receptacle Connector Solder Surface Mount, Right Angle"
				(at 33.02 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "10034814-001LF"
				(at 33.02 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 33.02 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, SMT, SATA, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Amphenol_SATA_1x22_10034814-001LF_1_1"
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "1A")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "3V3")
					(number "1B")
				)
				(pin output line
					(at 0 0 0)
					(length 3.81)
					(name "A+")
					(number "2A")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "2B")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 3.81)
					(name "A-")
					(number "3A")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "3B")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "4A")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "4B")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 3.81)
					(name "B-")
					(number "5A")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "5B")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 3.81)
					(name "B+")
					(number "6A")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "6B")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "7A")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "5V")
					(number "7B")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "5V")
					(number "8B")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "5V")
					(number "9B")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "GND")
					(number "10B")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "ACT/SPINUP")
					(number "11B")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "12B")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "12V")
					(number "13B")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "12V")
					(number "14B")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "12V")
					(number "15B")
				)
			)
			(embedded_fonts no)
		)
)
