(footprint "SD_10067847-001RLF"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -11.325 -18.56 0)
		(layer "F.SilkS")
	)
	(property "Value" "SD_10067847-001RLF"
		(at 0.739 -16.88 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -15.74 28.114 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -15.74 29.314 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -15.74 30.514 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -12.6 9.625)
		(size 1.5 1.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 11.598 9.625)
		(size 1.5 1.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at 6.373 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 3.873 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.574 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.125 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.625 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -6.125 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.551 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -10.25 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 8.874 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "CD" smd rect
		(at 2.225 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd rect
		(at -14.1 7.524)
		(size 1.2 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd rect
		(at 13.9 6.325)
		(size 1.2 2.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "WP" smd rect
		(at -13.6 -14.676)
		(size 1 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -15.2 -4.875) (xy -14 -4.875) (xy -14 1.425) (xy -15.2 1.425)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -10.811 -7.976) (xy -9.712 -7.976) (xy -9.712 -5.975) (xy -10.811 -5.975)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -9.11 -7.976) (xy -8.01 -7.976) (xy -8.01 -5.975) (xy -9.11 -5.975)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -6.68 -7.976) (xy -5.58 -7.976) (xy -5.58 -5.975) (xy -6.68 -5.975)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -4.181 -7.976) (xy -3.081 -7.976) (xy -3.081 -5.975) (xy -4.181 -5.975)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -1.68 -7.575) (xy -0.58 -7.575) (xy -0.58 -5.575) (xy -1.68 -5.575)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 0.42 -8.075) (xy 2.318 -8.075) (xy 2.318 -5.575) (xy 0.42 -5.575)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 3.317 -7.875) (xy 4.418 -7.875) (xy 4.418 -5.875) (xy 3.317 -5.875)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 5.82 -8.676) (xy 6.916 -8.676) (xy 6.916 -6.176) (xy 5.82 -6.176)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 8.32 -5.575) (xy 9.419 -5.575) (xy 9.419 -3.575) (xy 8.32 -3.575)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_10067847_001rlf.glb"
		(offset
			(xyz 0 13.874851 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 180 180)
		)
	)
)
