(footprint "USB-Micro-B_Receptacle_Amphenol_10118192"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-Micro-B_Receptacle_Amphenol_10118192"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5 6.7 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5 7.9 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5 9.099 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.301 -2.226)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.651 -2.226)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 -2.226)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0.65 -2.226)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.3 -2.226)
		(size 0.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd roundrect
		(at -3.801 0.449)
		(size 1.8 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at -3.101 -2.101)
		(size 2.1 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at -1.2 0.449)
		(size 1.9 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at 1.199 0.449)
		(size 1.9 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at 3.1 -2.101)
		(size 2.1 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "SH" smd roundrect
		(at 3.8 0.449)
		(size 1.8 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "antmicro_10118192_0001lf.glb"
		(offset
			(xyz -97.99917 2.75 -0.32)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
