(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCIe_x16_10146070-113Y0LF-vertical"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCIe_x16_10146070-113Y0LF-vertical"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCIe_x16_10146070-113Y0LF-vertical"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/3212936.pdf"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "164 Position Female Connector PCI Express™ Gold 0.039\" (1.00mm) Black"
				(at 35.56 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "PARTREV" "E"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "STANDARD" "Manufacturer Recommendations"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MAXIMUM_PACKAGE_HEIGHT" "11.25mm"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Amphenol"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "10146070-113Y0LF"
				(at 35.56 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCIe_x16_10146070-113Y0LF-vertical_1_1"
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "A1")
					(number "A1")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "A2")
					(number "A2")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "A3")
					(number "A3")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "A4")
					(number "A4")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "A5")
					(number "A5")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "A6")
					(number "A6")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "A7")
					(number "A7")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "A8")
					(number "A8")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "A9")
					(number "A9")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "A10")
					(number "A10")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "A11")
					(number "A11")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "A12")
					(number "A12")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "A13")
					(number "A13")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "A14")
					(number "A14")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "A15")
					(number "A15")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "A16")
					(number "A16")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "A17")
					(number "A17")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "A18")
					(number "A18")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "A19")
					(number "A19")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "A20")
					(number "A20")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "A21")
					(number "A21")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "A22")
					(number "A22")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "A23")
					(number "A23")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "A24")
					(number "A24")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "A25")
					(number "A25")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "A26")
					(number "A26")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "A27")
					(number "A27")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "A28")
					(number "A28")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "A29")
					(number "A29")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "A30")
					(number "A30")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "A31")
					(number "A31")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "A32")
					(number "A32")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "A33")
					(number "A33")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "A34")
					(number "A34")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "A35")
					(number "A35")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "A36")
					(number "A36")
				)
				(pin passive line
					(at 22.86 -91.44 180)
					(length 3.81)
					(name "A37")
					(number "A37")
				)
				(pin passive line
					(at 22.86 -93.98 180)
					(length 3.81)
					(name "A38")
					(number "A38")
				)
				(pin passive line
					(at 22.86 -96.52 180)
					(length 3.81)
					(name "A39")
					(number "A39")
				)
				(pin passive line
					(at 22.86 -99.06 180)
					(length 3.81)
					(name "A40")
					(number "A40")
				)
				(pin passive line
					(at 22.86 -101.6 180)
					(length 3.81)
					(name "A41")
					(number "A41")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "B1")
					(number "B1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "B2")
					(number "B2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "B3")
					(number "B3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "B4")
					(number "B4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "B5")
					(number "B5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "B6")
					(number "B6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "B7")
					(number "B7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "B8")
					(number "B8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "B9")
					(number "B9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "B10")
					(number "B10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "B11")
					(number "B11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "B12")
					(number "B12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "B13")
					(number "B13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "B14")
					(number "B14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "B15")
					(number "B15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "B16")
					(number "B16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "B17")
					(number "B17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "B18")
					(number "B18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "B19")
					(number "B19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "B20")
					(number "B20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "B21")
					(number "B21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "B22")
					(number "B22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "B23")
					(number "B23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "B24")
					(number "B24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "B25")
					(number "B25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "B26")
					(number "B26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "B27")
					(number "B27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "B28")
					(number "B28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "B29")
					(number "B29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "B30")
					(number "B30")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "B31")
					(number "B31")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "B32")
					(number "B32")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "B33")
					(number "B33")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "B34")
					(number "B34")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "B35")
					(number "B35")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "B36")
					(number "B36")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "B37")
					(number "B37")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "B38")
					(number "B38")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "B39")
					(number "B39")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "B40")
					(number "B40")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 3.81)
					(name "B41")
					(number "B41")
				)
			)
			(symbol "PCIe_x16_10146070-113Y0LF-vertical_2_1"
				(pin passive line
					(at 22.86 0 180)
					(length 3.81)
					(name "A42")
					(number "A42")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "A43")
					(number "A43")
				)
				(pin passive line
					(at 22.86 -5.08 180)
					(length 3.81)
					(name "A44")
					(number "A44")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 3.81)
					(name "A45")
					(number "A45")
				)
				(pin passive line
					(at 22.86 -10.16 180)
					(length 3.81)
					(name "A46")
					(number "A46")
				)
				(pin passive line
					(at 22.86 -12.7 180)
					(length 3.81)
					(name "A47")
					(number "A47")
				)
				(pin passive line
					(at 22.86 -15.24 180)
					(length 3.81)
					(name "A48")
					(number "A48")
				)
				(pin passive line
					(at 22.86 -17.78 180)
					(length 3.81)
					(name "A49")
					(number "A49")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 3.81)
					(name "A50")
					(number "A50")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 3.81)
					(name "A51")
					(number "A51")
				)
				(pin passive line
					(at 22.86 -25.4 180)
					(length 3.81)
					(name "A52")
					(number "A52")
				)
				(pin passive line
					(at 22.86 -27.94 180)
					(length 3.81)
					(name "A53")
					(number "A53")
				)
				(pin passive line
					(at 22.86 -30.48 180)
					(length 3.81)
					(name "A54")
					(number "A54")
				)
				(pin passive line
					(at 22.86 -33.02 180)
					(length 3.81)
					(name "A55")
					(number "A55")
				)
				(pin passive line
					(at 22.86 -35.56 180)
					(length 3.81)
					(name "A56")
					(number "A56")
				)
				(pin passive line
					(at 22.86 -38.1 180)
					(length 3.81)
					(name "A57")
					(number "A57")
				)
				(pin passive line
					(at 22.86 -40.64 180)
					(length 3.81)
					(name "A58")
					(number "A58")
				)
				(pin passive line
					(at 22.86 -43.18 180)
					(length 3.81)
					(name "A59")
					(number "A59")
				)
				(pin passive line
					(at 22.86 -45.72 180)
					(length 3.81)
					(name "A60")
					(number "A60")
				)
				(pin passive line
					(at 22.86 -48.26 180)
					(length 3.81)
					(name "A61")
					(number "A61")
				)
				(pin passive line
					(at 22.86 -50.8 180)
					(length 3.81)
					(name "A62")
					(number "A62")
				)
				(pin passive line
					(at 22.86 -53.34 180)
					(length 3.81)
					(name "A63")
					(number "A63")
				)
				(pin passive line
					(at 22.86 -55.88 180)
					(length 3.81)
					(name "A64")
					(number "A64")
				)
				(pin passive line
					(at 22.86 -58.42 180)
					(length 3.81)
					(name "A65")
					(number "A65")
				)
				(pin passive line
					(at 22.86 -60.96 180)
					(length 3.81)
					(name "A66")
					(number "A66")
				)
				(pin passive line
					(at 22.86 -63.5 180)
					(length 3.81)
					(name "A67")
					(number "A67")
				)
				(pin passive line
					(at 22.86 -66.04 180)
					(length 3.81)
					(name "A68")
					(number "A68")
				)
				(pin passive line
					(at 22.86 -68.58 180)
					(length 3.81)
					(name "A69")
					(number "A69")
				)
				(pin passive line
					(at 22.86 -71.12 180)
					(length 3.81)
					(name "A70")
					(number "A70")
				)
				(pin passive line
					(at 22.86 -73.66 180)
					(length 3.81)
					(name "A71")
					(number "A71")
				)
				(pin passive line
					(at 22.86 -76.2 180)
					(length 3.81)
					(name "A72")
					(number "A72")
				)
				(pin passive line
					(at 22.86 -78.74 180)
					(length 3.81)
					(name "A73")
					(number "A73")
				)
				(pin passive line
					(at 22.86 -81.28 180)
					(length 3.81)
					(name "A74")
					(number "A74")
				)
				(pin passive line
					(at 22.86 -83.82 180)
					(length 3.81)
					(name "A75")
					(number "A75")
				)
				(pin passive line
					(at 22.86 -86.36 180)
					(length 3.81)
					(name "A76")
					(number "A76")
				)
				(pin passive line
					(at 22.86 -88.9 180)
					(length 3.81)
					(name "A77")
					(number "A77")
				)
				(pin passive line
					(at 22.86 -91.44 180)
					(length 3.81)
					(name "A78")
					(number "A78")
				)
				(pin passive line
					(at 22.86 -93.98 180)
					(length 3.81)
					(name "A79")
					(number "A79")
				)
				(pin passive line
					(at 22.86 -96.52 180)
					(length 3.81)
					(name "A80")
					(number "A80")
				)
				(pin passive line
					(at 22.86 -99.06 180)
					(length 3.81)
					(name "A81")
					(number "A81")
				)
				(pin passive line
					(at 22.86 -101.6 180)
					(length 3.81)
					(name "A82")
					(number "A82")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "B42")
					(number "B42")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "B43")
					(number "B43")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "B44")
					(number "B44")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "B45")
					(number "B45")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "B46")
					(number "B46")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "B47")
					(number "B47")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "B48")
					(number "B48")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(name "B49")
					(number "B49")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(name "B50")
					(number "B50")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "B51")
					(number "B51")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "B52")
					(number "B52")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(name "B53")
					(number "B53")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(name "B54")
					(number "B54")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 3.81)
					(name "B55")
					(number "B55")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 3.81)
					(name "B56")
					(number "B56")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 3.81)
					(name "B57")
					(number "B57")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 3.81)
					(name "B58")
					(number "B58")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 3.81)
					(name "B59")
					(number "B59")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 3.81)
					(name "B60")
					(number "B60")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 3.81)
					(name "B61")
					(number "B61")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 3.81)
					(name "B62")
					(number "B62")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 3.81)
					(name "B63")
					(number "B63")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "B64")
					(number "B64")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "B65")
					(number "B65")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(name "B66")
					(number "B66")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 3.81)
					(name "B67")
					(number "B67")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 3.81)
					(name "B68")
					(number "B68")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 3.81)
					(name "B69")
					(number "B69")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(name "B70")
					(number "B70")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 3.81)
					(name "B71")
					(number "B71")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 3.81)
					(name "B72")
					(number "B72")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(name "B73")
					(number "B73")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 3.81)
					(name "B74")
					(number "B74")
				)
				(pin passive line
					(at 0 -83.82 0)
					(length 3.81)
					(name "B75")
					(number "B75")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 3.81)
					(name "B76")
					(number "B76")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 3.81)
					(name "B77")
					(number "B77")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 3.81)
					(name "B78")
					(number "B78")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 3.81)
					(name "B79")
					(number "B79")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 3.81)
					(name "B80")
					(number "B80")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 3.81)
					(name "B81")
					(number "B81")
				)
				(pin passive line
					(at 0 -101.6 0)
					(length 3.81)
					(name "B82")
					(number "B82")
				)
				(pin passive line
					(at 0 -106.68 0)
					(length 3.81)
					(name "S1")
					(number "S1")
				)
				(pin passive line
					(at 22.86 -106.68 180)
					(length 3.81)
					(name "S2")
					(number "S2")
				)
			)
			(embedded_fonts no)
		)
)
