(footprint "Conn_Molex_Nano-Fit_1x2_105313-2202_Horizontal"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Molex Nano-Fit Power Connectors, 2 Pins per row")
	(tags "connector Molex Nano-Fit NanoFit top entry 2.50mm horizontal")
	(property "Reference" "REF**"
		(at 0 -2.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Molex_Nano-Fit_1x2_105313-2202_Horizontal"
		(at 0 5.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.1 7.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.1 8.6 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.1 9.8 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 7.179 0)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.179 2.499)
		(size 1.7 1.7)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole custom
		(at 0 0)
		(size 1.417157 1.417157)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.85 -0.6) (xy 0.85 -0.6) (xy 0.85 0.6) (xy -0.45 0.6) (xy -0.85 0.2)
				)
				(width 0.5)
				(fill yes)
			)
		)
	)
	(pad "2" thru_hole oval
		(at 0 2.499)
		(size 2.2 1.7)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_105313_2202.glb"
		(offset
			(xyz 6.15 -1.25 2.1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -90)
		)
	)
)
