(footprint "Conn_Molex_Nano-Fit_2x5_105405-1110"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Pin Header, Horizontal, Power, 2.5 mm, 2 Rows, 10 Contacts, SMD, Nano-Fit 105310")
	(tags "Connector Molex Nano-Fit")
	(property "Reference" "REF**"
		(at 5.5 -10.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Molex_Nano-Fit_2x5_105405-1110"
		(at 3.7 5.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -7.3 8.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -7.3 9.6 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -3.5 6.8 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at 5 -7.985)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "2" smd roundrect
		(at 2.5 -7.985)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "3" smd roundrect
		(at 0 -7.985)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "4" smd roundrect
		(at -2.5 -7.985)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "5" smd roundrect
		(at -5 -7.985)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "6" smd roundrect
		(at 5 -4.685)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "7" smd roundrect
		(at 2.5 -4.685)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "8" smd roundrect
		(at 0 -4.685)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "9" smd roundrect
		(at -2.5 -4.685)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "10" smd roundrect
		(at -5 -4.685)
		(size 1.24 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "MP" smd roundrect
		(at -7.57 0.245)
		(size 1.1 8.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "MP" smd roundrect
		(at 6.97 0.245)
		(size 1.1 8.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(embedded_fonts no)
	(model "antmicro_105405_1110.glb"
		(offset
			(xyz 0.3 4.3 3.25)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
