(footprint "Conn_Molex_Nano-Fit_2x5_105429-1210"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Pin Header, Vertical, Power, 2.5 mm, 2 Rows, 10 Contacts, SMD, Nano-Fit 105429")
	(tags "connector Molex Nano-Fit")
	(property "Reference" "REF**"
		(at 5.3 -6.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Molex_Nano-Fit_2x5_105429-1210"
		(at 2.9 6.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8.2 8.5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.2 9.7 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.2 10.9 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at 5 -2.775)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "2" smd roundrect
		(at 2.5 -2.775)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "3" smd roundrect
		(at 0 -2.775)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "4" smd roundrect
		(at -2.5 -2.775)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "5" smd roundrect
		(at -5 -2.775)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "6" smd roundrect
		(at 5 3.725)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "7" smd roundrect
		(at 2.5 3.725)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "8" smd roundrect
		(at 0 3.725)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "9" smd roundrect
		(at -2.5 3.725)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "10" smd roundrect
		(at -5 3.725)
		(size 1.24 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2016129032)
	)
	(pad "MP" smd roundrect
		(at -6.805 0.475)
		(size 1.1 10.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "MP" smd roundrect
		(at 6.805 0.475)
		(size 1.1 10.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(embedded_fonts no)
	(model "antmicro_105429_1210.glb"
		(offset
			(xyz 0 -0.5 1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
