(footprint "Conn_Molex_Nano-Fit_1x2_SMD_1054301202"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Molex Nano-Fit Power Connectors, 105430-xx02, 2 Pins per row")
	(tags "connector Molex Nano-Fit")
	(property "Reference" "REF**"
		(at 0 -6.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Molex_Nano-Fit_1x2_SMD_1054301202"
		(at 0 7.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -4.77 8.11 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.77 9.31 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.77 10.51 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at 1.528 -4.901 90)
		(size 2.5 1.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.97 -4.901 90)
		(size 2.5 1.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -3.54 0.029)
		(size 1.1 8.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at 3.499 0.029)
		(size 1.1 8.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_105430_1202.glb"
		(offset
			(xyz 0.28 4.9 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
