(footprint "RJ45_1149611"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1 -4.8 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_1149611"
		(at 4.464 12.538 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8.6 14.538 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8.6 15.739 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8.6 16.938 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.427 -9.051)
		(size 0.7 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.156 -9.051)
		(size 0.7 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.885 -9.051)
		(size 0.7 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.615 -9.051)
		(size 0.7 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0.654 -9.051)
		(size 0.7 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.923 -9.051)
		(size 0.7 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.193 -9.051)
		(size 0.7 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.464 -9.051)
		(size 0.7 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -2.98 9.249)
		(size 3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 3.019 9.249)
		(size 3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_1149611.glb"
		(offset
			(xyz 8.05 10.05 13)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 180)
		)
	)
)
