(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB-C_Amphenol_12401598E4"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB-C_Amphenol_12401598E4"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB-C_Amphenol_12401598E4"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.amphenol-icc.com/media/wysiwyg/files/drawing/12401598xxx2a.pdf"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB-C (USB TYPE-C) USB 3.2 Gen 2 (USB 3.1 Gen 2, Superspeed + (USB 3.1)) Receptacle Connector 24 Position Surface Mount, Right Angle"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "12401598E4#2A"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "USB, CONNECTOR, SMT, HORIZONTAL"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB-C_Amphenol_12401598E4_1_1"
				(pin power_in line
					(at 0 -63.5 180)
					(length 3.81)
					(name "GND")
					(number "A1")
				)
				(pin bidirectional line
					(at 0 -33.02 180)
					(length 3.81)
					(name "TX_{1}+")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 -35.56 180)
					(length 3.81)
					(name "TX_{1}-")
					(number "A3")
				)
				(pin passive line
					(at 0 0 180)
					(length 3.81)
					(name "VBUS")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 3.81)
					(name "CC_{1}")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 3.81)
					(name "D_{A}+")
					(number "A6")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 3.81)
					(name "D_{A}-")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -55.88 180)
					(length 3.81)
					(name "SBU_{1}")
					(number "A8")
				)
				(pin passive line
					(at 0 0 180)
					(length 3.81)
					(name "VBUS")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -43.18 180)
					(length 3.81)
					(name "RX_{2}-")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -40.64 180)
					(length 3.81)
					(name "RX_{2}+")
					(number "A11")
				)
				(pin passive line
					(at 0 -63.5 180)
					(length 3.81)
					(name "GND")
					(number "A12")
				)
				(pin passive line
					(at 0 -63.5 180)
					(length 3.81)
					(name "GND")
					(number "B1")
				)
				(pin bidirectional line
					(at 0 -48.26 180)
					(length 3.81)
					(name "TX_{2}+")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -50.8 180)
					(length 3.81)
					(name "TX_{2}-")
					(number "B3")
				)
				(pin passive line
					(at 0 0 180)
					(length 3.81)
					(name "VBUS")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 3.81)
					(name "CC_{2}")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 3.81)
					(name "D_{B}+")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 3.81)
					(name "D_{B}-")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -58.42 180)
					(length 3.81)
					(name "SBU_{2}")
					(number "B8")
				)
				(pin passive line
					(at 0 0 180)
					(length 3.81)
					(name "VBUS")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 3.81)
					(name "RX_{1}-")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 3.81)
					(name "RX_{1}+")
					(number "B11")
				)
				(pin passive line
					(at 0 -63.5 180)
					(length 3.81)
					(name "GND")
					(number "B12")
				)
				(pin passive line
					(at 0 -66.04 180)
					(length 3.81)
					(name "SH")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
