(footprint "Conn_Phoenix_XS_1x2_1778764_Horizontal"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5.3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Phoenix_XS_1x2_1778764_Horizontal"
		(at 0 6.15 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -6.55 14.29 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -6.55 15.49 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.55 16.69 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.327 -1.874 180)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.374 -1.874 180)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Mask")
	)
	(pad "1" smd rect
		(at 1.274 3.475 180)
		(size 1.2 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.225 3.475 180)
		(size 1.2 3.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -4.825 -0.726 180)
		(size 2.2 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 4.873 -0.726 180)
		(size 2.2 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_1778764.glb"
		(offset
			(xyz -3.301 4.79 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 -180 -90)
		)
	)
)
