(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_M.2_1-2199230-6"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_M.2_1-2199230-6"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_M.2_1-2199230-6"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=2199230&DocType=Customer+Drawing&DocLang=English"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Key M Card Edge Connector, 0, Dual Side, 67 Contacts, Surface Mount, Right Angle, Solder"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "1-2199230-6"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, SMT, PCIE, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_M.2_1-2199230-6_0_0"
				(text "KEY M"
					(at 15.24 0 0)
				)
			)
			(symbol "Bus_M.2_1-2199230-6_1_1"
				(pin power_in line
					(at 30.48 -77.47 180)
					(length 3.81)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "2")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "4")
				)
				(pin output line
					(at 0 -77.47 0)
					(length 3.81)
					(name "PER3_N")
					(number "5")
				)
				(pin no_connect line
					(at 26.67 -39.37 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin output line
					(at 0 -74.93 0)
					(length 3.81)
					(name "PER3_P")
					(number "7")
				)
				(pin no_connect line
					(at 26.67 -64.77 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin passive line
					(at 30.48 -54.61 180)
					(length 3.81)
					(name "LED")
					(number "10")
				)
				(pin input line
					(at 0 -69.85 0)
					(length 3.81)
					(name "PET3_N")
					(number "11")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(name "3V3")
					(number "12")
				)
				(pin input line
					(at 0 -67.31 0)
					(length 3.81)
					(name "PET3_P")
					(number "13")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "14")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "15")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "16")
				)
				(pin output line
					(at 0 -62.23 0)
					(length 3.81)
					(name "PER2_N")
					(number "17")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "18")
				)
				(pin output line
					(at 0 -59.69 0)
					(length 3.81)
					(name "PER2_P")
					(number "19")
				)
				(pin no_connect line
					(at 26.67 -44.45 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin no_connect line
					(at 26.67 -45.72 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "22")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 3.81)
					(name "PET2_N")
					(number "23")
				)
				(pin no_connect line
					(at 26.67 -46.99 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "24")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 3.81)
					(name "PET2_P")
					(number "25")
				)
				(pin no_connect line
					(at 26.67 -59.69 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "26")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "27")
				)
				(pin no_connect line
					(at 26.67 -60.96 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "28")
				)
				(pin output line
					(at 0 -46.99 0)
					(length 3.81)
					(name "PER1_N")
					(number "29")
				)
				(pin no_connect line
					(at 26.67 -62.23 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin output line
					(at 0 -44.45 0)
					(length 3.81)
					(name "PER1_P")
					(number "31")
				)
				(pin no_connect line
					(at 26.67 -63.5 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "32")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "33")
				)
				(pin no_connect line
					(at 26.67 -66.04 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "34")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 3.81)
					(name "PET1_N")
					(number "35")
				)
				(pin no_connect line
					(at 26.67 -67.31 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "36")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 3.81)
					(name "PET1_P")
					(number "37")
				)
				(pin no_connect line
					(at 26.67 -69.85 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "38")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin input line
					(at 30.48 -31.75 180)
					(length 3.81)
					(name "SMB_CLK")
					(number "40")
				)
				(pin output line
					(at 0 -31.75 0)
					(length 3.81)
					(name "PER0_N")
					(number "41")
				)
				(pin bidirectional line
					(at 30.48 -29.21 180)
					(length 3.81)
					(name "SMB_DATA")
					(number "42")
				)
				(pin output line
					(at 0 -29.21 0)
					(length 3.81)
					(name "PER0_P")
					(number "43")
				)
				(pin output line
					(at 30.48 -26.67 180)
					(length 3.81)
					(name "ALERT")
					(number "44")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "45")
				)
				(pin no_connect line
					(at 26.67 -68.58 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "46")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "PET0_N")
					(number "47")
				)
				(pin no_connect line
					(at 26.67 -41.91 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "48")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 3.81)
					(name "PET0_P")
					(number "49")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "~{PERST}")
					(number "50")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "51")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 3.81)
					(name "~{CLKREQ}")
					(number "52")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "REFCLK_N")
					(number "53")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "~{PEWAKE}")
					(number "54")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "REFCLK_P")
					(number "55")
				)
				(pin no_connect line
					(at 26.67 -43.18 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "56")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "57")
				)
				(pin no_connect line
					(at 26.67 -71.12 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "58")
				)
				(pin no_connect line
					(at 26.67 -40.64 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "67")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "SUSCLK")
					(number "68")
				)
				(pin no_connect line
					(at 26.67 -38.1 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "69")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "70")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "71")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "72")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "73")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "3V3")
					(number "74")
				)
				(pin passive line
					(at 30.48 -77.47 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "75")
				)
				(pin passive line
					(at 30.48 -74.93 180)
					(length 3.81)
					(name "MP")
					(number "MP1")
				)
				(pin passive line
					(at 30.48 -74.93 180)
					(length 3.81)
					(hide yes)
					(name "MP")
					(number "MP2")
				)
			)
			(embedded_fonts no)
		)
)
