(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Socket_TE_MULTI-BEAM_2x5_1-2212115-4"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 19.05 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Socket_TE_MULTI-BEAM_2x5_1-2212115-4"
				(at 19.05 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Socket_TE_MULTI-BEAM_2x5_1-2212115-4"
				(at 19.05 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/usa-en/product-1-2212115-4.datasheet.pdf"
				(at 19.05 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Card Edge Power Connectors, Board-to-Board, 10 Position, 7.26mm"
				(at 19.05 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "1-2212115-4"
				(at 19.05 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 19.05 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 19.05 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 19.05 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "RECEPTACLE,  CONNECTOR, FEMALE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Socket_TE_MULTI-BEAM_2x5_1-2212115-4_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "P1")
					(number "1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "P2")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "S1")
					(number "7")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "S2")
					(number "8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "S3")
					(number "9")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "S4")
					(number "10")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "S5")
					(number "11")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "S6")
					(number "12")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "S7")
					(number "13")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "S8")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
