(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Socket_TE_2x84_1-2340321-2"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 58.42 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Socket_TE_2x84_1-2340321-2"
				(at 58.42 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Socket_TE_2x84_1-2340321-2"
				(at 58.42 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=2340321&DocType=Customer%20Drawing&DocLang=English&DocFormat=pdf&PartCntxt=1-2340321-2"
				(at 58.42 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "PCB Edge Card, Straddle Mount, 168 Position"
				(at 58.42 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "1-2340321-2"
				(at 58.42 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 58.42 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 58.42 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "RECEPTACLE,  CONNECTOR, FEMALE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Socket_TE_2x84_1-2340321-2_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "SGND_OA1")
					(number "OA1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "SIG_OA2")
					(number "OA2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "SIG_OA3")
					(number "OA3")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "SGND_OA4")
					(number "OA4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SIG_OA5")
					(number "OA5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "SIG_OA6")
					(number "OA6")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "SGND_OA7")
					(number "OA7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "SIG_OA8")
					(number "OA8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "SIG_OA9")
					(number "OA9")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "SGND_OA10")
					(number "OA10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "SIG_OA11")
					(number "OA11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "SIG_OA12")
					(number "OA12")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "SGND_OA13")
					(number "OA13")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 5.08)
					(name "SGND_OA14")
					(number "OA14")
				)
				(pin power_in line
					(at 45.72 0 180)
					(length 5.08)
					(name "SGND_OB1")
					(number "OB1")
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "SIG_OB2")
					(number "OB2")
				)
				(pin passive line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "SIG_OB3")
					(number "OB3")
				)
				(pin power_in line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "SGND_OB4")
					(number "OB4")
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "SIG_OB5")
					(number "OB5")
				)
				(pin passive line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "SIG_OB6")
					(number "OB6")
				)
				(pin power_in line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "SGND_OB7")
					(number "OB7")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "SIG_OB8")
					(number "OB8")
				)
				(pin passive line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "SIG_OB9")
					(number "OB9")
				)
				(pin power_in line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "SGND_OB10")
					(number "OB10")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "SIG_OB11")
					(number "OB11")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(name "SIG_OB12")
					(number "OB12")
				)
				(pin power_in line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "SGND_OB13")
					(number "OB13")
				)
				(pin power_in line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "SGND_OB14")
					(number "OB14")
				)
			)
			(symbol "Socket_TE_2x84_1-2340321-2_2_1"
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "SGND_A1")
					(number "A1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "SIG_A2")
					(number "A2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "SIG_A3")
					(number "A3")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "SGND_A4")
					(number "A4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SIG_A5")
					(number "A5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "SIG_A6")
					(number "A6")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "SGND_A7")
					(number "A7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "SIG_A8")
					(number "A8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "SIG_A9")
					(number "A9")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "SGND_A10")
					(number "A10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "SIG_A11")
					(number "A11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "SIG_A12")
					(number "A12")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "SGND_A13")
					(number "A13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "SIG_A14")
					(number "A14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "SIG_A15")
					(number "A15")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 5.08)
					(name "SGND_A16")
					(number "A16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "SIG_A17")
					(number "A17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "SIG_A18")
					(number "A18")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 5.08)
					(name "SGND_A19")
					(number "A19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "SIG_A20")
					(number "A20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "SIG_A21")
					(number "A21")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 5.08)
					(name "SGND_A22")
					(number "A22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "SIG_A23")
					(number "A23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "SIG_A24")
					(number "A24")
				)
				(pin power_in line
					(at 0 -60.96 0)
					(length 5.08)
					(name "SGND_A25")
					(number "A25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "SIG_A26")
					(number "A26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "SIG_A27")
					(number "A27")
				)
				(pin power_in line
					(at 0 -68.58 0)
					(length 5.08)
					(name "SGND_A28")
					(number "A28")
				)
				(pin power_in line
					(at 45.72 0 180)
					(length 5.08)
					(name "SGND_B1")
					(number "B1")
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "SIG_B2")
					(number "B2")
				)
				(pin passive line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "SIG_B3")
					(number "B3")
				)
				(pin power_in line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "SGND_B4")
					(number "B4")
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "SIG_B5")
					(number "B5")
				)
				(pin passive line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "SIG_B6")
					(number "B6")
				)
				(pin power_in line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "SGND_B7")
					(number "B7")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "SIG_B8")
					(number "B8")
				)
				(pin passive line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "SIG_B9")
					(number "B9")
				)
				(pin power_in line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "SGND_B10")
					(number "B10")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "SIG_B11")
					(number "B11")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(name "SIG_B12")
					(number "B12")
				)
				(pin power_in line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "SGND_B13")
					(number "B13")
				)
				(pin passive line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "SIG_B14")
					(number "B14")
				)
				(pin passive line
					(at 45.72 -35.56 180)
					(length 5.08)
					(name "SIG_B15")
					(number "B15")
				)
				(pin power_in line
					(at 45.72 -38.1 180)
					(length 5.08)
					(name "SGND_B16")
					(number "B16")
				)
				(pin passive line
					(at 45.72 -40.64 180)
					(length 5.08)
					(name "SIG_B17")
					(number "B17")
				)
				(pin passive line
					(at 45.72 -43.18 180)
					(length 5.08)
					(name "SIG_B18")
					(number "B18")
				)
				(pin power_in line
					(at 45.72 -45.72 180)
					(length 5.08)
					(name "SGND_B19")
					(number "B19")
				)
				(pin passive line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "SIG_B20")
					(number "B20")
				)
				(pin passive line
					(at 45.72 -50.8 180)
					(length 5.08)
					(name "SIG_B21")
					(number "B21")
				)
				(pin power_in line
					(at 45.72 -53.34 180)
					(length 5.08)
					(name "SGND_B22")
					(number "B22")
				)
				(pin passive line
					(at 45.72 -55.88 180)
					(length 5.08)
					(name "SIG_B23")
					(number "B23")
				)
				(pin passive line
					(at 45.72 -58.42 180)
					(length 5.08)
					(name "SIG_B24")
					(number "B24")
				)
				(pin power_in line
					(at 45.72 -60.96 180)
					(length 5.08)
					(name "SGND_B25")
					(number "B25")
				)
				(pin passive line
					(at 45.72 -63.5 180)
					(length 5.08)
					(name "SIG_B26")
					(number "B26")
				)
				(pin passive line
					(at 45.72 -66.04 180)
					(length 5.08)
					(name "SIG_B27")
					(number "B27")
				)
				(pin power_in line
					(at 45.72 -68.58 180)
					(length 5.08)
					(name "SGND_B28")
					(number "B28")
				)
			)
			(symbol "Socket_TE_2x84_1-2340321-2_3_1"
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "SGND_A29")
					(number "A29")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "SIG_A30")
					(number "A30")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "SIG_A31")
					(number "A31")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "SGND_A32")
					(number "A32")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SIG_A33")
					(number "A33")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "SIG_A34")
					(number "A34")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "SGND_A35")
					(number "A35")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "SIG_A36")
					(number "A36")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "SIG_A37")
					(number "A37")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "SGND_A38")
					(number "A38")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "SIG_A39")
					(number "A39")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "SIG_A40")
					(number "A40")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "SGND_A41")
					(number "A41")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 5.08)
					(name "SGND_A42")
					(number "A42")
				)
				(pin power_in line
					(at 45.72 0 180)
					(length 5.08)
					(name "SGND_B29")
					(number "B29")
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "SIG_B30")
					(number "B30")
				)
				(pin passive line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "SIG_B31")
					(number "B31")
				)
				(pin power_in line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "SGND_B32")
					(number "B32")
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "SIG_B33")
					(number "B33")
				)
				(pin passive line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "SIG_B34")
					(number "B34")
				)
				(pin power_in line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "SGND_B35")
					(number "B35")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "SIG_B36")
					(number "B36")
				)
				(pin passive line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "SIG_B37")
					(number "B37")
				)
				(pin power_in line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "SGND_B38")
					(number "B38")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "SIG_B39")
					(number "B39")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(name "SIG_B40")
					(number "B40")
				)
				(pin power_in line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "SGND_B41")
					(number "B41")
				)
				(pin power_in line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "SGND_B42")
					(number "B42")
				)
			)
			(symbol "Socket_TE_2x84_1-2340321-2_4_1"
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "SGND_A43")
					(number "A43")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "SIG_A44")
					(number "A44")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "SIG_A45")
					(number "A45")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "SGND_A46")
					(number "A46")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SIG_A47")
					(number "A47")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "SIG_A48")
					(number "A48")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "SGND_A49")
					(number "A49")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "SIG_A50")
					(number "A50")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "SIG_A51")
					(number "A51")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "SGND_A52")
					(number "A52")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "SIG_A53")
					(number "A53")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "SIG_A54")
					(number "A54")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "SGND_A55")
					(number "A55")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "SIG_A56")
					(number "A56")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "SIG_A57")
					(number "A57")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 5.08)
					(name "SGND_A58")
					(number "A58")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "SIG_A59")
					(number "A59")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "SIG_A60")
					(number "A60")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 5.08)
					(name "SGND_A61")
					(number "A61")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "SIG_A62")
					(number "A62")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "SIG_A63")
					(number "A63")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 5.08)
					(name "SGND_A64")
					(number "A64")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "SIG_A65")
					(number "A65")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "SIG_A66")
					(number "A66")
				)
				(pin power_in line
					(at 0 -60.96 0)
					(length 5.08)
					(name "SGND_A67")
					(number "A67")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "SIG_A68")
					(number "A68")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "SIG_A69")
					(number "A69")
				)
				(pin power_in line
					(at 0 -68.58 0)
					(length 5.08)
					(name "SGND_A70")
					(number "A70")
				)
				(pin power_in line
					(at 45.72 0 180)
					(length 5.08)
					(name "SGND_B43")
					(number "B43")
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "SIG_B44")
					(number "B44")
				)
				(pin passive line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "SIG_B45")
					(number "B45")
				)
				(pin power_in line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "SGND_B46")
					(number "B46")
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "SIG_B47")
					(number "B47")
				)
				(pin passive line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "SIG_B48")
					(number "B48")
				)
				(pin power_in line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "SGND_B49")
					(number "B49")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "SIG_B50")
					(number "B50")
				)
				(pin passive line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "SIG_B51")
					(number "B51")
				)
				(pin power_in line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "SGND_B52")
					(number "B52")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "SIG_B53")
					(number "B53")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(name "SIG_B54")
					(number "B54")
				)
				(pin power_in line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "SGND_B55")
					(number "B55")
				)
				(pin passive line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "SIG_B56")
					(number "B56")
				)
				(pin passive line
					(at 45.72 -35.56 180)
					(length 5.08)
					(name "SIG_B57")
					(number "B57")
				)
				(pin power_in line
					(at 45.72 -38.1 180)
					(length 5.08)
					(name "SGND_B58")
					(number "B58")
				)
				(pin passive line
					(at 45.72 -40.64 180)
					(length 5.08)
					(name "SIG_B59")
					(number "B59")
				)
				(pin passive line
					(at 45.72 -43.18 180)
					(length 5.08)
					(name "SIG_B60")
					(number "B60")
				)
				(pin power_in line
					(at 45.72 -45.72 180)
					(length 5.08)
					(name "SGND_B61")
					(number "B61")
				)
				(pin passive line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "SIG_B62")
					(number "B62")
				)
				(pin passive line
					(at 45.72 -50.8 180)
					(length 5.08)
					(name "SIG_B63")
					(number "B63")
				)
				(pin power_in line
					(at 45.72 -53.34 180)
					(length 5.08)
					(name "SGND_B64")
					(number "B64")
				)
				(pin passive line
					(at 45.72 -55.88 180)
					(length 5.08)
					(name "SIG_B65")
					(number "B65")
				)
				(pin passive line
					(at 45.72 -58.42 180)
					(length 5.08)
					(name "SIG_B66")
					(number "B66")
				)
				(pin power_in line
					(at 45.72 -60.96 180)
					(length 5.08)
					(name "SGND_B67")
					(number "B67")
				)
				(pin passive line
					(at 45.72 -63.5 180)
					(length 5.08)
					(name "SIG_B68")
					(number "B68")
				)
				(pin passive line
					(at 45.72 -66.04 180)
					(length 5.08)
					(name "SIG_B69")
					(number "B69")
				)
				(pin power_in line
					(at 45.72 -68.58 180)
					(length 5.08)
					(name "SGND_B70")
					(number "B70")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "SHIELD")
					(number "S1")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "SHIELD__1")
					(number "S2")
				)
			)
			(embedded_fonts no)
		)
)
