(footprint "Conn_Hermaphroditic_Molex_203456-0003"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Footprint based on: https://www.molex.com/content/dam/molex/molex-dot-com/products/automated/en-us/salesdrawingpdf/203/203456/2034560003_sd.pdf")
	(property "Reference" "J**"
		(at 0.115 -12.405 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Hermaphroditic_Molex_203456-0003"
		(at 0.115 12.895 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.102 -0.201 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.102 -0.201 0)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin 0.05)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -33.245 13.795 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -33.245 14.995 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -33.245 16.195 0)
		(layer "F.Fab")
	)
	(pad "A3" smd circle
		(at -28.4 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -27.5 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -26.6 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at -25.7 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at -24.8 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at -23.9 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at -23 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at -22.1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at -21.2 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at -20.3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at -19 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd circle
		(at -18.1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd circle
		(at -17.2 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd circle
		(at -16.3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd circle
		(at -15 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd circle
		(at -14.1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd circle
		(at -13.2 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd circle
		(at -12.3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd circle
		(at -11 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd circle
		(at -10.1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd circle
		(at -9.2 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A24" smd circle
		(at -8.3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A25" smd circle
		(at -7 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A26" smd circle
		(at -6.1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A27" smd circle
		(at -5.2 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A28" smd circle
		(at -4.3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A29" smd circle
		(at -3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A30" smd circle
		(at -2.1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A31" smd circle
		(at -1.2 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A32" smd circle
		(at -0.3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A33" smd circle
		(at 1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A34" smd circle
		(at 1.9 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A35" smd circle
		(at 2.8 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A36" smd circle
		(at 3.7 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A37" smd circle
		(at 5 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A38" smd circle
		(at 5.9 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A39" smd circle
		(at 6.8 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A40" smd circle
		(at 7.7 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A41" smd circle
		(at 8.6 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A42" smd circle
		(at 9.5 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A43" smd circle
		(at 10.4 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A44" smd circle
		(at 11.3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A45" smd circle
		(at 12.2 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A46" smd circle
		(at 13.1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A47" smd circle
		(at 14 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A48" smd circle
		(at 14.9 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A49" smd circle
		(at 15.8 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A50" smd circle
		(at 16.7 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A51" smd circle
		(at 17.6 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A52" smd circle
		(at 18.5 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A53" smd circle
		(at 19.4 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A54" smd circle
		(at 20.3 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A55" smd circle
		(at 21.2 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A56" smd circle
		(at 22.1 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A57" smd circle
		(at 23 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A58" smd circle
		(at 23.9 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A59" smd circle
		(at 24.8 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A60" smd circle
		(at 25.7 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A61" smd circle
		(at 26.6 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A62" smd circle
		(at 27.5 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A63" smd circle
		(at 28.4 -7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -28.2 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -27.3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -26.4 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -25.5 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -24.6 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at -23.7 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at -22.8 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at -21.9 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at -21 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at -20.1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at -19.2 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at -18.3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd circle
		(at -17 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd circle
		(at -16.1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd circle
		(at -15.2 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd circle
		(at -14.3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd circle
		(at -13 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd circle
		(at -12.1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B21" smd circle
		(at -11.2 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B22" smd circle
		(at -10.3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B23" smd circle
		(at -9 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B24" smd circle
		(at -8.1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B25" smd circle
		(at -7.2 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B26" smd circle
		(at -6.3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B27" smd circle
		(at -5 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B28" smd circle
		(at -4.1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B29" smd circle
		(at -3.2 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B30" smd circle
		(at -2.3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B31" smd circle
		(at -1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B32" smd circle
		(at -0.1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B33" smd circle
		(at 0.8 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B34" smd circle
		(at 1.7 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B35" smd circle
		(at 3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B36" smd circle
		(at 3.9 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B37" smd circle
		(at 4.8 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B38" smd circle
		(at 5.7 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B39" smd circle
		(at 7 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B40" smd circle
		(at 7.9 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B41" smd circle
		(at 8.8 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B42" smd circle
		(at 9.7 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B43" smd circle
		(at 10.6 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B44" smd circle
		(at 11.5 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B45" smd circle
		(at 12.4 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B46" smd circle
		(at 13.3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B47" smd circle
		(at 14.2 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B48" smd circle
		(at 15.1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B49" smd circle
		(at 16 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B50" smd circle
		(at 16.9 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B51" smd circle
		(at 17.8 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B52" smd circle
		(at 18.7 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B53" smd circle
		(at 19.6 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B54" smd circle
		(at 20.5 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B55" smd circle
		(at 21.4 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B56" smd circle
		(at 22.3 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B57" smd circle
		(at 23.2 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B58" smd circle
		(at 24.1 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B59" smd circle
		(at 25 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B60" smd circle
		(at 25.9 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B61" smd circle
		(at 26.8 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B62" smd circle
		(at 27.7 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B63" smd circle
		(at 28.6 -6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -30.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -29.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -28.4 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -27.5 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at -26.6 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at -25.7 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at -24.8 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at -23.9 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at -23 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at -22.1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at -21.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C12" smd circle
		(at -20.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C13" smd circle
		(at -19 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C14" smd circle
		(at -18.1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C15" smd circle
		(at -17.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C16" smd circle
		(at -16.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C17" smd circle
		(at -15 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C18" smd circle
		(at -14.1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C19" smd circle
		(at -13.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C20" smd circle
		(at -12.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C21" smd circle
		(at -11 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C22" smd circle
		(at -10.1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C23" smd circle
		(at -9.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C24" smd circle
		(at -8.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C25" smd circle
		(at -7 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C26" smd circle
		(at -6.1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C27" smd circle
		(at -5.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C28" smd circle
		(at -4.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C29" smd circle
		(at -3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C30" smd circle
		(at -2.1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C31" smd circle
		(at -1.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C32" smd circle
		(at -0.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C33" smd circle
		(at 1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C34" smd circle
		(at 1.9 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C35" smd circle
		(at 2.8 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C36" smd circle
		(at 3.7 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C37" smd circle
		(at 5 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C38" smd circle
		(at 5.9 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C39" smd circle
		(at 6.8 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C40" smd circle
		(at 7.7 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C41" smd circle
		(at 8.6 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C42" smd circle
		(at 9.5 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C43" smd circle
		(at 10.4 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C44" smd circle
		(at 11.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C45" smd circle
		(at 12.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C46" smd circle
		(at 13.1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C47" smd circle
		(at 14 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C48" smd circle
		(at 14.9 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C49" smd circle
		(at 15.8 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C50" smd circle
		(at 16.7 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C51" smd circle
		(at 17.6 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C52" smd circle
		(at 18.5 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C53" smd circle
		(at 19.4 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C54" smd circle
		(at 20.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C55" smd circle
		(at 21.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C56" smd circle
		(at 22.1 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C57" smd circle
		(at 23 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C58" smd circle
		(at 23.9 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C59" smd circle
		(at 24.8 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C60" smd circle
		(at 25.7 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C61" smd circle
		(at 26.6 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C62" smd circle
		(at 27.5 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C63" smd circle
		(at 28.4 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C64" smd circle
		(at 29.3 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C65" smd circle
		(at 30.2 -4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -30 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -29.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -28.2 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -27.3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -26.4 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -25.5 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D7" smd circle
		(at -24.6 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at -23.7 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at -22.8 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at -21.9 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at -21 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at -20.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at -19.2 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D14" smd circle
		(at -18.3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D15" smd circle
		(at -17 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D16" smd circle
		(at -16.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D17" smd circle
		(at -15.2 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D18" smd circle
		(at -14.3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D19" smd circle
		(at -13 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D20" smd circle
		(at -12.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D21" smd circle
		(at -11.2 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D22" smd circle
		(at -10.3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D23" smd circle
		(at -9 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D24" smd circle
		(at -8.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D25" smd circle
		(at -7.2 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D26" smd circle
		(at -6.3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D27" smd circle
		(at -5 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D28" smd circle
		(at -4.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D29" smd circle
		(at -3.2 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D30" smd circle
		(at -2.3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D31" smd circle
		(at -1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D32" smd circle
		(at -0.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D33" smd circle
		(at 0.8 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D34" smd circle
		(at 1.7 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D35" smd circle
		(at 3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D36" smd circle
		(at 3.9 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D37" smd circle
		(at 4.8 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D38" smd circle
		(at 5.7 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D39" smd circle
		(at 7 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D40" smd circle
		(at 7.9 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D41" smd circle
		(at 8.8 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D42" smd circle
		(at 9.7 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D43" smd circle
		(at 10.6 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D44" smd circle
		(at 11.5 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D45" smd circle
		(at 12.4 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D46" smd circle
		(at 13.3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D47" smd circle
		(at 14.2 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D48" smd circle
		(at 15.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D49" smd circle
		(at 16 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D50" smd circle
		(at 16.9 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D51" smd circle
		(at 17.8 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D52" smd circle
		(at 18.7 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D53" smd circle
		(at 19.6 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D54" smd circle
		(at 20.5 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D55" smd circle
		(at 21.4 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D56" smd circle
		(at 22.3 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D57" smd circle
		(at 23.2 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D58" smd circle
		(at 24.1 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D59" smd circle
		(at 25 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D60" smd circle
		(at 25.9 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D61" smd circle
		(at 26.8 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D62" smd circle
		(at 27.7 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D63" smd circle
		(at 28.6 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D64" smd circle
		(at 29.5 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D65" smd circle
		(at 30.4 -3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -30.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -29.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -28.4 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -27.5 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at -26.6 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at -25.7 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E7" smd circle
		(at -24.8 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at -23.9 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at -23 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E10" smd circle
		(at -22.1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at -21.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E12" smd circle
		(at -20.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E13" smd circle
		(at -19 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E14" smd circle
		(at -18.1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E15" smd circle
		(at -17.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E16" smd circle
		(at -16.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E17" smd circle
		(at -15 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E18" smd circle
		(at -14.1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E19" smd circle
		(at -13.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E20" smd circle
		(at -12.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E21" smd circle
		(at -11 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E22" smd circle
		(at -10.1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E23" smd circle
		(at -9.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E24" smd circle
		(at -8.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E25" smd circle
		(at -7 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E26" smd circle
		(at -6.1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E27" smd circle
		(at -5.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E28" smd circle
		(at -4.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E29" smd circle
		(at -3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E30" smd circle
		(at -2.1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E31" smd circle
		(at -1.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E32" smd circle
		(at -0.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E33" smd circle
		(at 1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E34" smd circle
		(at 1.9 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E35" smd circle
		(at 2.8 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E36" smd circle
		(at 3.7 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E37" smd circle
		(at 5 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E38" smd circle
		(at 5.9 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E39" smd circle
		(at 6.8 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E40" smd circle
		(at 7.7 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E41" smd circle
		(at 8.6 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E42" smd circle
		(at 9.5 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E43" smd circle
		(at 10.4 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E44" smd circle
		(at 11.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E45" smd circle
		(at 12.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E46" smd circle
		(at 13.1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E47" smd circle
		(at 14 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E48" smd circle
		(at 14.9 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E49" smd circle
		(at 15.8 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E50" smd circle
		(at 16.7 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E51" smd circle
		(at 17.6 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E52" smd circle
		(at 18.5 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E53" smd circle
		(at 19.4 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E54" smd circle
		(at 20.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E55" smd circle
		(at 21.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E56" smd circle
		(at 22.1 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E57" smd circle
		(at 23 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E58" smd circle
		(at 23.9 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E59" smd circle
		(at 24.8 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E60" smd circle
		(at 25.7 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E61" smd circle
		(at 26.6 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E62" smd circle
		(at 27.5 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E63" smd circle
		(at 28.4 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E64" smd circle
		(at 29.3 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E65" smd circle
		(at 30.2 -1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -30 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -29.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -28.2 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -27.3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at -26.4 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at -25.5 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F7" smd circle
		(at -24.6 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at -23.7 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at -22.8 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F10" smd circle
		(at -21.9 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at -21 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F12" smd circle
		(at -20.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F13" smd circle
		(at -19.2 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F14" smd circle
		(at -18.3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F15" smd circle
		(at -17 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F16" smd circle
		(at -16.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F17" smd circle
		(at -15.2 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F18" smd circle
		(at -14.3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F19" smd circle
		(at -13 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F20" smd circle
		(at -12.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F21" smd circle
		(at -11.2 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F22" smd circle
		(at -10.3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F23" smd circle
		(at -9 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F24" smd circle
		(at -8.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F25" smd circle
		(at -7.2 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F26" smd circle
		(at -6.3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F27" smd circle
		(at -5 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F28" smd circle
		(at -4.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F29" smd circle
		(at -3.2 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F30" smd circle
		(at -2.3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F31" smd circle
		(at -1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F32" smd circle
		(at -0.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F33" smd circle
		(at 0.8 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F34" smd circle
		(at 1.7 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F35" smd circle
		(at 3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F36" smd circle
		(at 3.9 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F37" smd circle
		(at 4.8 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F38" smd circle
		(at 5.7 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F39" smd circle
		(at 7 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F40" smd circle
		(at 7.9 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F41" smd circle
		(at 8.8 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F42" smd circle
		(at 9.7 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F43" smd circle
		(at 10.6 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F44" smd circle
		(at 11.5 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F45" smd circle
		(at 12.4 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F46" smd circle
		(at 13.3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F47" smd circle
		(at 14.2 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F48" smd circle
		(at 15.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F49" smd circle
		(at 16 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F50" smd circle
		(at 16.9 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F51" smd circle
		(at 17.8 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F52" smd circle
		(at 18.7 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F53" smd circle
		(at 19.6 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F54" smd circle
		(at 20.5 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F55" smd circle
		(at 21.4 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F56" smd circle
		(at 22.3 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F57" smd circle
		(at 23.2 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F58" smd circle
		(at 24.1 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F59" smd circle
		(at 25 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F60" smd circle
		(at 25.9 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F61" smd circle
		(at 26.8 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F62" smd circle
		(at 27.7 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F63" smd circle
		(at 28.6 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F64" smd circle
		(at 29.5 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F65" smd circle
		(at 30.4 0 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -30.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -29.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -28.4 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -27.5 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at -26.6 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G6" smd circle
		(at -25.7 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G7" smd circle
		(at -24.8 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at -23.9 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at -23 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G10" smd circle
		(at -22.1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at -21.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G12" smd circle
		(at -20.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G13" smd circle
		(at -19 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G14" smd circle
		(at -18.1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G15" smd circle
		(at -17.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G16" smd circle
		(at -16.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G17" smd circle
		(at -15 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G18" smd circle
		(at -14.1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G19" smd circle
		(at -13.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G20" smd circle
		(at -12.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G21" smd circle
		(at -11 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G22" smd circle
		(at -10.1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G23" smd circle
		(at -9.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G24" smd circle
		(at -8.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G25" smd circle
		(at -7 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G26" smd circle
		(at -6.1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G27" smd circle
		(at -5.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G28" smd circle
		(at -4.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G29" smd circle
		(at -3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G30" smd circle
		(at -2.1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G31" smd circle
		(at -1.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G32" smd circle
		(at -0.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G33" smd circle
		(at 1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G34" smd circle
		(at 1.9 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G35" smd circle
		(at 2.8 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G36" smd circle
		(at 3.7 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G37" smd circle
		(at 5 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G38" smd circle
		(at 5.9 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G39" smd circle
		(at 6.8 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G40" smd circle
		(at 7.7 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G41" smd circle
		(at 8.6 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G42" smd circle
		(at 9.5 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G43" smd circle
		(at 10.4 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G44" smd circle
		(at 11.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G45" smd circle
		(at 12.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G46" smd circle
		(at 13.1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G47" smd circle
		(at 14 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G48" smd circle
		(at 14.9 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G49" smd circle
		(at 15.8 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G50" smd circle
		(at 16.7 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G51" smd circle
		(at 17.6 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G52" smd circle
		(at 18.5 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G53" smd circle
		(at 19.4 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G54" smd circle
		(at 20.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G55" smd circle
		(at 21.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G56" smd circle
		(at 22.1 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G57" smd circle
		(at 23 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G58" smd circle
		(at 23.9 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G59" smd circle
		(at 24.8 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G60" smd circle
		(at 25.7 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G61" smd circle
		(at 26.6 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G62" smd circle
		(at 27.5 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G63" smd circle
		(at 28.4 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G64" smd circle
		(at 29.3 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G65" smd circle
		(at 30.2 1.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -30 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -29.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -28.2 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -27.3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at -26.4 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at -25.5 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H7" smd circle
		(at -24.6 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at -23.7 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at -22.8 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at -21.9 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at -21 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at -20.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at -19.2 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H14" smd circle
		(at -18.3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H15" smd circle
		(at -17 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H16" smd circle
		(at -16.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H17" smd circle
		(at -15.2 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H18" smd circle
		(at -14.3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H19" smd circle
		(at -13 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H20" smd circle
		(at -12.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H21" smd circle
		(at -11.2 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H22" smd circle
		(at -10.3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H23" smd circle
		(at -9 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H24" smd circle
		(at -8.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H25" smd circle
		(at -7.2 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H26" smd circle
		(at -6.3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H27" smd circle
		(at -5 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H28" smd circle
		(at -4.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H29" smd circle
		(at -3.2 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H30" smd circle
		(at -2.3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H31" smd circle
		(at -1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H32" smd circle
		(at -0.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H33" smd circle
		(at 0.8 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H34" smd circle
		(at 1.7 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H35" smd circle
		(at 3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H36" smd circle
		(at 3.9 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H37" smd circle
		(at 4.8 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H38" smd circle
		(at 5.7 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H39" smd circle
		(at 7 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H40" smd circle
		(at 7.9 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H41" smd circle
		(at 8.8 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H42" smd circle
		(at 9.7 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H43" smd circle
		(at 10.6 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H44" smd circle
		(at 11.5 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H45" smd circle
		(at 12.4 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H46" smd circle
		(at 13.3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H47" smd circle
		(at 14.2 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H48" smd circle
		(at 15.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H49" smd circle
		(at 16 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H50" smd circle
		(at 16.9 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H51" smd circle
		(at 17.8 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H52" smd circle
		(at 18.7 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H53" smd circle
		(at 19.6 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H54" smd circle
		(at 20.5 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H55" smd circle
		(at 21.4 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H56" smd circle
		(at 22.3 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H57" smd circle
		(at 23.2 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H58" smd circle
		(at 24.1 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H59" smd circle
		(at 25 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H60" smd circle
		(at 25.9 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H61" smd circle
		(at 26.8 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H62" smd circle
		(at 27.7 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H63" smd circle
		(at 28.6 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H64" smd circle
		(at 29.5 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H65" smd circle
		(at 30.4 3 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -30.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -29.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -28.4 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -27.5 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -26.6 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at -25.7 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J7" smd circle
		(at -24.8 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at -23.9 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at -23 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at -22.1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at -21.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at -20.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J13" smd circle
		(at -19 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J14" smd circle
		(at -18.1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J15" smd circle
		(at -17.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J16" smd circle
		(at -16.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J17" smd circle
		(at -15 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J18" smd circle
		(at -14.1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J19" smd circle
		(at -13.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J20" smd circle
		(at -12.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J21" smd circle
		(at -11 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J22" smd circle
		(at -10.1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J23" smd circle
		(at -9.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J24" smd circle
		(at -8.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J25" smd circle
		(at -7 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J26" smd circle
		(at -6.1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J27" smd circle
		(at -5.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J28" smd circle
		(at -4.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J29" smd circle
		(at -3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J30" smd circle
		(at -2.1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J31" smd circle
		(at -1.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J32" smd circle
		(at -0.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J33" smd circle
		(at 1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J34" smd circle
		(at 1.9 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J35" smd circle
		(at 2.8 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J36" smd circle
		(at 3.7 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J37" smd circle
		(at 5 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J38" smd circle
		(at 5.9 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J39" smd circle
		(at 6.8 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J40" smd circle
		(at 7.7 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J41" smd circle
		(at 8.6 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J42" smd circle
		(at 9.5 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J43" smd circle
		(at 10.4 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J44" smd circle
		(at 11.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J45" smd circle
		(at 12.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J46" smd circle
		(at 13.1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J47" smd circle
		(at 14 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J48" smd circle
		(at 14.9 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J49" smd circle
		(at 15.8 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J50" smd circle
		(at 16.7 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J51" smd circle
		(at 17.6 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J52" smd circle
		(at 18.5 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J53" smd circle
		(at 19.4 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J54" smd circle
		(at 20.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J55" smd circle
		(at 21.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J56" smd circle
		(at 22.1 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J57" smd circle
		(at 23 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J58" smd circle
		(at 23.9 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J59" smd circle
		(at 24.8 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J60" smd circle
		(at 25.7 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J61" smd circle
		(at 26.6 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J62" smd circle
		(at 27.5 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J63" smd circle
		(at 28.4 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J64" smd circle
		(at 29.3 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J65" smd circle
		(at 30.2 4.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -28.2 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -27.3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at -26.4 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K6" smd circle
		(at -25.5 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K7" smd circle
		(at -24.6 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at -23.7 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at -22.8 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K10" smd circle
		(at -21.9 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at -21 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K12" smd circle
		(at -20.1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K13" smd circle
		(at -19.2 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K14" smd circle
		(at -18.3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K15" smd circle
		(at -17 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K16" smd circle
		(at -16.1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K17" smd circle
		(at -15.2 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K18" smd circle
		(at -14.3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K19" smd circle
		(at -13 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K20" smd circle
		(at -12.1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K21" smd circle
		(at -11.2 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K22" smd circle
		(at -10.3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K23" smd circle
		(at -9 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K24" smd circle
		(at -8.1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K25" smd circle
		(at -7.2 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K26" smd circle
		(at -6.3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K27" smd circle
		(at -5 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K28" smd circle
		(at -4.1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K29" smd circle
		(at -3.2 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K30" smd circle
		(at -2.3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K31" smd circle
		(at -1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K32" smd circle
		(at -0.1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K33" smd circle
		(at 0.8 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K34" smd circle
		(at 1.7 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K35" smd circle
		(at 3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K36" smd circle
		(at 3.9 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K37" smd circle
		(at 4.8 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K38" smd circle
		(at 5.7 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K39" smd circle
		(at 7 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K40" smd circle
		(at 7.9 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K41" smd circle
		(at 8.8 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K42" smd circle
		(at 9.7 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K43" smd circle
		(at 10.6 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K44" smd circle
		(at 11.5 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K45" smd circle
		(at 12.4 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K46" smd circle
		(at 13.3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K47" smd circle
		(at 14.2 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K48" smd circle
		(at 15.1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K49" smd circle
		(at 16 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K50" smd circle
		(at 16.9 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K51" smd circle
		(at 17.8 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K52" smd circle
		(at 18.7 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K53" smd circle
		(at 19.6 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K54" smd circle
		(at 20.5 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K55" smd circle
		(at 21.4 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K56" smd circle
		(at 22.3 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K57" smd circle
		(at 23.2 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K58" smd circle
		(at 24.1 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K59" smd circle
		(at 25 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K60" smd circle
		(at 25.9 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K61" smd circle
		(at 26.8 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K62" smd circle
		(at 27.7 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K63" smd circle
		(at 28.6 6 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -28.4 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -27.5 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L5" smd circle
		(at -26.6 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L6" smd circle
		(at -25.7 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L7" smd circle
		(at -24.8 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at -23.9 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at -23 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L10" smd circle
		(at -22.1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L11" smd circle
		(at -21.2 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L12" smd circle
		(at -20.3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L13" smd circle
		(at -19 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L14" smd circle
		(at -18.1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L15" smd circle
		(at -17.2 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L16" smd circle
		(at -16.3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L17" smd circle
		(at -15 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L18" smd circle
		(at -14.1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L19" smd circle
		(at -13.2 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L20" smd circle
		(at -12.3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L21" smd circle
		(at -11 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L22" smd circle
		(at -10.1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L23" smd circle
		(at -9.2 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L24" smd circle
		(at -8.3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L25" smd circle
		(at -7 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L26" smd circle
		(at -6.1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L27" smd circle
		(at -5.2 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L28" smd circle
		(at -4.3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L29" smd circle
		(at -3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L30" smd circle
		(at -2.1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L31" smd circle
		(at -1.2 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L32" smd circle
		(at -0.3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L33" smd circle
		(at 1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L34" smd circle
		(at 1.9 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L35" smd circle
		(at 2.8 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L36" smd circle
		(at 3.7 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L37" smd circle
		(at 5 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L38" smd circle
		(at 5.9 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L39" smd circle
		(at 6.8 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L40" smd circle
		(at 7.7 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L41" smd circle
		(at 8.6 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L42" smd circle
		(at 9.5 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L43" smd circle
		(at 10.4 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L44" smd circle
		(at 11.3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L45" smd circle
		(at 12.2 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L46" smd circle
		(at 13.1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L47" smd circle
		(at 14 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L48" smd circle
		(at 14.9 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L49" smd circle
		(at 15.8 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L50" smd circle
		(at 16.7 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L51" smd circle
		(at 17.6 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L52" smd circle
		(at 18.5 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L53" smd circle
		(at 19.4 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L54" smd circle
		(at 20.3 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L55" smd circle
		(at 21.2 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L56" smd circle
		(at 22.1 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L57" smd circle
		(at 23 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L58" smd circle
		(at 23.9 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L59" smd circle
		(at 24.8 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L60" smd circle
		(at 25.7 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L61" smd circle
		(at 26.6 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L62" smd circle
		(at 27.5 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L63" smd circle
		(at 28.4 7.5 90)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_203456_0003.glb"
		(offset
			(xyz -23.865 46.705 25.215)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 90)
		)
	)
)
