(footprint "Conn_Molex_Pico-Lock_1x2_205338-0002"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "J"
		(at -1.325 -6.81 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Molex_Pico-Lock_1x2_205338-0002"
		(at 5.66 6.19 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.99 8.19 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.99 9.39 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.99 10.59 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1 -2.725 180)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste")
	)
	(pad "2" smd rect
		(at 1 -2.725 180)
		(size 1.1 1.45)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at -3.895 3.25 180)
		(size 1.35 2.9)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 3.895 3.25 180)
		(size 1.35 2.9)
		(layers "F.Cu" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_205338_0002.glb"
		(offset
			(xyz 1 -8.775 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
