(footprint "Conn_Plug_I-PEX_NOVASTACK-35-HDP_2x14+4_20697-028E-01"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.956 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Plug_I-PEX_NOVASTACK-35-HDP_2x14+4_20697-028E-01"
		(at 0 3.156 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.14 5.156 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.14 6.356 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.14 7.556 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.275 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "2" smd rect
		(at -2.275 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "3" smd rect
		(at -1.925 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "4" smd rect
		(at -1.925 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "5" smd rect
		(at -1.575 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "6" smd rect
		(at -1.575 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "7" smd rect
		(at -1.225 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "8" smd rect
		(at -1.225 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "9" smd rect
		(at -0.875 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "10" smd rect
		(at -0.875 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "11" smd rect
		(at -0.525 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "12" smd rect
		(at -0.525 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "13" smd rect
		(at -0.175 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "14" smd rect
		(at -0.175 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "15" smd rect
		(at 0.175 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "16" smd rect
		(at 0.175 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "17" smd rect
		(at 0.525 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "18" smd rect
		(at 0.525 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "19" smd rect
		(at 0.875 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "20" smd rect
		(at 0.875 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "21" smd rect
		(at 1.225 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "22" smd rect
		(at 1.225 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "23" smd rect
		(at 1.575 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "24" smd rect
		(at 1.575 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "25" smd rect
		(at 1.925 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "26" smd rect
		(at 1.925 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "27" smd rect
		(at 2.275 0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "28" smd rect
		(at 2.275 -0.725)
		(size 0.2 0.45)
		(layers "F.Cu")
	)
	(pad "P1" smd rect
		(at -2.8 0.725)
		(size 0.5 0.45)
		(layers "F.Cu")
	)
	(pad "P2" smd rect
		(at -2.8 -0.725)
		(size 0.5 0.45)
		(layers "F.Cu")
	)
	(pad "P3" smd rect
		(at 2.8 0.725)
		(size 0.5 0.45)
		(layers "F.Cu")
	)
	(pad "P4" smd rect
		(at 2.8 -0.725)
		(size 0.5 0.45)
		(layers "F.Cu")
	)
	(pad "SH" smd rect
		(at -4.62 -1.08)
		(size 0.35 0.6)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at -4.62 1.08)
		(size 0.35 0.6)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at -2.45 -1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at -2.45 1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at -1.75 -1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at -1.75 1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at -0.7 -1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at -0.7 1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 0.7 -1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 0.7 1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 1.75 -1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 1.75 1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 2.45 -1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 2.45 1.75)
		(size 0.22 0.4)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 4.62 -1.08)
		(size 0.35 0.6)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" smd rect
		(at 4.62 1.08)
		(size 0.35 0.6)
		(layers "F.Cu" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_20697_028e_01.glb"
		(offset
			(xyz 0 0 0.655)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 0 0)
		)
	)
)
