(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RJ45_ATTEND_210A-11C0A-RA10"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 39.37 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RJ45_ATTEND_210A-11C0A-RA10"
				(at 39.116 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RJ45_ATTEND_210A-11C0A-RA10"
				(at 39.116 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.attend.com.tw/en/product.php?act=view&id=292"
				(at 39.116 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Jack Modular Connector RJ45, Vertical, Shielded, THT"
				(at 39.116 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "210A-11C0A-RA10"
				(at 39.37 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ATTEND"
				(at 39.116 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 39.116 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.116 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "THT, CONNECTOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RJ45_ATTEND_210A-11C0A-RA10_1_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "4")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "5")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "6")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "7")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "8")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "SH")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
