(footprint "DisplayPort-Mini_Receptacle_TE_2129320-3"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -3.125 -5.334 0)
		(layer "F.SilkS")
	)
	(property "Value" "DisplayPort-Mini_Receptacle_TE_2129320-3"
		(at 0 9.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "PCB_EDGE"
		(at 0 1.8 0)
		(unlocked yes)
		(layer "Dwgs.User")
	)
	(fp_text user "${REFERENCE}"
		(at -5.842 10.55 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.842 11.75 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.842 12.95 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -2.05 -4.151)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.45 -4.151)
		(size 1 1)
		(drill 1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 -3.351)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0.45 -0.804)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0.45 -4.151)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 1.35 -0.804)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 1.35 -4.151)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 1.8 0)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 1.8 -3.351)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 2.249 -0.804)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 2.249 -4.151)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 3.148 -0.804)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 3.148 -4.151)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 3.6 0)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 3.6 -3.351)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 4.049 -0.804)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 4.049 -4.151)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 4.95 -0.804)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 4.95 -4.151)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at 5.4 0)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 5.4 -3.351)
		(size 0.75 0.75)
		(drill 0.55)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -2.802 -0.804)
		(size 1.4 2.85)
		(drill oval 0.9 2.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at -2.5 4.498)
		(size 1.2 2.25)
		(drill oval 0.7 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 7.9 4.498)
		(size 1.2 2.25)
		(drill oval 0.7 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 8.198 -0.804)
		(size 1.4 2.85)
		(drill oval 0.9 2.35)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_2129320_3.glb"
		(offset
			(xyz 2.7 -8.05 1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 -180 180)
		)
	)
)
