(footprint "Conn_Molex_Micro-Lock_1x2_2159310270"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.82 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Molex_Micro-Lock_1x2_2159310270"
		(at -5.05 5.09 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -5.05 6.17 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.05 7.37 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -5.05 8.57 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 0 0)
		(layer "User.5")
	)
	(pad "1" smd rect
		(at 1.25 -2.86)
		(size 1.397 2.3114)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "1" smd rect
		(at 1.25 2.57)
		(size 1.397 2.1082)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.25 -2.86)
		(size 1.397 2.3114)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.25 2.57)
		(size 1.397 2.1082)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at -3.9 -0.07)
		(size 1.4478 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP" smd rect
		(at 3.9 -0.07)
		(size 1.4478 3.048)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_2159310270.glb"
		(offset
			(xyz -0 3.13 12.75)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 -0 -180)
		)
	)
)
