(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bus_M.2_2199230-2"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 45.72 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bus_M.2_2199230-2"
				(at 45.72 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bus_M.2_2199230-2"
				(at 45.72 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/418/9/ENG_DS_1_1773702_1NGFFQRG_EN_0214_1_1773702_1NGFF_-3328593.pdf"
				(at 45.72 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Key E, PCI connector"
				(at 45.72 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "2199230-2"
				(at 45.72 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 45.72 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, SMT, PCIE, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bus_M.2_2199230-2_0_0"
				(text "KEY E"
					(at 15.24 0 0)
				)
			)
			(symbol "Bus_M.2_2199230-2_1_1"
				(pin power_in line
					(at 30.48 -104.14 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 30.48 0 180)
					(length 2.54)
					(name "3.3V")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 2.54)
					(name "USB_D_P")
					(number "3")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "3.3V")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 2.54)
					(name "USB_D_N")
					(number "5")
				)
				(pin output line
					(at 30.48 -85.09 180)
					(length 2.54)
					(name "~{LED_1}")
					(number "6")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "PCM_CLK")
					(number "8")
				)
				(pin input line
					(at 0 -86.36 0)
					(length 2.54)
					(name "SDIO_CLK")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "PCM_SYNC")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 2.54)
					(name "SDIO_CMD")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "PCM_IN")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 2.54)
					(name "SDIO_D0")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "PCM_OUT")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 2.54)
					(name "SDIO_D1")
					(number "15")
				)
				(pin output line
					(at 30.48 -90.17 180)
					(length 2.54)
					(name "~{LED_2}")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 2.54)
					(name "SDIO_D2")
					(number "17")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 2.54)
					(name "SDIO_D3")
					(number "19")
				)
				(pin output line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "~{UART_WAKE}")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 2.54)
					(name "SDIO_~{WAKE}")
					(number "21")
				)
				(pin bidirectional line
					(at 30.48 -48.26 180)
					(length 2.54)
					(name "UART_RXD")
					(number "22")
				)
				(pin input line
					(at 0 -104.14 0)
					(length 2.54)
					(name "SDIO_~{RESET}")
					(number "23")
				)
				(pin bidirectional line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "UART_TXD")
					(number "32")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
				(pin bidirectional line
					(at 30.48 -53.34 180)
					(length 2.54)
					(name "UART_CTS")
					(number "34")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "PET0_P")
					(number "35")
				)
				(pin bidirectional line
					(at 30.48 -50.8 180)
					(length 2.54)
					(name "UART_RTS")
					(number "36")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "PET0_N")
					(number "37")
				)
				(pin bidirectional line
					(at 30.48 -74.93 180)
					(length 2.54)
					(name "VENDOR_1")
					(number "38")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin bidirectional line
					(at 30.48 -77.47 180)
					(length 2.54)
					(name "VENDOR_2")
					(number "40")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PER0_P")
					(number "41")
				)
				(pin bidirectional line
					(at 30.48 -80.01 180)
					(length 2.54)
					(name "VENDOR_3")
					(number "42")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "PER0_N")
					(number "43")
				)
				(pin bidirectional line
					(at 30.48 -68.58 180)
					(length 2.54)
					(name "COEX3")
					(number "44")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "45")
				)
				(pin bidirectional line
					(at 30.48 -66.04 180)
					(length 2.54)
					(name "COEX_TXD")
					(number "46")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "REFCLK0_P")
					(number "47")
				)
				(pin bidirectional line
					(at 30.48 -63.5 180)
					(length 2.54)
					(name "COEX_RXD")
					(number "48")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "REFCLK0_N")
					(number "49")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "SUSCLK")
					(number "50")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "51")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{PERST0}")
					(number "52")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{CLKREQ0}")
					(number "53")
				)
				(pin input line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "W_DISABLE2")
					(number "54")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{PEWAKE0}")
					(number "55")
				)
				(pin input line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "W_DISABLE1")
					(number "56")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "57")
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "I2C_DATA")
					(number "58")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PET1_P")
					(number "59")
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "I2C_CLK")
					(number "60")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PET1_N")
					(number "61")
				)
				(pin output line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "~{ALERT}")
					(number "62")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "63")
				)
				(pin no_connect line
					(at 27.94 -93.98 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "64")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PER1_P")
					(number "65")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "UIM_SWP")
					(number "66")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PER1_N")
					(number "67")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "UIM_POWER_SNK")
					(number "68")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "69")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "UIM_POWER_SRC")
					(number "70")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "REFCLK1_P")
					(number "71")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "3.3V")
					(number "72")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "REFCLK1_N")
					(number "73")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(hide yes)
					(name "3.3V")
					(number "74")
				)
				(pin passive line
					(at 30.48 -104.14 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "75")
				)
				(pin passive line
					(at 30.48 -101.6 180)
					(length 2.54)
					(name "MP")
					(number "MP")
				)
			)
			(embedded_fonts no)
		)
)
