(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Phone_TRS_MiniJack_35RASMT4BHNTRX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Phone_TRS_MiniJack_35RASMT4BHNTRX"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Phone_TRS_MiniJack_35RASMT4BHNTRX"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/393/35rasmt4bhntrx_cd-2942952.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Phone Connectors SMT 3.5MM PHONE JACK, AUDIO Headphone Connector"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Switchcraft"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "35RASMT4BHNTRX"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, JACK, AUDIO, THT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Phone_TRS_MiniJack_35RASMT4BHNTRX_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "SLEEVE")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RING")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "TIP")
					(number "3")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 2.54)
					(name "RING_SWITCH")
					(number "4")
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 2.54)
					(name "TIP_SWITCH")
					(number "5")
				)
			)
			(embedded_fonts no)
		)
)
