(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Molex_Mini-Fit-Jr_2x5_39-28-1103"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 25.4 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Molex_Mini-Fit-Jr_2x5_39-28-1103"
				(at 25.4 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Molex_Mini-Fit-Jr_2x5_39-28-1103"
				(at 25.4 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.molex.com/pdm_docs/sd/039281103_sd.pdf"
				(at 25.4 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pin Header, THT, Vertical, UL94V-2, Power, Wire-to-Board, 4.2 mm, 2 Rows, 10 Contacts, Mini-fit Jr, 5566 series"
				(at 25.4 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "39-28-1103"
				(at 25.4 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Molex"
				(at 25.4 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 25.4 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 25.4 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "VERTICAL, THT, HEADER, CONNECTOR, MALE, WIRE-BOARD, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Molex_Mini-Fit-Jr_2x5_39-28-1103_1_1"
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "4")
					(number "4")
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "5")
					(number "5")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "6")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "7")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "8")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "9")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "10")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
