(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Plug_Bus_CE7_EPT_401-51501-51"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Plug_Bus_CE7_EPT_401-51501-51"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Plug_Bus_CE7_EPT_401-51501-51"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.farnell.com/datasheets/1905093.pdf"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Mezzanine Connector, 5mm Height, COM Express, Header, 0.5 mm, 2 Rows, 440 Contacts, Surface Mount"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "ept"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "401-51501-51"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "CONNECTOR, B2B, PLUG, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_1_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "NCSI"
					(at -31.75 -24.13 0)
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "NCSI_TX_EN")
					(number "A84")
				)
				(pin input line
					(at 0 -17.78 180)
					(length 5.08)
					(name "NCSI_RX_ER")
					(number "B89")
				)
				(pin input line
					(at 0 -20.32 180)
					(length 5.08)
					(name "NCSI_CLK_IN")
					(number "B91")
				)
				(pin input line
					(at 0 -5.08 180)
					(length 5.08)
					(name "NCSI_RXD1")
					(number "B92")
				)
				(pin input line
					(at 0 -2.54 180)
					(length 5.08)
					(name "NCSI_RXD0")
					(number "B93")
				)
				(pin output line
					(at 0 -22.86 180)
					(length 5.08)
					(name "NCSI_CRS_DV")
					(number "B94")
				)
				(pin output line
					(at 0 -10.16 180)
					(length 5.08)
					(name "NCSI_TXD1")
					(number "B95")
				)
				(pin output line
					(at 0 -7.62 180)
					(length 5.08)
					(name "NCSI_TXD0")
					(number "B96")
				)
				(pin input line
					(at 0 -12.7 180)
					(length 5.08)
					(name "NCSI_ARB_IN")
					(number "B98")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "NCSI_ARB_OUT")
					(number "B99")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_2_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "GBE0"
					(at -31.75 -49.53 0)
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "GBE0_MDI3-")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "GBE0_MDI3+")
					(number "A3")
				)
				(pin output line
					(at 0 -38.1 180)
					(length 5.08)
					(name "~{GBE0_LINK100}")
					(number "A4")
				)
				(pin output line
					(at 0 -35.56 180)
					(length 5.08)
					(name "~{GBE0_LINK1000}")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GBE0_MDI2-")
					(number "A6")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GBE0_MDI2+")
					(number "A7")
				)
				(pin output line
					(at 0 -40.64 180)
					(length 5.08)
					(name "~{GBE0_LINK}")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "GBE0_MDI1-")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -20.32 180)
					(length 5.08)
					(name "GBE0_MDI1+")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "GBE0_MDI0-")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -27.94 180)
					(length 5.08)
					(name "GBE0_MDI0+")
					(number "A13")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "GBE0_CTREF")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -48.26 180)
					(length 5.08)
					(name "GBE0_SDP")
					(number "A49")
				)
				(pin output line
					(at 0 -43.18 180)
					(length 5.08)
					(name "~{GBE0_ACT}")
					(number "B2")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_3_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "LS"
					(at -31.75 -34.29 0)
				)
				(pin power_out line
					(at 0 0 180)
					(length 5.08)
					(name "SPI_POWER")
					(number "A91")
				)
				(pin input line
					(at 0 -2.54 180)
					(length 5.08)
					(name "SPI_MISO")
					(number "A92")
				)
				(pin output line
					(at 0 -5.08 180)
					(length 5.08)
					(name "SPI_CLK")
					(number "A94")
				)
				(pin output line
					(at 0 -7.62 180)
					(length 5.08)
					(name "SPI_MOSI")
					(number "A95")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "SER0_TX")
					(number "A98")
				)
				(pin input line
					(at 0 -17.78 180)
					(length 5.08)
					(name "SER0_RX")
					(number "A99")
				)
				(pin output line
					(at 0 -22.86 180)
					(length 5.08)
					(name "SER1_TX")
					(number "A101")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "SER1_RX")
					(number "A102")
				)
				(pin open_collector line
					(at 0 -30.48 180)
					(length 5.08)
					(name "I2C_CK")
					(number "B33")
				)
				(pin open_collector line
					(at 0 -33.02 180)
					(length 5.08)
					(name "I2C_DAT")
					(number "B34")
				)
				(pin output line
					(at 0 -10.16 180)
					(length 5.08)
					(name "~{SPI_CS}")
					(number "B97")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_4_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "MGMT"
					(at -31.75 -90.17 0)
				)
				(pin output line
					(at 0 -60.96 180)
					(length 5.08)
					(name "~{SUS_S3}")
					(number "A15")
				)
				(pin output line
					(at 0 -63.5 180)
					(length 5.08)
					(name "~{SUS_S4}")
					(number "A18")
				)
				(pin output line
					(at 0 -66.04 180)
					(length 5.08)
					(name "~{SUS_S5}")
					(number "A24")
				)
				(pin input line
					(at 0 -73.66 180)
					(length 5.08)
					(name "~{BATLOW}")
					(number "A27")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "~{BIOS_DIS0}/ESPI_SAFS")
					(number "A34")
				)
				(pin output line
					(at 0 -58.42 180)
					(length 5.08)
					(name "~{THRMTRIP}")
					(number "A35")
				)
				(pin bidirectional line
					(at 0 -12.7 180)
					(length 5.08)
					(name "LPC_SERIRQ/~{ESPI_CS1}")
					(number "A50")
				)
				(pin input line
					(at 0 -78.74 180)
					(length 5.08)
					(name "TPM_PP")
					(number "A96")
				)
				(pin passive line
					(at 0 -76.2 180)
					(length 5.08)
					(name "~{TYPE10}")
					(number "A97")
				)
				(pin input line
					(at 0 -43.18 180)
					(length 5.08)
					(name "~{LID}")
					(number "A103")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "~{LPC_FRAME}/~{ESPI_CS0}")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "LPC_AD0/ESPI_IO_0")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 5.08)
					(name "LPC_AD1/ESPI_IO_1")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "LPC_AD2/ESPI_IO_2")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "LPC_AD3/ESPI_IO_3")
					(number "B7")
				)
				(pin input line
					(at 0 -17.78 180)
					(length 5.08)
					(name "~{LPC_DRQ0}/~{ESPI_ALERT0}")
					(number "B8")
				)
				(pin input line
					(at 0 -20.32 180)
					(length 5.08)
					(name "~{LPC_DRQ1}/~{ESPI_ALERT1}")
					(number "B9")
				)
				(pin output line
					(at 0 -10.16 180)
					(length 5.08)
					(name "LPC_CLK/ESPI_CK")
					(number "B10")
				)
				(pin input line
					(at 0 -40.64 180)
					(length 5.08)
					(name "~{PWRBTN}")
					(number "B12")
				)
				(pin open_collector line
					(at 0 -50.8 180)
					(length 5.08)
					(name "SMB_CK")
					(number "B13")
				)
				(pin open_collector line
					(at 0 -53.34 180)
					(length 5.08)
					(name "SMB_DAT")
					(number "B14")
				)
				(pin input line
					(at 0 -48.26 180)
					(length 5.08)
					(name "~{SMB_ALERT}")
					(number "B15")
				)
				(pin output line
					(at 0 -22.86 180)
					(length 5.08)
					(name "~{SUS_STAT}/~{ESPI_RESET}")
					(number "B18")
				)
				(pin input line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PWR_OK")
					(number "B24")
				)
				(pin output line
					(at 0 -81.28 180)
					(length 5.08)
					(name "WDT")
					(number "B27")
				)
				(pin output line
					(at 0 -83.82 180)
					(length 5.08)
					(name "SPKR")
					(number "B32")
				)
				(pin input line
					(at 0 -55.88 180)
					(length 5.08)
					(name "~{THRM}")
					(number "B35")
				)
				(pin input line
					(at 0 -30.48 180)
					(length 5.08)
					(name "~{ESPI_EN}")
					(number "B47")
				)
				(pin input line
					(at 0 -35.56 180)
					(length 5.08)
					(name "~{SYS_RESET}")
					(number "B49")
				)
				(pin output line
					(at 0 -33.02 180)
					(length 5.08)
					(name "~{CB_RESET}")
					(number "B50")
				)
				(pin input line
					(at 0 -68.58 180)
					(length 5.08)
					(name "~{WAKE0}")
					(number "B66")
				)
				(pin input line
					(at 0 -71.12 180)
					(length 5.08)
					(name "~{WAKE1}")
					(number "B67")
				)
				(pin input line
					(at 0 -27.94 180)
					(length 5.08)
					(name "~{BIOS_DIS1}")
					(number "B88")
				)
				(pin output line
					(at 0 -86.36 180)
					(length 5.08)
					(name "FAN_PWMOUT")
					(number "B101")
				)
				(pin input line
					(at 0 -88.9 180)
					(length 5.08)
					(name "FAN_TACHIN")
					(number "B102")
				)
				(pin input line
					(at 0 -45.72 180)
					(length 5.08)
					(name "~{SLEEP}")
					(number "B103")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_5_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "GPIO"
					(at -31.75 -19.05 0)
				)
				(pin input line
					(at 0 -10.16 180)
					(length 5.08)
					(name "GPI0")
					(number "A54")
				)
				(pin input line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GPI1")
					(number "A63")
				)
				(pin input line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GPI2")
					(number "A67")
				)
				(pin input line
					(at 0 -17.78 180)
					(length 5.08)
					(name "GPI3")
					(number "A85")
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "GPO0")
					(number "A93")
				)
				(pin output line
					(at 0 -2.54 180)
					(length 5.08)
					(name "GPO1")
					(number "B54")
				)
				(pin output line
					(at 0 -5.08 180)
					(length 5.08)
					(name "GPO2")
					(number "B57")
				)
				(pin output line
					(at 0 -7.62 180)
					(length 5.08)
					(name "GPO3")
					(number "B63")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_6_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "SATA"
					(at -31.75 -31.75 0)
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "SATA0_TX+")
					(number "A16")
				)
				(pin output line
					(at 0 -2.54 180)
					(length 5.08)
					(name "SATA0_TX-")
					(number "A17")
				)
				(pin input line
					(at 0 -7.62 180)
					(length 5.08)
					(name "SATA0_RX+")
					(number "A19")
				)
				(pin input line
					(at 0 -10.16 180)
					(length 5.08)
					(name "SATA0_RX-")
					(number "A20")
				)
				(pin bidirectional line
					(at 0 -30.48 180)
					(length 5.08)
					(name "~{(S)ATA_ACT}")
					(number "A28")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "SATA1_TX+")
					(number "B16")
				)
				(pin output line
					(at 0 -17.78 180)
					(length 5.08)
					(name "SATA1_TX-")
					(number "B17")
				)
				(pin input line
					(at 0 -22.86 180)
					(length 5.08)
					(name "SATA1_RX+")
					(number "B19")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "SATA1_RX-")
					(number "B20")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_7_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "USB"
					(at -31.75 -36.83 0)
				)
				(pin bidirectional line
					(at 0 -10.16 180)
					(length 5.08)
					(name "USB2-")
					(number "A42")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 5.08)
					(name "USB2+")
					(number "A43")
				)
				(pin input line
					(at 0 -35.56 180)
					(length 5.08)
					(name "~{USB_2_3_OC}")
					(number "A44")
				)
				(pin bidirectional line
					(at 0 -25.4 180)
					(length 5.08)
					(name "USB0-")
					(number "A45")
				)
				(pin bidirectional line
					(at 0 -22.86 180)
					(length 5.08)
					(name "USB0+")
					(number "A46")
				)
				(pin bidirectional line
					(at 0 -2.54 180)
					(length 5.08)
					(name "USB3-")
					(number "B42")
				)
				(pin bidirectional line
					(at 0 0 180)
					(length 5.08)
					(name "USB3+")
					(number "B43")
				)
				(pin input line
					(at 0 -33.02 180)
					(length 5.08)
					(name "~{USB_0_1_OC}")
					(number "B44")
				)
				(pin bidirectional line
					(at 0 -17.78 180)
					(length 5.08)
					(name "USB1-")
					(number "B45")
				)
				(pin bidirectional line
					(at 0 -15.24 180)
					(length 5.08)
					(name "USB1+")
					(number "B46")
				)
				(pin input line
					(at 0 -30.48 180)
					(length 5.08)
					(name "USB0_HOST_PRSNT")
					(number "B48")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_8_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "POWER"
					(at -31.75 -16.51 0)
				)
				(pin power_in line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A1")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A11")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A21")
				)
				(pin no_connect line
					(at -33.02 -2.54 0)
					(length 5.08)
					(name "RSVD")
					(number "A29")
				)
				(pin no_connect line
					(at -33.02 -3.81 0)
					(length 5.08)
					(name "RSVD")
					(number "A30")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A31")
				)
				(pin no_connect line
					(at -33.02 -5.08 0)
					(length 5.08)
					(name "RSVD")
					(number "A32")
				)
				(pin no_connect line
					(at -33.02 -6.35 0)
					(length 5.08)
					(name "RSVD")
					(number "A33")
				)
				(pin power_in line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "A38")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A41")
				)
				(pin power_in line
					(at 0 -2.54 180)
					(length 5.08)
					(name "VCC_RTC")
					(number "A47")
				)
				(pin no_connect line
					(at -33.02 -7.62 0)
					(length 5.08)
					(name "RSVD")
					(number "A48")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A51")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "A57")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A60")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "A66")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A70")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "A73")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "A76")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "A79")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A80")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "A83")
				)
				(pin no_connect line
					(at -33.02 -8.89 0)
					(length 5.08)
					(name "RSVD")
					(number "A86")
				)
				(pin no_connect line
					(at -33.02 -10.16 0)
					(length 5.08)
					(name "RSVD")
					(number "A87")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A90")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A100")
				)
				(pin power_in line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "A104")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "A105")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "A106")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "A107")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "A108")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "A109")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "A110")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B1")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B11")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B21")
				)
				(pin no_connect line
					(at -33.02 -11.43 0)
					(length 5.08)
					(name "RSVD")
					(number "B28")
				)
				(pin no_connect line
					(at -33.02 -12.7 0)
					(length 5.08)
					(name "RSVD")
					(number "B29")
				)
				(pin no_connect line
					(at -33.02 -13.97 0)
					(length 5.08)
					(name "RSVD")
					(number "B30")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B31")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "B38")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B41")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B51")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B60")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B70")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "B73")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "B76")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "B79")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B80")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "B83")
				)
				(pin power_in line
					(at 0 -5.08 180)
					(length 5.08)
					(name "VCC_5V_SBY")
					(number "B84")
				)
				(pin passive line
					(at 0 -5.08 180)
					(length 5.08)
					(name "VCC_5V_SBY")
					(number "B85")
				)
				(pin passive line
					(at 0 -5.08 180)
					(length 5.08)
					(name "VCC_5V_SBY")
					(number "B86")
				)
				(pin passive line
					(at 0 -5.08 180)
					(length 5.08)
					(name "VCC_5V_SBY")
					(number "B87")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B90")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B100")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "B104")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "B105")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "B106")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "B107")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "B108")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "B109")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "B110")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_9_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "PCIe"
					(at -31.75 -118.11 0)
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "PCIE_TX15+")
					(number "A22")
				)
				(pin output line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PCIE_TX15-")
					(number "A23")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PCIE_TX14+")
					(number "A25")
				)
				(pin output line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PCIE_TX14-")
					(number "A26")
				)
				(pin output line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PCIE_TX13+")
					(number "A36")
				)
				(pin output line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PCIE_TX13-")
					(number "A37")
				)
				(pin output line
					(at 0 -45.72 180)
					(length 5.08)
					(name "PCIE_TX12+")
					(number "A39")
				)
				(pin output line
					(at 0 -48.26 180)
					(length 5.08)
					(name "PCIE_TX12-")
					(number "A40")
				)
				(pin output line
					(at 0 -106.68 180)
					(length 5.08)
					(name "PCIE_TX8+")
					(number "A71")
				)
				(pin output line
					(at 0 -109.22 180)
					(length 5.08)
					(name "PCIE_TX8-")
					(number "A72")
				)
				(pin output line
					(at 0 -91.44 180)
					(length 5.08)
					(name "PCIE_TX9+")
					(number "A74")
				)
				(pin output line
					(at 0 -93.98 180)
					(length 5.08)
					(name "PCIE_TX9-")
					(number "A75")
				)
				(pin output line
					(at 0 -76.2 180)
					(length 5.08)
					(name "PCIE_TX10+")
					(number "A77")
				)
				(pin output line
					(at 0 -78.74 180)
					(length 5.08)
					(name "PCIE_TX10-")
					(number "A78")
				)
				(pin output line
					(at 0 -60.96 180)
					(length 5.08)
					(name "PCIE_TX11+")
					(number "A81")
				)
				(pin output line
					(at 0 -63.5 180)
					(length 5.08)
					(name "PCIE_TX11-")
					(number "A82")
				)
				(pin input line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PCIE_RX15+")
					(number "B22")
				)
				(pin input line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PCIE_RX15-")
					(number "B23")
				)
				(pin input line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PCIE_RX14+")
					(number "B25")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PCIE_RX14-")
					(number "B26")
				)
				(pin input line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PCIE_RX13+")
					(number "B36")
				)
				(pin input line
					(at 0 -40.64 180)
					(length 5.08)
					(name "PCIE_RX13-")
					(number "B37")
				)
				(pin input line
					(at 0 -53.34 180)
					(length 5.08)
					(name "PCIE_RX12+")
					(number "B39")
				)
				(pin input line
					(at 0 -55.88 180)
					(length 5.08)
					(name "PCIE_RX12-")
					(number "B40")
				)
				(pin input line
					(at 0 -114.3 180)
					(length 5.08)
					(name "PCIE_RX8+")
					(number "B71")
				)
				(pin input line
					(at 0 -116.84 180)
					(length 5.08)
					(name "PCIE_RX8-")
					(number "B72")
				)
				(pin input line
					(at 0 -99.06 180)
					(length 5.08)
					(name "PCIE_RX9+")
					(number "B74")
				)
				(pin input line
					(at 0 -101.6 180)
					(length 5.08)
					(name "PCIE_RX9-")
					(number "B75")
				)
				(pin input line
					(at 0 -83.82 180)
					(length 5.08)
					(name "PCIE_RX10+")
					(number "B77")
				)
				(pin input line
					(at 0 -86.36 180)
					(length 5.08)
					(name "PCIE_RX10-")
					(number "B78")
				)
				(pin input line
					(at 0 -68.58 180)
					(length 5.08)
					(name "PCIE_RX11+")
					(number "B81")
				)
				(pin input line
					(at 0 -71.12 180)
					(length 5.08)
					(name "PCIE_RX11-")
					(number "B82")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_10_1"
				(text "C/D"
					(at -31.75 0 0)
				)
				(text "USBSS"
					(at -31.75 -57.15 0)
				)
				(pin input line
					(at 0 -55.88 180)
					(length 5.08)
					(name "USB_SSRX0-")
					(number "C3")
				)
				(pin input line
					(at 0 -53.34 180)
					(length 5.08)
					(name "USB_SSRX0+")
					(number "C4")
				)
				(pin input line
					(at 0 -40.64 180)
					(length 5.08)
					(name "USB_SSRX1-")
					(number "C6")
				)
				(pin input line
					(at 0 -38.1 180)
					(length 5.08)
					(name "USB_SSRX1+")
					(number "C7")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "USB_SSRX2-")
					(number "C9")
				)
				(pin input line
					(at 0 -22.86 180)
					(length 5.08)
					(name "USB_SSRX2+")
					(number "C10")
				)
				(pin input line
					(at 0 -10.16 180)
					(length 5.08)
					(name "USB_SSRX3-")
					(number "C12")
				)
				(pin input line
					(at 0 -7.62 180)
					(length 5.08)
					(name "USB_SSRX3+")
					(number "C13")
				)
				(pin output line
					(at 0 -48.26 180)
					(length 5.08)
					(name "USB_SSTX0-")
					(number "D3")
				)
				(pin output line
					(at 0 -45.72 180)
					(length 5.08)
					(name "USB_SSTX0+")
					(number "D4")
				)
				(pin output line
					(at 0 -33.02 180)
					(length 5.08)
					(name "USB_SSTX1-")
					(number "D6")
				)
				(pin output line
					(at 0 -30.48 180)
					(length 5.08)
					(name "USB_SSTX1+")
					(number "D7")
				)
				(pin output line
					(at 0 -17.78 180)
					(length 5.08)
					(name "USB_SSTX2-")
					(number "D9")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "USB_SSTX2+")
					(number "D10")
				)
				(pin output line
					(at 0 -2.54 180)
					(length 5.08)
					(name "USB_SSTX3-")
					(number "D12")
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "USB_SSTX3+")
					(number "D13")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_11_1"
				(text "C/D"
					(at -31.75 0 0)
				)
				(text "10GBaseKR"
					(at -31.75 -153.67 0)
				)
				(pin open_collector line
					(at 0 -129.54 180)
					(length 5.08)
					(name "10G_PHY_MDC_SCL3")
					(number "C15")
				)
				(pin open_collector line
					(at 0 -114.3 180)
					(length 5.08)
					(name "10G_PHY_MDC_SCL2")
					(number "C16")
				)
				(pin bidirectional line
					(at 0 -142.24 180)
					(length 5.08)
					(name "10G_SDP2")
					(number "C17")
				)
				(pin input line
					(at 0 -116.84 180)
					(length 5.08)
					(name "10G_INT2")
					(number "C24")
				)
				(pin input line
					(at 0 -7.62 180)
					(length 5.08)
					(name "10G_KR_RX3+")
					(number "C26")
				)
				(pin input line
					(at 0 -10.16 180)
					(length 5.08)
					(name "10G_KR_RX3-")
					(number "C27")
				)
				(pin input line
					(at 0 -22.86 180)
					(length 5.08)
					(name "10G_KR_RX2+")
					(number "C29")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "10G_KR_RX2-")
					(number "C30")
				)
				(pin open_collector line
					(at 0 -121.92 180)
					(length 5.08)
					(name "10G_SFP_SDA3")
					(number "C32")
				)
				(pin open_collector line
					(at 0 -106.68 180)
					(length 5.08)
					(name "10G_SFP_SDA2")
					(number "C33")
				)
				(pin output line
					(at 0 -99.06 180)
					(length 5.08)
					(name "10G_PHY_RST_23")
					(number "C34")
				)
				(pin output line
					(at 0 -60.96 180)
					(length 5.08)
					(name "10G_PHY_RST_01")
					(number "C35")
				)
				(pin open_collector line
					(at 0 -149.86 180)
					(length 5.08)
					(name "10G_LED_SDA")
					(number "C36")
				)
				(pin open_collector line
					(at 0 -152.4 180)
					(length 5.08)
					(name "10G_LED_SCL")
					(number "C37")
				)
				(pin open_collector line
					(at 0 -83.82 180)
					(length 5.08)
					(name "10G_SFP_SDA1")
					(number "C38")
				)
				(pin open_collector line
					(at 0 -68.58 180)
					(length 5.08)
					(name "10G_SFP_SDA0")
					(number "C39")
				)
				(pin bidirectional line
					(at 0 -137.16 180)
					(length 5.08)
					(name "10G_SDP0")
					(number "C40")
				)
				(pin input line
					(at 0 -38.1 180)
					(length 5.08)
					(name "10G_KR_RX1+")
					(number "C42")
				)
				(pin input line
					(at 0 -40.64 180)
					(length 5.08)
					(name "10G_KR_RX1-")
					(number "C43")
				)
				(pin open_collector line
					(at 0 -91.44 180)
					(length 5.08)
					(name "10G_PHY_MDC_SCL1")
					(number "C45")
				)
				(pin open_collector line
					(at 0 -76.2 180)
					(length 5.08)
					(name "10G_PHY_MDC_SCL0")
					(number "C46")
				)
				(pin input line
					(at 0 -78.74 180)
					(length 5.08)
					(name "10G_INT0")
					(number "C47")
				)
				(pin input line
					(at 0 -53.34 180)
					(length 5.08)
					(name "10G_KR_RX0+")
					(number "C49")
				)
				(pin input line
					(at 0 -55.88 180)
					(length 5.08)
					(name "10G_KR_RX0-")
					(number "C50")
				)
				(pin open_collector line
					(at 0 -127 180)
					(length 5.08)
					(name "10G_PHY_MDIO_SDA3")
					(number "D15")
				)
				(pin open_collector line
					(at 0 -111.76 180)
					(length 5.08)
					(name "10G_PHY_MDIO_SDA2")
					(number "D16")
				)
				(pin bidirectional line
					(at 0 -144.78 180)
					(length 5.08)
					(name "10G_SDP3")
					(number "D17")
				)
				(pin input line
					(at 0 -132.08 180)
					(length 5.08)
					(name "10G_INT3")
					(number "D24")
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "10G_KR_TX3+")
					(number "D26")
				)
				(pin output line
					(at 0 -2.54 180)
					(length 5.08)
					(name "10G_KR_TX3-")
					(number "D27")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "10G_KR_TX2+")
					(number "D29")
				)
				(pin output line
					(at 0 -17.78 180)
					(length 5.08)
					(name "10G_KR_TX2-")
					(number "D30")
				)
				(pin open_collector line
					(at 0 -124.46 180)
					(length 5.08)
					(name "10G_SFP_SCL3")
					(number "D32")
				)
				(pin open_collector line
					(at 0 -109.22 180)
					(length 5.08)
					(name "10G_SFP_SCL2")
					(number "D33")
				)
				(pin input line
					(at 0 -101.6 180)
					(length 5.08)
					(name "10G_PHY_CAP_23")
					(number "D34")
				)
				(pin input line
					(at 0 -63.5 180)
					(length 5.08)
					(name "10G_PHY_CAP_01")
					(number "D35")
				)
				(pin open_collector line
					(at 0 -86.36 180)
					(length 5.08)
					(name "10G_SFP_SCL1")
					(number "D38")
				)
				(pin open_collector line
					(at 0 -71.12 180)
					(length 5.08)
					(name "10G_SFP_SCL0")
					(number "D39")
				)
				(pin bidirectional line
					(at 0 -139.7 180)
					(length 5.08)
					(name "10G_SDP1")
					(number "D40")
				)
				(pin output line
					(at 0 -30.48 180)
					(length 5.08)
					(name "10G_KR_TX1+")
					(number "D42")
				)
				(pin output line
					(at 0 -33.02 180)
					(length 5.08)
					(name "10G_KR_TX1-")
					(number "D43")
				)
				(pin open_collector line
					(at 0 -88.9 180)
					(length 5.08)
					(name "10G_PHY_MDIO_SDA1")
					(number "D45")
				)
				(pin open_collector line
					(at 0 -73.66 180)
					(length 5.08)
					(name "10G_PHY_MDIO_SDA0")
					(number "D46")
				)
				(pin input line
					(at 0 -93.98 180)
					(length 5.08)
					(name "10G_INT1")
					(number "D47")
				)
				(pin output line
					(at 0 -45.72 180)
					(length 5.08)
					(name "10G_KR_TX0+")
					(number "D49")
				)
				(pin output line
					(at 0 -48.26 180)
					(length 5.08)
					(name "10G_KR_TX0-")
					(number "D50")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_12_1"
				(text "C/D"
					(at -31.75 0 0)
				)
				(text "MGMT"
					(at -31.75 -8.89 0)
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "~{TYPE0}")
					(number "C54")
				)
				(pin passive line
					(at 0 -2.54 180)
					(length 5.08)
					(name "~{TYPE1}")
					(number "C57")
				)
				(pin input line
					(at 0 -7.62 180)
					(length 5.08)
					(name "RAPID_SHUTDOWN")
					(number "C67")
				)
				(pin passive line
					(at 0 -5.08 180)
					(length 5.08)
					(name "~{TYPE2}")
					(number "D57")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_13_1"
				(text "C/D"
					(at -31.75 0 0)
				)
				(text "POWER"
					(at -31.75 -16.51 0)
				)
				(pin power_in line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C1")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C2")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C8")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C11")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C14")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C18")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C21")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C25")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C28")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C31")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C41")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C44")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C48")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C51")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C60")
				)
				(pin no_connect line
					(at -33.02 -2.54 0)
					(length 5.08)
					(name "RSVD")
					(number "C63")
				)
				(pin no_connect line
					(at -33.02 -3.81 0)
					(length 5.08)
					(name "RSVD")
					(number "C64")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C70")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C73")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C76")
				)
				(pin no_connect line
					(at -33.02 -5.08 0)
					(length 5.08)
					(name "RSVD")
					(number "C77")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C80")
				)
				(pin no_connect line
					(at -33.02 -6.35 0)
					(length 5.08)
					(name "RSVD")
					(number "C83")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C84")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C87")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C90")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C93")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C96")
				)
				(pin no_connect line
					(at -33.02 -7.62 0)
					(length 5.08)
					(name "RSVD")
					(number "C97")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C100")
				)
				(pin power_in line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "C103")
				)
				(pin power_in line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "C104")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "C105")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "C106")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "C107")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "C108")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "C109")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "C110")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D1")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D2")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D5")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D8")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D11")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D14")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D18")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D21")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D25")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D28")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D31")
				)
				(pin no_connect line
					(at -33.02 -13.97 0)
					(length 5.08)
					(name "RSVD")
					(number "D36")
				)
				(pin no_connect line
					(at -33.02 -12.7 0)
					(length 5.08)
					(name "RSVD")
					(number "D37")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D41")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D44")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D48")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D51")
				)
				(pin no_connect line
					(at -33.02 -8.89 0)
					(length 5.08)
					(name "RSVD")
					(number "D54")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D60")
				)
				(pin no_connect line
					(at -33.02 -11.43 0)
					(length 5.08)
					(name "RSVD")
					(number "D63")
				)
				(pin no_connect line
					(at -33.02 -10.16 0)
					(length 5.08)
					(name "RSVD")
					(number "D64")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D67")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D70")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D73")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D76")
				)
				(pin no_connect line
					(at -33.02 0 0)
					(length 5.08)
					(name "RSVD")
					(number "D77")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D80")
				)
				(pin no_connect line
					(at -33.02 -15.24 0)
					(length 5.08)
					(name "RSVD")
					(number "D83")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D84")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D87")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D90")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D93")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D96")
				)
				(pin no_connect line
					(at -33.02 -1.27 0)
					(length 5.08)
					(name "RSVD")
					(number "D97")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D100")
				)
				(pin passive line
					(at 0 -15.24 180)
					(length 5.08)
					(name "GND")
					(number "D103")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "D104")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "D105")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "D106")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "D107")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "D108")
				)
				(pin passive line
					(at 0 0 180)
					(length 5.08)
					(name "VCC_12V")
					(number "D109")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 5.08)
					(name "GND(FIXED)")
					(number "D110")
				)
				(pin passive line
					(at 0 -10.16 180)
					(length 5.08)
					(name "MP")
					(number "MP")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_14_1"
				(text "C/D"
					(at -31.75 0 0)
				)
				(text "PCIe"
					(at -31.75 -240.03 0)
				)
				(pin input line
					(at 0 -236.22 180)
					(length 5.08)
					(name "PCIE_RX16+")
					(number "C52")
				)
				(pin input line
					(at 0 -238.76 180)
					(length 5.08)
					(name "PCIE_RX16-")
					(number "C53")
				)
				(pin input line
					(at 0 -220.98 180)
					(length 5.08)
					(name "PCIE_RX17+")
					(number "C55")
				)
				(pin input line
					(at 0 -223.52 180)
					(length 5.08)
					(name "PCIE_RX17-")
					(number "C56")
				)
				(pin input line
					(at 0 -205.74 180)
					(length 5.08)
					(name "PCIE_RX18+")
					(number "C58")
				)
				(pin input line
					(at 0 -208.28 180)
					(length 5.08)
					(name "PCIE_RX18-")
					(number "C59")
				)
				(pin input line
					(at 0 -190.5 180)
					(length 5.08)
					(name "PCIE_RX19+")
					(number "C61")
				)
				(pin input line
					(at 0 -193.04 180)
					(length 5.08)
					(name "PCIE_RX19-")
					(number "C62")
				)
				(pin input line
					(at 0 -175.26 180)
					(length 5.08)
					(name "PCIE_RX20+")
					(number "C65")
				)
				(pin input line
					(at 0 -177.8 180)
					(length 5.08)
					(name "PCIE_RX20-")
					(number "C66")
				)
				(pin input line
					(at 0 -160.02 180)
					(length 5.08)
					(name "PCIE_RX21+")
					(number "C68")
				)
				(pin input line
					(at 0 -162.56 180)
					(length 5.08)
					(name "PCIE_RX21-")
					(number "C69")
				)
				(pin input line
					(at 0 -144.78 180)
					(length 5.08)
					(name "PCIE_RX22+")
					(number "C71")
				)
				(pin input line
					(at 0 -147.32 180)
					(length 5.08)
					(name "PCIE_RX22-")
					(number "C72")
				)
				(pin input line
					(at 0 -129.54 180)
					(length 5.08)
					(name "PCIE_RX23+")
					(number "C74")
				)
				(pin input line
					(at 0 -132.08 180)
					(length 5.08)
					(name "PCIE_RX23-")
					(number "C75")
				)
				(pin input line
					(at 0 -114.3 180)
					(length 5.08)
					(name "PCIE_RX24+")
					(number "C78")
				)
				(pin input line
					(at 0 -116.84 180)
					(length 5.08)
					(name "PCIE_RX24-")
					(number "C79")
				)
				(pin input line
					(at 0 -99.06 180)
					(length 5.08)
					(name "PCIE_RX25+")
					(number "C81")
				)
				(pin input line
					(at 0 -101.6 180)
					(length 5.08)
					(name "PCIE_RX25-")
					(number "C82")
				)
				(pin input line
					(at 0 -83.82 180)
					(length 5.08)
					(name "PCIE_RX26+")
					(number "C85")
				)
				(pin input line
					(at 0 -86.36 180)
					(length 5.08)
					(name "PCIE_RX26-")
					(number "C86")
				)
				(pin input line
					(at 0 -68.58 180)
					(length 5.08)
					(name "PCIE_RX27+")
					(number "C88")
				)
				(pin input line
					(at 0 -71.12 180)
					(length 5.08)
					(name "PCIE_RX27-")
					(number "C89")
				)
				(pin input line
					(at 0 -53.34 180)
					(length 5.08)
					(name "PCIE_RX28+")
					(number "C91")
				)
				(pin input line
					(at 0 -55.88 180)
					(length 5.08)
					(name "PCIE_RX28-")
					(number "C92")
				)
				(pin input line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PCIE_RX29+")
					(number "C94")
				)
				(pin input line
					(at 0 -40.64 180)
					(length 5.08)
					(name "PCIE_RX29-")
					(number "C95")
				)
				(pin input line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PCIE_RX30+")
					(number "C98")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PCIE_RX30-")
					(number "C99")
				)
				(pin input line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PCIE_RX31+")
					(number "C101")
				)
				(pin input line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PCIE_RX31-")
					(number "C102")
				)
				(pin output line
					(at 0 -228.6 180)
					(length 5.08)
					(name "PCIE_TX16+")
					(number "D52")
				)
				(pin output line
					(at 0 -231.14 180)
					(length 5.08)
					(name "PCIE_TX16-")
					(number "D53")
				)
				(pin output line
					(at 0 -213.36 180)
					(length 5.08)
					(name "PCIE_TX17+")
					(number "D55")
				)
				(pin output line
					(at 0 -215.9 180)
					(length 5.08)
					(name "PCIE_TX17-")
					(number "D56")
				)
				(pin output line
					(at 0 -198.12 180)
					(length 5.08)
					(name "PCIE_TX18+")
					(number "D58")
				)
				(pin output line
					(at 0 -200.66 180)
					(length 5.08)
					(name "PCIE_TX18-")
					(number "D59")
				)
				(pin output line
					(at 0 -182.88 180)
					(length 5.08)
					(name "PCIE_TX19+")
					(number "D61")
				)
				(pin output line
					(at 0 -185.42 180)
					(length 5.08)
					(name "PCIE_TX19-")
					(number "D62")
				)
				(pin output line
					(at 0 -167.64 180)
					(length 5.08)
					(name "PCIE_TX20+")
					(number "D65")
				)
				(pin output line
					(at 0 -170.18 180)
					(length 5.08)
					(name "PCIE_TX20-")
					(number "D66")
				)
				(pin output line
					(at 0 -152.4 180)
					(length 5.08)
					(name "PCIE_TX21+")
					(number "D68")
				)
				(pin output line
					(at 0 -154.94 180)
					(length 5.08)
					(name "PCIE_TX21-")
					(number "D69")
				)
				(pin output line
					(at 0 -137.16 180)
					(length 5.08)
					(name "PCIE_TX22+")
					(number "D71")
				)
				(pin output line
					(at 0 -139.7 180)
					(length 5.08)
					(name "PCIE_TX22-")
					(number "D72")
				)
				(pin output line
					(at 0 -121.92 180)
					(length 5.08)
					(name "PCIE_TX23+")
					(number "D74")
				)
				(pin output line
					(at 0 -124.46 180)
					(length 5.08)
					(name "PCIE_TX23-")
					(number "D75")
				)
				(pin output line
					(at 0 -106.68 180)
					(length 5.08)
					(name "PCIE_TX24+")
					(number "D78")
				)
				(pin output line
					(at 0 -109.22 180)
					(length 5.08)
					(name "PCIE_TX24-")
					(number "D79")
				)
				(pin output line
					(at 0 -91.44 180)
					(length 5.08)
					(name "PCIE_TX25+")
					(number "D81")
				)
				(pin output line
					(at 0 -93.98 180)
					(length 5.08)
					(name "PCIE_TX25-")
					(number "D82")
				)
				(pin output line
					(at 0 -76.2 180)
					(length 5.08)
					(name "PCIE_TX26+")
					(number "D85")
				)
				(pin output line
					(at 0 -78.74 180)
					(length 5.08)
					(name "PCIE_TX26-")
					(number "D86")
				)
				(pin output line
					(at 0 -60.96 180)
					(length 5.08)
					(name "PCIE_TX27+")
					(number "D88")
				)
				(pin output line
					(at 0 -63.5 180)
					(length 5.08)
					(name "PCIE_TX27-")
					(number "D89")
				)
				(pin output line
					(at 0 -45.72 180)
					(length 5.08)
					(name "PCIE_TX28+")
					(number "D91")
				)
				(pin output line
					(at 0 -48.26 180)
					(length 5.08)
					(name "PCIE_TX28-")
					(number "D92")
				)
				(pin output line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PCIE_TX29+")
					(number "D94")
				)
				(pin output line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PCIE_TX29-")
					(number "D95")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PCIE_TX30+")
					(number "D98")
				)
				(pin output line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PCIE_TX30-")
					(number "D99")
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "PCIE_TX31+")
					(number "D101")
				)
				(pin output line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PCIE_TX31-")
					(number "D102")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_15_1"
				(text "C/D"
					(at -31.75 0 0)
				)
				(text "PCIe"
					(at -31.75 -26.67 0)
				)
				(pin input line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PCIE_RX6+")
					(number "C19")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PCIE_RX6-")
					(number "C20")
				)
				(pin input line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PCIE_RX7+")
					(number "C22")
				)
				(pin input line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PCIE_RX7-")
					(number "C23")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PCIE_TX6+")
					(number "D19")
				)
				(pin output line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PCIE_TX6-")
					(number "D20")
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "PCIE_TX7+")
					(number "D22")
				)
				(pin output line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PCIE_TX7-")
					(number "D23")
				)
			)
			(symbol "Plug_Bus_CE7_EPT_401-51501-51_16_1"
				(text "A/B"
					(at -31.75 0 0)
				)
				(text "PCIe"
					(at -31.75 -95.25 0)
				)
				(pin output line
					(at 0 0 180)
					(length 5.08)
					(name "PCIE_TX5+")
					(number "A52")
				)
				(pin output line
					(at 0 -2.54 180)
					(length 5.08)
					(name "PCIE_TX5-")
					(number "A53")
				)
				(pin output line
					(at 0 -15.24 180)
					(length 5.08)
					(name "PCIE_TX4+")
					(number "A55")
				)
				(pin output line
					(at 0 -17.78 180)
					(length 5.08)
					(name "PCIE_TX4-")
					(number "A56")
				)
				(pin output line
					(at 0 -30.48 180)
					(length 5.08)
					(name "PCIE_TX3+")
					(number "A58")
				)
				(pin output line
					(at 0 -33.02 180)
					(length 5.08)
					(name "PCIE_TX3-")
					(number "A59")
				)
				(pin output line
					(at 0 -45.72 180)
					(length 5.08)
					(name "PCIE_TX2+")
					(number "A61")
				)
				(pin output line
					(at 0 -48.26 180)
					(length 5.08)
					(name "PCIE_TX2-")
					(number "A62")
				)
				(pin output line
					(at 0 -60.96 180)
					(length 5.08)
					(name "PCIE_TX1+")
					(number "A64")
				)
				(pin output line
					(at 0 -63.5 180)
					(length 5.08)
					(name "PCIE_TX1-")
					(number "A65")
				)
				(pin output line
					(at 0 -76.2 180)
					(length 5.08)
					(name "PCIE_TX0+")
					(number "A68")
				)
				(pin output line
					(at 0 -78.74 180)
					(length 5.08)
					(name "PCIE_TX0-")
					(number "A69")
				)
				(pin output line
					(at 0 -91.44 180)
					(length 5.08)
					(name "PCIE_CK_REF+")
					(number "A88")
				)
				(pin output line
					(at 0 -93.98 180)
					(length 5.08)
					(name "PCIE_CK_REF-")
					(number "A89")
				)
				(pin input line
					(at 0 -7.62 180)
					(length 5.08)
					(name "PCIE_RX5+")
					(number "B52")
				)
				(pin input line
					(at 0 -10.16 180)
					(length 5.08)
					(name "PCIE_RX5-")
					(number "B53")
				)
				(pin input line
					(at 0 -22.86 180)
					(length 5.08)
					(name "PCIE_RX4+")
					(number "B55")
				)
				(pin input line
					(at 0 -25.4 180)
					(length 5.08)
					(name "PCIE_RX4-")
					(number "B56")
				)
				(pin input line
					(at 0 -38.1 180)
					(length 5.08)
					(name "PCIE_RX3+")
					(number "B58")
				)
				(pin input line
					(at 0 -40.64 180)
					(length 5.08)
					(name "PCIE_RX3-")
					(number "B59")
				)
				(pin input line
					(at 0 -53.34 180)
					(length 5.08)
					(name "PCIE_RX2+")
					(number "B61")
				)
				(pin input line
					(at 0 -55.88 180)
					(length 5.08)
					(name "PCIE_RX2-")
					(number "B62")
				)
				(pin input line
					(at 0 -68.58 180)
					(length 5.08)
					(name "PCIE_RX1+")
					(number "B64")
				)
				(pin input line
					(at 0 -71.12 180)
					(length 5.08)
					(name "PCIE_RX1-")
					(number "B65")
				)
				(pin input line
					(at 0 -83.82 180)
					(length 5.08)
					(name "PCIE_RX0+")
					(number "B68")
				)
				(pin input line
					(at 0 -86.36 180)
					(length 5.08)
					(name "PCIE_RX0-")
					(number "B69")
				)
			)
			(embedded_fonts no)
		)
)
