(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Molex_Micro-Fit_2x4_430450801"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 29.21 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Molex_Micro-Fit_2x4_430450801"
				(at 29.21 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Molex_Micro-Fit_2x4_430450801"
				(at 29.21 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://tools.molex.com/pdm_docs/sd/430450801_sd.pdf"
				(at 29.21 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Pin Header, Wire-to-Board, 3 mm, 2 Rows, 8 Contacts, Through Hole Right-Angle, Micro-Fit 3.0 43045"
				(at 29.21 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "43045-0801"
				(at 29.21 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Molex"
				(at 29.21 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 29.21 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 29.21 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, THT, WIRE-BOARD, HORIZONTAL, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Molex_Micro-Fit_2x4_430450801_1_1"
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin input line
					(at 11.43 0 180)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin input line
					(at 11.43 -2.54 180)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin input line
					(at 11.43 -5.08 180)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin input line
					(at 11.43 -7.62 180)
					(length 2.54)
					(name "")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
