(footprint "Conn_M12_43-02740"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Connector M12, 8 pins")
	(property "Reference" "REF**"
		(at -8.996 0.648 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_M12_43-02740"
		(at -6.746 -13.102 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -12.36 4.41 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -12.36 5.61 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -12.36 6.81 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -8.995 -6.1)
		(size 2.8 2.8)
		(drill 2.8)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -8.995 -2.1)
		(size 2.05 2.05)
		(drill 2.05)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 6.005 -6.1)
		(size 2.8 2.8)
		(drill 2.8)
		(layers "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 6.005 -2.1)
		(size 2.05 2.05)
		(drill 2.05)
		(layers "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -3 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -4.215 -2.1)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -3.575 -4.2)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -1.495 -4.2)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 0.585 -4.2)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 1.225 -2.1)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at -1.495 -2.1)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -1.495 -6.1)
		(size 1.7 1.7)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_43_02740.glb"
		(offset
			(xyz -1.51 30.59 8.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 45 180)
		)
	)
)
