(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Conn_M12_43-02740"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 19.05 2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Conn_M12_43-02740"
				(at 19.05 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Conn_M12_43-02740"
				(at 19.05 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/81/43-02740_e-1520754.pdf"
				(at 19.05 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "M12 connector, 8 pins, Female"
				(at 19.05 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "43-02740"
				(at 19.05 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 19.05 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 19.05 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 19.05 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "HORIZONTAL, THT, CONNECTOR, FEMALE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Conn_M12_43-02740_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "")
					(number "6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "")
					(number "7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "")
					(number "8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
