(footprint "Conn_Plug_Molex_SlimStack_2x12_5037722410"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.1 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Plug_Molex_SlimStack_2x12_5037722410"
		(at 0 2.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -4.35 4.9 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.35 6.1 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.35 7.3 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.2 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "2" smd rect
		(at -2.2 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "3" smd rect
		(at -1.8 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "4" smd rect
		(at -1.8 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "5" smd rect
		(at -1.4 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "6" smd rect
		(at -1.4 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "7" smd rect
		(at -1 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "8" smd rect
		(at -1 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "9" smd rect
		(at -0.6 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "10" smd rect
		(at -0.6 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "11" smd rect
		(at -0.2 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "12" smd rect
		(at -0.2 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "13" smd rect
		(at 0.2 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "14" smd rect
		(at 0.2 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "15" smd rect
		(at 0.6 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "16" smd rect
		(at 0.6 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "17" smd rect
		(at 1 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "18" smd rect
		(at 1 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "19" smd rect
		(at 1.4 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "20" smd rect
		(at 1.4 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "21" smd rect
		(at 1.8 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "22" smd rect
		(at 1.8 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "23" smd rect
		(at 2.2 1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "24" smd rect
		(at 2.2 -1.175)
		(size 0.24 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.0381)
	)
	(pad "MP" smd rect
		(at -2.95 -1.145)
		(size 0.5 0.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "MP" smd rect
		(at -2.95 1.145)
		(size 0.5 0.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "MP" smd rect
		(at 2.95 -1.145)
		(size 0.5 0.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(pad "MP" smd rect
		(at 2.95 1.145)
		(size 0.5 0.47)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_5037722410.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
