(footprint "Conn_Molex_Pico-Lock_1x2_504050-0291"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -0.749 -3.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Molex_Pico-Lock_1x2_504050-0291"
		(at -0.749 4.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.481 10.175 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.481 11.374 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.481 12.573 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.749 -2.85)
		(size 0.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.75 -2.85)
		(size 0.6 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP1" smd roundrect
		(at -3.354 2.338)
		(size 1.25 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP2" smd roundrect
		(at 3.356 2.338)
		(size 1.25 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_504050_0291.glb"
		(offset
			(xyz 0 -2 1)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 180)
		)
	)
)
