(footprint "Conn_Molex_PicoBlade_1x12_532611271"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Molex PicoBlade series connector, 53261-1271")
	(tags "CONNECTOR, SMT")
	(property "Reference" "REF**"
		(at -5.8 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Molex_PicoBlade_1x12_532611271"
		(at -10.6 4.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -10.88 5.2 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -10.88 6.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -10.88 7.6 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -6.875 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -5.625 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.375 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.125 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.875 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -0.625 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.625 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.875 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 3.125 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 4.375 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 5.625 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 6.875 -2.4)
		(size 0.8 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -9.425 0.5)
		(size 2.1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.119048)
	)
	(pad "MP" smd roundrect
		(at 9.425 0.5)
		(size 2.1 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.119048)
	)
	(embedded_fonts no)
	(model "antmicro_53261_1271.glb"
		(offset
			(xyz 0 -3.6 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
