(footprint "Conn_Plug_Molex_SlimStack_2x20_537480408"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Plug_Molex_SlimStack_2x20_537480408"
		(at 0 3.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -7.4 6 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -7.4 7.2 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -7.2 4.7 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -4.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -4.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -4.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -4.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -2.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -2.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -2.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -1.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -1.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -0.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -0.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -0.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -0.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 0.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 0.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 1.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 1.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 1.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 1.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 2.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 2.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 2.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 2.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 2.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 3.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 3.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 4.25 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 4.25 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 4.75 -1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 4.75 1.7 90)
		(size 1.2 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_537480408.glb"
		(offset
			(xyz 0 0 1.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
