(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RJ12_TE_5555154-1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 34.29 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RJ12_TE_5555154-1"
				(at 34.29 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RJ12_TE_5555154-1"
				(at 34.29 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=5555154&DocType=Customer+Drawing&DocLang=English&PartCntxt=5555154-1&DocFormat=pdf"
				(at 34.29 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Modular Jack, 1 x 1 (Port), 6P6C, Shielded, Through Hole Mount"
				(at 34.29 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "TE Connectivity"
				(at 34.29 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "5555154-1"
				(at 34.29 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 34.29 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, ETHERNET, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RJ12_TE_5555154-1_1_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "")
					(number "6")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "")
					(number "SH1")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "")
					(number "SH2")
				)
			)
			(embedded_fonts no)
		)
)
