(footprint "RJ45_X-2337992-8_Horizontal"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -2.2 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_X-2337992-8_Horizontal"
		(at -2.6 22 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.644 23.4 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.644 24.8 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.644 26.2 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 8.9)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 11.429 8.9)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.269 2.539)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.539 0)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.809 2.539)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 5.078 0)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 6.349 2.539)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 7.618 0)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at 8.89 2.539)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 10.159 0)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 11.429 2.539)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 0 5.078)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 2.539 6.339)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 8.89 6.339)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 11.429 5.07)
		(size 1.397 1.397)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at -0.927 12.958)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole circle
		(at 1.614 12.958)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 9.814 12.958)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole circle
		(at 12.355 12.958)
		(size 1.524 1.524)
		(drill 1.016)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole circle
		(at -2.136 5.85)
		(size 2.1 2.1)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole circle
		(at 13.563 5.85)
		(size 2.1082 2.1082)
		(drill 1.6002)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_5_2337992_8.glb"
		(offset
			(xyz 5.75 -19.75 6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
