(footprint "USB-A_Receptacle_WE_614004184726"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "USB-A (USB TYPE-A) USB 2.0 Receptacle Connector 4 Position Through Hole, Right Angle")
	(property "Reference" "REF**"
		(at 0 -1.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-A_Receptacle_WE_614004184726"
		(at 0 11.5 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.96 12.425 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.96 13.625 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.96 14.825 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.25 1.25)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.4 0)
		(size 1.25 1.25)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 2.798 0)
		(size 1.25 1.25)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.2 0)
		(size 1.25 1.25)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole roundrect
		(at -0.651 2.499)
		(size 1.8 3.3)
		(drill oval 1.2 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "SH" thru_hole roundrect
		(at 2.1 5.599)
		(size 1.5 2)
		(drill oval 1 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "SH" thru_hole roundrect
		(at 4.849 2.499)
		(size 1.8 3.3)
		(drill oval 1.2 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_614004184726.glb"
		(offset
			(xyz 2.1 -0.1 7.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
	(model "antmicro_614004184726.glb"
		(offset
			(xyz 2 -22 7.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 90 90 0)
		)
	)
)
