(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB-A_WE_614004184726"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 15.24 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB-A_WE_614004184726"
				(at 15.24 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB-A_WE_614004184726"
				(at 15.24 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.we-online.com/katalog/datasheet/614004184726.pdf"
				(at 15.24 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB-A (USB TYPE-A) USB 2.0 Receptacle Connector 4 Position Through Hole, Right Angle"
				(at 15.24 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "614004184726"
				(at 15.24 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 15.24 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 15.24 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 15.24 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "USB, CONNECTOR, THT, HORIZONTAL, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB-A_WE_614004184726_1_1"
				(pin passive line
					(at 0 0 180)
					(length 2.54)
					(name "VBUS")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -7.62 180)
					(length 2.54)
					(name "D-")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 180)
					(length 2.54)
					(name "D+")
					(number "3")
				)
				(pin power_in line
					(at 0 -10.16 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin passive line
					(at 0 -12.7 180)
					(length 2.54)
					(name "SH")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
