(footprint "RJ45_Wurth_615008137421"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -9.7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_Wurth_615008137421"
		(at 0 10.3 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -13.446 10.095 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -13.446 11.294 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -13.446 12.493 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -9.92 2.539)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 2.777 2.539 180)
		(size 3.25 3.25)
		(drill 3.25)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -1.02 -1.782)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -2.04 0)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -3.06 -1.782)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -4.08 0)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -5.101 -1.782)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at -6.12 0)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at -7.141 -1.782)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 3.289 -6.601)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole circle
		(at 0.989 -6.601)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at -8.141 -6.601)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at -10.43 -6.601)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -11.696 -0.891)
		(size 2.3 2.3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 4.554 -0.891)
		(size 2.3 2.3)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_615008137421.glb"
		(offset
			(xyz -3.57 -0.04 6.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 180 0 90)
		)
	)
)
