(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RJ45_Wurth_615008137421"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RJ45_Wurth_615008137421"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RJ45_Wurth_615008137421"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.we-online.com/components/products/datasheet/615008141321.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Modular Jack, 1 x 1 (Port), 8P8C, Cat5, Through Hole Mount"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "615008137421"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Würth Elektronik"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RJ45, THT, ETHERNET, HORIZONTAL, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RJ45_Wurth_615008137421_1_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "4")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "5")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "6")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "7")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "8")
					(number "8")
				)
				(pin passive line
					(at 22.86 -2.54 180)
					(length 2.54)
					(name "LED_Y-")
					(number "9")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(name "LED_Y+")
					(number "10")
				)
				(pin passive line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "LED_G-")
					(number "11")
				)
				(pin passive line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "LED_G+")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SH")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
