(footprint "Conn_FFC_Amphenol_1x40_62684-401100AHLF"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_FFC_Amphenol_1x40_62684-401100AHLF"
		(at 0 4.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -13.75 6.313 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -13.75 7.513 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -13.75 8.713 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -9.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "2" smd rect
		(at -9.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "3" smd rect
		(at -8.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "4" smd rect
		(at -8.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "5" smd rect
		(at -7.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "6" smd rect
		(at -7.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "7" smd rect
		(at -6.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "8" smd rect
		(at -6.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "9" smd rect
		(at -5.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "10" smd rect
		(at -5.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "11" smd rect
		(at -4.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "12" smd rect
		(at -4.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "13" smd rect
		(at -3.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "14" smd rect
		(at -3.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "15" smd rect
		(at -2.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "16" smd rect
		(at -2.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "17" smd rect
		(at -1.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "18" smd rect
		(at -1.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "19" smd rect
		(at -0.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "20" smd rect
		(at -0.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "21" smd rect
		(at 0.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "22" smd rect
		(at 0.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "23" smd rect
		(at 1.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "24" smd rect
		(at 1.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "25" smd rect
		(at 2.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "26" smd rect
		(at 2.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "27" smd rect
		(at 3.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "28" smd rect
		(at 3.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "29" smd rect
		(at 4.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "30" smd rect
		(at 4.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "31" smd rect
		(at 5.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "32" smd rect
		(at 5.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "33" smd rect
		(at 6.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "34" smd rect
		(at 6.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "35" smd rect
		(at 7.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "36" smd rect
		(at 7.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "37" smd rect
		(at 8.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "38" smd rect
		(at 8.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "39" smd rect
		(at 9.25 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "40" smd rect
		(at 9.75 -2.55 180)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.09)
	)
	(pad "SH" smd custom
		(at -11.45 0.565)
		(size 1.4 1.4)
		(layers "F.Cu")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.8 -1.6) (xy -0.8 -1.6) (xy -0.8 -0.8) (xy -1.6 -0.8) (xy -1.6 0.8) (xy 0.8 0.8)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(pad "SH" smd custom
		(at 11.45 0.565)
		(size 1.4 1.4)
		(layers "F.Cu")
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.8 -1.6) (xy 0.8 -1.6) (xy 0.8 -0.8) (xy 1.6 -0.8) (xy 1.6 0.8) (xy -0.8 0.8)
				)
				(width 0.01)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_62684_401100ahlf.glb"
		(offset
			(xyz 0 -0.338 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
